{"text_format":"1","workbook":"xlsx","n_sheets":19,"sheets":["Input impactbeoordeing","Input bijkomende maatregelen","Input financiële kengetallen","Input huidige maatreg. (fac.)","Input overige investeringen","Dashboard beslissing","Expressielijsten","Matrix Stof x impact","Info per OWL","Keuzelijst parameters","Toetswaarden spec wl","Criteria volgens stofcategorie","Samenvatting econ kengetallen","KE afleiding NL - Algemene par","MKN - Max","MKN - JG","Toetswaarden STAP 4-7","MKN opgeschoond","BBT+ Criteria"],"not_rendered":{"charts":4,"images":1,"macros":1,"external_links":3,"defined_names":24,"comments":3,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Input impactbeoordeing","index":0,"n_rows":43,"n_cols":58,"rows_kept":43,"cut":false,"hidden":false,"merged":[[34,0,34,3],[33,0,33,3],[35,5,42,11],[17,0,18,0],[17,1,18,1],[17,2,18,2],[17,7,18,7],[17,9,18,9],[17,3,18,3],[17,4,18,4],[17,6,18,6],[11,2,11,3],[10,2,10,3],[17,26,17,27],[17,8,18,8],[17,5,18,5],[17,10,18,10],[17,11,18,11],[17,12,18,12]]}
["Vul de oranje en groene cellen in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ingavelijst",null,null,"Keuzelijst eenheid"]
[]
["Huidig geloosde volume afvalwater ",null,null,"m³/dag",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"selecteer eenheid",null,null,"ng/L"]
["Aantal lozingsdagen",null,null,"dagen/jaar",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"m³/uur",null,null,"µg/L"]
["Aantal uren lozing per dag",null,null,"uur/dag",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"m³/dag",null,null,"mg/L"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"m³/jaar",null,null,"g/L",null,null,null,null,null,null,null,null,null,null,null,null,"Na update stappenplan impactbeoordeling is deze berekening niet langer relevant. Dit wordt dan ook niet langer weergegeven op dit dashboard. "]
["Lozing",null,{"$f":"IFERROR(C8/C5,\"\")","v":""},"m³/uur",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mg O2/L"]
[null,null,{"$f":"IFERROR(C9/C4,\"\")","v":""},"m³/dag",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"µS/cm"]
[null,null,{"$f":"IF(D3=$AA$4,$C$3*$C$4*$C$5,IF(D3=$AA$5,$C$3*$C$4,IF(D3=AA6,$C$3,\"\")))","v":0},"m³/jaar"]
[]
["Waterloop Code"]
["Waterloop naam",null,{"$f":"IFERROR(VLOOKUP(C11,'Info per OWL'!$A:$B,2,FALSE),\"\")","v":""}]
["Q gem pegase waterloop",null,null,"m³/s"]
[null,null,{"$f":"C13*60*60*24*365","v":0},"m³/jaar"]
[]
[]
["Probleemparameters impactbeoordeling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hoeveel % mag bedrijf innemen van overige ruimte",1]
[null,"Parameternaam","Afkorting","Max. procentuele bijdrage parameter (%)","Duidelijke verslechtering klasse","Eenheid","MKN - JG*","Concentratie lozing","Stroomopwaartse concentratie - Jaargemiddelde ","Gewenste effluentconcentratie impactbeoordeling afvalwater","Waterrelevante stof Vlaanderen","Stofcategorie",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Uniformisatie eenheden",null,"Geloosde vuilvracht","Toegestane vuilvracht","Vereiste vuilvrachtreductie","MKN omrekening naar µg/L voor bezwaarlijkheid","Waterbezwaarlijkheid",null,null,null,null,null,null,null,null,null,null,"Meetonzekerheid opzoeken","Toetswaarden opzoeken",null,null,null,"Reductiedoelberekening"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Uniforme eenheid","Factor omrekening eenheden","kg/jaar","kg/jaar","kg/jaar","µg/L","1/MKN",null,null,null,null,null,null,null,null,null,"MKN opzoeken","Meetonzekerheid","MKN","TW G-M","TW M-O","Doel waterlichaam",null,{"$f":"AA19","v":"Uniforme eenheid"},"Factor","VV max (kg/jaar)","VV oppervlaktewater (kg/jaar)","VV Lozing ruimte (kg/jaar)","Individeel bedrijf: max xx% inname overige ruimte (kg/jaar)","Concentratie (mg/L)","Terugrekening eenheid","Finale beslissing"]
[1,null,{"$f":"IFERROR(VLOOKUP(B20,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},null,null,{"$f":"IFERROR(VLOOKUP(B20,'Keuzelijst parameters'!C:F,4,FALSE),\"\")","v":""},{"$f":"AS20","v":""},null,null,null,{"$f":"IFERROR(VLOOKUP(C20,'Keuzelijst parameters'!E:I,4,FALSE),\"\")","v":""},{"$f":"IF(ISBLANK(D20)=TRUE,\"\",'Dashboard beslissing'!M5)","v":""},{"$f":"IF(ISBLANK(D20)=TRUE,\"\",IF(L20=3,\"Geen verdere beoordeling nodig voor deze parameter\",\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(B20,'Keuzelijst parameters'!C:G,5,FALSE),\"\")","v":""},{"$f":"IF(AA20=\"mg/L\",1,IF(AA20=\"µg/L\",1000,IF(AA20=\"ng/L\",1000*1000,IF(AA20=\"µS/cm\",1000,\"\"))))","v":""},{"$f":"IFERROR(H20/AB20*$C$9/1000,\"\")","v":""},{"$f":"IFERROR(J20/AB20*$C$9/1000,\"\")","v":""},{"$f":"IFERROR(AC20-AD20,\"\")","v":""},{"$f":"IFERROR(IF(AA20=\"mg/L\",G20*1000,IF(AA20=\"µg/L\",G20,IF(AA20=\"ng/L\",G20/1000,\"\"))),\"\")","v":""},{"$f":"IFERROR(1/AF20,\"\")","v":""},null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(VLOOKUP(C20,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C20),'Toetswaarden spec wl'!$F:$N,6,FALSE),VLOOKUP(C20,'Keuzelijst parameters'!$B:$M,12,FALSE)),\"\")","v":""},{"$f":"VLOOKUP(B20,'Keuzelijst parameters'!$W:$Z,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(IF(VLOOKUP(C20,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C20),'Toetswaarden spec wl'!$F:$N,4,FALSE),VLOOKUP(C20,'Keuzelijst parameters'!$B:$M,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(VLOOKUP(C20,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C20),'Toetswaarden spec wl'!$F:$N,8,FALSE),AS20),\"\")","v":""},{"$f":"IFERROR(IF(VLOOKUP(C20,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C20),'Toetswaarden spec wl'!$F:$N,9,FALSE),VLOOKUP(C20,'Keuzelijst parameters'!$B:$P,15,FALSE)),\"\")","v":0},{"$f":"AS20","v":""},{"$f":"B20","v":0},{"$f":"AA20","v":""},{"$f":"IF(AX20=\"mg/L\",1,IF(AX20=\"µg/L\",1000,IF(AX20=\"ng/L\",1000*1000,IF(AX20=\"µS/cm\",1000,\"\"))))","v":""},{"$f":"(AV20/AY20*($C$14+$C$9))/1000","v":{"$error":"#VALUE!"}},{"$f":"(I20/AY20*$C$14)/1000","v":{"$error":"#VALUE!"}},{"$f":"AZ20-BA20","v":{"$error":"#VALUE!"}},{"$f":"IF(BB20<=0,0,BB20*$BC$17)","v":{"$error":"#VALUE!"}},{"$f":"BC20/$C$9*1000","v":{"$error":"#VALUE!"}},{"$f":"BD20*AY20","v":{"$error":"#VALUE!"}},{"$f":"IF(I20=\"\",\"\",IF(I20<AV20,BE20,AV20))","v":""}]
[2,null,{"$f":"IFERROR(VLOOKUP(B21,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},null,null,{"$f":"IFERROR(VLOOKUP(B21,'Keuzelijst parameters'!C:F,4,FALSE),\"\")","v":""},"",null,null,null,{"$f":"IFERROR(VLOOKUP(C21,'Keuzelijst parameters'!E:I,4,FALSE),\"\")","v":""},{"$f":"IF(ISBLANK(D21)=TRUE,\"\",'Dashboard beslissing'!M6)","v":""},{"$f":"IF(ISBLANK(D21)=TRUE,\"\",IF(L21=3,\"Geen verdere beoordeling nodig voor deze parameter\",\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(B21,'Keuzelijst parameters'!C:G,5,FALSE),\"\")","v":""},{"$f":"IF(AA21=\"mg/L\",1,IF(AA21=\"µg/L\",1000,IF(AA21=\"ng/L\",1000*1000,IF(AA21=\"µS/cm\",1000,\"\"))))","v":""},"","",{"$f":"IFERROR(AC21-AD21,\"\")","v":""},"",{"$f":"IFERROR(1/AF21,\"\")","v":""},null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(VLOOKUP(C21,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C21),'Toetswaarden spec wl'!$F:$N,6,FALSE),VLOOKUP(C21,'Keuzelijst parameters'!$B:$M,12,FALSE)),\"\")","v":""},{"$f":"VLOOKUP(B21,'Keuzelijst parameters'!$W:$Z,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(IF(VLOOKUP(C21,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C21),'Toetswaarden spec wl'!$F:$N,4,FALSE),VLOOKUP(C21,'Keuzelijst parameters'!$B:$M,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(VLOOKUP(C21,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C21),'Toetswaarden spec wl'!$F:$N,8,FALSE),AS21),\"\")","v":""},{"$f":"IFERROR(IF(VLOOKUP(C21,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C21),'Toetswaarden spec wl'!$F:$N,9,FALSE),VLOOKUP(C21,'Keuzelijst parameters'!$B:$P,15,FALSE)),\"\")","v":0},{"$f":"AS21","v":""},0,{"$f":"AA21","v":""},{"$f":"IF(AX21=\"mg/L\",1,IF(AX21=\"µg/L\",1000,IF(AX21=\"ng/L\",1000*1000,IF(AX21=\"µS/cm\",1000,\"\"))))","v":""},{"$f":"(AV21/AY21*($C$14+$C$9))/1000","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"AZ21-BA21","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"BC21/$C$9*1000","v":{"$error":"#VALUE!"}},{"$f":"BD21*AY21","v":{"$error":"#VALUE!"}},""]
[3,null,{"$f":"IFERROR(VLOOKUP(B22,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},null,null,{"$f":"IFERROR(VLOOKUP(B22,'Keuzelijst parameters'!C:F,4,FALSE),\"\")","v":""},"",null,null,null,{"$f":"IFERROR(VLOOKUP(C22,'Keuzelijst parameters'!E:I,4,FALSE),\"\")","v":""},{"$f":"IF(ISBLANK(D22)=TRUE,\"\",'Dashboard beslissing'!M7)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(B22,'Keuzelijst parameters'!C:G,5,FALSE),\"\")","v":""},"","","","","","",null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(VLOOKUP(C22,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C22),'Toetswaarden spec wl'!$F:$N,6,FALSE),VLOOKUP(C22,'Keuzelijst parameters'!$B:$M,12,FALSE)),\"\")","v":""},{"$f":"VLOOKUP(B22,'Keuzelijst parameters'!$W:$Z,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(IF(VLOOKUP(C22,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C22),'Toetswaarden spec wl'!$F:$N,4,FALSE),VLOOKUP(C22,'Keuzelijst parameters'!$B:$M,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(VLOOKUP(C22,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C22),'Toetswaarden spec wl'!$F:$N,8,FALSE),AS22),\"\")","v":""},{"$f":"IFERROR(IF(VLOOKUP(C22,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C22),'Toetswaarden spec wl'!$F:$N,9,FALSE),VLOOKUP(C22,'Keuzelijst parameters'!$B:$P,15,FALSE)),\"\")","v":0},"",0,"","",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},""]
[4,null,{"$f":"IFERROR(VLOOKUP(B23,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},null,null,{"$f":"IFERROR(VLOOKUP(B23,'Keuzelijst parameters'!C:F,4,FALSE),\"\")","v":""},"",null,null,null,{"$f":"IFERROR(VLOOKUP(C23,'Keuzelijst parameters'!E:I,4,FALSE),\"\")","v":""},{"$f":"IF(ISBLANK(D23)=TRUE,\"\",'Dashboard beslissing'!M8)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(B23,'Keuzelijst parameters'!C:G,5,FALSE),\"\")","v":""},"","","","","","",null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(VLOOKUP(C23,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C23),'Toetswaarden spec wl'!$F:$N,6,FALSE),VLOOKUP(C23,'Keuzelijst parameters'!$B:$M,12,FALSE)),\"\")","v":""},{"$f":"VLOOKUP(B23,'Keuzelijst parameters'!$W:$Z,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(IF(VLOOKUP(C23,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C23),'Toetswaarden spec wl'!$F:$N,4,FALSE),VLOOKUP(C23,'Keuzelijst parameters'!$B:$M,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(VLOOKUP(C23,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C23),'Toetswaarden spec wl'!$F:$N,8,FALSE),AS23),\"\")","v":""},{"$f":"IFERROR(IF(VLOOKUP(C23,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C23),'Toetswaarden spec wl'!$F:$N,9,FALSE),VLOOKUP(C23,'Keuzelijst parameters'!$B:$P,15,FALSE)),\"\")","v":0},"",0,"","",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},""]
[5,null,{"$f":"IFERROR(VLOOKUP(B24,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},null,null,{"$f":"IFERROR(VLOOKUP(B24,'Keuzelijst parameters'!C:F,4,FALSE),\"\")","v":""},"",null,null,null,{"$f":"IFERROR(VLOOKUP(C24,'Keuzelijst parameters'!E:I,4,FALSE),\"\")","v":""},{"$f":"IF(ISBLANK(D24)=TRUE,\"\",'Dashboard beslissing'!M9)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(B24,'Keuzelijst parameters'!C:G,5,FALSE),\"\")","v":""},"","","","","","",null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(VLOOKUP(C24,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C24),'Toetswaarden spec wl'!$F:$N,6,FALSE),VLOOKUP(C24,'Keuzelijst parameters'!$B:$M,12,FALSE)),\"\")","v":""},{"$f":"VLOOKUP(B24,'Keuzelijst parameters'!$W:$Z,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(IF(VLOOKUP(C24,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C24),'Toetswaarden spec wl'!$F:$N,4,FALSE),VLOOKUP(C24,'Keuzelijst parameters'!$B:$M,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(VLOOKUP(C24,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C24),'Toetswaarden spec wl'!$F:$N,8,FALSE),AS24),\"\")","v":""},{"$f":"IFERROR(IF(VLOOKUP(C24,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C24),'Toetswaarden spec wl'!$F:$N,9,FALSE),VLOOKUP(C24,'Keuzelijst parameters'!$B:$P,15,FALSE)),\"\")","v":0},"",0,"","",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},""]
[6,null,{"$f":"IFERROR(VLOOKUP(B25,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},null,null,{"$f":"IFERROR(VLOOKUP(B25,'Keuzelijst parameters'!C:F,4,FALSE),\"\")","v":""},"",null,null,null,{"$f":"IFERROR(VLOOKUP(C25,'Keuzelijst parameters'!E:I,4,FALSE),\"\")","v":""},{"$f":"IF(ISBLANK(D25)=TRUE,\"\",'Dashboard beslissing'!M10)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(B25,'Keuzelijst parameters'!C:G,5,FALSE),\"\")","v":""},"","","","","","",null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(VLOOKUP(C25,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C25),'Toetswaarden spec wl'!$F:$N,6,FALSE),VLOOKUP(C25,'Keuzelijst parameters'!$B:$M,12,FALSE)),\"\")","v":""},{"$f":"VLOOKUP(B25,'Keuzelijst parameters'!$W:$Z,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(IF(VLOOKUP(C25,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C25),'Toetswaarden spec wl'!$F:$N,4,FALSE),VLOOKUP(C25,'Keuzelijst parameters'!$B:$M,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(VLOOKUP(C25,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C25),'Toetswaarden spec wl'!$F:$N,8,FALSE),AS25),\"\")","v":""},{"$f":"IFERROR(IF(VLOOKUP(C25,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C25),'Toetswaarden spec wl'!$F:$N,9,FALSE),VLOOKUP(C25,'Keuzelijst parameters'!$B:$P,15,FALSE)),\"\")","v":0},"",0,"","",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},""]
[7,null,{"$f":"IFERROR(VLOOKUP(B26,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},null,null,{"$f":"IFERROR(VLOOKUP(B26,'Keuzelijst parameters'!C:F,4,FALSE),\"\")","v":""},"",null,null,null,{"$f":"IFERROR(VLOOKUP(C26,'Keuzelijst parameters'!E:I,4,FALSE),\"\")","v":""},{"$f":"IF(ISBLANK(D26)=TRUE,\"\",'Dashboard beslissing'!M11)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(B26,'Keuzelijst parameters'!C:G,5,FALSE),\"\")","v":""},"","","","","","",null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(VLOOKUP(C26,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C26),'Toetswaarden spec wl'!$F:$N,6,FALSE),VLOOKUP(C26,'Keuzelijst parameters'!$B:$M,12,FALSE)),\"\")","v":""},{"$f":"VLOOKUP(B26,'Keuzelijst parameters'!$W:$Z,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(IF(VLOOKUP(C26,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C26),'Toetswaarden spec wl'!$F:$N,4,FALSE),VLOOKUP(C26,'Keuzelijst parameters'!$B:$M,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(VLOOKUP(C26,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C26),'Toetswaarden spec wl'!$F:$N,8,FALSE),AS26),\"\")","v":""},{"$f":"IFERROR(IF(VLOOKUP(C26,'Keuzelijst parameters'!$B:$M,11,FALSE)=\"ja\",VLOOKUP(_xlfn.CONCAT($C$11,C26),'Toetswaarden spec wl'!$F:$N,9,FALSE),VLOOKUP(C26,'Keuzelijst parameters'!$B:$P,15,FALSE)),\"\")","v":0},"",0,"","",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},""]
[]
[]
[]
["Huidige index der consumptieprijzen met als basisjaar 2013 (2013=100)"]
[134.44,"Huidige consumptieprijsindex raadplegen"]
[]
[]
[]
["Niet-genormeerde parameters"]
["Volgnummer","Naam stof","Toetswaarde","Eenheid"]
["E1"]
["E2"]
["E3"]
["E4"]
["E5"]
["E6"]
["E7"]

{"sheet":"Input bijkomende maatregelen","index":1,"n_rows":114,"n_cols":50,"rows_kept":114,"cut":false,"hidden":false,"merged":[[46,1,46,2],[41,1,41,4],[42,1,42,4],[43,1,43,2],[37,1,37,10],[40,1,40,2],[39,1,39,3],[45,1,45,4],[8,3,8,4],[10,1,10,2],[9,1,9,2],[11,1,11,2],[24,1,24,2],[7,1,8,2],[17,1,17,2],[20,1,20,11],[24,10,25,10],[24,11,25,11],[24,7,25,7],[24,3,25,3],[24,4,25,4],[24,5,25,5],[17,3,17,9],[24,6,25,6],[0,1,0,2],[4,1,4,2],[5,1,5,2],[6,1,6,2],[2,1,2,9],[4,3,4,4],[5,3,5,4],[47,1,47,2],[48,1,48,2],[53,1,53,2],[55,1,55,2],[54,1,54,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[73,1,73,2],[63,1,63,2],[64,1,64,2],[56,1,56,2],[57,1,57,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[58,1,58,2],[59,1,59,2],[60,1,60,2],[61,1,61,2],[70,1,70,2],[71,1,71,2],[72,1,72,2],[62,1,62,2],[112,1,112,11],[114,1,114,11],[84,1,84,11],[85,1,86,11],[3,1,3,4],[87,1,87,3],[99,1,99,3],[111,1,111,3],[113,1,113,3],[13,1,14,2],[68,1,68,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[69,1,69,2]]}
[null,"Vul groene velden in"]
[]
[null,"1. Bijkomende maatregelen: Informatie"]
[]
[null,"Deze maatregel is een:",null,null,null,{"$f":"VLOOKUP(D5,O19:P24,2,FALSE)","v":{"$error":"#N/A"}}]
[null,"Type Technologie"]
[]
[null,{"$f":"IF(F5=4,\"Jaarlijks volume water waar maatregel een effect op heeft\",\"Behandeld volume door bijkomende maatregel\")","v":{"$error":"#N/A"}},null,null,"m³/j"]
[null,null,null,{"$f":"IF(ISBLANK(D8)=TRUE,\"\",IF(D8='Input huidige maatreg. (fac.)'!D10,\"Volledige behandeling stroom\",IF(D8<'Input huidige maatreg. (fac.)'!D10,\"Deelstroombehandeling\",\"Fout - check behandelingsdebiet\")))","v":""}]
[]
[null,"Heeft deze maatregel ook een effect op het volume (vb. indamping of membraantechniek)?"]
[null,"Geloosd volume na maatregel",null,null,"m³/j"]
[]
[null,"Geloosd totaal volume - lozingspunt"]
[null,null,null,{"$f":"IF(D11=\"ja\",'Input impactbeoordeing'!$C$9-(D8-D12),'Input impactbeoordeing'!$C$9)","v":0},"m³/j"]
[]
[]
[null,"Omschrijving maatregel",null,null,null,null,null,null,null,null,null,null,null,null,"Lijstje","Code",null,"Lijst","Code",null,"Lijst"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Afwalwaterbehandeling op deelstroomniveau",1,null,"Membraan technieken + afvoer",1,null,"ja",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Afwalwaterbehandeling op de volledige waterstroom",1,null,"Membraan technieken",3,null,"nee",0]
[null,"2. Bijkomende maatreglen: Vuilvrachtreductie",null,null,null,null,null,null,null,null,null,null,null,null,"Bronmaatregel",4,null,"Indamping + afvoer",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Procesgeïntegreerde maatregel",4,null,"Indamping",2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Adsorptie technieken",3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oxidatieve technieken",3]
[null,"Probleemparameter(s)",null,{"$f":"IF($F$5=1,\"Influentconcentratie bijkomende techniek\",\"Vermeden emissies (kg/jaar)\")","v":{"$error":"#N/A"}},{"$f":"IF($F$5=1,\"Concentratie lozing na bijkomende techniek - gemiddeld\",\"\")","v":{"$error":"#N/A"}},"Berekende effluentconcentratie ter hoogte van lozingspunt",{"$f":"'Input impactbeoordeing'!J18","v":"Gewenste effluentconcentratie impactbeoordeling afvalwater"},"Eenheid","Verwijderde vuilvracht","Resterende vuilvracht geloosd","Inkomend volume bijkomende techniek (m³/jaar)","Geloosd volume na bijkomende techniek (m³/jaar)",null,null,null,null,null,"fysico-chemische behandeling",3,null,null,null,null,null,null,null,null,"Probleemparameter(s)","Eenheid uniform",null,"Influentconcentratie bijkomende techniek - UNIF mg/L ","Effluentconcentratie na implementatie bijkomende techniek - gemiddeld","Ingaande vuilvracht","Uitgaande vuilvracht","Verijderde vuilvracht","Totale vuilvracht voor maatregel","Totale resterende vuilvracht","Totaal volume","C lozingspunt","C lozingspunt terugrekening basiseenheid",null,"Probleemparameter(s)","Eenheid uniform",null,"Verijderde vuilvracht","Totale vuilvracht voor maatregel","Totale resterende vuilvracht","Totaal volume","C lozingspunt","C lozingspunt terugrekening basiseenheid"]
[null,"Nr","Naam",null,null,null,null,null,"kg/jaar","kg/jaar",null,null,null,null,null,null,null,"Andere technieken of combinaties",4,null,null,null,null,null,null,null,null,null,null,"UNIF factor","mg/L","mg/L","kg/jaar","kg/jaar","kg/jaar","kg/jaar","kg/jaar","m³/jaar","mg/L",null,null,null,null,"UNIF factor","kg/jaar","kg/jaar","kg/jaar","m³/jaar","mg/L"]
[null,1,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!B20)","v":""},null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",IF($F$5=1,AN27,AX27))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!J20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!F20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",IF($F$5=1,AI27,AS27))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",IF($F$5=1,AK27,AU27))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",$D$8)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",IF($D$11=\"ja\",$D$12,$D$8))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!B20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!AA20)","v":""},{"$f":"IF($AC27=\"mg/L\",1,IF($AC27=\"µg/L\",1000,IF($AC27=\"ng/L\",1000*1000,IF($AC27=\"µS/cm\",1000,\"\"))))","v":""},{"$f":"IF($F$5=1,D27/AD27,\"\")","v":{"$error":"#N/A"}},{"$f":"IF($F$5=1,E27/AD27,\"\")","v":{"$error":"#N/A"}},{"$f":"AE27*K27/1000","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"AG27-AH27","v":{"$error":"#N/A"}},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!AC20)","v":""},{"$f":"AJ27-AI27","v":{"$error":"#VALUE!"}},{"$f":"$D$15","v":0},{"$f":"AK27/AL27*1000","v":{"$error":"#VALUE!"}},{"$f":"AM27*AD27","v":{"$error":"#VALUE!"}},1,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!B20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!AA20)","v":""},{"$f":"IF($AC27=\"mg/L\",1,IF($AC27=\"µg/L\",1000,IF($AC27=\"ng/L\",1000*1000,IF($AC27=\"µS/cm\",1000,\"\"))))","v":""},{"$f":"D27","v":0},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!AC20)","v":""},{"$f":"AT27-AS27","v":{"$error":"#VALUE!"}},{"$f":"$D$15","v":0},{"$f":"AU27/AV27*1000","v":{"$error":"#VALUE!"}},{"$f":"AW27*AR27","v":{"$error":"#VALUE!"}}]
[null,2,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!B21)","v":""},null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",IF($F$5=1,AN28,AX28))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!J21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!F21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",IF($F$5=1,AI28,AS28))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",IF($F$5=1,AK28,AU28))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",$D$8)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",IF($D$11=\"ja\",$D$12,$D$8))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!B21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!AA21)","v":""},{"$f":"IF($AC28=\"mg/L\",1,IF($AC28=\"µg/L\",1000,IF($AC28=\"ng/L\",1000*1000,IF($AC28=\"µS/cm\",1000,\"\"))))","v":""},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"AG28-AH28","v":{"$error":"#N/A"}},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!AC21)","v":""},{"$f":"AJ28-AI28","v":{"$error":"#VALUE!"}},{"$f":"$D$15","v":0},{"$f":"AK28/AL28*1000","v":{"$error":"#VALUE!"}},{"$f":"AM28*AD28","v":{"$error":"#VALUE!"}},2,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!B21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!AA21)","v":""},{"$f":"IF($AC28=\"mg/L\",1,IF($AC28=\"µg/L\",1000,IF($AC28=\"ng/L\",1000*1000,IF($AC28=\"µS/cm\",1000,\"\"))))","v":""},0,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!AC21)","v":""},{"$f":"AT28-AS28","v":{"$error":"#VALUE!"}},{"$f":"$D$15","v":0},{"$f":"AU28/AV28*1000","v":{"$error":"#VALUE!"}},{"$f":"AW28*AR28","v":{"$error":"#VALUE!"}}]
[null,3,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!B22)","v":""},null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",IF($F$5=1,AN29,AX29))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!J22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!F22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",IF($F$5=1,AI29,AS29))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",IF($F$5=1,AK29,AU29))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",$D$8)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",IF($D$11=\"ja\",$D$12,$D$8))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!B22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!AA22)","v":""},"",{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!AC22)","v":""},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!B22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!AA22)","v":""},"",0,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!AC22)","v":""},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,4,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!B23)","v":""},null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",IF($F$5=1,AN30,AX30))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!J23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!F23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",IF($F$5=1,AI30,AS30))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",IF($F$5=1,AK30,AU30))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",$D$8)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",IF($D$11=\"ja\",$D$12,$D$8))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!B23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!AA23)","v":""},"",{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!AC23)","v":""},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},4,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!B23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!AA23)","v":""},"",0,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!AC23)","v":""},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,5,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!B24)","v":""},null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",IF($F$5=1,AN31,AX31))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!J24)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!F24)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",IF($F$5=1,AI31,AS31))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",IF($F$5=1,AK31,AU31))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",$D$8)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",IF($D$11=\"ja\",$D$12,$D$8))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!B24)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!AA24)","v":""},"",{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!AC24)","v":""},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},5,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!B24)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!AA24)","v":""},"",0,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!AC24)","v":""},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,6,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!B25)","v":""},null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",IF($F$5=1,AN32,AX32))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!J25)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!F25)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",IF($F$5=1,AI32,AS32))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",IF($F$5=1,AK32,AU32))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",$D$8)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",IF($D$11=\"ja\",$D$12,$D$8))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!B25)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!AA25)","v":""},"",{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!AC25)","v":""},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},6,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!B25)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!AA25)","v":""},"",0,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!AC25)","v":""},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,7,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!B26)","v":""},null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",IF($F$5=1,AN33,AX33))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!J26)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!F26)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",IF($F$5=1,AI33,AS33))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",IF($F$5=1,AK33,AU33))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",$D$8)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",IF($D$11=\"ja\",$D$12,$D$8))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!B26)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!AA26)","v":""},"",{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!AC26)","v":""},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},7,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!B26)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!AA26)","v":""},"",0,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!AC26)","v":""},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[]
[]
[]
[null,"3. Bijkomende maatregelen: Financiële informatie "]
[]
[null,"Ik wens de eenvoudige kostenstructuur in te vullen",null,null,"ja"]
[]
[null,"CAPEX / Investeringskosten - eenvoudig",null,null,null,"OPEX / werkingskosten",null,null,"Baten"]
[]
[null,"Totale CAPEX",null,null,"EUR","Totale OPEX",null,"EUR/jaar","Totale baten ",null,"EUR/jaar"]
[]
[null,"CAPEX / Investeringskosten - uitgebreid",null,null,null,"OPEX / werkingskosten",null,null,"Baten"]
[]
[null,"Directe constructie kosten",null,{"$f":"SUM(D49:D53)","v":0},"EUR","VARIABLE",{"$f":"SUM(G49:G54)","v":0},"EUR/jaar","verminderde heffing",null,"EUR/jaar"]
[null,"Unit kostprijs waterzuivering",null,null,"EUR","Energie",null,"EUR/jaar","verminderde aankoop water",null,"EUR/jaar"]
[null,"Elektriciteit & instrumentatie",null,null,"EUR","Chemicaliën",null,"EUR/jaar","verkoop reststoffen",null,"EUR/jaar"]
[null,"Equipment & utilities",null,null,"EUR","Verbruiksmateriaal (bv. membranen)",null,"EUR/jaar","andere baten",null,"EUR/jaar"]
[null,"Gebouw",null,null,"EUR","Afvoer afval",null,"EUR/jaar","andere baten 2",null,"EUR/jaar"]
[null,"Varia",null,null,"EUR","Varia",null,"EUR/jaar"]
[null,"Emissies tijdens bouw (CO2)",null,null,"EUR","Emissies tijdens exploitatie (CO2 eq)",null,"EUR/jaar"]
[]
[null,"Indirecte kosten",null,{"$f":"SUM(D57:D60)","v":0},"EUR","FIXED",{"$f":"SUM(G57:G60)","v":0},"EUR/jaar"]
[null,"Engineering",null,null,"EUR","Manuren",null,"EUR/jaar"]
[null,"Project ontwikkeling (admin, vergunningen, legal, …)",null,null,"EUR","Onderhoud",null,"EUR/jaar"]
[null,"Financiering",null,null,"EUR","Opvolging (data analyse, …)",null,"EUR/jaar"]
[null,"Varia",null,null,"EUR","Varia",null,"EUR/jaar"]
[]
[null,"onvoorzien",null,null,"EUR","onvoorzien",null,"EUR/jaar"]
[]
[null,"Totale CAPEX",null,{"$f":"D62+D56+D48","v":0},"EUR","Totale OPEX",{"$f":"G62+G56+G48","v":0},"EUR/jaar","Totale baten ",{"$f":" SUM(J48:J61)","v":0},"EUR/jaar"]
[]
[]
[]
[null,"Totale CAPEX",null,{"$f":"IF(E40=\"ja\",D44,D64)","v":0},"EUR","Totale OPEX",{"$f":"IF(E40=\"ja\",G44,G64)","v":0},"EUR/jaar","Totale baten",{"$f":"IF(E40=\"ja\",J44,J64)","v":0},"EUR/jaar"]
[null,"Afschrijvingsperiode",null,10,"jaar"]
[null,"Rente",null,0.04,"%"]
[]
[null,"Jaarslijkse kapitaalkost (YCC)",null,{"$f":"-PMT(D70,D69,D68)","v":0},"EUR/jaar","OPEX (exclusief YCC en baten)",{"$f":"G68","v":0},"EUR/jaar","Totale baten ",{"$f":"J68","v":0},"EUR/jaar"]
[]
[null,null,null,{"$f":"IFERROR(D72/D8,0)","v":0},"EUR/m³",null,{"$f":"IFERROR(G72/D8,0)","v":0},"EUR/m³"]
[]
[]
[null,"Totale kost (=YCC+OPEX-baten)",null,{"$f":"D72+G72-J72","v":0},"EUR/jaar"]
[null,null,null,{"$f":"IFERROR(D77/D8,0)","v":0},"EUR/m³"]
[]
[]
[]
[]
[]
[]
[null,"4. Bijkomende maatregelen: Mogelijke cross-media effecten"]
[null,"De voorgestelde maatregel geeft aanleiding tot volgende cross-media effecten"]
[]
[null,"A Emissies naar water - opconcentratie reeds aanwezige polluent",null,null,"nee"]
[]
[null,null,"Parameternaam","Afkorting","Eenheid","MKN - JG/Toetswaarde","Volume (m³/jaar)","CSOW","Ceffluent ter hoogte van lozingspunt","CSAW (berekend)","Abs Bijdrage onder realistische omstandigheden","Proc. Bijdrage onder realistische omstandigheden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Probleemparameter(s)",null,null,"CSOW","CSAW","TW","CSOW < TW","CSAW > TW","Beoordeling",null,null,null,"Expressie"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"µg/L","µg/L","µg/L"]
[null,1,{"$f":"IFERROR(IF(F27>'Input impactbeoordeing'!H20,'Input bijkomende maatregelen'!C27,\"\"),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(C92,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},{"$f":"IFERROR(IF(F27>'Input impactbeoordeing'!H20,'Input impactbeoordeing'!F20,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F27>'Input impactbeoordeing'!H20,'Input impactbeoordeing'!G20,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F27>'Input impactbeoordeing'!H20,$D$15,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F27>'Input impactbeoordeing'!H20,'Input impactbeoordeing'!I20,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F27>'Input impactbeoordeing'!H20,F27,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",((I92*G92)+(H92*'Input impactbeoordeing'!$C$14))/(G92+'Input impactbeoordeing'!$C$14)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",((I92*G92)/(G92+'Input impactbeoordeing'!$C$14))),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",K92/F92),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"C92","v":""},null,null,{"$f":"H92","v":""},{"$f":"J92","v":""},{"$f":"F92","v":""},{"$f":"IF(H92>=F92,\"Nee\",\"Ja\")","v":"Nee"},{"$f":"IF(J92>F92,\"Ja\",\"Nee\")","v":"Nee"},{"$f":"IF(AND(AH92=\"Ja\",AI92=\"Nee\"),$AN$105,IF(AND(AH92=\"Ja\",AI92=\"Ja\"),$AN$106,$AN$104))","v":"Toetswaarde SOW niet gehaald. Maatregel draagt bij tot het niet halen doelstellingen voor deze parameter"},null,null,null,"Toetswaarde SOW niet gehaald. Maatregel draagt bij tot het niet halen doelstellingen voor deze parameter"]
[null,2,{"$f":"IFERROR(IF(F28>'Input impactbeoordeing'!H21,'Input bijkomende maatregelen'!C28,\"\"),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(C93,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},{"$f":"IFERROR(IF(F28>'Input impactbeoordeing'!H21,'Input impactbeoordeing'!F21,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F28>'Input impactbeoordeing'!H21,'Input impactbeoordeing'!G21,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F28>'Input impactbeoordeing'!H21,$D$15,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F28>'Input impactbeoordeing'!H21,'Input impactbeoordeing'!I21,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F28>'Input impactbeoordeing'!H21,F28,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",((I93*G93)+(H93*'Input impactbeoordeing'!$C$14))/(G93+'Input impactbeoordeing'!$C$14)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",((I93*G93)/(G93+'Input impactbeoordeing'!$C$14))),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",K93/F93),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"C93","v":""},null,null,"","","","Nee","Nee","Toetswaarde SOW niet gehaald. Maatregel draagt bij tot het niet halen doelstellingen voor deze parameter",null,null,null,"Toetswaarde SOW en SAW gehaald. Maatregel zorgt niet voor achteruitgang klasse voor deze parameter"]
[null,3,{"$f":"IFERROR(IF(F29>'Input impactbeoordeing'!H22,'Input bijkomende maatregelen'!C29,\"\"),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(C94,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},{"$f":"IFERROR(IF(F29>'Input impactbeoordeing'!H22,'Input impactbeoordeing'!F22,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F29>'Input impactbeoordeing'!H22,'Input impactbeoordeing'!G22,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F29>'Input impactbeoordeing'!H22,$D$15,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F29>'Input impactbeoordeing'!H22,'Input impactbeoordeing'!I22,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F29>'Input impactbeoordeing'!H22,F29,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",((I94*G94)+(H94*'Input impactbeoordeing'!$C$14))/(G94+'Input impactbeoordeing'!$C$14)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",((I94*G94)/(G94+'Input impactbeoordeing'!$C$14))),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",K94/F94),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,"",null,null,"","","","Nee","Nee","Toetswaarde SOW niet gehaald. Maatregel draagt bij tot het niet halen doelstellingen voor deze parameter",null,null,null,"Toetswaarde SOW gehaald, SAW niet. Maatregel zorgt  voor achteruitgang klasse voor deze parameter"]
[null,4,{"$f":"IFERROR(IF(F30>'Input impactbeoordeing'!H23,'Input bijkomende maatregelen'!C30,\"\"),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(C95,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},{"$f":"IFERROR(IF(F30>'Input impactbeoordeing'!H23,'Input impactbeoordeing'!F23,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F30>'Input impactbeoordeing'!H23,'Input impactbeoordeing'!G23,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F30>'Input impactbeoordeing'!H23,$D$15,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F30>'Input impactbeoordeing'!H23,'Input impactbeoordeing'!I23,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F30>'Input impactbeoordeing'!H23,F30,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",((I95*G95)+(H95*'Input impactbeoordeing'!$C$14))/(G95+'Input impactbeoordeing'!$C$14)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",((I95*G95)/(G95+'Input impactbeoordeing'!$C$14))),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",K95/F95),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"",null,null,"","","","Nee","Nee","Toetswaarde SOW niet gehaald. Maatregel draagt bij tot het niet halen doelstellingen voor deze parameter"]
[null,5,{"$f":"IFERROR(IF(F31>'Input impactbeoordeing'!H24,'Input bijkomende maatregelen'!C31,\"\"),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(C96,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},{"$f":"IFERROR(IF(F31>'Input impactbeoordeing'!H24,'Input impactbeoordeing'!F24,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F31>'Input impactbeoordeing'!H24,'Input impactbeoordeing'!G24,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F31>'Input impactbeoordeing'!H24,$D$15,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F31>'Input impactbeoordeing'!H24,'Input impactbeoordeing'!I24,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F31>'Input impactbeoordeing'!H24,F31,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",((I96*G96)+(H96*'Input impactbeoordeing'!$C$14))/(G96+'Input impactbeoordeing'!$C$14)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",((I96*G96)/(G96+'Input impactbeoordeing'!$C$14))),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",K96/F96),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"",null,null,"","","","Nee","Nee","Toetswaarde SOW niet gehaald. Maatregel draagt bij tot het niet halen doelstellingen voor deze parameter"]
[null,6,{"$f":"IFERROR(IF(F32>'Input impactbeoordeing'!H25,'Input bijkomende maatregelen'!C32,\"\"),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(C97,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},{"$f":"IFERROR(IF(F32>'Input impactbeoordeing'!H25,'Input impactbeoordeing'!F25,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F32>'Input impactbeoordeing'!H25,'Input impactbeoordeing'!G25,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F32>'Input impactbeoordeing'!H25,$D$15,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F32>'Input impactbeoordeing'!H25,'Input impactbeoordeing'!I25,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F32>'Input impactbeoordeing'!H25,F32,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",((I97*G97)+(H97*'Input impactbeoordeing'!$C$14))/(G97+'Input impactbeoordeing'!$C$14)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",((I97*G97)/(G97+'Input impactbeoordeing'!$C$14))),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",K97/F97),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"",null,null,"","","","Nee","Nee","Toetswaarde SOW niet gehaald. Maatregel draagt bij tot het niet halen doelstellingen voor deze parameter"]
[null,7,{"$f":"IFERROR(IF(F33>'Input impactbeoordeing'!H26,'Input bijkomende maatregelen'!C33,\"\"),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(C98,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},{"$f":"IFERROR(IF(F33>'Input impactbeoordeing'!H26,'Input impactbeoordeing'!F26,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F33>'Input impactbeoordeing'!H26,'Input impactbeoordeing'!G26,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F33>'Input impactbeoordeing'!H26,$D$15,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F33>'Input impactbeoordeing'!H26,'Input impactbeoordeing'!I26,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(F33>'Input impactbeoordeing'!H26,F33,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",((I98*G98)+(H98*'Input impactbeoordeing'!$C$14))/(G98+'Input impactbeoordeing'!$C$14)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",((I98*G98)/(G98+'Input impactbeoordeing'!$C$14))),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",K98/F98),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"",null,null,"","","","Nee","Nee","Toetswaarde SOW niet gehaald. Maatregel draagt bij tot het niet halen doelstellingen voor deze parameter"]
[]
[null,"B Emissies naar water - Toename lozing andere componenten",null,null,"nee"]
[]
[null,null,"Parameternaam","Afkorting","Eenheid","MKN - JG/Toetswaarde","Volume","CSOW","Ceffluent ter hoogte van het lozingspunt","CSAW (berekend)","Abs Bijdrage onder realistische omstandigheden","Proc. Bijdrage onder realistische omstandigheden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Probleemparameter(s)",null,null,"CSOW","CSAW","TW","CSOW < TW","CSAW > TW","Beoordeling",null,null,null,"Expressie"]
[null,null,null,null,null,null,"m³/jaar","µg/L","µg/L","µg/L","µg/L",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"µg/L","µg/L","µg/L"]
[null,1,null,{"$f":"IFERROR(VLOOKUP(C104,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(C104,'Keuzelijst parameters'!C:F,4,FALSE),\"\")","v":""},null,null,null,null,{"$f":"IF(ISBLANK(C104)=TRUE,\"\",((I104*G104)+(H104*'Input impactbeoordeing'!$C$14))/(G104+'Input impactbeoordeing'!$C$14))","v":""},{"$f":"IF(ISBLANK(C104)=TRUE,\"\",((I104*G104))/(G104+'Input impactbeoordeing'!$C$14))","v":""},{"$f":"IFERROR(IF(ISBLANK(C104)=TRUE,\"\",K104/F104),0)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"C104","v":0},null,null,{"$f":"H104","v":0},{"$f":"J104","v":""},{"$f":"F104","v":0},{"$f":"IF(H104>=F104,\"Nee\",\"Ja\")","v":"Nee"},{"$f":"IF(J104>F104,\"Ja\",\"Nee\")","v":"Nee"},{"$f":"IF(AND(AH104=\"Ja\",AI104=\"Nee\"),$AN$105,IF(AND(AH104=\"Ja\",AI104=\"Ja\"),$AN$106,$AN$104))","v":"Toetswaarde SOW niet gehaald. Maatregel draagt bij tot het niet halen doelstellingen voor deze parameter"},null,null,null,"Toetswaarde SOW niet gehaald. Maatregel draagt bij tot het niet halen doelstellingen voor deze parameter"]
[null,2,null,{"$f":"IFERROR(VLOOKUP(C105,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(C105,'Keuzelijst parameters'!C:F,4,FALSE),\"\")","v":""},null,null,null,null,{"$f":"IF(ISBLANK(C105)=TRUE,\"\",((I105*G105)+(H105*'Input impactbeoordeing'!$C$14))/(G105+'Input impactbeoordeing'!$C$14))","v":""},{"$f":"IF(ISBLANK(C105)=TRUE,\"\",((I105*G105))/(G105+'Input impactbeoordeing'!$C$14))","v":""},{"$f":"IFERROR(IF(ISBLANK(C105)=TRUE,\"\",K105/F105),0)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"C105","v":0},null,null,0,"",0,"Nee","Nee","Toetswaarde SOW niet gehaald. Maatregel draagt bij tot het niet halen doelstellingen voor deze parameter",null,null,null,"Toetswaarde SOW en SAW gehaald. Maatregel zorgt niet voor achteruitgang klasse voor deze parameter"]
[null,3,null,{"$f":"IFERROR(VLOOKUP(C106,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(C106,'Keuzelijst parameters'!C:F,4,FALSE),\"\")","v":""},null,null,null,null,{"$f":"IF(ISBLANK(C106)=TRUE,\"\",((I106*G106)+(H106*'Input impactbeoordeing'!$C$14))/(G106+'Input impactbeoordeing'!$C$14))","v":""},{"$f":"IF(ISBLANK(C106)=TRUE,\"\",((I106*G106))/(G106+'Input impactbeoordeing'!$C$14))","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,0,null,null,0,"",0,"Nee","Nee","Toetswaarde SOW niet gehaald. Maatregel draagt bij tot het niet halen doelstellingen voor deze parameter",null,null,null,"Toetswaarde SOW gehaald, SAW niet. Maatregel zorgt  voor achteruitgang klasse voor deze parameter"]
[null,4,null,{"$f":"IFERROR(VLOOKUP(C107,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(C107,'Keuzelijst parameters'!C:F,4,FALSE),\"\")","v":""},null,null,null,null,{"$f":"IF(ISBLANK(C107)=TRUE,\"\",((I107*G107)+(H107*'Input impactbeoordeing'!$C$14))/(G107+'Input impactbeoordeing'!$C$14))","v":""},{"$f":"IF(ISBLANK(C107)=TRUE,\"\",((I107*G107))/(G107+'Input impactbeoordeing'!$C$14))","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,0,null,null,0,"",0,"Nee","Nee","Toetswaarde SOW niet gehaald. Maatregel draagt bij tot het niet halen doelstellingen voor deze parameter"]
[null,5,null,{"$f":"IFERROR(VLOOKUP(C108,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(C108,'Keuzelijst parameters'!C:F,4,FALSE),\"\")","v":""},null,null,null,null,{"$f":"IF(ISBLANK(C108)=TRUE,\"\",((I108*G108)+(H108*'Input impactbeoordeing'!$C$14))/(G108+'Input impactbeoordeing'!$C$14))","v":""},{"$f":"IF(ISBLANK(C108)=TRUE,\"\",((I108*G108))/(G108+'Input impactbeoordeing'!$C$14))","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,0,null,null,0,"",0,"Nee","Nee","Toetswaarde SOW niet gehaald. Maatregel draagt bij tot het niet halen doelstellingen voor deze parameter"]
[null,6,null,{"$f":"IFERROR(VLOOKUP(C109,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(C109,'Keuzelijst parameters'!C:F,4,FALSE),\"\")","v":""},null,null,null,null,{"$f":"IF(ISBLANK(C109)=TRUE,\"\",((I109*G109)+(H109*'Input impactbeoordeing'!$C$14))/(G109+'Input impactbeoordeing'!$C$14))","v":""},{"$f":"IF(ISBLANK(C109)=TRUE,\"\",((I109*G109))/(G109+'Input impactbeoordeing'!$C$14))","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,0,null,null,0,"",0,"Nee","Nee","Toetswaarde SOW niet gehaald. Maatregel draagt bij tot het niet halen doelstellingen voor deze parameter"]
[null,7,null,{"$f":"IFERROR(VLOOKUP(C110,'Keuzelijst parameters'!C:E,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(C110,'Keuzelijst parameters'!C:F,4,FALSE),\"\")","v":""},null,null,null,null,{"$f":"IF(ISBLANK(C110)=TRUE,\"\",((I110*G110)+(H110*'Input impactbeoordeing'!$C$14))/(G110+'Input impactbeoordeing'!$C$14))","v":""},{"$f":"IF(ISBLANK(C110)=TRUE,\"\",((I110*G110))/(G110+'Input impactbeoordeing'!$C$14))","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,0,null,null,0,"",0,"Nee","Nee","Toetswaarde SOW niet gehaald. Maatregel draagt bij tot het niet halen doelstellingen voor deze parameter"]
[]
[null,"C Emissies naar lucht",null,null,"nee"]
[]
[null,"D Overige",null,null,"nee"]

{"sheet":"Input financiële kengetallen","index":2,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[[22,0,22,1],[22,2,22,5],[24,0,24,5],[23,2,23,5],[21,1,21,5],[6,1,6,5],[10,7,12,7],[14,7,21,7],[7,0,7,5],[9,0,9,5],[8,2,8,5]]}
["Vul groene velden in"]
[]
["Volledig schema (VOL)"]
["(Nummering jaarrekening rechter bovenhoek jaarrekening start met VOL)",null,null,"bronnen","https://cri.nbb.be/bc9/web/catalog?execution=e2s1"]
[null,null,null,null,"jaarrekeningen raadplegen via nationale bank - opgelet: pop up blocker disablen"]
["In dit kader worden de kengetallen van de holding gerapporteerd."]
["Financiële kengetallen van de holding","Naam Holding",null,null,null,null,null,"Definities"]
[]
["Recentste jaartal beschikbare informatie",2024,null,null,null,null,null,"Omzet (code 70), zijnde het totaal bedrag aan verkochte producten/diensten."]
[]
["Maatstaf","Jaartal",null,null,null,null,null,"Zuivere toegevoegde waarde = Bedrijfsopbrengsten (code 70/76A) - Handelsgoederen, grond- en hulpstoffen (code 60) - Diensten en diverse goederen (code 61) - Exploitatiesubsidies en vanwege de overheid ontvangen compenserende bedragen (code  740)."]
[null,{"$f":"B9","v":2024},{"$f":"B12-1","v":2023},{"$f":"C12-1","v":2022},{"$f":"D12-1","v":2021},{"$f":"E12-1","v":2020}]
[]
["Omzet"]
[null,null,null,null,null,null,null,"EBITDA = [Winst of verlies van het boekjaar (code 9903)-opbrengst uit financiële activa (code 750)-Opbrengst uit Vlottende activa (code 751)-andere financiële opbrengsten (code 752/9)+kosten van schulden (code 650)+Waardevermindering op vlottende activa (code 651)+andere financiële kosten (code652/9)] +Afschrijvingen en waardeverminderingen (code 630)+waardeverminderingen op voorraden,bestellingen,...(code 631/4)+uitzonderlijke afschrijvingen en waardeverminderingen (code 660)-Terugnemng avan afschrijvingen en van waardeverminderingen (code 760)"]
["Toegevoegde waarde"]
[]
["EBIDTA"]
[]
[]
["In dit kader worden de kengetallen van de vestiging gerapporteerd. Deze informatie wordt door het bedrijf opgegeven (vaak niet publiek)."]
["Financiële kengetallen van de vestiging","Naam Vestiging"]
[]
["Recentste jaartal beschikbare informatie",2024]
[]
["Maatstaf","Jaartal"]
[null,{"$f":"B24","v":2024},{"$f":"B27-1","v":2023},{"$f":"C27-1","v":2022},2021,2020]
[]
["Omzet"]
[]
["Toegevoegde waarde"]
[]
["EBIDTA"]

{"sheet":"Input huidige maatreg. (fac.)","index":3,"n_rows":42,"n_cols":29,"rows_kept":42,"cut":false,"hidden":false,"merged":[[40,5,40,10],[39,1,39,10],[8,1,8,10],[9,5,10,10],[1,1,1,11],[14,1,14,2],[13,1,13,10],[32,1,32,4],[40,1,40,2],[29,5,29,8],[3,3,7,10],[0,1,0,11],[11,1,11,11],[3,1,7,2],[9,1,10,2],[12,1,12,11],[41,1,41,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[29,1,29,4],[31,1,31,4],[35,1,35,4],[33,1,33,2],[34,1,34,2]]}
[null,"Vul de groene velden in"]
[]
[null,"1. Huidige maatregelen: Beschrijving van de case - bestaande maatreglen en lozing"]
[null,"Omschrijving huidige technieken en maatregelen: "]
[]
[]
[]
[]
[null,"Gegevens lozing"]
[null,"Lozing TOTAAL volume afvalwater",null,{"$f":"'Input impactbeoordeing'!$C$9","v":0},"m³/jaar"]
[null,null,null,{"$f":"'Input impactbeoordeing'!C8","v":""},"m³/d"]
[]
[]
[null,"2. Huidige maatreglen: Vuilvrachtreductie door huidige maatregelen"]
[null,"Probleemparameter(s)",null,"Inkomende concentratie huidige waterzuivering","Huidige effluentconcentratie thv lozingspunt",{"$f":"'Input impactbeoordeing'!J18","v":"Gewenste effluentconcentratie impactbeoordeling afvalwater"},"Eenheid","Inkomende vuilvracht huidige waterzuivering","Huidig geloosde vuilvrachten","Gem. bijkomend te verwijderen per jaar","Gem. vuilvracht reeds verwijderd door huidige WZ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Probleemparameter(s)","Eenheid uniform","Factor"]
[null,"nr","naam",null,null,null,null,"kg/jaar","kg/jaar","kg/jaar","kg/jaar"]
[null,1,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!B20)","v":""},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!H20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!J20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!F20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",D17*$D$10/AC17/1000)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",$D$10*E17/AC17/1000)","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",($D$10*(E17-F17))/AC17)/1000,\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK(D17)=TRUE,\"\",(H17-I17)),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!B20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!AA20)","v":""},{"$f":"IF($AB17=\"mg/L\",1,IF($AB17=\"µg/L\",1000,IF($AB17=\"ng/L\",1000*1000,IF($AB17=\"µS/cm\",1000,\"\"))))","v":""}]
[null,2,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!B21)","v":""},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!H21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!J21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!F21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",D18*$D$10/AC18/1000)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",$D$10*E18/AC18/1000)","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",($D$10*(E18-F18))/AC18)/1000,\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK(D18)=TRUE,\"\",(H18-I18)),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!B21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!AA21)","v":""},{"$f":"IF($AB18=\"mg/L\",1,IF($AB18=\"µg/L\",1000,IF($AB18=\"ng/L\",1000*1000,IF($AB18=\"µS/cm\",1000,\"\"))))","v":""}]
[null,3,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!B22)","v":""},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!H22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!J22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!F22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",D19*$D$10/AC19/1000)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",$D$10*E19/AC19/1000)","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",($D$10*(E19-F19))/AC19)/1000,\"\")","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!B22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!AA22)","v":""},""]
[null,4,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!B23)","v":""},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!H23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!J23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!F23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",D20*$D$10/AC20/1000)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",$D$10*E20/AC20/1000)","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",($D$10*(E20-F20))/AC20)/1000,\"\")","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!B23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!AA23)","v":""},""]
[null,5,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!B24)","v":""},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!H24)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!J24)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!F24)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",D21*$D$10/AC21/1000)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",$D$10*E21/AC21/1000)","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",($D$10*(E21-F21))/AC21)/1000,\"\")","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!B24)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!AA24)","v":""},""]
[null,6,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!B25)","v":""},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!H25)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!J25)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!F25)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",D22*$D$10/AC22/1000)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",$D$10*E22/AC22/1000)","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",($D$10*(E22-F22))/AC22)/1000,\"\")","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!B25)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!AA25)","v":""},""]
[null,7,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!B26)","v":""},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!H26)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!J26)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!F26)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",D23*$D$10/AC23/1000)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",$D$10*E23/AC23/1000)","v":""},{"$f":"IFERROR(IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",($D$10*(E23-F23))/AC23)/1000,\"\")","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!B26)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!AA26)","v":""},""]
[null,null,null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B28)=TRUE,\"\",$D$10*E24/1000)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B28)=TRUE,\"\",($D$10*(E24-F24))/1000)","v":""},{"$f":"IFERROR(H24/1000,\"\")","v":""}]
[]
[]
[]
[]
[null,"3. Huidige maatregelen: Financiële informatie "]
[null,"CAPEX / Investeringskosten",null,null,null,"OPEX / Werkingskosten"]
[null,"Totale investeringskost huidige maatregelen",null,null,"EUR","Energie",null,null,"EUR/jaar"]
[null,null,null,null,null,"Chemiecaliën",null,null,"EUR/jaar"]
[null,null,null,null,null,"Verbruiksmateriaal",null,null,"EUR/jaar"]
[null,"Afschrijvingsperiode",null,10,"jaar","Manuren",null,null,"EUR/jaar"]
[null,"Rente",null,0.04,"%","Vervanging",null,null,"EUR/jaar"]
[null,null,null,null,null,"…",null,null,"EUR/jaar"]
[null,"Jaarlijkse kapitaalkost  (YCC)",null,{"$f":"IFERROR(-PMT(D35,D34,D31),0)","v":0},"EUR/jaar","OPEX ",null,{"$f":"SUM(H31:H36)","v":0},"EUR/jaar"]
[null,null,null,{"$f":"IFERROR(D37/D10,0)","v":0},"EUR/m³",null,null,{"$f":"IFERROR(H37/D10,0)","v":0},"EUR/m³"]
[]
[]
[null,"Totale kost huidige maatregelen (YCC + OPEX)",null,{"$f":"SUM(H37,D37)","v":0},"EUR/jaar"]
[null,null,null,{"$f":"IFERROR(D41/D10,0)","v":0},"EUR/m³"]

{"sheet":"Input overige investeringen","index":4,"n_rows":16,"n_cols":10,"rows_kept":16,"cut":false,"hidden":false,"merged":[[0,0,0,10],[1,0,1,10],[3,0,3,1],[8,9,8,10],[9,9,9,10],[6,1,6,4],[7,1,7,4],[8,1,8,4],[9,1,9,4],[2,0,2,10],[3,4,3,10],[4,4,4,10],[6,9,6,10],[7,9,7,10],[4,0,4,1],[5,0,5,10],[10,9,10,10],[14,9,14,10],[15,9,15,10],[11,1,11,4],[11,9,11,10],[12,1,12,4],[12,9,12,10],[13,1,13,4],[13,9,13,10],[15,0,15,4],[10,1,10,4],[14,1,14,4]]}
["1. Andere gelijktijdige investeringen i.k.v. impactbeoordeling afvalwater"]
["Indien er ook andere gelijktijdige investeringen nodig zijn in het kader van de impactbeoordeling afvalwater, dan kunnen deze hier worden weergegeven"]
[]
["Afschrijvingsperiode",null,10,"jaar"]
["Rente",null,0.04,"%"]
[]
["Nr","Omschrijving",null,null,null,"Capex (EUR)","Opex (EUR)","Baten (EUR)","YCC","Totale kost (=YCC+OPEX-baten)"]
[1,null,null,null,null,null,null,null,{"$f":"-PMT($C$5,$C$4,F8)","v":0},{"$f":"I8+G8-H8","v":0}]
[2,null,null,null,null,null,null,null,{"$f":"-PMT($C$5,$C$4,F9)","v":0},{"$f":"I9+G9-H9","v":0}]
[3,null,null,null,null,null,null,null,{"$f":"-PMT($C$5,$C$4,F10)","v":0},0]
[4,null,null,null,null,null,null,null,0,0]
[5,null,null,null,null,null,null,null,{"$f":"-PMT($C$5,$C$4,F12)","v":0},{"$f":"I12+G12-H12","v":0}]
[6,null,null,null,null,null,null,null,0,0]
[7,null,null,null,null,null,null,null,0,0]
[8,null,null,null,null,null,null,null,0,0]
["Totaal overige investeringen i.k.v. impactbeoordeling afvalwater",null,null,null,null,null,null,null,null,{"$f":"SUM(J8:K15)","v":0}]

{"sheet":"Dashboard beslissing","index":5,"n_rows":136,"n_cols":52,"rows_kept":136,"cut":false,"hidden":false,"merged":[[125,11,128,11],[125,12,128,12],[128,1,128,7],[131,1,131,2],[131,9,135,10],[132,11,135,11],[132,12,135,12],[126,1,126,2],[127,1,127,2],[133,1,133,2],[134,1,134,2],[31,9,31,10],[32,9,32,10],[33,9,33,10],[135,1,135,7],[132,1,132,2],[124,9,128,10],[37,6,37,8],[41,1,41,12],[35,9,35,10],[36,9,36,10],[37,9,37,10],[32,6,32,8],[33,6,33,8],[34,6,34,8],[35,6,35,8],[36,6,36,8],[1,1,1,12],[15,1,15,12],[28,1,28,12],[16,12,17,12],[29,12,30,12],[30,9,30,10],[2,6,2,10],[3,6,3,10],[4,6,4,10],[5,6,5,10],[6,6,6,10],[7,6,7,10],[8,6,8,10],[9,6,9,10],[10,6,10,10],[11,6,11,10],[54,12,57,12],[29,6,29,10],[99,2,99,10],[53,9,57,10],[62,1,62,12],[55,1,55,2],[57,1,57,7],[54,1,54,2],[53,1,53,2],[42,1,42,2],[43,1,43,2],[45,1,45,2],[30,6,30,8],[34,9,34,10],[46,9,50,10],[31,6,31,8],[103,1,103,12],[104,1,104,2],[105,1,105,2],[46,1,46,2],[47,1,47,2],[47,12,50,12],[76,1,76,3],[48,1,48,2],[50,1,50,7],[54,11,57,11],[47,11,50,11],[74,1,74,12],[86,1,86,3],[97,2,97,10],[56,1,56,2],[49,1,49,2],[107,1,107,2],[123,1,123,2],[124,1,124,2],[125,1,125,2],[108,1,108,3],[109,1,109,3],[119,1,119,3],[111,2,111,3],[112,2,112,3],[113,2,113,3],[114,2,114,3],[115,2,115,3],[116,2,116,3],[117,2,117,3],[118,2,118,3],[110,1,110,3]]}
[]
[null,"Overzicht: Aard van de impact en aanwijzing stofcategorie"]
[null,null,"Probleemparameter(s)",{"$f":"'Input impactbeoordeing'!D18","v":"Max. procentuele bijdrage parameter (%)"},{"$f":"'Input impactbeoordeing'!K18","v":"Waterrelevante stof Vlaanderen"},{"$f":"'Input impactbeoordeing'!AG18","v":"Waterbezwaarlijkheid"},null,null,null,null,null,"Code","Stof x impactcategorie",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Codering bijdrage","Codering speciale categorie","Codering duidelijke achteruitgang","Unieke code"]
[]
[null,1,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!B20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!D20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!K20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!AG20)","v":""},null,null,null,null,null,{"$f":"AI5","v":""},{"$f":"IFERROR(VLOOKUP(L5,'Matrix Stof x impact'!$I$2:$K$22,3,FALSE),\"\")","v":""},{"$f":"IF(M5=5,\"Geen verder onderzoek nodig, gelet op de stof x impactcategorie\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",IF(D5>='Matrix Stof x impact'!$B$32,'Matrix Stof x impact'!$C$32,IF(D5>='Matrix Stof x impact'!$B$33,'Matrix Stof x impact'!$C$33,IF(D5>='Matrix Stof x impact'!$B$34,'Matrix Stof x impact'!$C$34,IF(D5>='Matrix Stof x impact'!$B$35,'Matrix Stof x impact'!$C$35,'Matrix Stof x impact'!$C$36)))))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",IF(E5='Matrix Stof x impact'!$A$40,'Matrix Stof x impact'!$B$40,IF(E5='Matrix Stof x impact'!$A$41,'Matrix Stof x impact'!$B$41,\"ERROR\")))","v":""},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",IF(C5=\"\",\"\",SUM(AF5:AH5)))","v":""}]
[null,2,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!B21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!D21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!K21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!AG21)","v":""},null,null,null,null,null,{"$f":"AI6","v":""},{"$f":"IFERROR(VLOOKUP(L6,'Matrix Stof x impact'!$I$2:$K$22,3,FALSE),\"\")","v":""},{"$f":"IF(M6=5,\"Geen verder onderzoek nodig, gelet op de stof x impactcategorie\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",IF(D6>='Matrix Stof x impact'!$B$32,'Matrix Stof x impact'!$C$32,IF(D6>='Matrix Stof x impact'!$B$33,'Matrix Stof x impact'!$C$33,IF(D6>='Matrix Stof x impact'!$B$34,'Matrix Stof x impact'!$C$34,IF(D6>='Matrix Stof x impact'!$B$35,'Matrix Stof x impact'!$C$35,'Matrix Stof x impact'!$C$36)))))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",IF(E6='Matrix Stof x impact'!$A$40,'Matrix Stof x impact'!$B$40,IF(E6='Matrix Stof x impact'!$A$41,'Matrix Stof x impact'!$B$41,\"ERROR\")))","v":""},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",IF(C6=\"\",\"\",SUM(AF6:AH6)))","v":""}]
[null,3,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!B22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!D22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!K22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!AG22)","v":""},null,null,null,null,null,"",{"$f":"IFERROR(VLOOKUP(L7,'Matrix Stof x impact'!$I$2:$K$22,3,FALSE),\"\")","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",IF(D7>='Matrix Stof x impact'!$B$32,'Matrix Stof x impact'!$C$32,IF(D7>='Matrix Stof x impact'!$B$33,'Matrix Stof x impact'!$C$33,IF(D7>='Matrix Stof x impact'!$B$34,'Matrix Stof x impact'!$C$34,IF(D7>='Matrix Stof x impact'!$B$35,'Matrix Stof x impact'!$C$35,'Matrix Stof x impact'!$C$36)))))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",IF(E7='Matrix Stof x impact'!$A$40,'Matrix Stof x impact'!$B$40,IF(E7='Matrix Stof x impact'!$A$41,'Matrix Stof x impact'!$B$41,\"ERROR\")))","v":""},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",IF(C7=\"\",\"\",SUM(AF7:AH7)))","v":""}]
[null,4,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!B23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!D23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!K23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!AG23)","v":""},null,null,null,null,null,"",{"$f":"IFERROR(VLOOKUP(L8,'Matrix Stof x impact'!$I$2:$K$22,3,FALSE),\"\")","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",IF(D8>='Matrix Stof x impact'!$B$32,'Matrix Stof x impact'!$C$32,IF(D8>='Matrix Stof x impact'!$B$33,'Matrix Stof x impact'!$C$33,IF(D8>='Matrix Stof x impact'!$B$34,'Matrix Stof x impact'!$C$34,IF(D8>='Matrix Stof x impact'!$B$35,'Matrix Stof x impact'!$C$35,'Matrix Stof x impact'!$C$36)))))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",IF(E8='Matrix Stof x impact'!$A$40,'Matrix Stof x impact'!$B$40,IF(E8='Matrix Stof x impact'!$A$41,'Matrix Stof x impact'!$B$41,\"ERROR\")))","v":""},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",IF(C8=\"\",\"\",SUM(AF8:AH8)))","v":""}]
[null,5,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!B24)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!D24)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!K24)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!AG24)","v":""},null,null,null,null,null,"",{"$f":"IFERROR(VLOOKUP(L9,'Matrix Stof x impact'!$I$2:$K$22,3,FALSE),\"\")","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",IF(D9>='Matrix Stof x impact'!$B$32,'Matrix Stof x impact'!$C$32,IF(D9>='Matrix Stof x impact'!$B$33,'Matrix Stof x impact'!$C$33,IF(D9>='Matrix Stof x impact'!$B$34,'Matrix Stof x impact'!$C$34,IF(D9>='Matrix Stof x impact'!$B$35,'Matrix Stof x impact'!$C$35,'Matrix Stof x impact'!$C$36)))))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",IF(E9='Matrix Stof x impact'!$A$40,'Matrix Stof x impact'!$B$40,IF(E9='Matrix Stof x impact'!$A$41,'Matrix Stof x impact'!$B$41,\"ERROR\")))","v":""},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",IF(C9=\"\",\"\",SUM(AF9:AH9)))","v":""}]
[null,6,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!B25)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!D25)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!K25)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!AG25)","v":""},null,null,null,null,null,"",{"$f":"IFERROR(VLOOKUP(L10,'Matrix Stof x impact'!$I$2:$K$22,3,FALSE),\"\")","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",IF(D10>='Matrix Stof x impact'!$B$32,'Matrix Stof x impact'!$C$32,IF(D10>='Matrix Stof x impact'!$B$33,'Matrix Stof x impact'!$C$33,IF(D10>='Matrix Stof x impact'!$B$34,'Matrix Stof x impact'!$C$34,IF(D10>='Matrix Stof x impact'!$B$35,'Matrix Stof x impact'!$C$35,'Matrix Stof x impact'!$C$36)))))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",IF(E10='Matrix Stof x impact'!$A$40,'Matrix Stof x impact'!$B$40,IF(E10='Matrix Stof x impact'!$A$41,'Matrix Stof x impact'!$B$41,\"ERROR\")))","v":""},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",IF(C10=\"\",\"\",SUM(AF10:AH10)))","v":""}]
[null,7,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!B26)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!D26)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!K26)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!AG26)","v":""},null,null,null,null,null,"",{"$f":"IFERROR(VLOOKUP(L11,'Matrix Stof x impact'!$I$2:$K$22,3,FALSE),\"\")","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",IF(D11>='Matrix Stof x impact'!$B$32,'Matrix Stof x impact'!$C$32,IF(D11>='Matrix Stof x impact'!$B$33,'Matrix Stof x impact'!$C$33,IF(D11>='Matrix Stof x impact'!$B$34,'Matrix Stof x impact'!$C$34,IF(D11>='Matrix Stof x impact'!$B$35,'Matrix Stof x impact'!$C$35,'Matrix Stof x impact'!$C$36)))))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",IF(E11='Matrix Stof x impact'!$A$40,'Matrix Stof x impact'!$B$40,IF(E11='Matrix Stof x impact'!$A$41,'Matrix Stof x impact'!$B$41,\"ERROR\")))","v":""},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",IF(C11=\"\",\"\",SUM(AF11:AH11)))","v":""}]
[]
[]
[]
[]
[null,"Criterium 1: Bereiken verbeterdoelstelling  - streefwaarde impactbeoordeling"]
[null,null,"Probleemparameter(s)","Eenheid",{"$f":"'Input impactbeoordeing'!J18","v":"Gewenste effluentconcentratie impactbeoordeling afvalwater"},"Effluentconcentratie na implementatie bijkomende maatregelen","Verwijderde vuilvracht door bijkomende maatregel","Verwijderingsrendement maatregel","Finaal geloosd volume ","Initieel geloosd volume water",null,"Code opmaak","Beoordeling"]
[null,null,null,null,null,null,"kg/jaar","%","m³/jaar","m³/jaar"]
[null,1,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!B20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!F20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!J20)","v":""},{"$f":"IF(C19=\"\",\"\",'Input bijkomende maatregelen'!F27)","v":""},{"$f":"IF(C19=\"\",\"\",'Input bijkomende maatregelen'!I27)","v":""},{"$f":"IFERROR(('Input impactbeoordeing'!AC20-'Input bijkomende maatregelen'!J27)/'Input impactbeoordeing'!AC20,\"\")","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input bijkomende maatregelen'!$D$15)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!$C$9)","v":""},null,{"$f":"IFERROR(IF(F19<=(E19/2),Expressielijsten!$D$6,IF(F19<=E19,Expressielijsten!$D$7,IF(AND(F19>E19,H19>0.75),Expressielijsten!$D$8,Expressielijsten!$D$9))),\"\")","v":""},{"$f":"IFERROR(IF(F19<=(E19/2),Expressielijsten!$B$6,IF(F19<=E19,Expressielijsten!$B$7,IF(AND(F19>E19,H19>0.75),Expressielijsten!$B$8,Expressielijsten!$B$9))),\"\")","v":""}]
[null,2,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!B21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!F21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!J21)","v":""},{"$f":"IF(C20=\"\",\"\",'Input bijkomende maatregelen'!F28)","v":""},{"$f":"IF(C20=\"\",\"\",'Input bijkomende maatregelen'!I28)","v":""},{"$f":"IFERROR(('Input impactbeoordeing'!AC21-'Input bijkomende maatregelen'!J28)/'Input impactbeoordeing'!AC21,\"\")","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input bijkomende maatregelen'!$D$15)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!$C$9)","v":""},null,{"$f":"IFERROR(IF(F20<=(E20/2),Expressielijsten!$D$6,IF(F20<=E20,Expressielijsten!$D$7,IF(AND(F20>E20,H20>0.75),Expressielijsten!$D$8,Expressielijsten!$D$9))),\"\")","v":""},{"$f":"IFERROR(IF(F20<=(E20/2),Expressielijsten!$B$6,IF(F20<=E20,Expressielijsten!$B$7,IF(AND(F20>E20,H20>0.75),Expressielijsten!$B$8,Expressielijsten!$B$9))),\"\")","v":""}]
[null,3,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!B22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!F22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!J22)","v":""},{"$f":"IF(C21=\"\",\"\",'Input bijkomende maatregelen'!F29)","v":""},{"$f":"IF(C21=\"\",\"\",'Input bijkomende maatregelen'!I29)","v":""},{"$f":"IFERROR(('Input impactbeoordeing'!AC22-'Input bijkomende maatregelen'!J29)/'Input impactbeoordeing'!AC22,\"\")","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input bijkomende maatregelen'!$D$15)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!$C$9)","v":""},null,{"$f":"IFERROR(IF(F21<=(E21/2),Expressielijsten!$D$6,IF(F21<=E21,Expressielijsten!$D$7,IF(AND(F21>E21,H21>0.75),Expressielijsten!$D$8,Expressielijsten!$D$9))),\"\")","v":""},{"$f":"IFERROR(IF(F21<=(E21/2),Expressielijsten!$B$6,IF(F21<=E21,Expressielijsten!$B$7,IF(AND(F21>E21,H21>0.75),Expressielijsten!$B$8,Expressielijsten!$B$9))),\"\")","v":""}]
[null,4,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!B23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!F23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!J23)","v":""},{"$f":"IF(C22=\"\",\"\",'Input bijkomende maatregelen'!F30)","v":""},{"$f":"IF(C22=\"\",\"\",'Input bijkomende maatregelen'!I30)","v":""},{"$f":"IFERROR(('Input impactbeoordeing'!AC23-'Input bijkomende maatregelen'!J30)/'Input impactbeoordeing'!AC23,\"\")","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input bijkomende maatregelen'!$D$15)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!$C$9)","v":""},null,{"$f":"IFERROR(IF(F22<=(E22/2),Expressielijsten!$D$6,IF(F22<=E22,Expressielijsten!$D$7,IF(AND(F22>E22,H22>0.75),Expressielijsten!$D$8,Expressielijsten!$D$9))),\"\")","v":""},{"$f":"IFERROR(IF(F22<=(E22/2),Expressielijsten!$B$6,IF(F22<=E22,Expressielijsten!$B$7,IF(AND(F22>E22,H22>0.75),Expressielijsten!$B$8,Expressielijsten!$B$9))),\"\")","v":""}]
[null,5,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!B24)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!F24)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!J24)","v":""},{"$f":"IF(C23=\"\",\"\",'Input bijkomende maatregelen'!F31)","v":""},{"$f":"IF(C23=\"\",\"\",'Input bijkomende maatregelen'!I31)","v":""},{"$f":"IFERROR(('Input impactbeoordeing'!AC24-'Input bijkomende maatregelen'!J31)/'Input impactbeoordeing'!AC24,\"\")","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input bijkomende maatregelen'!$D$15)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!$C$9)","v":""},null,{"$f":"IFERROR(IF(F23<=(E23/2),Expressielijsten!$D$6,IF(F23<=E23,Expressielijsten!$D$7,IF(AND(F23>E23,H23>0.75),Expressielijsten!$D$8,Expressielijsten!$D$9))),\"\")","v":""},{"$f":"IFERROR(IF(F23<=(E23/2),Expressielijsten!$B$6,IF(F23<=E23,Expressielijsten!$B$7,IF(AND(F23>E23,H23>0.75),Expressielijsten!$B$8,Expressielijsten!$B$9))),\"\")","v":""}]
[null,6,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!B25)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!F25)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!J25)","v":""},{"$f":"IF(C24=\"\",\"\",'Input bijkomende maatregelen'!F32)","v":""},{"$f":"IF(C24=\"\",\"\",'Input bijkomende maatregelen'!I32)","v":""},{"$f":"IFERROR(('Input impactbeoordeing'!AC25-'Input bijkomende maatregelen'!J32)/'Input impactbeoordeing'!AC25,\"\")","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input bijkomende maatregelen'!$D$15)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!$C$9)","v":""},null,{"$f":"IFERROR(IF(F24<=(E24/2),Expressielijsten!$D$6,IF(F24<=E24,Expressielijsten!$D$7,IF(AND(F24>E24,H24>0.75),Expressielijsten!$D$8,Expressielijsten!$D$9))),\"\")","v":""},{"$f":"IFERROR(IF(F24<=(E24/2),Expressielijsten!$B$6,IF(F24<=E24,Expressielijsten!$B$7,IF(AND(F24>E24,H24>0.75),Expressielijsten!$B$8,Expressielijsten!$B$9))),\"\")","v":""}]
[null,7,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!B26)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!F26)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!J26)","v":""},{"$f":"IF(C25=\"\",\"\",'Input bijkomende maatregelen'!F33)","v":""},{"$f":"IF(C25=\"\",\"\",'Input bijkomende maatregelen'!I33)","v":""},{"$f":"IFERROR(('Input impactbeoordeing'!AC26-'Input bijkomende maatregelen'!J33)/'Input impactbeoordeing'!AC26,\"\")","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input bijkomende maatregelen'!$D$15)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!$C$9)","v":""},null,{"$f":"IFERROR(IF(F25<=(E25/2),Expressielijsten!$D$6,IF(F25<=E25,Expressielijsten!$D$7,IF(AND(F25>E25,H25>0.75),Expressielijsten!$D$8,Expressielijsten!$D$9))),\"\")","v":""},{"$f":"IFERROR(IF(F25<=(E25/2),Expressielijsten!$B$6,IF(F25<=E25,Expressielijsten!$B$7,IF(AND(F25>E25,H25>0.75),Expressielijsten!$B$8,Expressielijsten!$B$9))),\"\")","v":""}]
[]
[]
[]
[null,"Criterium 2: Kosteneffectiviteit saneringstechniek",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Berekening KE BBT model"]
[null,null,"Probleemparameter(s)","Stof x impactcategorie","KE bijkomende maatregel",{"$f":"AS30","v":"Toetscriterium KE "},"Duiding toetscriterium",null,null,null,null,null,"Beoordeling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Berekening KE BBT (alg)",null,"Berekening BBT+ (alg)",null,"Afwijking BBT",null,null,"Stofcategorie","BBT (na index)","BBT+ (na index)","BBT/BBT+ toetscriteria","Toetscriterium KE ","Expressie toetscriterium",null,null,null,null,"Index consumptieprijzen horende bij BBT NL model (BJ 2013 = 100)"]
[null,null,null,null,"EUR/kg",{"$f":"AS31","v":"EUR/kg"},null,null,null,null,null,"Code opmaak",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stof","Bezwaarlijkheid stof","Bezwaarlijkheid < 0.01","Bezwaarlijkheid >= 0.01","Bezwaarlijkheid < 0.01","Bezwaarlijkheid >= 0.01","BBT afwijkend","BBT","BBT+",null,null,null,null,"EUR/kg",null,null,null,null,null,"2018-01-01",106.22]
[null,1,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!B20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",M5)","v":""},{"$f":"'Samenvatting econ kengetallen'!F44","v":""},{"$error":"#VALUE!"},{"$f":"AR32","v":"Geen toetsing vereist - Cat 3"},null,null,{"$f":"AT32","v":"KE afgeleid uit NL model"},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",IF(AR32=\"Bovenste kostencurve\",IF(E32<AQ32,IF(E32<AP32,Expressielijsten!$D$18,Expressielijsten!$D$14),Expressielijsten!$D$15),IF(E32<F32,Expressielijsten!$D$16,Expressielijsten!$D$17)))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",IF(AR32=\"Bovenste kostencurve\",IF(E32<AQ32,IF(E32<AP32,Expressielijsten!$B$18,Expressielijsten!$B$14),Expressielijsten!$B$15),IF(E32<F32,Expressielijsten!$B$16,Expressielijsten!$B$17)))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"C32","v":""},{"$f":"F5","v":""},{"$f":"198282.668*AG32^1.148887","v":{"$error":"#VALUE!"}},{"$f":"660.23*LN(AG32)+3948.9","v":{"$error":"#VALUE!"}},{"$f":"1982826.68*AG32^1.148887","v":{"$error":"#VALUE!"}},{"$f":"6602.3*LN(AG32)+39489","v":{"$error":"#VALUE!"}},{"$f":"VLOOKUP($AF32,'Keuzelijst parameters'!$R$1:$U$378,2,FALSE)","v":0},{"$f":"IF(AL32=\"Ja\",VLOOKUP($AF32,'Keuzelijst parameters'!$R$1:$U$378,3,FALSE),\"\")","v":""},{"$f":"IF(AL32=\"Ja\",VLOOKUP($AF32,'Keuzelijst parameters'!$R$1:$U$378,4,FALSE),\"\")","v":""},{"$f":"IF(C5=\"\",\"\",M5)","v":""},{"$f":"IF(AL32=\"ja\",AM32,IF(AG32<0.01,AH32,AI32))*$AZ$32/$AZ$31","v":{"$error":"#VALUE!"}},{"$f":"IF(AL32=\"ja\",AN32,IF(AG32<0.01,AJ32,AK32))*$AZ$32/$AZ$31","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(VLOOKUP(AO32,'Criteria volgens stofcategorie'!$G$4:$AB$7,22,FALSE),\"Geen toetsing vereist - Cat 3\")","v":"Geen toetsing vereist - Cat 3"},{"$f":"IF(AO32=1,AQ32,AP32)","v":{"$error":"#VALUE!"}},{"$f":"IF(AL32=\"ja\",Expressielijsten!$B$23,Expressielijsten!$B$24)","v":"KE afgeleid uit NL model"},null,null,null,null,"Ingegeven index",{"$f":"'Input impactbeoordeing'!A31","v":134.44}]
[null,2,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!B21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",M6)","v":""},{"$f":"'Samenvatting econ kengetallen'!F45","v":""},{"$error":"#VALUE!"},{"$f":"AR33","v":"Geen toetsing vereist - Cat 3"},null,null,{"$f":"AT33","v":"KE afgeleid uit NL model"},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",IF(AR33=\"Bovenste kostencurve\",IF(E33<AQ33,IF(E33<AP33,Expressielijsten!$D$18,Expressielijsten!$D$14),Expressielijsten!$D$15),IF(E33<F33,Expressielijsten!$D$16,Expressielijsten!$D$17)))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",IF(AR33=\"Bovenste kostencurve\",IF(E33<AQ33,IF(E33<AP33,Expressielijsten!$B$18,Expressielijsten!$B$14),Expressielijsten!$B$15),IF(E33<F33,Expressielijsten!$B$16,Expressielijsten!$B$17)))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"198282.668*AG33^1.148887","v":{"$error":"#VALUE!"}},{"$f":"660.23*LN(AG33)+3948.9","v":{"$error":"#VALUE!"}},{"$f":"1982826.68*AG33^1.148887","v":{"$error":"#VALUE!"}},{"$f":"6602.3*LN(AG33)+39489","v":{"$error":"#VALUE!"}},{"$f":"VLOOKUP($AF33,'Keuzelijst parameters'!$R$1:$U$378,2,FALSE)","v":0},{"$f":"IF(AL33=\"Ja\",VLOOKUP($AF33,'Keuzelijst parameters'!$R$1:$U$378,3,FALSE),\"\")","v":""},{"$f":"IF(AL33=\"Ja\",VLOOKUP($AF33,'Keuzelijst parameters'!$R$1:$U$378,4,FALSE),\"\")","v":""},"",{"$f":"IF(AL33=\"ja\",AM33,IF(AG33<0.01,AH33,AI33))*$AZ$32/$AZ$31","v":{"$error":"#VALUE!"}},{"$f":"IF(AL33=\"ja\",AN33,IF(AG33<0.01,AJ33,AK33))*$AZ$32/$AZ$31","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(VLOOKUP(AO33,'Criteria volgens stofcategorie'!$G$4:$AB$7,22,FALSE),\"Geen toetsing vereist - Cat 3\")","v":"Geen toetsing vereist - Cat 3"},{"$f":"IF(AO33=1,AQ33,AP33)","v":{"$error":"#VALUE!"}},{"$f":"IF(AL33=\"ja\",Expressielijsten!$B$23,Expressielijsten!$B$24)","v":"KE afgeleid uit NL model"}]
[null,3,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!B22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",M7)","v":""},{"$f":"'Samenvatting econ kengetallen'!F46","v":""},{"$error":"#VALUE!"},"Geen toetsing vereist - Cat 3",null,null,"KE afgeleid uit NL model",null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",IF(AR34=\"Bovenste kostencurve\",IF(E34<AQ34,IF(E34<AP34,Expressielijsten!$D$18,Expressielijsten!$D$14),Expressielijsten!$D$15),IF(E34<F34,Expressielijsten!$D$16,Expressielijsten!$D$17)))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",IF(AR34=\"Bovenste kostencurve\",IF(E34<AQ34,IF(E34<AP34,Expressielijsten!$B$18,Expressielijsten!$B$14),Expressielijsten!$B$15),IF(E34<F34,Expressielijsten!$B$16,Expressielijsten!$B$17)))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP($AF34,'Keuzelijst parameters'!$R$1:$U$378,2,FALSE)","v":0},{"$f":"IF(AL34=\"Ja\",VLOOKUP($AF34,'Keuzelijst parameters'!$R$1:$U$378,3,FALSE),\"\")","v":""},{"$f":"IF(AL34=\"Ja\",VLOOKUP($AF34,'Keuzelijst parameters'!$R$1:$U$378,4,FALSE),\"\")","v":""},"",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IFERROR(VLOOKUP(AO34,'Criteria volgens stofcategorie'!$G$4:$AB$7,22,FALSE),\"Geen toetsing vereist - Cat 3\")","v":"Geen toetsing vereist - Cat 3"},{"$error":"#VALUE!"},{"$f":"IF(AL34=\"ja\",Expressielijsten!$B$23,Expressielijsten!$B$24)","v":"KE afgeleid uit NL model"}]
[null,4,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!B23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",M8)","v":""},{"$f":"'Samenvatting econ kengetallen'!F47","v":""},{"$error":"#VALUE!"},"Geen toetsing vereist - Cat 3",null,null,"KE afgeleid uit NL model",null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",IF(AR35=\"Bovenste kostencurve\",IF(E35<AQ35,IF(E35<AP35,Expressielijsten!$D$18,Expressielijsten!$D$14),Expressielijsten!$D$15),IF(E35<F35,Expressielijsten!$D$16,Expressielijsten!$D$17)))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",IF(AR35=\"Bovenste kostencurve\",IF(E35<AQ35,IF(E35<AP35,Expressielijsten!$B$18,Expressielijsten!$B$14),Expressielijsten!$B$15),IF(E35<F35,Expressielijsten!$B$16,Expressielijsten!$B$17)))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP($AF35,'Keuzelijst parameters'!$R$1:$U$378,2,FALSE)","v":0},{"$f":"IF(AL35=\"Ja\",VLOOKUP($AF35,'Keuzelijst parameters'!$R$1:$U$378,3,FALSE),\"\")","v":""},{"$f":"IF(AL35=\"Ja\",VLOOKUP($AF35,'Keuzelijst parameters'!$R$1:$U$378,4,FALSE),\"\")","v":""},"",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IFERROR(VLOOKUP(AO35,'Criteria volgens stofcategorie'!$G$4:$AB$7,22,FALSE),\"Geen toetsing vereist - Cat 3\")","v":"Geen toetsing vereist - Cat 3"},{"$error":"#VALUE!"},{"$f":"IF(AL35=\"ja\",Expressielijsten!$B$23,Expressielijsten!$B$24)","v":"KE afgeleid uit NL model"}]
[null,5,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!B24)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",M9)","v":""},{"$f":"'Samenvatting econ kengetallen'!F48","v":""},{"$error":"#VALUE!"},"Geen toetsing vereist - Cat 3",null,null,"KE afgeleid uit NL model",null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",IF(AR36=\"Bovenste kostencurve\",IF(E36<AQ36,IF(E36<AP36,Expressielijsten!$D$18,Expressielijsten!$D$14),Expressielijsten!$D$15),IF(E36<F36,Expressielijsten!$D$16,Expressielijsten!$D$17)))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",IF(AR36=\"Bovenste kostencurve\",IF(E36<AQ36,IF(E36<AP36,Expressielijsten!$B$18,Expressielijsten!$B$14),Expressielijsten!$B$15),IF(E36<F36,Expressielijsten!$B$16,Expressielijsten!$B$17)))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP($AF36,'Keuzelijst parameters'!$R$1:$U$378,2,FALSE)","v":0},{"$f":"IF(AL36=\"Ja\",VLOOKUP($AF36,'Keuzelijst parameters'!$R$1:$U$378,3,FALSE),\"\")","v":""},{"$f":"IF(AL36=\"Ja\",VLOOKUP($AF36,'Keuzelijst parameters'!$R$1:$U$378,4,FALSE),\"\")","v":""},"",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IFERROR(VLOOKUP(AO36,'Criteria volgens stofcategorie'!$G$4:$AB$7,22,FALSE),\"Geen toetsing vereist - Cat 3\")","v":"Geen toetsing vereist - Cat 3"},{"$error":"#VALUE!"},{"$f":"IF(AL36=\"ja\",Expressielijsten!$B$23,Expressielijsten!$B$24)","v":"KE afgeleid uit NL model"}]
[null,6,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!B25)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",M10)","v":""},{"$f":"'Samenvatting econ kengetallen'!F49","v":""},{"$error":"#VALUE!"},"Geen toetsing vereist - Cat 3",null,null,"KE afgeleid uit NL model",null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",IF(AR37=\"Bovenste kostencurve\",IF(E37<AQ37,IF(E37<AP37,Expressielijsten!$D$18,Expressielijsten!$D$14),Expressielijsten!$D$15),IF(E37<F37,Expressielijsten!$D$16,Expressielijsten!$D$17)))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",IF(AR37=\"Bovenste kostencurve\",IF(E37<AQ37,IF(E37<AP37,Expressielijsten!$B$18,Expressielijsten!$B$14),Expressielijsten!$B$15),IF(E37<F37,Expressielijsten!$B$16,Expressielijsten!$B$17)))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP($AF37,'Keuzelijst parameters'!$R$1:$U$378,2,FALSE)","v":0},{"$f":"IF(AL37=\"Ja\",VLOOKUP($AF37,'Keuzelijst parameters'!$R$1:$U$378,3,FALSE),\"\")","v":""},{"$f":"IF(AL37=\"Ja\",VLOOKUP($AF37,'Keuzelijst parameters'!$R$1:$U$378,4,FALSE),\"\")","v":""},"",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IFERROR(VLOOKUP(AO37,'Criteria volgens stofcategorie'!$G$4:$AB$7,22,FALSE),\"Geen toetsing vereist - Cat 3\")","v":"Geen toetsing vereist - Cat 3"},{"$error":"#VALUE!"},{"$f":"IF(AL37=\"ja\",Expressielijsten!$B$23,Expressielijsten!$B$24)","v":"KE afgeleid uit NL model"}]
[null,7,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!B26)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",M11)","v":""},{"$f":"'Samenvatting econ kengetallen'!F50","v":""},{"$error":"#VALUE!"},"Geen toetsing vereist - Cat 3",null,null,"KE afgeleid uit NL model",null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",IF(AR38=\"Bovenste kostencurve\",IF(E38<AQ38,IF(E38<AP38,Expressielijsten!$D$18,Expressielijsten!$D$14),Expressielijsten!$D$15),IF(E38<F38,Expressielijsten!$D$16,Expressielijsten!$D$17)))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",IF(AR38=\"Bovenste kostencurve\",IF(E38<AQ38,IF(E38<AP38,Expressielijsten!$B$18,Expressielijsten!$B$14),Expressielijsten!$B$15),IF(E38<F38,Expressielijsten!$B$16,Expressielijsten!$B$17)))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"198282.668*AG38^1.148887","v":{"$error":"#VALUE!"}},{"$f":"660.23*LN(AG38)+3948.9","v":{"$error":"#VALUE!"}},{"$f":"1982826.68*AG38^1.148887","v":{"$error":"#VALUE!"}},{"$f":"6602.3*LN(AG38)+39489","v":{"$error":"#VALUE!"}},{"$f":"VLOOKUP($AF38,'Keuzelijst parameters'!$R$1:$U$378,2,FALSE)","v":0},{"$f":"IF(AL38=\"Ja\",VLOOKUP($AF38,'Keuzelijst parameters'!$R$1:$U$378,3,FALSE),\"\")","v":""},{"$f":"IF(AL38=\"Ja\",VLOOKUP($AF38,'Keuzelijst parameters'!$R$1:$U$378,4,FALSE),\"\")","v":""},"",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IFERROR(VLOOKUP(AO38,'Criteria volgens stofcategorie'!$G$4:$AB$7,22,FALSE),\"Geen toetsing vereist - Cat 3\")","v":"Geen toetsing vereist - Cat 3"},{"$error":"#VALUE!"},{"$f":"IF(AL38=\"ja\",Expressielijsten!$B$23,Expressielijsten!$B$24)","v":"KE afgeleid uit NL model"}]
[]
[]
[]
[null,"Criterium 3: Economische draagkracht bedrijf"]
[null,"Categorie stof met hoogste impact",null,{"$f":"MIN(M5:M10)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lijst selectie"]
[null,"Toetscriterium stof met hoogste impact",null,{"$f":"VLOOKUP(D43,'Criteria volgens stofcategorie'!$G$3:$AB$7,22,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vestiging & Holding"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vestiging"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Holding"]
[null,"Holding",null,"Financiële data van de holding","Bijkomende maatregel \n(opex + ycc - baten)","Ratio","Criteria aanvaardbaar","Criteria intermediair bovengrens","Code",null,null,"Code opmaak","Beoordeling"]
[null,"Omzet",null,{"$f":"IFERROR('Samenvatting econ kengetallen'!$G$79,\"Nog niet ingevuld\")","v":"Nog niet ingevuld"},{"$f":"'Samenvatting econ kengetallen'!$B$25","v":0},{"$f":"E48/D48","v":{"$error":"#VALUE!"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,10,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,12,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(F48<G48,Expressielijsten!$B$30,IF(F48<(H48+G48)/2,Expressielijsten!$B$31,IF(F48>=H48,Expressielijsten!$B$33,Expressielijsten!$B$32)))","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(D43=1,VLOOKUP(I51,Expressielijsten!A53:E117,5,FALSE),VLOOKUP(I51,Expressielijsten!A53:E117,4,FALSE))","v":{"$error":"#VALUE!"}},{"$f":"IF(D43=1,VLOOKUP(I51,Expressielijsten!A53:C117,3,FALSE),VLOOKUP(I51,Expressielijsten!A53:C117,2,FALSE))","v":{"$error":"#VALUE!"}}]
[null,"Toegevoegde waarde",null,{"$f":"IFERROR('Samenvatting econ kengetallen'!$G$80,\"Nog niet ingevuld\")","v":"Nog niet ingevuld"},{"$f":"'Samenvatting econ kengetallen'!$B$25","v":0},{"$f":"IF(D49<=0,1,E49/D49)","v":{"$error":"#VALUE!"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,14,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,16,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(F49<G49,Expressielijsten!$B$37,IF(F49<(H49+G49)/2,Expressielijsten!$B$38,IF(F49>=H49,Expressielijsten!$B$40,Expressielijsten!$B$39)))","v":{"$error":"#VALUE!"}}]
[null,"EBITDA",null,{"$f":"IFERROR('Samenvatting econ kengetallen'!$G$81,\"Nog niet ingevuld\")","v":"Nog niet ingevuld"},{"$f":"'Samenvatting econ kengetallen'!$B$25","v":0},{"$f":"IF(D50<=0,1,E50/D50)","v":{"$error":"#VALUE!"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,18,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,20,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(F50<G50,Expressielijsten!$B$44,IF(F50<(H50+G50)/2,Expressielijsten!$B$45,IF(F50>=H50,Expressielijsten!$B$47,Expressielijsten!$B$46)))","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,{"$f":"I48+I49+I50","v":{"$error":"#VALUE!"}}]
[]
[]
[null,"Vestiging",null,"Financiële data van de vestiging","Bijkomende maatregel \n(opex + ycc - baten)","Ratio","Criteria aanvaardbaar","Criteria intermediair bovengrens","Code",null,null,"Code opmaak","Beoordeling"]
[null,"Omzet",null,{"$f":"IFERROR('Samenvatting econ kengetallen'!$G$70,\"Nog niet ingevuld\")","v":"Nog niet ingevuld"},{"$f":"'Samenvatting econ kengetallen'!$B$25","v":0},{"$f":"E55/D55","v":{"$error":"#VALUE!"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,10,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,12,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(F55<G55,Expressielijsten!$B$30,IF(F55<(H55+G55)/2,Expressielijsten!$B$31,IF(F55>=H55,Expressielijsten!$B$33,Expressielijsten!$B$32)))","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(D43=1,VLOOKUP(I58,Expressielijsten!A53:E117,5,FALSE),VLOOKUP(I58,Expressielijsten!A53:E117,4,FALSE))","v":{"$error":"#VALUE!"}},{"$f":"IF(D43=1,VLOOKUP(I58,Expressielijsten!A53:C117,3,FALSE),VLOOKUP(I58,Expressielijsten!A53:C117,2,FALSE))","v":{"$error":"#VALUE!"}}]
[null,"Toegevoegde waarde",null,{"$f":"IFERROR('Samenvatting econ kengetallen'!$G$71,\"Nog niet ingevuld\")","v":"Nog niet ingevuld"},{"$f":"'Samenvatting econ kengetallen'!$B$25","v":0},{"$f":"IF(D56<=0,1,E56/D56)","v":{"$error":"#VALUE!"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,14,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,16,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(F56<G56,Expressielijsten!$B$37,IF(F56<(H56+G56)/2,Expressielijsten!$B$38,IF(F56>=H56,Expressielijsten!$B$40,Expressielijsten!$B$39)))","v":{"$error":"#VALUE!"}}]
[null,"EBITDA",null,{"$f":"IFERROR('Samenvatting econ kengetallen'!$G$72,\"Nog niet ingevuld\")","v":"Nog niet ingevuld"},{"$f":"'Samenvatting econ kengetallen'!$B$25","v":0},{"$f":"IF(D57<=0,1,E57/D57)","v":{"$error":"#VALUE!"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,18,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,20,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(F57<G57,Expressielijsten!$B$44,IF(F57<(H57+G57)/2,Expressielijsten!$B$45,IF(F57>=H57,Expressielijsten!$B$47,Expressielijsten!$B$46)))","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,{"$f":"I55+I56+I57","v":{"$error":"#VALUE!"}}]
[]
[]
[]
[]
[null,"Criterium 4: Vergelijking t.o.v. huidige maatregelen"]
[null,null,"Probleemparameter(s)","Totale vuilvracht ","Verwijderde vuilvracht huidige maatregelen","Verwijderde vuilvracht bijkomende maatregelen","Bijdrage bestaande maatregelen aan halen doelstelling toegestane vuilvracht","Bijdrage bijkomende maatregelen aan halen doelstelling toegestane vuilvracht","Toegestane vuilvracht","KE bestaande maatregel","KE bijkomende maatregelen",null,"Beoordeling"]
[null,null,null,"kg/jaar","kg/jaar","kg/jaar","%","%","kg/jaar","EUR/kg","EUR/kg"]
[null,1,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!B20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",IF(ISBLANK('Input huidige maatreg. (fac.)'!D17)=TRUE,\"Inkomende vuilvracht niet gespecifieerd\",'Input huidige maatreg. (fac.)'!H17))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",IF(ISBLANK('Input huidige maatreg. (fac.)'!D17)=TRUE,\"Inkomende vuilvracht niet gespecifieerd\",'Input huidige maatreg. (fac.)'!K17))","v":""},{"$f":"'Input bijkomende maatregelen'!I27","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",IFERROR(E66/(D66-I66),\"Inkomende vuilvracht niet gespecifieerd\"))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",IFERROR(F66/(D66-I66),\"Inkomende vuilvracht niet gespecifieerd\"))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!AD20)","v":""},{"$f":"'Samenvatting econ kengetallen'!C44","v":""},{"$f":"E32","v":""},null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",_xlfn.CONCAT(IF(G66=\"Inkomende vuilvracht niet gespecifieerd\",\"\",IF(H66>G66,Expressielijsten!$B$122,Expressielijsten!$B$123)),\"; \",IF(K66<J66,Expressielijsten!$B$124,Expressielijsten!$B$125)))","v":""}]
[null,2,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!B21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",IF(ISBLANK('Input huidige maatreg. (fac.)'!D18)=TRUE,\"Inkomende vuilvracht niet gespecifieerd\",'Input huidige maatreg. (fac.)'!H18))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",IF(ISBLANK('Input huidige maatreg. (fac.)'!D18)=TRUE,\"Inkomende vuilvracht niet gespecifieerd\",'Input huidige maatreg. (fac.)'!K18))","v":""},{"$f":"'Input bijkomende maatregelen'!I28","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",IFERROR(E67/(D67-I67),\"Inkomende vuilvracht niet gespecifieerd\"))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",IFERROR(F67/(D67-I67),\"Inkomende vuilvracht niet gespecifieerd\"))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!AD21)","v":""},{"$f":"'Samenvatting econ kengetallen'!C45","v":""},"",null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",_xlfn.CONCAT(IF(G67=\"Inkomende vuilvracht niet gespecifieerd\",\"\",IF(H67>G67,Expressielijsten!$B$122,Expressielijsten!$B$123)),\"; \",IF(K67<J67,Expressielijsten!$B$124,Expressielijsten!$B$125)))","v":""}]
[null,3,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!B22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",IF(ISBLANK('Input huidige maatreg. (fac.)'!D19)=TRUE,\"Inkomende vuilvracht niet gespecifieerd\",'Input huidige maatreg. (fac.)'!H19))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",IF(ISBLANK('Input huidige maatreg. (fac.)'!D19)=TRUE,\"Inkomende vuilvracht niet gespecifieerd\",'Input huidige maatreg. (fac.)'!K19))","v":""},{"$f":"'Input bijkomende maatregelen'!I29","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",IFERROR(E68/(D68-I68),\"Inkomende vuilvracht niet gespecifieerd\"))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",IFERROR(F68/(D68-I68),\"Inkomende vuilvracht niet gespecifieerd\"))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!AD22)","v":""},{"$f":"'Samenvatting econ kengetallen'!C46","v":""},"",null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",_xlfn.CONCAT(IF(G68=\"Inkomende vuilvracht niet gespecifieerd\",\"\",IF(H68>G68,Expressielijsten!$B$122,Expressielijsten!$B$123)),\"; \",IF(K68<J68,Expressielijsten!$B$124,Expressielijsten!$B$125)))","v":""}]
[null,4,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!B23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",IF(ISBLANK('Input huidige maatreg. (fac.)'!D20)=TRUE,\"Inkomende vuilvracht niet gespecifieerd\",'Input huidige maatreg. (fac.)'!H20))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",IF(ISBLANK('Input huidige maatreg. (fac.)'!D20)=TRUE,\"Inkomende vuilvracht niet gespecifieerd\",'Input huidige maatreg. (fac.)'!K20))","v":""},{"$f":"'Input bijkomende maatregelen'!I30","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",IFERROR(E69/(D69-I69),\"Inkomende vuilvracht niet gespecifieerd\"))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",IFERROR(F69/(D69-I69),\"Inkomende vuilvracht niet gespecifieerd\"))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!AD23)","v":""},{"$f":"'Samenvatting econ kengetallen'!C47","v":""},"",null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",_xlfn.CONCAT(IF(G69=\"Inkomende vuilvracht niet gespecifieerd\",\"\",IF(H69>G69,Expressielijsten!$B$122,Expressielijsten!$B$123)),\"; \",IF(K69<J69,Expressielijsten!$B$124,Expressielijsten!$B$125)))","v":""}]
[null,5,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!B24)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",IF(ISBLANK('Input huidige maatreg. (fac.)'!D21)=TRUE,\"Inkomende vuilvracht niet gespecifieerd\",'Input huidige maatreg. (fac.)'!H21))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",IF(ISBLANK('Input huidige maatreg. (fac.)'!D21)=TRUE,\"Inkomende vuilvracht niet gespecifieerd\",'Input huidige maatreg. (fac.)'!K21))","v":""},{"$f":"'Input bijkomende maatregelen'!I31","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",IFERROR(E70/(D70-I70),\"Inkomende vuilvracht niet gespecifieerd\"))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",IFERROR(F70/(D70-I70),\"Inkomende vuilvracht niet gespecifieerd\"))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!AD24)","v":""},{"$f":"'Samenvatting econ kengetallen'!C48","v":""},"",null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",_xlfn.CONCAT(IF(G70=\"Inkomende vuilvracht niet gespecifieerd\",\"\",IF(H70>G70,Expressielijsten!$B$122,Expressielijsten!$B$123)),\"; \",IF(K70<J70,Expressielijsten!$B$124,Expressielijsten!$B$125)))","v":""}]
[null,6,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!B25)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",IF(ISBLANK('Input huidige maatreg. (fac.)'!D22)=TRUE,\"Inkomende vuilvracht niet gespecifieerd\",'Input huidige maatreg. (fac.)'!H22))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",IF(ISBLANK('Input huidige maatreg. (fac.)'!D22)=TRUE,\"Inkomende vuilvracht niet gespecifieerd\",'Input huidige maatreg. (fac.)'!K22))","v":""},{"$f":"'Input bijkomende maatregelen'!I32","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",IFERROR(E71/(D71-I71),\"Inkomende vuilvracht niet gespecifieerd\"))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",IFERROR(F71/(D71-I71),\"Inkomende vuilvracht niet gespecifieerd\"))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!AD25)","v":""},{"$f":"'Samenvatting econ kengetallen'!C49","v":""},"",null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",_xlfn.CONCAT(IF(G71=\"Inkomende vuilvracht niet gespecifieerd\",\"\",IF(H71>G71,Expressielijsten!$B$122,Expressielijsten!$B$123)),\"; \",IF(K71<J71,Expressielijsten!$B$124,Expressielijsten!$B$125)))","v":""}]
[null,7,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!B26)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",IF(ISBLANK('Input huidige maatreg. (fac.)'!D23)=TRUE,\"Inkomende vuilvracht niet gespecifieerd\",'Input huidige maatreg. (fac.)'!H23))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",IF(ISBLANK('Input huidige maatreg. (fac.)'!D23)=TRUE,\"Inkomende vuilvracht niet gespecifieerd\",'Input huidige maatreg. (fac.)'!K23))","v":""},{"$f":"'Input bijkomende maatregelen'!I33","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",IFERROR(E72/(D72-I72),\"Inkomende vuilvracht niet gespecifieerd\"))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",IFERROR(F72/(D72-I72),\"Inkomende vuilvracht niet gespecifieerd\"))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!AD26)","v":""},{"$f":"'Samenvatting econ kengetallen'!C50","v":""},"",null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",_xlfn.CONCAT(IF(G72=\"Inkomende vuilvracht niet gespecifieerd\",\"\",IF(H72>G72,Expressielijsten!$B$122,Expressielijsten!$B$123)),\"; \",IF(K72<J72,Expressielijsten!$B$124,Expressielijsten!$B$125)))","v":""}]
[]
[]
[null,"Criterium 5: Overzicht crossmedia-effecten"]
[]
[null,{"$f":"'Input bijkomende maatregelen'!B88","v":"A Emissies naar water - opconcentratie reeds aanwezige polluent"},null,null,{"$f":"'Input bijkomende maatregelen'!L90","v":"Proc. Bijdrage onder realistische omstandigheden"},"Significantiedrempel",null,null,null,null,null,"Code opmaak","Beoordeling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Significantiedrempel cross media ",0.01]
[null,1,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!B20)","v":""},null,{"$f":"IF(C78=\"\",\"\",IF('Input bijkomende maatregelen'!L92=\"\",\"niet van toepassing\",'Input bijkomende maatregelen'!L92))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",IF(E78=\"niet van toepassing\",\"-\",$AG$77))","v":""},null,null,null,null,null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C92)=TRUE,\"\",IF(E78=\"niet van toepassing\",1,IF(E78>F78,0,1)))","v":1},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C92)=TRUE,\"\",IF(E78=\"niet van toepassing\",Expressielijsten!$B$131,IF(E78>F78,Expressielijsten!$B$130,Expressielijsten!$B$131)))","v":"Geen significant cross media effect te verwachten"}]
[null,2,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!B21)","v":""},null,{"$f":"IF(C79=\"\",\"\",IF('Input bijkomende maatregelen'!L93=\"\",\"niet van toepassing\",'Input bijkomende maatregelen'!L93))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",IF(E79=\"niet van toepassing\",\"-\",$AG$77))","v":""},null,null,null,null,null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C93)=TRUE,\"\",IF(E79=\"niet van toepassing\",1,IF(E79>F79,0,1)))","v":1},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C93)=TRUE,\"\",IF(E79=\"niet van toepassing\",Expressielijsten!$B$131,IF(E79>F79,Expressielijsten!$B$130,Expressielijsten!$B$131)))","v":"Geen significant cross media effect te verwachten"}]
[null,3,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!B22)","v":""},null,{"$f":"IF(C80=\"\",\"\",IF('Input bijkomende maatregelen'!L94=\"\",\"niet van toepassing\",'Input bijkomende maatregelen'!L94))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",IF(E80=\"niet van toepassing\",\"-\",$AG$77))","v":""},null,null,null,null,null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C94)=TRUE,\"\",IF(E80=\"niet van toepassing\",1,IF(E80>F80,0,1)))","v":1},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C94)=TRUE,\"\",IF(E80=\"niet van toepassing\",Expressielijsten!$B$131,IF(E80>F80,Expressielijsten!$B$130,Expressielijsten!$B$131)))","v":"Geen significant cross media effect te verwachten"}]
[null,4,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!B23)","v":""},null,{"$f":"IF(C81=\"\",\"\",IF('Input bijkomende maatregelen'!L95=\"\",\"niet van toepassing\",'Input bijkomende maatregelen'!L95))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",IF(E81=\"niet van toepassing\",\"-\",$AG$77))","v":""},null,null,null,null,null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C95)=TRUE,\"\",IF(E81=\"niet van toepassing\",1,IF(E81>F81,0,1)))","v":1},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C95)=TRUE,\"\",IF(E81=\"niet van toepassing\",Expressielijsten!$B$131,IF(E81>F81,Expressielijsten!$B$130,Expressielijsten!$B$131)))","v":"Geen significant cross media effect te verwachten"}]
[null,5,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!B24)","v":""},null,{"$f":"IF(C82=\"\",\"\",IF('Input bijkomende maatregelen'!L96=\"\",\"niet van toepassing\",'Input bijkomende maatregelen'!L96))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",IF(E82=\"niet van toepassing\",\"-\",$AG$77))","v":""},null,null,null,null,null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C96)=TRUE,\"\",IF(E82=\"niet van toepassing\",1,IF(E82>F82,0,1)))","v":1},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C96)=TRUE,\"\",IF(E82=\"niet van toepassing\",Expressielijsten!$B$131,IF(E82>F82,Expressielijsten!$B$130,Expressielijsten!$B$131)))","v":"Geen significant cross media effect te verwachten"}]
[null,6,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!B25)","v":""},null,{"$f":"IF(C83=\"\",\"\",IF('Input bijkomende maatregelen'!L97=\"\",\"niet van toepassing\",'Input bijkomende maatregelen'!L97))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",IF(E83=\"niet van toepassing\",\"-\",$AG$77))","v":""},null,null,null,null,null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C97)=TRUE,\"\",IF(E83=\"niet van toepassing\",1,IF(E83>F83,0,1)))","v":1},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C97)=TRUE,\"\",IF(E83=\"niet van toepassing\",Expressielijsten!$B$131,IF(E83>F83,Expressielijsten!$B$130,Expressielijsten!$B$131)))","v":"Geen significant cross media effect te verwachten"}]
[null,7,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!B26)","v":""},null,{"$f":"IF(C84=\"\",\"\",IF('Input bijkomende maatregelen'!L98=\"\",\"niet van toepassing\",'Input bijkomende maatregelen'!L98))","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",IF(E84=\"niet van toepassing\",\"-\",$AG$77))","v":""},null,null,null,null,null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C98)=TRUE,\"\",IF(E84=\"niet van toepassing\",1,IF(E84>F84,0,1)))","v":1},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C98)=TRUE,\"\",IF(E84=\"niet van toepassing\",Expressielijsten!$B$131,IF(E84>F84,Expressielijsten!$B$130,Expressielijsten!$B$131)))","v":"Geen significant cross media effect te verwachten"}]
[]
[]
[null,{"$f":"'Input bijkomende maatregelen'!B100","v":"B Emissies naar water - Toename lozing andere componenten"},null,null,{"$f":"'Input bijkomende maatregelen'!L102","v":"Proc. Bijdrage onder realistische omstandigheden"},"Significantiedrempel",null,null,null,null,null,null,"Beoordeling"]
[null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C104)=TRUE,\"\",'Input bijkomende maatregelen'!B104)","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C104)=TRUE,\"\",'Input bijkomende maatregelen'!C104)","v":""},null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C104)=TRUE,\"\",IF('Input bijkomende maatregelen'!L104=\"\",\"niet van toepassing\",'Input bijkomende maatregelen'!L104))","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C104)=TRUE,\"\",IF(E88=\"niet van toepassing\",\"-\",$AG$77))","v":""},null,null,null,null,null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C104)=TRUE,1,IF(E88=\"niet van toepassing\",1,IF(E88>F88,0,1)))","v":1},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C104)=TRUE,\"Geen effect\",IF(E88=\"niet van toepassing\",Expressielijsten!$B$131,IF(E88>F88,Expressielijsten!$B$130,Expressielijsten!$B$131)))","v":"Geen effect"}]
[null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C105)=TRUE,\"\",'Input bijkomende maatregelen'!B105)","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C105)=TRUE,\"\",'Input bijkomende maatregelen'!C105)","v":""},null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C105)=TRUE,\"\",IF('Input bijkomende maatregelen'!L105=\"\",\"niet van toepassing\",'Input bijkomende maatregelen'!L105))","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C105)=TRUE,\"\",IF(E89=\"niet van toepassing\",\"-\",$AG$77))","v":""},null,null,null,null,null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C105)=TRUE,\"\",IF(E89=\"niet van toepassing\",1,IF(E89>F89,0,1)))","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C105)=TRUE,\"\",IF(E89=\"niet van toepassing\",Expressielijsten!$B$131,IF(E89>F89,Expressielijsten!$B$130,Expressielijsten!$B$131)))","v":""}]
[null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C106)=TRUE,\"\",'Input bijkomende maatregelen'!B106)","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C106)=TRUE,\"\",'Input bijkomende maatregelen'!C106)","v":""},null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C106)=TRUE,\"\",IF('Input bijkomende maatregelen'!L106=\"\",\"niet van toepassing\",'Input bijkomende maatregelen'!L106))","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C106)=TRUE,\"\",IF(E90=\"niet van toepassing\",\"-\",$AG$77))","v":""},null,null,null,null,null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C106)=TRUE,\"\",IF(E90=\"niet van toepassing\",1,IF(E90>F90,0,1)))","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C106)=TRUE,\"\",IF(E90=\"niet van toepassing\",Expressielijsten!$B$131,IF(E90>F90,Expressielijsten!$B$130,Expressielijsten!$B$131)))","v":""}]
[null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C107)=TRUE,\"\",'Input bijkomende maatregelen'!B107)","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C107)=TRUE,\"\",'Input bijkomende maatregelen'!C107)","v":""},null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C107)=TRUE,\"\",IF('Input bijkomende maatregelen'!L107=\"\",\"niet van toepassing\",'Input bijkomende maatregelen'!L107))","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C107)=TRUE,\"\",IF(E91=\"niet van toepassing\",\"-\",$AG$77))","v":""},null,null,null,null,null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C107)=TRUE,\"\",IF(E91=\"niet van toepassing\",1,IF(E91>F91,0,1)))","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C107)=TRUE,\"\",IF(E91=\"niet van toepassing\",Expressielijsten!$B$131,IF(E91>F91,Expressielijsten!$B$130,Expressielijsten!$B$131)))","v":""}]
[null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C108)=TRUE,\"\",'Input bijkomende maatregelen'!B108)","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C108)=TRUE,\"\",'Input bijkomende maatregelen'!C108)","v":""},null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C108)=TRUE,\"\",IF('Input bijkomende maatregelen'!L108=\"\",\"niet van toepassing\",'Input bijkomende maatregelen'!L108))","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C108)=TRUE,\"\",IF(E92=\"niet van toepassing\",\"-\",$AG$77))","v":""},null,null,null,null,null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C108)=TRUE,\"\",IF(E92=\"niet van toepassing\",1,IF(E92>F92,0,1)))","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C108)=TRUE,\"\",IF(E92=\"niet van toepassing\",Expressielijsten!$B$131,IF(E92>F92,Expressielijsten!$B$130,Expressielijsten!$B$131)))","v":""}]
[null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C109)=TRUE,\"\",'Input bijkomende maatregelen'!B109)","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C109)=TRUE,\"\",'Input bijkomende maatregelen'!C109)","v":""},null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C109)=TRUE,\"\",IF('Input bijkomende maatregelen'!L109=\"\",\"niet van toepassing\",'Input bijkomende maatregelen'!L109))","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C109)=TRUE,\"\",IF(E93=\"niet van toepassing\",\"-\",$AG$77))","v":""},null,null,null,null,null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C109)=TRUE,\"\",IF(E93=\"niet van toepassing\",1,IF(E93>F93,0,1)))","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C109)=TRUE,\"\",IF(E93=\"niet van toepassing\",Expressielijsten!$B$131,IF(E93>F93,Expressielijsten!$B$130,Expressielijsten!$B$131)))","v":""}]
[null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C110)=TRUE,\"\",'Input bijkomende maatregelen'!B110)","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C110)=TRUE,\"\",'Input bijkomende maatregelen'!C110)","v":""},null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C110)=TRUE,\"\",IF('Input bijkomende maatregelen'!L110=\"\",\"niet van toepassing\",'Input bijkomende maatregelen'!L110))","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C110)=TRUE,\"\",IF(E94=\"niet van toepassing\",\"-\",$AG$77))","v":""},null,null,null,null,null,{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C110)=TRUE,\"\",IF(E94=\"niet van toepassing\",1,IF(E94>F94,0,1)))","v":""},{"$f":"IF(ISBLANK('Input bijkomende maatregelen'!C110)=TRUE,\"\",IF(E94=\"niet van toepassing\",Expressielijsten!$B$131,IF(E94>F94,Expressielijsten!$B$130,Expressielijsten!$B$131)))","v":""}]
[]
[]
[null,null,{"$f":"'Input bijkomende maatregelen'!B112","v":"C Emissies naar lucht"},null,null,null,null,null,null,null,null,null,"Beoordeling"]
[null,null,{"$f":"IF('Input bijkomende maatregelen'!E112=\"ja\",'Input bijkomende maatregelen'!B113,\"\")","v":""},null,null,null,null,null,null,null,null,{"$f":"IF('Input bijkomende maatregelen'!E112=\"Ja\",0,1)","v":1},{"$f":"IF('Input bijkomende maatregelen'!E112=\"Ja\",Expressielijsten!$B$133,Expressielijsten!$B$134)","v":"Geen effect"}]
[null,null,{"$f":"'Input bijkomende maatregelen'!B114","v":"D Overige"},null,null,null,null,null,null,null,null,null,"Beoordeling"]
[null,null,{"$f":"IF('Input bijkomende maatregelen'!E114=\"ja\",'Input bijkomende maatregelen'!B115,\"\")","v":""},null,null,null,null,null,null,null,null,{"$f":"IF('Input bijkomende maatregelen'!E114=\"ja\",0,1)","v":1},{"$f":"IF('Input bijkomende maatregelen'!E114=\"ja\",Expressielijsten!$B$133,Expressielijsten!$B$134)","v":"Geen effect"}]
[]
[]
[]
[null,"Criterium 6: Effect overige investeringen i.k.v. impactbeoordeling op economische draagkracht"]
[null,"Categorie stof met hoogste impact",null,{"$f":"MIN(M5:M10)","v":0}]
[null,"Toetscriterium stof met hoogste impact",null,{"$f":"VLOOKUP(D105,'Criteria volgens stofcategorie'!$G$3:$AB$7,22,FALSE)","v":{"$error":"#N/A"}}]
[]
[]
[null,"Overzicht investeringen i.k.v. impactbeoordeling water",null,null,"Totale jaarlijkse kost "]
[null,"Maatregel zoals ingevuld in deze tool",null,null,{"$f":"'Samenvatting econ kengetallen'!$B$25","v":0}]
[null,"Overige investeringen",null,null,"Totale jaarlijkse kost "]
[null,{"$f":"IF(ISBLANK('Input overige investeringen'!F8)=TRUE,\"\",'Input overige investeringen'!A8)","v":""},{"$f":"IF(ISBLANK('Input overige investeringen'!B8)=TRUE,\"\",'Input overige investeringen'!B8)","v":""},null,{"$f":"IF(ISBLANK('Input overige investeringen'!F8)=TRUE,\"\",'Input overige investeringen'!J8)","v":""}]
[null,{"$f":"IF(ISBLANK('Input overige investeringen'!F9)=TRUE,\"\",'Input overige investeringen'!A9)","v":""},{"$f":"IF(ISBLANK('Input overige investeringen'!B9)=TRUE,\"\",'Input overige investeringen'!B9)","v":""},null,{"$f":"IF(ISBLANK('Input overige investeringen'!F9)=TRUE,\"\",'Input overige investeringen'!J9)","v":""}]
[null,{"$f":"IF(ISBLANK('Input overige investeringen'!F10)=TRUE,\"\",'Input overige investeringen'!A10)","v":""},{"$f":"IF(ISBLANK('Input overige investeringen'!B10)=TRUE,\"\",'Input overige investeringen'!B10)","v":""},null,{"$f":"IF(ISBLANK('Input overige investeringen'!F10)=TRUE,\"\",'Input overige investeringen'!J10)","v":""}]
[null,{"$f":"IF(ISBLANK('Input overige investeringen'!F11)=TRUE,\"\",'Input overige investeringen'!A11)","v":""},{"$f":"IF(ISBLANK('Input overige investeringen'!B11)=TRUE,\"\",'Input overige investeringen'!B11)","v":""},null,{"$f":"IF(ISBLANK('Input overige investeringen'!F11)=TRUE,\"\",'Input overige investeringen'!J11)","v":""}]
[null,{"$f":"IF(ISBLANK('Input overige investeringen'!F12)=TRUE,\"\",'Input overige investeringen'!A12)","v":""},{"$f":"IF(ISBLANK('Input overige investeringen'!B12)=TRUE,\"\",'Input overige investeringen'!B12)","v":""},null,{"$f":"IF(ISBLANK('Input overige investeringen'!F12)=TRUE,\"\",'Input overige investeringen'!J12)","v":""}]
[null,{"$f":"IF(ISBLANK('Input overige investeringen'!F13)=TRUE,\"\",'Input overige investeringen'!A13)","v":""},{"$f":"IF(ISBLANK('Input overige investeringen'!B13)=TRUE,\"\",'Input overige investeringen'!B13)","v":""},null,{"$f":"IF(ISBLANK('Input overige investeringen'!F13)=TRUE,\"\",'Input overige investeringen'!J13)","v":""}]
[null,{"$f":"IF(ISBLANK('Input overige investeringen'!F14)=TRUE,\"\",'Input overige investeringen'!A14)","v":""},{"$f":"IF(ISBLANK('Input overige investeringen'!B14)=TRUE,\"\",'Input overige investeringen'!B14)","v":""},null,{"$f":"IF(ISBLANK('Input overige investeringen'!F14)=TRUE,\"\",'Input overige investeringen'!J14)","v":""}]
[null,{"$f":"IF(ISBLANK('Input overige investeringen'!F15)=TRUE,\"\",'Input overige investeringen'!A15)","v":""},{"$f":"IF(ISBLANK('Input overige investeringen'!B15)=TRUE,\"\",'Input overige investeringen'!B15)","v":""},null,{"$f":"IF(ISBLANK('Input overige investeringen'!F15)=TRUE,\"\",'Input overige investeringen'!J15)","v":""}]
[null,{"$f":"'Input overige investeringen'!A16","v":"Totaal overige investeringen i.k.v. impactbeoordeling afvalwater"},null,null,{"$f":"IF(ISBLANK('Input overige investeringen'!J16)=TRUE,\"\",'Input overige investeringen'!J16)","v":0}]
[]
[null,"Som totale maatregelen i.k.v. impactbeoordeling afvalwater",null,null,{"$f":"E120+E110","v":0}]
[]
[]
[null,"Holding",null,"Financiële data van de holding","Bijkomende maatregel + overige investeringen\n(opex + ycc - baten)","Ratio","Criteria aanvaardbaar","Criteria intermediair bovengrens","Code",null,null,"Code opmaak","Beoordeling"]
[null,"Omzet",null,{"$f":"'Samenvatting econ kengetallen'!$G$79","v":{"$error":"#DIV/0!"}},{"$f":"$E$122","v":0},{"$f":"E126/D126","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,10,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,12,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(F126<G126,Expressielijsten!$B$30,IF(F126<(H126+G126)/2,Expressielijsten!$B$31,IF(F126>=H126,Expressielijsten!$B$33,Expressielijsten!$B$32)))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"IF(D105=1,VLOOKUP(I129,Expressielijsten!A53:E117,5,FALSE),VLOOKUP(I129,Expressielijsten!A53:E117,4,FALSE))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D105=1,VLOOKUP(I129,Expressielijsten!A53:C117,3,FALSE),VLOOKUP(I129,Expressielijsten!A53:C117,2,FALSE))","v":{"$error":"#DIV/0!"}}]
[null,"Toegevoegde waarde",null,{"$f":"'Samenvatting econ kengetallen'!$G$80","v":{"$error":"#DIV/0!"}},{"$f":"$E$122","v":0},{"$f":"IF(D127<=0,1,E127/D127)","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,14,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,16,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(F127<G127,Expressielijsten!$B$37,IF(F127<(H127+G127)/2,Expressielijsten!$B$38,IF(F127>=H127,Expressielijsten!$B$40,Expressielijsten!$B$39)))","v":{"$error":"#DIV/0!"}}]
[null,"EBITDA",null,{"$f":"'Samenvatting econ kengetallen'!$G$81","v":{"$error":"#DIV/0!"}},{"$f":"$E$122","v":0},{"$f":"IF(D128<=0,1,E128/D128)","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,18,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,20,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(F128<G128,Expressielijsten!$B$44,IF(F128<(H128+G128)/2,Expressielijsten!$B$45,IF(F128>=H128,Expressielijsten!$B$47,Expressielijsten!$B$46)))","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,{"$f":"I126+I127+I128","v":{"$error":"#DIV/0!"}}]
[]
[]
[null,"Vestiging",null,"Financiële data van de vestiging","Bijkomende maatregel + overige investeringen\n(opex + ycc - baten)","Ratio","Criteria aanvaardbaar","Criteria intermediair bovengrens","Code",null,null,"Code opmaak","Beoordeling"]
[null,"Omzet",null,{"$f":"'Samenvatting econ kengetallen'!$G$70","v":{"$error":"#DIV/0!"}},{"$f":"$E$122","v":0},{"$f":"E133/D133","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,10,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,12,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(F133<G133,Expressielijsten!$B$30,IF(F133<(H133+G133)/2,Expressielijsten!$B$31,IF(F133>=H133,Expressielijsten!$B$33,Expressielijsten!$B$32)))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"IF(D105=1,VLOOKUP(I136,Expressielijsten!A53:E117,5,FALSE),VLOOKUP(I136,Expressielijsten!A53:E117,4,FALSE))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D105=1,VLOOKUP(I136,Expressielijsten!A53:C117,3,FALSE),VLOOKUP(I136,Expressielijsten!A53:C117,2,FALSE))","v":{"$error":"#DIV/0!"}}]
[null,"Toegevoegde waarde",null,{"$f":"'Samenvatting econ kengetallen'!$G$71","v":{"$error":"#DIV/0!"}},{"$f":"$E$122","v":0},{"$f":"IF(D134<=0,1,E134/D134)","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,14,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,16,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(F134<G134,Expressielijsten!$B$37,IF(F134<(H134+G134)/2,Expressielijsten!$B$38,IF(F134>=H134,Expressielijsten!$B$40,Expressielijsten!$B$39)))","v":{"$error":"#DIV/0!"}}]
[null,"EBITDA",null,{"$f":"'Samenvatting econ kengetallen'!$G$72","v":{"$error":"#DIV/0!"}},{"$f":"$E$122","v":0},{"$f":"IF(D135<=0,1,E135/D135)","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,18,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($D$43,'Criteria volgens stofcategorie'!$G$4:$AB$7,20,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(F135<G135,Expressielijsten!$B$44,IF(F135<(H135+G135)/2,Expressielijsten!$B$45,IF(F135>=H135,Expressielijsten!$B$47,Expressielijsten!$B$46)))","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,{"$f":"I133+I134+I135","v":{"$error":"#DIV/0!"}}]

{"sheet":"Expressielijsten","index":6,"n_rows":134,"n_cols":12,"rows_kept":134,"cut":false,"hidden":true,"merged":[]}
["Criterium 0"]
["Zie tabblad stof x impactcategorie; zie ook dashboard beslissing cel M7"]
[]
["Criterium 1"]
["Toetsing","Expressie",null,"Codering - gunstigheid"]
["C effluent < 1/2 C impactbeoordeling","Gunstig: Reductie door de beschouwde bijkomende maatregelen zou ruimschoots voldoende moeten zijn om vooropgestelde streefwaarde te halen",null,1]
["C effluent < C impactbeoordeling","Gunstig: Reductie door de beschouwde bijkomende maatregelen zou voldoende moeten zijn om vooropgestelde streefwaarde te halen",null,1]
["C effluent > C impactbeoordeling AND VR% > 75%","Gunstig: Reductie door de beschouwde bijkomende maatregelen is niet voldoende om de vooropgestelde streefwaarde te halen. De toegepaste maatregelen zorgen echter wel voor een significante reductie (>75%) van de vuilvrachtlozing voor deze parameter.",null,1]
["C effluent > C impactbeoordeling AND VR% < 75%","Te beoordelen: Reductie door de beschouwde bijkomende maatregelen is niet voldoende om de vooropgestelde streefwaarde te halen en de toegepaste maatregelen zorgen  ook niet voor een significante reductie (>75%) van de vuilvrachtlozing voor deze parameter. In specifieke gevallen, kan echter geoordeeld worden dat ook een lager verwijderingsrendement acceptabel is.",null,0]
[]
[]
["Criterium 2"]
["Toetsing","Expressielijst",null,"Codering - gunstigheid"]
["Kosten Verdergaand dan BBT AND KE(maatregel) < KE BBT+NL","Maatregel is KE voor deze parameter: Gelet op de impact van de stof op het ontvangende waterlichaam dient hier getoetst te worden aan de bovenste kosteneffectiviteitsdrempel. De kosteneffectiviteit van de bijkomende maatregel ligt onder deze drempel. Deze maatregel is dus kosteneffectief voor deze parameter.",null,1]
["Kosten Verdergaand dan BBT AND KE(maatregel) > KE BBT+NL","Maatregel is niet KE voor deze parameter: Gelet op de impact van de stof op het ontvangende waterlichaam dient hier getoetst te worden aan de bovenste kosteneffectiviteitsdrempel. De kosteneffectiviteit van de bijkomende maatregel ligt boven deze drempel. Deze maatregel is niet kosteneffectief voor deze parameter.",null,0]
["Kosten gelijkgesteld met BBT AND KE(maatregel < KE BBT NL","Maatregel is KE voor deze parameter: Gelet op de beperkte impact van de stof/lozing in het ontvangende waterlichaam dient hier getoetst te worden aan de onderste kosteneffectiviteitsdrempel. De kosteneffectiviteit van de bijkomende maatregel ligt onder deze drempel. Deze maatregel is dus kosteneffectief voor deze parameter.",null,1]
["Kosten gelijkgesteld met BBT AND KE(maatregel > KE BBT NL)","Maatregel is niet KE voor deze parameter: Gelet op de beperkte impact van de stof/lozing in het ontvangende waterlichaam dient hier getoetst te worden aan de onderste kosteneffectiviteitsdrempel. De kosteneffectiviteit van de bijkomende maatregel ligt boven deze drempel. Deze maatregel is dus niet kosteneffectief voor deze parameter.",null,0]
["Kosten Verdergaand dan BBT AND KE(maatregel) < KE BBT NL","Maatregel is zeer KE voor deze parameter: Gelet op de impact van de stof op het ontvangende waterlichaam dient hier getoetst te worden aan de bovenste kosteneffectiviteitsdrempel. De kosteneffectiviteit van de bijkomende maatregel ligt onder deze drempel. Bijkomstig ligt de kosteneffectiviteit ook onder de drempel die gelijkgesteld wordt met BBT maatregelen. Deze maatregel is dus zeer kosteneffectief voor deze parameter.",null,1]
[null,null,null,1]
["Criterium 2 expressies BBT/BBT+"]
["Onderste kostencurve","Maximale bijkomende kosten gelijkgesteld met BBT"]
["Bovenste kostencurve","Maximale bijkomende kosten verdergaand dan BBT (10 x BBT)"]
["Afwijking kostencurve","KE afgeleid uit praktijkvoorbeelden"]
["Geen afwijking kostencurve","KE afgeleid uit NL model"]
[]
[]
[]
["Criterium 3 - interpretatie toetswaarde omzet"]
["Toetsing","Omzetcode"]
["Kosten/omzet < 0.5%",0]
["Kosten/omzet 0.5-2.75%",1]
["Kosten/omzet 2.75-5%",10]
["Kosten/omzet > 5%",100]
[]
["Criterium 3- interpretatie toetswaarde toegevoegde waarde"]
["Toetsing","Omzetcode"]
["Kosten/toegevoegde waarde <2%",0]
["kosten/toegevoegde waarde 2-26%",1]
["Kosten/toegevoegde waarde 26-50%",10]
["Kosten/toegevoegde waarde >50%",100]
[]
["Criterium 3- interpretatie toetswaarde EBIDTA"]
["Toetsing","Omzetcode"]
["Kosten/EBIDTA <10%",0]
["Kosten/EBIDTA 10-45%",1]
["Kosten/EBIDTA 45-100%",10]
["Kosten/EBIDTA >100%",100]
[]
[]
[]
["Criterium 3 - interpretatie somcode",null,null,null,null,null,"Coderingsmatrix"]
["Somcode","Interpretatie BBT","Interpretatie BBT+","Codering - gunstigheid BBT","Codering - gunstigheid verdergaand dan BBT","Column1","Omzet - codering","expressie","Toegevoegde waarde - codering","expressie2","EBIDTA - codering","Column3"]
[{"$f":"Expressielijsten!G53+Expressielijsten!I53+K53","v":0},"Maatregel haalbaar","Maatregel haalbaar",1,1,null,{"$f":"$B$30","v":0},{"$f":"$A$30","v":"Kosten/omzet < 0.5%"},{"$f":"$B$37","v":0},{"$f":"$A$37","v":"Kosten/toegevoegde waarde <2%"},{"$f":"$B$44","v":0},{"$f":"$A$44","v":"Kosten/EBIDTA <10%"}]
[{"$f":"Expressielijsten!G54+Expressielijsten!I54+K54","v":1},"Maatregel haalbaar: één van de toetscriteria bevindt zich in de intermediaire zone, maar wel in het ondergebied. Hierdoor kan de maatregel alsnog als haalbaar beschouwd kan worden.","Maatregel haalbaar: één van de toetscriteria bevindt zich in de intermediaire zone, maar wel in het ondergebied. Hierdoor kan de maatregel alsnog als haalbaar beschouwd kan worden.",1,1,null,{"$f":"$B$30","v":0},{"$f":"$A$30","v":"Kosten/omzet < 0.5%"},{"$f":"$B$38","v":1},{"$f":"$A$38","v":"kosten/toegevoegde waarde 2-26%"},{"$f":"$B$44","v":0},{"$f":"$A$44","v":"Kosten/EBIDTA <10%"}]
[{"$f":"Expressielijsten!G55+Expressielijsten!I55+K55","v":10},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel haalbaar: Gelet op de stof x impactcategorie (1) is de maatregel als haalbaar te beschouwen, ondanks het feit dat ten minste één van de toetscriteria zich in het bovengebied van de intermediaire zone bevindt.",0,1,null,0,{"$f":"$A$30","v":"Kosten/omzet < 0.5%"},{"$f":"$B$39","v":10},{"$f":"$A$39","v":"Kosten/toegevoegde waarde 26-50%"},0,"Kosten/EBIDTA <10%"]
[{"$f":"Expressielijsten!G56+Expressielijsten!I56+K56","v":100},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,0,{"$f":"$A$30","v":"Kosten/omzet < 0.5%"},{"$f":"$B$40","v":100},{"$f":"$A$40","v":"Kosten/toegevoegde waarde >50%"},0,"Kosten/EBIDTA <10%"]
[{"$f":"Expressielijsten!G57+Expressielijsten!I57+K57","v":1},"Maatregel haalbaar: één van de toetscriteria ligt in de intermediaire zone, maar in het ondergebied van de zone waardoor de maatregel alsnog als haalbaar beschouwd kan worden","Maatregel haalbaar: één van de toetscriteria ligt in de intermediaire zone, maar in het ondergebied van de zone waardoor de maatregel alsnog als haalbaar beschouwd kan worden",1,1,null,{"$f":"$B$31","v":1},{"$f":"$A$31","v":"Kosten/omzet 0.5-2.75%"},{"$f":"$B$37","v":0},{"$f":"$A$37","v":"Kosten/toegevoegde waarde <2%"},0,"Kosten/EBIDTA <10%"]
[{"$f":"Expressielijsten!G58+Expressielijsten!I58+K58","v":2},"Maatregel haalbaar: twee toetscriteria liggen in de intermediaire zone, maar in het ondergebied van de zone waardoor de maatregel alsnog als haalbaar beschouwd kan worden","Maatregel haalbaar: twee toetscriteria liggen in de intermediaire zone, maar in het ondergebied van de zone waardoor de maatregel alsnog als haalbaar beschouwd kan worden",1,1,null,{"$f":"$B$31","v":1},{"$f":"$A$31","v":"Kosten/omzet 0.5-2.75%"},{"$f":"$B$38","v":1},{"$f":"$A$38","v":"kosten/toegevoegde waarde 2-26%"},0,"Kosten/EBIDTA <10%"]
[{"$f":"Expressielijsten!G59+Expressielijsten!I59+K59","v":11},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel haalbaar: Gelet op de stof x impactcategorie (1) is de maatregel als haalbaar te beschouwen, ondanks het feit dat ten minste één van de toetscriteria zich in het bovengebied van de intermediaire zone bevindt.",0,1,null,1,{"$f":"$A$31","v":"Kosten/omzet 0.5-2.75%"},{"$f":"$B$39","v":10},{"$f":"$A$39","v":"Kosten/toegevoegde waarde 26-50%"},0,"Kosten/EBIDTA <10%"]
[{"$f":"Expressielijsten!G60+Expressielijsten!I60+K60","v":101},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,1,{"$f":"$A$31","v":"Kosten/omzet 0.5-2.75%"},{"$f":"$B$40","v":100},{"$f":"$A$40","v":"Kosten/toegevoegde waarde >50%"},0,"Kosten/EBIDTA <10%"]
[{"$f":"Expressielijsten!G61+Expressielijsten!I61+K61","v":10},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel haalbaar: Gelet op de stof x impactcategorie (1) is de maatregel als haalbaar te beschouwen, ondanks het feit dat ten minste één van de toetscriteria zich in het bovengebied van de intermediaire zone bevindt.",0,1,null,{"$f":"$B$32","v":10},{"$f":"$A$32","v":"Kosten/omzet 2.75-5%"},{"$f":"$B$37","v":0},{"$f":"$A$37","v":"Kosten/toegevoegde waarde <2%"},0,"Kosten/EBIDTA <10%"]
[{"$f":"Expressielijsten!G62+Expressielijsten!I62+K62","v":11},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel haalbaar: Gelet op de stof x impactcategorie (1) is de maatregel als haalbaar te beschouwen, ondanks het feit dat ten minste één van de toetscriteria zich in het bovengebied van de intermediaire zone bevindt.",0,1,null,{"$f":"$B$32","v":10},{"$f":"$A$32","v":"Kosten/omzet 2.75-5%"},{"$f":"$B$38","v":1},{"$f":"$A$38","v":"kosten/toegevoegde waarde 2-26%"},0,"Kosten/EBIDTA <10%"]
[{"$f":"Expressielijsten!G63+Expressielijsten!I63+K63","v":20},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel onhaalbaar: ten minste twee toetscriteria bevinden zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.",0,0,null,10,{"$f":"$A$32","v":"Kosten/omzet 2.75-5%"},{"$f":"$B$39","v":10},{"$f":"$A$39","v":"Kosten/toegevoegde waarde 26-50%"},0,"Kosten/EBIDTA <10%"]
[{"$f":"Expressielijsten!G64+Expressielijsten!I64+K64","v":110},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,10,{"$f":"$A$32","v":"Kosten/omzet 2.75-5%"},{"$f":"$B$40","v":100},{"$f":"$A$40","v":"Kosten/toegevoegde waarde >50%"},0,"Kosten/EBIDTA <10%"]
[{"$f":"Expressielijsten!G65+Expressielijsten!I65+K65","v":100},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,{"$f":"$B$33","v":100},{"$f":"$A$33","v":"Kosten/omzet > 5%"},{"$f":"$B$37","v":0},{"$f":"$A$37","v":"Kosten/toegevoegde waarde <2%"},0,"Kosten/EBIDTA <10%"]
[{"$f":"Expressielijsten!G66+Expressielijsten!I66+K66","v":101},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,{"$f":"$B$33","v":100},{"$f":"$A$33","v":"Kosten/omzet > 5%"},{"$f":"$B$38","v":1},{"$f":"$A$38","v":"kosten/toegevoegde waarde 2-26%"},0,"Kosten/EBIDTA <10%"]
[{"$f":"Expressielijsten!G67+Expressielijsten!I67+K67","v":110},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,100,{"$f":"$A$33","v":"Kosten/omzet > 5%"},{"$f":"$B$39","v":10},{"$f":"$A$39","v":"Kosten/toegevoegde waarde 26-50%"},0,"Kosten/EBIDTA <10%"]
[{"$f":"Expressielijsten!G68+Expressielijsten!I68+K68","v":200},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,100,{"$f":"$A$33","v":"Kosten/omzet > 5%"},{"$f":"$B$40","v":100},{"$f":"$A$40","v":"Kosten/toegevoegde waarde >50%"},0,"Kosten/EBIDTA <10%"]
[{"$f":"Expressielijsten!G69+Expressielijsten!I69+K69","v":1},"Maatregel haalbaar: één van de toetscriteria ligt in de intermediaire zone, maar in het ondergebied van de zone waardoor de maatregel alsnog als haalbaar beschouwd kan worden","Maatregel haalbaar: één van de toetscriteria ligt in de intermediaire zone, maar in het ondergebied van de zone waardoor de maatregel alsnog als haalbaar beschouwd kan worden",1,1,null,{"$f":"$B$30","v":0},{"$f":"$A$30","v":"Kosten/omzet < 0.5%"},{"$f":"$B$37","v":0},{"$f":"$A$37","v":"Kosten/toegevoegde waarde <2%"},{"$f":"$B$45","v":1},{"$f":"$A$45","v":"Kosten/EBIDTA 10-45%"}]
[{"$f":"Expressielijsten!G70+Expressielijsten!I70+K70","v":2},"Maatregel haalbaar: twee toetscriteria liggen in de intermediaire zone, maar in het ondergebied van de zone waardoor de maatregel alsnog als haalbaar beschouwd kan worden","Maatregel haalbaar: twee toetscriteria liggen in de intermediaire zone, maar in het ondergebied van de zone waardoor de maatregel alsnog als haalbaar beschouwd kan worden",1,1,null,{"$f":"$B$30","v":0},{"$f":"$A$30","v":"Kosten/omzet < 0.5%"},{"$f":"$B$38","v":1},{"$f":"$A$38","v":"kosten/toegevoegde waarde 2-26%"},{"$f":"$B$45","v":1},{"$f":"$A$45","v":"Kosten/EBIDTA 10-45%"}]
[{"$f":"Expressielijsten!G71+Expressielijsten!I71+K71","v":11},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel haalbaar: Gelet op de stof x impactcategorie (1) is de maatregel als haalbaar te beschouwen, ondanks het feit dat ten minste één van de toetscriteria zich in het bovengebied van de intermediaire zone bevindt.",0,1,null,0,{"$f":"$A$30","v":"Kosten/omzet < 0.5%"},{"$f":"$B$39","v":10},{"$f":"$A$39","v":"Kosten/toegevoegde waarde 26-50%"},1,"Kosten/EBIDTA 10-45%"]
[{"$f":"Expressielijsten!G72+Expressielijsten!I72+K72","v":101},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,0,{"$f":"$A$30","v":"Kosten/omzet < 0.5%"},{"$f":"$B$40","v":100},{"$f":"$A$40","v":"Kosten/toegevoegde waarde >50%"},1,"Kosten/EBIDTA 10-45%"]
[{"$f":"Expressielijsten!G73+Expressielijsten!I73+K73","v":2},"Maatregel haalbaar: twee toetscriteria liggen in de intermediaire zone, maar in het ondergebied van de zone waardoor de maatregel alsnog als haalbaar beschouwd kan worden","Maatregel haalbaar: twee toetscriteria liggen in de intermediaire zone, maar in het ondergebied van de zone waardoor de maatregel alsnog als haalbaar beschouwd kan worden",1,1,null,{"$f":"$B$31","v":1},{"$f":"$A$31","v":"Kosten/omzet 0.5-2.75%"},{"$f":"$B$37","v":0},{"$f":"$A$37","v":"Kosten/toegevoegde waarde <2%"},1,"Kosten/EBIDTA 10-45%"]
[{"$f":"Expressielijsten!G74+Expressielijsten!I74+K74","v":3},"Maatregel onhaalbaar: de drie toetscriteria liggen in de intermedaire zone","Maatregel haalbaar: Gelet op de stof x impactcategorie (1) is de maatregel als haalbaar te beschouwen, ondanks het feit dat alle toetscriteria zich in de intermediaire zone bevinden.",0,1,null,{"$f":"$B$31","v":1},{"$f":"$A$31","v":"Kosten/omzet 0.5-2.75%"},{"$f":"$B$38","v":1},{"$f":"$A$38","v":"kosten/toegevoegde waarde 2-26%"},1,"Kosten/EBIDTA 10-45%"]
[{"$f":"Expressielijsten!G75+Expressielijsten!I75+K75","v":12},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel onhaalbaar: één toetscriterium bevindt zich in het bovengebied van de intermediaire zone en de twee andere in het ondergebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.",0,0,null,1,{"$f":"$A$31","v":"Kosten/omzet 0.5-2.75%"},{"$f":"$B$39","v":10},{"$f":"$A$39","v":"Kosten/toegevoegde waarde 26-50%"},1,"Kosten/EBIDTA 10-45%"]
[{"$f":"Expressielijsten!G76+Expressielijsten!I76+K76","v":102},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,1,{"$f":"$A$31","v":"Kosten/omzet 0.5-2.75%"},{"$f":"$B$40","v":100},{"$f":"$A$40","v":"Kosten/toegevoegde waarde >50%"},1,"Kosten/EBIDTA 10-45%"]
[{"$f":"Expressielijsten!G77+Expressielijsten!I77+K77","v":11},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel haalbaar: Gelet op de stof x impactcategorie (1) is de maatregel als haalbaar te beschouwen, ondanks het feit dat ten minste één van de toetscriteria zich in het bovengebied van de intermediaire zone bevindt.",0,1,null,{"$f":"$B$32","v":10},{"$f":"$A$32","v":"Kosten/omzet 2.75-5%"},{"$f":"$B$37","v":0},{"$f":"$A$37","v":"Kosten/toegevoegde waarde <2%"},1,"Kosten/EBIDTA 10-45%"]
[{"$f":"Expressielijsten!G78+Expressielijsten!I78+K78","v":12},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel onhaalbaar: één toetscriterium bevindt zich in het bovengebied van de intermediaire zone en de twee andere in het ondergebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.",0,0,null,{"$f":"$B$32","v":10},{"$f":"$A$32","v":"Kosten/omzet 2.75-5%"},{"$f":"$B$38","v":1},{"$f":"$A$38","v":"kosten/toegevoegde waarde 2-26%"},1,"Kosten/EBIDTA 10-45%"]
[{"$f":"Expressielijsten!G79+Expressielijsten!I79+K79","v":21},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel onhaalbaar: ten minste twee toetscriteria bevinden zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.",0,0,null,10,{"$f":"$A$32","v":"Kosten/omzet 2.75-5%"},{"$f":"$B$39","v":10},{"$f":"$A$39","v":"Kosten/toegevoegde waarde 26-50%"},1,"Kosten/EBIDTA 10-45%"]
[{"$f":"Expressielijsten!G80+Expressielijsten!I80+K80","v":111},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,10,{"$f":"$A$32","v":"Kosten/omzet 2.75-5%"},{"$f":"$B$40","v":100},{"$f":"$A$40","v":"Kosten/toegevoegde waarde >50%"},1,"Kosten/EBIDTA 10-45%"]
[{"$f":"Expressielijsten!G81+Expressielijsten!I81+K81","v":101},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,{"$f":"$B$33","v":100},{"$f":"$A$33","v":"Kosten/omzet > 5%"},{"$f":"$B$37","v":0},{"$f":"$A$37","v":"Kosten/toegevoegde waarde <2%"},1,"Kosten/EBIDTA 10-45%"]
[{"$f":"Expressielijsten!G82+Expressielijsten!I82+K82","v":102},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,{"$f":"$B$33","v":100},{"$f":"$A$33","v":"Kosten/omzet > 5%"},{"$f":"$B$38","v":1},{"$f":"$A$38","v":"kosten/toegevoegde waarde 2-26%"},1,"Kosten/EBIDTA 10-45%"]
[{"$f":"Expressielijsten!G83+Expressielijsten!I83+K83","v":111},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,100,{"$f":"$A$33","v":"Kosten/omzet > 5%"},{"$f":"$B$39","v":10},{"$f":"$A$39","v":"Kosten/toegevoegde waarde 26-50%"},1,"Kosten/EBIDTA 10-45%"]
[{"$f":"Expressielijsten!G84+Expressielijsten!I84+K84","v":201},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,100,{"$f":"$A$33","v":"Kosten/omzet > 5%"},{"$f":"$B$40","v":100},{"$f":"$A$40","v":"Kosten/toegevoegde waarde >50%"},1,"Kosten/EBIDTA 10-45%"]
[{"$f":"Expressielijsten!G85+Expressielijsten!I85+K85","v":10},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel haalbaar: Gelet op de stof x impactcategorie (1) is de maatregel als haalbaar te beschouwen, ondanks het feit dat ten minste één van de toetscriteria zich in het bovengebied van de intermediaire zone bevindt.",0,1,null,{"$f":"$B$30","v":0},{"$f":"$A$30","v":"Kosten/omzet < 0.5%"},{"$f":"$B$37","v":0},{"$f":"$A$37","v":"Kosten/toegevoegde waarde <2%"},{"$f":"$B$46","v":10},{"$f":"$A$46","v":"Kosten/EBIDTA 45-100%"}]
[{"$f":"Expressielijsten!G86+Expressielijsten!I86+K86","v":11},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel haalbaar: Gelet op de stof x impactcategorie (1) is de maatregel als haalbaar te beschouwen, ondanks het feit dat ten minste één van de toetscriteria zich in het bovengebied van de intermediaire zone bevindt.",0,1,null,{"$f":"$B$30","v":0},{"$f":"$A$30","v":"Kosten/omzet < 0.5%"},{"$f":"$B$38","v":1},{"$f":"$A$38","v":"kosten/toegevoegde waarde 2-26%"},{"$f":"$B$46","v":10},{"$f":"$A$46","v":"Kosten/EBIDTA 45-100%"}]
[{"$f":"Expressielijsten!G87+Expressielijsten!I87+K87","v":20},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel onhaalbaar: ten minste twee toetscriteria bevinden zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.",0,0,null,0,{"$f":"$A$30","v":"Kosten/omzet < 0.5%"},{"$f":"$B$39","v":10},{"$f":"$A$39","v":"Kosten/toegevoegde waarde 26-50%"},10,"Kosten/EBIDTA 45-100%"]
[{"$f":"Expressielijsten!G88+Expressielijsten!I88+K88","v":110},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,0,{"$f":"$A$30","v":"Kosten/omzet < 0.5%"},{"$f":"$B$40","v":100},{"$f":"$A$40","v":"Kosten/toegevoegde waarde >50%"},10,"Kosten/EBIDTA 45-100%"]
[{"$f":"Expressielijsten!G89+Expressielijsten!I89+K89","v":11},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel haalbaar: Gelet op de stof x impactcategorie (1) is de maatregel als haalbaar te beschouwen, ondanks het feit dat ten minste één van de toetscriteria zich in het bovengebied van de intermediaire zone bevindt.",0,1,null,{"$f":"$B$31","v":1},{"$f":"$A$31","v":"Kosten/omzet 0.5-2.75%"},{"$f":"$B$37","v":0},{"$f":"$A$37","v":"Kosten/toegevoegde waarde <2%"},10,"Kosten/EBIDTA 45-100%"]
[{"$f":"Expressielijsten!G90+Expressielijsten!I90+K90","v":12},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel onhaalbaar: één toetscriterium bevindt zich in het bovengebied van de intermediaire zone en de twee andere in het ondergebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.",0,0,null,{"$f":"$B$31","v":1},{"$f":"$A$31","v":"Kosten/omzet 0.5-2.75%"},{"$f":"$B$38","v":1},{"$f":"$A$38","v":"kosten/toegevoegde waarde 2-26%"},10,"Kosten/EBIDTA 45-100%"]
[{"$f":"Expressielijsten!G91+Expressielijsten!I91+K91","v":21},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel onhaalbaar: ten minste twee toetscriteria bevinden zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.",0,0,null,1,{"$f":"$A$31","v":"Kosten/omzet 0.5-2.75%"},{"$f":"$B$39","v":10},{"$f":"$A$39","v":"Kosten/toegevoegde waarde 26-50%"},10,"Kosten/EBIDTA 45-100%"]
[{"$f":"Expressielijsten!G92+Expressielijsten!I92+K92","v":111},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,1,{"$f":"$A$31","v":"Kosten/omzet 0.5-2.75%"},{"$f":"$B$40","v":100},{"$f":"$A$40","v":"Kosten/toegevoegde waarde >50%"},10,"Kosten/EBIDTA 45-100%"]
[{"$f":"Expressielijsten!G93+Expressielijsten!I93+K93","v":20},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel onhaalbaar: ten minste twee toetscriteria bevinden zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.",0,0,null,{"$f":"$B$32","v":10},{"$f":"$A$32","v":"Kosten/omzet 2.75-5%"},{"$f":"$B$37","v":0},{"$f":"$A$37","v":"Kosten/toegevoegde waarde <2%"},10,"Kosten/EBIDTA 45-100%"]
[{"$f":"Expressielijsten!G94+Expressielijsten!I94+K94","v":21},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel onhaalbaar: ten minste twee toetscriteria bevinden zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.",0,0,null,{"$f":"$B$32","v":10},{"$f":"$A$32","v":"Kosten/omzet 2.75-5%"},{"$f":"$B$38","v":1},{"$f":"$A$38","v":"kosten/toegevoegde waarde 2-26%"},10,"Kosten/EBIDTA 45-100%"]
[{"$f":"Expressielijsten!G95+Expressielijsten!I95+K95","v":30},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.","Maatregel onhaalbaar: ten minste twee toetscriteria bevinden zich in het bovengebied van de intermediaire zone. Hierdoor kan de maatregel als onhaalbaar beschouwd worden.",0,0,null,10,{"$f":"$A$32","v":"Kosten/omzet 2.75-5%"},{"$f":"$B$39","v":10},{"$f":"$A$39","v":"Kosten/toegevoegde waarde 26-50%"},10,"Kosten/EBIDTA 45-100%"]
[{"$f":"Expressielijsten!G96+Expressielijsten!I96+K96","v":120},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,10,{"$f":"$A$32","v":"Kosten/omzet 2.75-5%"},{"$f":"$B$40","v":100},{"$f":"$A$40","v":"Kosten/toegevoegde waarde >50%"},10,"Kosten/EBIDTA 45-100%"]
[{"$f":"Expressielijsten!G97+Expressielijsten!I97+K97","v":110},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,{"$f":"$B$33","v":100},{"$f":"$A$33","v":"Kosten/omzet > 5%"},{"$f":"$B$37","v":0},{"$f":"$A$37","v":"Kosten/toegevoegde waarde <2%"},10,"Kosten/EBIDTA 45-100%"]
[{"$f":"Expressielijsten!G98+Expressielijsten!I98+K98","v":111},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,{"$f":"$B$33","v":100},{"$f":"$A$33","v":"Kosten/omzet > 5%"},{"$f":"$B$38","v":1},{"$f":"$A$38","v":"kosten/toegevoegde waarde 2-26%"},10,"Kosten/EBIDTA 45-100%"]
[{"$f":"Expressielijsten!G99+Expressielijsten!I99+K99","v":120},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,100,{"$f":"$A$33","v":"Kosten/omzet > 5%"},{"$f":"$B$39","v":10},{"$f":"$A$39","v":"Kosten/toegevoegde waarde 26-50%"},10,"Kosten/EBIDTA 45-100%"]
[{"$f":"Expressielijsten!G100+Expressielijsten!I100+K100","v":210},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,100,{"$f":"$A$33","v":"Kosten/omzet > 5%"},{"$f":"$B$40","v":100},{"$f":"$A$40","v":"Kosten/toegevoegde waarde >50%"},10,"Kosten/EBIDTA 45-100%"]
[{"$f":"Expressielijsten!G101+Expressielijsten!I101+K101","v":100},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,{"$f":"$B$30","v":0},{"$f":"$A$30","v":"Kosten/omzet < 0.5%"},{"$f":"$B$37","v":0},{"$f":"$A$37","v":"Kosten/toegevoegde waarde <2%"},{"$f":"$B$47","v":100},{"$f":"$A$47","v":"Kosten/EBIDTA >100%"}]
[{"$f":"Expressielijsten!G102+Expressielijsten!I102+K102","v":101},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,{"$f":"$B$30","v":0},{"$f":"$A$30","v":"Kosten/omzet < 0.5%"},{"$f":"$B$38","v":1},{"$f":"$A$38","v":"kosten/toegevoegde waarde 2-26%"},{"$f":"$B$47","v":100},{"$f":"$A$47","v":"Kosten/EBIDTA >100%"}]
[{"$f":"Expressielijsten!G103+Expressielijsten!I103+K103","v":110},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,0,{"$f":"$A$30","v":"Kosten/omzet < 0.5%"},{"$f":"$B$39","v":10},{"$f":"$A$39","v":"Kosten/toegevoegde waarde 26-50%"},100,"Kosten/EBIDTA >100%"]
[{"$f":"Expressielijsten!G104+Expressielijsten!I104+K104","v":200},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,0,{"$f":"$A$30","v":"Kosten/omzet < 0.5%"},{"$f":"$B$40","v":100},{"$f":"$A$40","v":"Kosten/toegevoegde waarde >50%"},100,"Kosten/EBIDTA >100%"]
[{"$f":"Expressielijsten!G105+Expressielijsten!I105+K105","v":101},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,{"$f":"$B$31","v":1},{"$f":"$A$31","v":"Kosten/omzet 0.5-2.75%"},{"$f":"$B$37","v":0},{"$f":"$A$37","v":"Kosten/toegevoegde waarde <2%"},100,"Kosten/EBIDTA >100%"]
[{"$f":"Expressielijsten!G106+Expressielijsten!I106+K106","v":102},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,{"$f":"$B$31","v":1},{"$f":"$A$31","v":"Kosten/omzet 0.5-2.75%"},{"$f":"$B$38","v":1},{"$f":"$A$38","v":"kosten/toegevoegde waarde 2-26%"},100,"Kosten/EBIDTA >100%"]
[{"$f":"Expressielijsten!G107+Expressielijsten!I107+K107","v":111},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,1,{"$f":"$A$31","v":"Kosten/omzet 0.5-2.75%"},{"$f":"$B$39","v":10},{"$f":"$A$39","v":"Kosten/toegevoegde waarde 26-50%"},100,"Kosten/EBIDTA >100%"]
[{"$f":"Expressielijsten!G108+Expressielijsten!I108+K108","v":201},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,1,{"$f":"$A$31","v":"Kosten/omzet 0.5-2.75%"},{"$f":"$B$40","v":100},{"$f":"$A$40","v":"Kosten/toegevoegde waarde >50%"},100,"Kosten/EBIDTA >100%"]
[{"$f":"Expressielijsten!G109+Expressielijsten!I109+K109","v":110},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,{"$f":"$B$32","v":10},{"$f":"$A$32","v":"Kosten/omzet 2.75-5%"},{"$f":"$B$37","v":0},{"$f":"$A$37","v":"Kosten/toegevoegde waarde <2%"},100,"Kosten/EBIDTA >100%"]
[{"$f":"Expressielijsten!G110+Expressielijsten!I110+K110","v":111},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,{"$f":"$B$32","v":10},{"$f":"$A$32","v":"Kosten/omzet 2.75-5%"},{"$f":"$B$38","v":1},{"$f":"$A$38","v":"kosten/toegevoegde waarde 2-26%"},100,"Kosten/EBIDTA >100%"]
[{"$f":"Expressielijsten!G111+Expressielijsten!I111+K111","v":120},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,10,{"$f":"$A$32","v":"Kosten/omzet 2.75-5%"},{"$f":"$B$39","v":10},{"$f":"$A$39","v":"Kosten/toegevoegde waarde 26-50%"},100,"Kosten/EBIDTA >100%"]
[{"$f":"Expressielijsten!G112+Expressielijsten!I112+K112","v":210},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,10,{"$f":"$A$32","v":"Kosten/omzet 2.75-5%"},{"$f":"$B$40","v":100},{"$f":"$A$40","v":"Kosten/toegevoegde waarde >50%"},100,"Kosten/EBIDTA >100%"]
[{"$f":"Expressielijsten!G113+Expressielijsten!I113+K113","v":200},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,{"$f":"$B$33","v":100},{"$f":"$A$33","v":"Kosten/omzet > 5%"},{"$f":"$B$37","v":0},{"$f":"$A$37","v":"Kosten/toegevoegde waarde <2%"},100,"Kosten/EBIDTA >100%"]
[{"$f":"Expressielijsten!G114+Expressielijsten!I114+K114","v":201},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,{"$f":"$B$33","v":100},{"$f":"$A$33","v":"Kosten/omzet > 5%"},{"$f":"$B$38","v":1},{"$f":"$A$38","v":"kosten/toegevoegde waarde 2-26%"},100,"Kosten/EBIDTA >100%"]
[{"$f":"Expressielijsten!G115+Expressielijsten!I115+K115","v":210},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,100,{"$f":"$A$33","v":"Kosten/omzet > 5%"},{"$f":"$B$39","v":10},{"$f":"$A$39","v":"Kosten/toegevoegde waarde 26-50%"},100,"Kosten/EBIDTA >100%"]
[{"$f":"Expressielijsten!G116+Expressielijsten!I116+K116","v":300},"Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone","Maatregel onhaalbaar: ten minste één van de toetscriteria bevindt zich in de onhaalbare zone",0,0,null,100,{"$f":"$A$33","v":"Kosten/omzet > 5%"},{"$f":"$B$40","v":100},{"$f":"$A$40","v":"Kosten/toegevoegde waarde >50%"},100,"Kosten/EBIDTA >100%"]
[]
[]
[]
["Criterium 4"]
["Toetsing","Expressielijst"]
["VV reductie bijkomende maatregel > VV reductie huidige maatregel","Bijkomende maatregelen zorgen voor een grotere bijdrage aan de vuilvrachtreductie dan de bestaande maatregelen"]
["VV reductie bijkomende maatregel < VV reductie huidige maatregel","Bijkomende maatregelen zorgen niet voor een grotere bijdrage aan de vuilvrachtreductie dan de bestaande maatregelen"]
["KE bijkomende maatregel (EUR) < KE huidige maatregelen","De kosteneffectiviteit van de bijkomende maatregelen is gunstiger dan die van de bestaande maatregelen"]
["KE bijkomende maatregel (EUR) > KE huidige maatregelen","De kosteneffectiviteit van de bijkomende maatregelen is niet gunstiger dan die van de bestaande maatregelen"]
[]
[]
["Criterium 5 cross media effecten"]
["Toetsing","Expressielijst"]
["Bijdrage > drempel","Significant cross media effect te verwachten"]
["Bijdrage < drempel","Geen significant cross media effect te verwachten"]
[]
["Overige: Ja","Evalueer effecten"]
["Overige: nee","Geen effect"]

{"sheet":"Matrix Stof x impact","index":7,"n_rows":47,"n_cols":12,"rows_kept":47,"cut":false,"hidden":true,"merged":[[0,0,0,1],[38,0,38,1],[29,0,29,1],[43,0,43,1],[0,5,0,9]]}
["Bijdrage",null,null,null,"Deze kolom te checken door VMM","Prio cat"]
["Bovengrens","Ondergrens","Waterrelevante stof Vlaanderen","Duidelijke verslechtering klasse","Prio categorie","Bijdrage","ZZS/PGS/PS (ja=10, nee=20)","Duidelijke achteruitgang/verslechtering klasse","Unieke code","Prio cat_OLD","Priocat_NEW"]
[">100%",0.2,"Ja","Ja",1,{"$f":"IF(B3>=$B$32,$C$32,IF(B3>=$B$33,$C$33,IF(B3>=$B$34,$C$34,IF(B3>=$B$35,$C$35,$C$36))))","v":100},{"$f":"IF(C3=$A$40,$B$40,IF(C3=$A$41,$B$41,\"ERROR\"))","v":10},{"$f":"IF(D3=$A$45,$B$45,IF(D3=$A$46,$B$46,IF(D3=$A$47,$B$47,\"ERROR\")))","v":0},{"$f":"F3+G3+H3","v":110},{"$f":"E3","v":1},1]
[">100%",0.2,"Nee","Ja",1,{"$f":"IF(B4>=$B$32,$C$32,IF(B4>=$B$33,$C$33,IF(B4>=$B$34,$C$34,IF(B4>=$B$35,$C$35,$C$36))))","v":100},{"$f":"IF(C4=$A$40,$B$40,IF(C4=$A$41,$B$41,\"ERROR\"))","v":20},{"$f":"IF(D4=$A$45,$B$45,IF(D4=$A$46,$B$46,IF(D4=$A$47,$B$47,\"ERROR\")))","v":0},120,{"$f":"E4","v":1},1]
[">100%",0.2,"Ja","Nee",1,100,10,0,110,{"$f":"E5","v":1},1]
[">100%",0.2,"Nee","Nee",1,100,20,0,120,{"$f":"E6","v":1},1]
[0.2,0.1,"Ja","Ja",1,200,10,0,210,{"$f":"E7","v":1},1]
[0.2,0.1,"Nee","Ja",2,200,20,0,220,2,1]
[0.2,0.1,"Ja","Nee",2,200,10,0,210,2,1]
[0.2,0.1,"Nee","Nee",2,200,20,0,220,2,1]
[0.1,0.05,"Ja","Niet bepaald",2,300,10,0,310,2,1]
[0.1,0.05,"Nee","Niet bepaald",3,300,20,0,320,3,2]
[0.1,0.05,"Ja","Niet bepaald",2,300,10,0,310,2,1]
[0.1,0.05,"Nee","Niet bepaald",3,300,20,0,320,3,2]
[0.05,0.01,"Ja","Niet bepaald",3,400,10,0,410,3,1]
[0.05,0.01,"Nee","Niet bepaald",4,400,20,0,420,4,2]
[0.05,0.01,"Ja","Niet bepaald",3,400,10,0,410,3,1]
[0.05,0.01,"Nee","Niet bepaald",4,400,20,0,420,4,2,"Checken of je in impacttool dan doorverwezen wordt naar BBT + of niet in dit geval"]
[0.01,0,"Ja","Niet bepaald",5,500,10,0,510,5,3,"Checken of je in impacttool dan doorverwezen wordt naar BBT + of niet in dit geval"]
[0.01,0,"Nee","Niet bepaald",5,500,20,0,520,5,3,"Checken of je in impacttool dan doorverwezen wordt naar BBT + of niet in dit geval"]
[0.01,0,"Ja","Niet bepaald",5,500,10,0,510,5,3,"Checken of je in impacttool dan doorverwezen wordt naar BBT + of niet in dit geval"]
[0.01,0,"Nee","Niet bepaald",5,500,20,0,520,5,3,"Checken of je in impacttool dan doorverwezen wordt naar BBT + of niet in dit geval"]
[]
[]
[]
[]
[]
[]
[]
["Codering bijdrage"]
["Bovengrens","Ondergrens"]
[1,0.2,100]
[0.2,0.1,200]
[0.1,0.05,300]
[0.05,0.01,400]
[0.01,0,500]
[]
[]
["Codering speciale categorie"]
["Ja",10]
["Nee",20]
[]
[]
["Codering achteruitgang",null,"(OLD)"]
["Ja",0,1]
["Nee",0,2]
["Niet bepaald",0,2]

{"sheet":"Info per OWL","index":8,"n_rows":516,"n_cols":8,"rows_kept":516,"cut":false,"hidden":true,"merged":[]}
["Code","Naam waterlichaam","Afstroomzone","Categorie","Type","Stroomgebiedsdistrict","Bekken","Prioritering Code"]
["L107_10","KEMMELBEEK","A0_VL05_2","rivier","Bk"," Schelde","Ijzer",4]
["L107_104","NEERBEEK","A0_VL17_48","rivier","Bk"," Schelde","Leie",5]
["L107_105","PALINGBEEK","A0_VL17_48","rivier","Bk"," Schelde","Leie",5]
["L107_11","WANEBEEK","A0_VL05_2","rivier","Bk"," Schelde","Ijzer",4]
["L107_112","LA HAUTE PLANCHE","A0_VL17_48","rivier","Bk"," Schelde","Leie",5]
["L107_113","DOUVEBEEK","A0_G_L107_113","rivier","Bk"," Schelde","Leie",6]
["L107_116","GROTE SPIERE","A0_G_L107_116","rivier","Bk"," Schelde","Boven-Schelde",5]
["L107_12","VLETERBEEK","A0_VL05_12","rivier","Bk"," Schelde","Ijzer",4]
["L107_120","SCHEEBEEK","A0_VL17_204","rivier","Bk"," Schelde","Boven-Schelde",5]
["L107_122","HET GELEED","A0_VL08_173","rivier","Pb"," Schelde","Brugse Polders",6]
["L107_123","KANAAL VAN BRUGGE NAAR SLUIS","A0_G_L107_123","rivier","Pz"," Schelde","Brugse Polders",6]
["L107_124","RONSELAREBEEK","A0_VL08_173","rivier","Pb"," Schelde","Brugse Polders",6]
["L107_130","KLEINE GEUL","A0_VL05_17","rivier","Pb"," Schelde","Brugse Polders",6]
["L107_131","LISSEWEEGSEVAART","A0_VL17_186","rivier","Pb"," Schelde","Brugse Polders",6]
["L107_133","BLANKENBERGSEVAART L1","A0_VL08_16","rivier","Pb"," Schelde","Brugse Polders",4]
["L107_135","JABBEEKSE BEEK","A0_VL08_164","rivier","Bk"," Schelde","Brugse Polders",5]
["L107_136","HOGE WATERING","A0_VL08_173","rivier","Pz"," Schelde","Brugse Polders",6]
["L107_140","SCHELLEVLIET","A0_VL08_164","rivier","Pb"," Schelde","Brugse Polders",5]
["L107_143","GROOT ZWIN - NOORDGELEED","A0_VL08_164","rivier","Pb"," Schelde","Brugse Polders",5]
["L107_149","PROVINCIEGELEED","A0_VL11_19","rivier","Pb"," Schelde","Ijzer",6]
["L107_150","GRANINGATEVLIET","A0_VL05_6","rivier","Pb"," Schelde","Ijzer",6]
["L107_16","HARINGEBEEK","A0_VL08_7","rivier","Bk"," Schelde","Ijzer",5]
["L107_202","OOSTPOLDERKREEK","A0_VL08_172","rivier","Pb"," Schelde","Gentse Kanalen",4]
["L107_209","ZWARTESLUISBEEK L1","A0_VL08_27","rivier","Pz"," Schelde","Gentse Kanalen",3]
["L107_213","EEKLOSE WATERGANG","A0_VL08_173","rivier","Pb"," Schelde","Brugse Polders",6]
["L107_218","SLEIDINGSVAARDEKEN","A0_VL05_152","rivier","Bk"," Schelde","Gentse Kanalen",3]
["L107_225","KEUTELBEEK","A0_VL08_164","rivier","Bk"," Schelde","Brugse Polders",5]
["L107_234","POEKEBEEK L1","A0_VL21_26","rivier","Bk"," Schelde","Gentse Kanalen",3]
["L107_235","REIGERBEEK","A0_VL21_26","rivier","Bk"," Schelde","Gentse Kanalen",3]
["L107_236","NEERSCHUURBEEK","A0_VL21_26","rivier","Bk"," Schelde","Gentse Kanalen",3]
["L107_237","SPEIBEEK","A0_VL05_53","rivier","Bk"," Schelde","Leie",4]
["L107_239","OUDE MANDEL L1","A0_VL05_53","rivier","Bk"," Schelde","Leie",4]
["L107_240","ZOUBEEK","A0_VL05_50","rivier","Bk"," Schelde","Leie",5]
["L107_241","KATTEBEEK","A0_VL17_54","rivier","Bk"," Schelde","Leie",5]
["L107_242","DUIVEBEEK","A0_VL17_54","rivier","Bk"," Schelde","Leie",5]
["L107_246","STAMPKOTBEEK - MOLENBEEK","A0_VL05_62","rivier","Bk"," Schelde","Boven-Schelde",4]
["L107_247","STAMPKOTBEEK - WALLEBEEK","A0_VL05_62","rivier","Bk"," Schelde","Boven-Schelde",4]
["L107_253","STAMPKOTBEEK - MUNKBOSBEEK","A0_VL05_58","rivier","Bk"," Schelde","Boven-Schelde",5]
["L107_254","MOLENBEEK - BEIAARDBEEK","A0_VL17_204","rivier","Bk"," Schelde","Boven-Schelde",5]
["L107_266","PEERDESTOKBEEK","A0_VL11_63","rivier","Bk"," Schelde","Boven-Schelde",3]
["L107_272","OPHASSELTBEEK","A0_VL05_73","rivier","Bk"," Schelde","Dender",3]
["L107_273","MOLENBEEK - PACHTBOSBEEK L1","A0_VL05_73","rivier","Bk"," Schelde","Dender",3]
["L107_274","MOLENBEEK - KALSTERBEEK","A0_VL05_67","rivier","Bk"," Schelde","Dender",5]
["L107_275","TER ERPENBEEK","A0_VL21_74","rivier","Bk"," Schelde","Dender",3]
["L107_276","MOLENBEEK - GRAADBEEK","A0_VL08_71","rivier","Bk"," Schelde","Dender",5]
["L107_277","WILDEBEEK","A0_VL05_70","rivier","Bk"," Schelde","Dender",5]
["L107_279","MOLENBEEK - VOGELENZANGBEEK","A0_VL17_206","rivier","Bk"," Schelde","Dender",5]
["L107_282","MOLENBEEK - GONDEBEEK","A0_VL11_40","rivier","Bk"," Schelde","Beneden-Schelde",5]
["L107_287","MOLENBEEK - GROTE BEEK","A0_VL05_32","rivier","Bk"," Schelde","Beneden-Schelde",4]
["L107_289","DAMSLOOT","A0_VL11_40","rivier","Bk"," Schelde","Beneden-Schelde",5]
["L107_296","VOORSTESLOOT","A0_VL11_40","rivier","Bk"," Schelde","Beneden-Schelde",5]
["L107_299","VONDELBEEK L1","A0_VL05_75","rivier","Bk"," Schelde","Dender",6]
["L107_3","BROENBEEK","A0_VL11_10","rivier","Bk"," Schelde","Ijzer",6]
["L107_305","ZELEBEEK","A0_VL08_39","rivier","Bk"," Schelde","Beneden-Schelde",4]
["L107_325","GROTE ASTBEEK","A0_VL05_175","rivier","Bk"," Schelde","Gentse Kanalen",4]
["L107_328","ZUIDELIJKE WATERGANG","A0_VL05_34","rivier","Pb"," Schelde","Beneden-Schelde",4]
["L107_329","BLOKSTRAATBEEK","A0_VL11_37","rivier","Pz"," Schelde","Beneden-Schelde",5]
["L107_33","BOMMELAREVAART","A0_VL11_13","rivier","Pb"," Schelde","Ijzer",6]
["L107_330","WATERLOOP VAN DE HOGE LANDEN L1","A0_VL11_37","rivier","Bk"," Schelde","Beneden-Schelde",5]
["L107_333","DOORLOOP","A0_VL17_43","rivier","Pb"," Schelde","Beneden-Schelde",5]
["L107_335","MOLENBEEK - BEVERBEEK","A0_VL17_206","rivier","Bk"," Schelde","Dender",5]
["L107_336","DE RIJT","A0_VL17_206","rivier","Bk"," Schelde","Dender",5]
["L107_34","RINGSLOT","A0_G_L107_34","rivier","Pb"," Schelde","Ijzer",5]
["L107_37","LANGGELEED","A0_VL17_15","rivier","Pb"," Schelde","Ijzer",5]
["L107_4","KORVERSBEEK","A0_VL11_10","rivier","Bk"," Schelde","Ijzer",6]
["L107_40","STENENSLUISVAART","A0_VL21_1","rivier","Pz"," Schelde","Ijzer",3]
["L107_403","MOLENBEEK - NEERPEDEBEEK","A0_G_L107_403","rivier","Bk"," Schelde","Beneden-Schelde",5]
["L107_404","LOTBEEK","A0_VL08_92","rivier","Bk"," Schelde","Dijle Zenne",4]
["L107_407","GROEBENGRACHT","A0_VL08_92","rivier","Bk"," Schelde","Dijle Zenne",4]
["L107_409","KLEINE MAALBEEK","A0_VL11_91","rivier","Bk"," Schelde","Dijle Zenne",4]
["L107_411","MOLENBEEK - PARKBEEK","A0_VL21_79","rivier","Bk"," Schelde","Dijle Zenne",4]
["L107_413","TANGEBEEK","A0_VL05_93","rivier","Bk"," Schelde","Dijle Zenne",5]
["L107_417","DE GROTE LAAK","A0_VL05_81","rivier","Bk"," Schelde","Dijle Zenne",4]
["L107_418","MENE","A0_VL21_107","rivier","Bk"," Schelde","Demer",3]
["L107_421","GENOVEVABEEK","A0_VL21_107","rivier","Bk"," Schelde","Demer",3]
["L107_422","'S HERTOGENGRACHT","A0_VL21_107","rivier","Bk"," Schelde","Demer",3]
["L107_423","BEGIJNEBEEK L1","A0_VL20_96","rivier","Bk"," Schelde","Demer",3]
["L107_424","VIJVERSLOOP","A0_VL20_96","rivier","Bk"," Schelde","Demer",3]
["L107_431","ST-ODULPHUSBEEK","A0_VL11_109","rivier","Bk"," Schelde","Demer",3]
["L107_432","DORMAALBEEK","A0_VL11_109","rivier","Bk"," Schelde","Demer",3]
["L107_433","BEVERBEEK","A0_VL08_72","rivier","Bk"," Schelde","Dender",3]
["L107_434","SCHEIBEEK","A0_VL08_72","rivier","Bk"," Schelde","Dender",3]
["L107_435","AREBEEK","A0_VL08_72","rivier","Bk"," Schelde","Dender",3]
["L107_439","IJSE L1","A0_VL11_83","rivier","Bk"," Schelde","Dijle Zenne",3]
["L107_441","LANGEGRACHT","A0_VL11_83","rivier","Bk"," Schelde","Dijle Zenne",3]
["L107_449","VOER (BERTEM)","A0_VL05_87","rivier","Bk"," Schelde","Dijle Zenne",3]
["L107_451","GROTE LAAK - GROTE LOOP - MESTENLOOP","A0_VL05_103","rivier","BkK"," Schelde","Demer",4]
["L107_452","LAARBEEK","A0_VL05_103","rivier","Bk"," Schelde","Demer",4]
["L107_453","ZWARTEBEEK (SCHERPENHEUVEL-ZICHEM)","A0_VL05_103","rivier","BkK"," Schelde","Demer",4]
["L107_454","KLEINEBEEK - RIJSELSESTRAATVLIET","A0_VL21_97","rivier","BkK"," Schelde","Demer",3]
["L107_462","LEMINGSBEEK","A0_VL05_89","rivier","Bk"," Schelde","Dijle Zenne",3]
["L107_463","AABEEK (MECHELEN)","A0_VL08_95","rivier","Bk"," Schelde","Dijle Zenne",5]
["L107_464","LEYBEEK","A0_VL08_95","rivier","Bk"," Schelde","Dijle Zenne",5]
["L107_47","ZARRENBEEK L1","A0_VL05_180","rivier","Bk"," Schelde","Ijzer",6]
["L107_48","KANAAL VAN ESEN","A0_VL05_3","rivier","Pz"," Schelde","Ijzer",6]
["L107_5","BOLLAERTBEEK","A0_VL05_5","rivier","Bk"," Schelde","Ijzer",5]
["L107_56","REYGAERTSVLIET","A0_VL05_6","rivier","Pb"," Schelde","Ijzer",6]
["L107_6","DIKKEBUSBEEK","A0_VL05_166","rivier","Bk"," Schelde","Ijzer",5]
["L107_60","GROOTGELEED","A0_VL11_11","rivier","Pb"," Schelde","Ijzer",5]
["L107_600","LEYLOOP","A0_G_L107_600","rivier","BkK"," Maas","Maas",4]
["L107_601","DE AA (RAVELS)","A0_G_L107_601","rivier","BkK"," Maas","Maas",4]
["L107_602","BLAUWPUTTEN EN LEILOOP","A0_VL11_145","rivier","BkK"," Maas","Maas",3]
["L107_603","HEERLESE LOOP","A0_VL11_145","rivier","BkK"," Maas","Maas",3]
["L107_607","MERKSKE L1","A0_VL05_146","rivier","BkK"," Maas","Maas",2]
["L107_609","KLEINE MARK","A0_VL11_145","rivier","BkK"," Maas","Maas",3]
["L107_61","VAARTDIJKGELEED","A0_VL11_11","rivier","Pz"," Schelde","Ijzer",5]
["L107_610","MARK L1","A0_VL11_145","rivier","BkK"," Maas","Maas",3]
["L107_613","SLUISKENSVIJVER","A0_VL05_148","rivier","BkK"," Maas","Maas",3]
["L107_614","WEERIJSEBEEK L1","A0_VL05_148","rivier","BkK"," Maas","Maas",3]
["L107_615","KLEINE BEEK (WUUSTWEZEL)","A0_VL05_148","rivier","BkK"," Maas","Maas",3]
["L107_629","KLEIN WILBOEREBEEK","A0_VL21_129","rivier","BkK"," Schelde","Nete",2]
["L107_63","BOERGONJEVAART","A0_VL11_11","rivier","Pz"," Schelde","Ijzer",5]
["L107_631","MOLENBEEK - BOLLAAK L1","A0_VL21_129","rivier","BkK"," Schelde","Nete",2]
["L107_632","DE DELFTE BEEK","A0_VL21_129","rivier","BkK"," Schelde","Nete",2]
["L107_633","BOSBEEK - DIEPTELOOP","A0_VL05_121","rivier","BkK"," Schelde","Nete",3]
["L107_638","GROTE CALIE","A0_VL11_120","rivier","BkK"," Schelde","Nete",3]
["L107_640","DE AA - NATTENLOOP","A0_VL11_120","rivier","BkK"," Schelde","Nete",3]
["L107_644","ITTERBEEK (DUFFEL)","A0_VL08_132","rivier","Bk"," Schelde","Nete",4]
["L107_648","BRUINBEEK","A0_VL11_88","rivier","Bk"," Schelde","Dijle Zenne",3]
["L107_650","REEHAGENBEEK","A0_VL11_88","rivier","Bk"," Schelde","Dijle Zenne",3]
["L107_654","LARUMSE LOOP","A0_VL11_127","rivier","BkK"," Schelde","Nete",2]
["L107_655","DALEMANSLOOP","A0_VL11_127","rivier","BkK"," Schelde","Nete",2]
["L107_656","BEGGELBEEK","A0_VL08_132","rivier","Bk"," Schelde","Nete",4]
["L107_66","KERKBEEK","A0_VL05_18","rivier","Bk"," Schelde","Brugse Polders",4]
["L107_664","MOLENBEEK - ZIJP","A0_VL05_30","rivier","Bk"," Schelde","Beneden-Schelde",3]
["L107_665","BOUWBEEK","A0_VL05_30","rivier","Bk"," Schelde","Beneden-Schelde",3]
["L107_67","LIJSTERBEEK","A0_VL05_18","rivier","Bk"," Schelde","Brugse Polders",4]
["L107_677","DIEPE BEEK","A0_VL17_29","rivier","BkK"," Schelde","Beneden-Schelde",3]
["L107_681","KOUDE BEEK","A0_VL17_29","rivier","BkK"," Schelde","Beneden-Schelde",3]
["L107_684","SCHOON SCHIJN","A0_VL20_36","rivier","Pz"," Schelde","Beneden-Schelde",4]
["L107_688","LAARSE BEEK","A0_VL17_35","rivier","BkK"," Schelde","Beneden-Schelde",4]
["L107_695","VARENDONKSE BEEK","A0_VL05_124","rivier","BkK"," Schelde","Nete",4]
["L107_702","MILLEGEMLOOP","A0_VL11_128","rivier","BkK"," Schelde","Nete",3]
["L107_705","SCHEPPELIJKE NETE","A0_VL11_128","rivier","BkK"," Schelde","Nete",3]
["L107_706","MOLSE NETE L1","A0_VL11_128","rivier","BkK"," Schelde","Nete",3]
["L107_708","GROTE NETE L1","A0_VL11_123","rivier","BkK"," Schelde","Nete",2]
["L107_722","WAMP L1","A0_VL05_130","rivier","BkK"," Schelde","Nete",2]
["L107_723","RODE LOOP","A0_VL05_130","rivier","BkK"," Schelde","Nete",2]
["L107_729","STAPKENSLOOP","A0_VL05_131","rivier","BkK"," Schelde","Nete",3]
["L107_735","GESTELBEEK","A0_VL08_132","rivier","BkK"," Schelde","Nete",4]
["L107_740","BERGEBEEK","A0_VL08_125","rivier","Bk"," Schelde","Nete",4]
["L107_741","SPILLEBEEK","A0_G_L107_741","rivier","BkK"," Maas","Maas",4]
["L107_742","PLATTE BEEK","A0_VL05_121","rivier","BkK"," Schelde","Nete",3]
["L107_78","DEVEBEEK L1","A0_VL05_44","rivier","Bk"," Schelde","Leie",6]
["L107_8","IEPERLEE","A0_VL05_166","rivier","Bk"," Schelde","Ijzer",6]
["L107_809","KLEINE HERK L1","A0_VL05_108","rivier","Bk"," Schelde","Demer",3]
["L107_810","WINTERBEEK (KORTESSEM)","A0_VL05_113","rivier","Bk"," Schelde","Demer",3]
["L107_812","MOMBEEK L1","A0_VL05_113","rivier","Bk"," Schelde","Demer",3]
["L107_814","STEENLAAK","A0_VL11_205","rivier","BkK"," Schelde","Demer",3]
["L107_82","BABILLEBEEK","A0_VL05_51","rivier","Bk"," Schelde","Leie",6]
["L107_824","ROELBEEK","A0_VL05_105","rivier","Bk"," Schelde","Demer",4]
["L107_83","ROOBEEK","A0_VL05_51","rivier","Bk"," Schelde","Leie",6]
["L107_836","LAAMBEEK","A0_VL05_110","rivier","BkK"," Schelde","Demer",2]
["L107_839","ZONDERIKBEEK","A0_VL11_205","rivier","BkK"," Schelde","Demer",3]
["L107_84","KROMMEBEEK","A0_VL05_51","rivier","Bk"," Schelde","Leie",6]
["L107_846","KAATSBEEK","A0_VL05_99","rivier","BkK"," Schelde","Demer",3]
["L107_847","WINTERBEEK (BILZEN)","A0_VL05_98","rivier","Bk"," Schelde","Demer",3]
["L107_848","DEMER L1","A0_VL05_98","rivier","Bk"," Schelde","Demer",3]
["L107_852","MUNSTERBEEK L1","A0_VL05_114","rivier","BkK"," Schelde","Demer",2]
["L107_853","ZUTENDAALBEEK","A0_VL05_114","rivier","BkK"," Schelde","Demer",2]
["L107_854","BOLLISENBEEK","A0_VL05_136","rivier","BkK"," Maas","Maas",3]
["L107_855","DOMMEL L1","A0_VL05_136","rivier","BkK"," Maas","Maas",3]
["L107_856","HOLVENLOOP","A0_VL05_136","rivier","BkK"," Maas","Maas",3]
["L107_857","EINDERGATLOOP","A0_VL05_136","rivier","BkK"," Maas","Maas",3]
["L107_858","WARMBEEK L1","A0_VL17_147","rivier","BkK"," Maas","Maas",2]
["L107_859","PRINSENLOOP","A0_G_L107_859","rivier","BkK"," Maas","Maas",2]
["L107_861","ABEEK L1","A0_VL11_133","rivier","BkK"," Maas","Maas",3]
["L107_866","LOSSING L1","A0_VL05_141","rivier","BkK"," Maas","Maas",3]
["L107_869","SOERBEEK","A0_VL11_133","rivier","BkK"," Maas","Maas",3]
["L107_876","BOSBEEK L1","A0_VL05_135","rivier","BkK"," Maas","Maas",3]
["L107_879","VRIETSELBEEK - OUDE MAAS (DILSEN)","A0_VL11_203","rivier","BkK"," Maas","Maas",4]
["L107_883","ZIEPBEEK","A0_VL11_203","rivier","BkK"," Maas","Maas",4]
["L107_885","HEESWATER","A0_VL22_208","rivier","Bk"," Maas","Beneden-Schelde",3]
["L107_890","BEEK - DE BUTH (TONGEREN)","A0_VL21_139","rivier","Bk"," Maas","Maas",5]
["L107_891","VOER (VOEREN)","A0_G_L107_891","rivier","Bk"," Maas","Maas",4]
["L107_892","BEEK (VOEREN)","A0_G_L107_892","rivier","Bk"," Maas","Maas",4]
["L107_893","GULP","A0_G_L107_893","rivier","Bk"," Maas","Maas",4]
["L107_91","PLAATSBEEK","A0_VL17_49","rivier","Bk"," Schelde","Leie",5]
["L107_92","MAALBEEK (LEIEBEKKEN)","A0_VL05_45","rivier","Bk"," Schelde","Leie",4]
["L107_97","KASSELRIJBEEK - WEST","A0_VL05_45","rivier","Bk"," Schelde","Leie",4]
["L107_98","GAVERBEEK","A0_VL05_45","rivier","Bk"," Schelde","Leie",4]
["L110_1100","ZILVERBEEK","A0_G_L110_1100","rivier","Bk"," Schelde","Dijle Zenne",2]
["L111_1001","MARTJEVAART - LEKKERBOTERBEEK","A0_VL11_10","rivier","Bk"," Schelde","Ijzer",6]
["L111_1003","GELUWEBEEK","A0_VL17_48","rivier","Bk"," Schelde","Leie",5]
["L111_1004","RIJTGRACHT","A0_VL17_204","rivier","Bk"," Schelde","Boven-Schelde",5]
["L111_1005","KALSIJDEADER","A0_VL08_173","rivier","Pb"," Schelde","Brugse Polders",6]
["L111_1006","HOOFDSLOOT","A0_VL08_164","rivier","Bk"," Schelde","Brugse Polders",5]
["L111_1007","STEGERSZWIN","A0_VL08_164","rivier","Pb"," Schelde","Brugse Polders",5]
["L111_1010","OOSTKERKEVAART","A0_VL11_13","rivier","Pb"," Schelde","Ijzer",6]
["L111_1011","BOEREKREEK","A0_VL08_172","rivier","Pb"," Schelde","Gentse Kanalen",4]
["L111_1014","MEREBEEK","A0_VL05_24","rivier","Bk"," Schelde","Gentse Kanalen",3]
["L111_1015","OUDE AVAART","A0_VL11_13","rivier","Pb"," Schelde","Ijzer",6]
["L111_1016","WANTEBEEK","A0_VL21_26","rivier","Bk"," Schelde","Gentse Kanalen",3]
["L111_1018","LEEBEEK","A0_VL05_58","rivier","Bk"," Schelde","Boven-Schelde",5]
["L111_1019","MOLENBEEK - MARKEBEEK","A0_VL17_60","rivier","Bk"," Schelde","Boven-Schelde",3]
["L111_1020","OOSSEBEEK","A0_VL17_204","rivier","Bk"," Schelde","Boven-Schelde",5]
["L111_1021","ZWALMBEEK","A0_VL11_63","rivier","Bk"," Schelde","Boven-Schelde",3]
["L111_1022","MOLENBEEK (RONSE)","A0_G_L111_1022","rivier","Bk"," Schelde","Boven-Schelde",5]
["L111_1024","BAVEGEMSE BEEK","A0_VL21_33","rivier","Bk"," Schelde","Beneden-Schelde",4]
["L111_1025","MAANBEEK","A0_VL05_31","rivier","Bk"," Schelde","Beneden-Schelde",2]
["L111_1027","GROOTEBEEK","A0_VL08_71","rivier","Bk"," Schelde","Dender",5]
["L111_1028","LANGELEDE","A0_VL05_175","rivier","Bk"," Schelde","Gentse Kanalen",4]
["L111_1029","KLEINE WATERGANG","A0_VL05_182","rivier","Bk"," Schelde","Gentse Kanalen",3]
["L111_1030","WATERGANG VAN DE MOERBEKEPOLDER","A0_G_L111_1030","rivier","Bk"," Schelde","Gentse Kanalen",4]
["L111_1031","KANAAL VAN STEKENE","A0_VL05_175","rivier","Bk"," Schelde","Gentse Kanalen",4]
["L111_1032","DIJKGRACHT","A0_VL11_37","rivier","Pz"," Schelde","Beneden-Schelde",5]
["L111_1033","PAPENMEERSBEEK","A0_VL17_206","rivier","Bk"," Schelde","Dender",5]
["L111_1034","NIEUWE GRACHT","A0_VL05_153","rivier","Pb"," Schelde","Ijzer",6]
["L111_1035","KOEVAARDEKEN","A0_VL21_1","rivier","Pz"," Schelde","Ijzer",3]
["L111_1037","MOLENBEEK - LAKEBEEK","A0_VL08_92","rivier","Bk"," Schelde","Dijle Zenne",4]
["L111_1038","MAALBEEK - AMELVONNEBEEK","A0_VL22_215","rivier","Bk"," Schelde","Beneden-Schelde",5]
["L111_1039","STEENVOORDBEEK (TERNAT)","A0_VL17_66","rivier","Bk"," Schelde","Dender",3]
["L111_1040","BELLEBEEK L1","A0_VL17_66","rivier","Bk"," Schelde","Dender",3]
["L111_1041","WINGE L1","A0_VL05_116","rivier","Bk"," Schelde","Demer",2]
["L111_1042","LEIBEEK - LIPSEBEEK L1","A0_VL05_85","rivier","Bk"," Schelde","Dijle Zenne",4]
["L111_1043","WEESBEEK L1","A0_VL05_90","rivier","Bk"," Schelde","Dijle Zenne",2]
["L111_1044","KASTEELBEEK","A0_VL05_3","rivier","Bk"," Schelde","Ijzer",6]
["L111_1046","GROTE MOTTE","A0_VL05_104","rivier","Bk"," Schelde","Demer",4]
["L111_1047","BAREBEEK L1","A0_VL11_76","rivier","Bk"," Schelde","Dijle Zenne",3]
["L111_1048","ZIJDELINGSGELEED","A0_VL05_14","rivier","Pb"," Schelde","Ijzer",6]
["L111_1049","MUNTLOOP","A0_VL11_145","rivier","BkK"," Maas","Maas",3]
["L111_1050","WEHAGENBEEK","A0_VL05_148","rivier","BkK"," Maas","Maas",3]
["L111_1052","LAAKBEEK","A0_VL05_121","rivier","BkK"," Schelde","Nete",3]
["L111_1053","MOUBEEK","A0_VL05_18","rivier","Bk"," Schelde","Brugse Polders",4]
["L111_1054","GOORBOSBEEK","A0_VL08_132","rivier","Bk"," Schelde","Nete",4]
["L111_1056","VROUWVLIET L1","A0_VL11_88","rivier","Bk"," Schelde","Dijle Zenne",3]
["L111_1057","GROTE MOLENBEEK L1","A0_VL05_30","rivier","Bk"," Schelde","Beneden-Schelde",3]
["L111_1058","ZWARTE BEEK (WILLEBROEK)","A0_VL17_42","rivier","Bk"," Schelde","Beneden-Schelde",5]
["L111_1059","ZIELBEEK - BOSBEEK L1","A0_VL05_38","rivier","Bk"," Schelde","Beneden-Schelde",4]
["L111_1060","GROOT SCHIJN L1","A0_VL17_29","rivier","BkK"," Schelde","Beneden-Schelde",3]
["L111_1062","HERSELTSELOOP","A0_VL08_125","rivier","Bk"," Schelde","Nete",4]
["L111_1063","STEENKENSBEEK","A0_VL05_124","rivier","Bk"," Schelde","Nete",4]
["L111_1064","ST. TRUDOLEKEN","A0_VL05_21","rivier","Bk"," Schelde","Brugse Polders",4]
["L111_1065","ASBEEK","A0_VL11_123","rivier","BkK"," Schelde","Nete",2]
["L111_1066","LOEIJENS NEETJE","A0_VL11_126","rivier","BkK"," Schelde","Nete",2]
["L111_1067","KLEINE NETE L1","A0_VL11_126","rivier","BkK"," Schelde","Nete",2]
["L111_1069","AFWATERINGSGRACHT","A0_VL20_36","rivier","Pb"," Schelde","Beneden-Schelde",4]
["L111_1070","WIMP L1","A0_VL05_131","rivier","BkK"," Schelde","Nete",3]
["L111_1071","GOORLOOP","A0_VL08_132","rivier","BkK"," Schelde","Nete",4]
["L111_1072","POVERSBEEK","A0_VL05_20","rivier","Bk"," Schelde","Brugse Polders",4]
["L111_1075","MELSTERBEEK L1","A0_VL11_207","rivier","Bk"," Schelde","Demer",4]
["L111_1076","CICINDRIA","A0_VL11_207","rivier","Bk"," Schelde","Demer",4]
["L111_1077","MOLENBEEK (SINT-TRUIDEN)","A0_VL11_207","rivier","Bk"," Schelde","Demer",4]
["L111_1078","GRONDBEEK","A0_VL05_106","rivier","Bk"," Schelde","Demer",4]
["L111_1079","HELDERBEEK","A0_VL11_117","rivier","BkK"," Schelde","Demer",2]
["L111_1080","ZWARTEBEEK L1","A0_VL11_117","rivier","BkK"," Schelde","Demer",2]
["L111_1081","MANGELBEEK L1","A0_VL05_110","rivier","BkK"," Schelde","Demer",2]
["L111_1082","SLANGBEEK","A0_VL11_205","rivier","BkK"," Schelde","Demer",3]
["L111_1083","MISERIKBEEK","A0_VL05_99","rivier","BkK"," Schelde","Demer",3]
["L111_1084","MANDEL L1","A0_VL05_51","rivier","Bk"," Schelde","Leie",6]
["L111_1086","LOZERBROEKBEEK","A0_G_L111_1086","rivier","BkK"," Maas","Maas",4]
["L111_1087","HORSTGATERBEEK","A0_VL05_141","rivier","BkK"," Maas","Maas",3]
["L111_1088","ITTERBEEK L1","A0_VL05_137","rivier","BkK"," Maas","Maas",3]
["L111_1089","WITBEEK","A0_G_L111_1089","rivier","BkK"," Maas","Maas",3]
["L111_1090","ZANDERBEEK","A0_VL11_203","rivier","BkK"," Maas","Maas",4]
["L111_1091","KIKBEEK","A0_VL11_203","rivier","BkK"," Maas","Maas",4]
["L111_1092","ZOUW","A0_G_L111_1092","rivier","Bk"," Maas","Maas",5]
["L111_1093","EZELSBEEK","A0_VL21_139","rivier","Bk"," Maas","Maas",5]
["L111_1094","HEULEBEEK L1","A0_VL21_47","rivier","Bk"," Schelde","Leie",5]
["L111_1095","KLEINE LAAK","A0_VL05_122","rivier","BkK"," Schelde","Nete",4]
["L111_1096","GROTE LAAK L1","A0_VL05_122","rivier","BkK"," Schelde","Nete",4]
["L111_1098","KEIBEEK","A0_VL05_46","rivier","Bk"," Schelde","Leie",4]
["L111_1099","GAVERSE BEEK (BECQUE DE NEUVILLE)","A0_VL17_48","rivier","Bk"," Schelde","Leie",5]
["L111_1101","GROTE KEIGNAERT","A0_VL11_19","rivier","Pb"," Schelde","Ijzer",6]
["L111_1102","KLEINE A - WILDERTSE BEEK","A0_G_L111_1102","rivier","BkK"," Maas","Maas",4]
["L111_1104","DESPIERREBEEK","A0_G_L111_1104","rivier","Bk"," Schelde","Leie",6]
["L111_1105","MELSENBEEK","A0_VL11_40","rivier","Bk"," Schelde","Beneden-Schelde",5]
["L111_1106","DONKSE BEEK","A0_VL17_35","rivier","Pz"," Schelde","Beneden-Schelde",4]
["L111_1107","SLIJKVAART","A0_VL11_13","rivier","Pb"," Schelde","Ijzer",6]
["L111_1108","STEENGRACHT","A0_VL11_13","rivier","Pb"," Schelde","Ijzer",6]
["L111_1109","MOERDIJKVAART L1","A0_VL11_11","rivier","Bk"," Schelde","Ijzer",5]
["L111_1110","EDE","A0_VL22_218","rivier","Bk"," Schelde","Brugse Polders",5]
["L111_1111","GELEEDBEEK - PASSENDALEGELEED","A0_VL08_164","rivier","Pb"," Schelde","Brugse Polders",5]
["L111_1112","ISABELLASTROOM","A0_VL08_157","rivier","Bk"," Schelde","Gentse Kanalen",4]
["L111_1113","LACHENEBEEK","A0_VL08_132","rivier","Bk"," Schelde","Nete",4]
["L111_1114","ANTITANKGRACHT ZUID","A0_VL17_29","rivier","Bk"," Schelde","Beneden-Schelde",3]
["L111_1201","S HERTOGENDIJKSE BEEK","A0_VL20_36","rivier","Pz"," Schelde","Beneden-Schelde",4]
["L111_15","HEIDEBEEK (VLETEREN)","A0_VL05_12","rivier","Pz"," Schelde","Ijzer",4]
["L111_18","ST-MACHUITSBEEK","A0_VL11_13","rivier","Pb"," Schelde","Ijzer",6]
["L111_298","OUDE DENDER","A0_VL08_71","rivier","Bk"," Schelde","Dender",5]
["L111_315","FONDATIEGRACHT","A0_VL05_182","rivier","Bk"," Schelde","Gentse Kanalen",3]
["L111_326","BARBIERBEEK","A0_VL17_42","rivier","Bk"," Schelde","Beneden-Schelde",5]
["L111_419","SCHOORBROEKBEEK","A0_VL21_107","rivier","Bk"," Schelde","Demer",3]
["L111_436","VELPE L1","A0_VL05_115","rivier","Bk"," Schelde","Demer",3]
["L111_624","TAPPELBEEK","A0_VL21_129","rivier","BkK"," Schelde","Nete",2]
["L111_627","KLEINE BEEK (ZANDHOVEN)","A0_VL21_129","rivier","BkK"," Schelde","Nete",2]
["L111_639","VISBEEK","A0_VL11_120","rivier","BkK"," Schelde","Nete",3]
["L111_674","BENEDENVLIET L1","A0_VL05_28","rivier","Bk"," Schelde","Beneden-Schelde",3]
["L111_676","WEZELSE BEEK","A0_VL17_29","rivier","BkK"," Schelde","Beneden-Schelde",3]
["L111_699","SCHERPENBERGLOOP","A0_VL11_123","rivier","BkK"," Schelde","Nete",2]
["L111_707","KLEINE HOOFDGRACHT","A0_VL11_123","rivier","BkK"," Schelde","Nete",2]
["L111_717","DESSELSE NEET","A0_VL11_126","rivier","BkK"," Schelde","Nete",2]
["L111_724","ANTITANKGRACHT NOORD","A0_VL20_36","rivier","Bk"," Schelde","Beneden-Schelde",4]
["L111_844","STIEMER","A0_VL05_99","rivier","BkK"," Schelde","Demer",3]
["L117_1036","ZUUNBEEK L1","A0_VL21_94","rivier","Bk"," Schelde","Dijle Zenne",4]
["L117_1068","HERTSBERGEBEEK - GETEBEEK","A0_VL05_20","rivier","Bk"," Schelde","Brugse Polders",4]
["L117_1073","RIVIERBEEK","A0_VL05_20","rivier","Bk"," Schelde","Brugse Polders",4]
["L117_1074","HERK L1","A0_VL05_108","rivier","Bk"," Schelde","Demer",3]
["L117_1085","WILDERBEEK","A0_VL05_114","rivier","Bk"," Schelde","Demer",2]
["L117_17","STEENVOORDEBEEK (WATOU)","A0_VL05_4","rivier","Bk"," Schelde","Ijzer",6]
["L117_219","BURGGRAVENSTROOM","A0_VL05_152","rivier","Bk"," Schelde","Gentse Kanalen",3]
["L117_232","JOBEEK","A0_VL05_20","rivier","Bk"," Schelde","Brugse Polders",4]
["L117_233","RINGBEEK","A0_VL05_20","rivier","Bk"," Schelde","Brugse Polders",4]
["L117_402","MOLENBEEK - SLAGVIJVERBEEK","A0_VL21_94","rivier","Bk"," Schelde","Dijle Zenne",4]
["L117_659","KREKELBEEK","A0_VL08_132","rivier","BkK"," Schelde","Nete",4]
["L117_673","KLEIN SCHIJN (NOORDELIJK DEEL)","A0_VL22_211","rivier","BkK"," Schelde","Beneden-Schelde",3]
["L117_813","HERKEBEEK","A0_VL05_108","rivier","Bk"," Schelde","Demer",3]
["L118_238","KROMMEDIJKBEEK","A0_VL05_52","rivier","Bk"," Schelde","Onbekend",6]
["L119_675","KLEIN SCHIJN (ZUIDELIJK DEEL)","A0_VL22_211","rivier","BkK"," Schelde","Beneden-Schelde",3]
["L120_1097","KASSELRIJBEEK - OOST","A0_VL05_45","rivier","Bk"," Schelde","Leie",4]
["L121_1045","GROTEBEEK - WINTERBEEK","A0_VL21_97","rivier","BkK"," Schelde","Demer",3]
["L2 Bk","L2 Kleine Beek","nvt","rivier","Bk","nvt","nvt","nvt"]
["VL05_102","DEMER V","A0_VL05_102","rivier","Rg"," Schelde","Demer",4]
["VL05_103","DEMER VI","A0_VL05_103","rivier","Rg"," Schelde","Demer",4]
["VL05_104","DEMER VII","A0_VL05_104","rivier","Rg"," Schelde","Demer",4]
["VL05_105","GETE I","A0_VL05_105","rivier","Rk"," Schelde","Demer",4]
["VL05_106","GETE II","A0_VL05_106","rivier","Rg"," Schelde","Demer",4]
["VL05_108","HERK + KLEINE HERK","A0_VL05_108","rivier","Bg"," Schelde","Demer",3]
["VL05_110","MANGELBEEK","A0_VL05_110","rivier","BgK"," Schelde","Demer",2]
["VL05_113","MOMBEEK","A0_VL05_113","rivier","Bg"," Schelde","Demer",3]
["VL05_114","MUNSTERBEEK","A0_VL05_114","rivier","BgK"," Schelde","Demer",2]
["VL05_115","VELPE","A0_VL05_115","rivier","Bg"," Schelde","Demer",3]
["VL05_116","WINGE","A0_VL05_116","rivier","Bg"," Schelde","Demer",2]
["VL05_118","ZWARTWATER","A0_VL05_118","rivier","Bg"," Schelde","Demer",3]
["VL05_119","VINNE","A0_VL05_119","meer","Ami"," Schelde","Demer",3]
["VL05_12","POPERINGEVAART","A0_VL05_12","rivier","Bg"," Schelde","Ijzer",4]
["VL05_121","AA II","A0_VL05_121","rivier","BgK"," Schelde","Nete",3]
["VL05_122","GROTE LAAK","A0_VL05_122","rivier","BgK"," Schelde","Nete",4]
["VL05_124","GROTE NETE II","A0_VL05_124","rivier","BgK"," Schelde","Nete",4]
["VL05_130","WAMP","A0_VL05_130","rivier","BgK"," Schelde","Nete",2]
["VL05_131","WIMP","A0_VL05_131","rivier","BgK"," Schelde","Nete",3]
["VL05_134","BERWIJN","A0_VL05_134","rivier","Bg"," Maas","Maas",3]
["VL05_135","BOSBEEK","A0_VL05_135","rivier","BgK"," Maas","Maas",3]
["VL05_136","DOMMEL","A0_VL05_136","rivier","BgK"," Maas","Maas",3]
["VL05_137","ITTERBEEK I","A0_VL05_137","rivier","BgK"," Maas","Maas",3]
["VL05_138","ITTERBEEK II","A0_VL05_138","rivier","BgK"," Maas","Maas",3]
["VL05_14","VLADSLOVAART","A0_VL05_14","rivier","Pb"," Schelde","Ijzer",6]
["VL05_140","JEKER II","A0_VL05_140","rivier","Rk"," Maas","Maas",5]
["VL05_141","LOSSING","A0_VL05_141","rivier","BgK"," Maas","Maas",3]
["VL05_146","MERKSKE","A0_VL05_146","rivier","BgK"," Maas","Maas",2]
["VL05_148","WEERIJSEBEEK","A0_VL05_148","rivier","BgK"," Maas","Maas",3]
["VL05_150","AFLEIDINGSKANAAL van de LEIE/SCHIPDONKKANAAL I","A0_VL05_150","rivier","Rg"," Schelde","Gentse Kanalen",6]
["VL05_152","AVRIJEVAART + SLEIDINGSVAARDEKE","A0_VL05_152","rivier","Rk"," Schelde","Gentse Kanalen",3]
["VL05_153","BERGENVAART","A0_VL05_153","rivier","Pb"," Schelde","Ijzer",6]
["VL05_159","KANAAL CHARLEROI-BRUSSEL","A0_VL05_159","rivier","Rg"," Schelde","Dijle Zenne",6]
["VL05_163","KANAAL GENT-OOSTENDE II","A0_VL05_163","rivier","Rg"," Schelde","Gentse Kanalen",6]
["VL05_166","KANAAL IEPER-IJZER","A0_VL05_166","rivier","Rg"," Schelde","Ijzer",6]
["VL05_167","KANAAL LEUVEN-DIJLE","A0_VL05_167","rivier","Rg"," Schelde","Dijle Zenne",6]
["VL05_17","ISABELLAVAART","A0_VL05_17","rivier","Pb"," Schelde","Brugse Polders",6]
["VL05_170","KANAAL VAN BEVERLO","A0_VL05_170","rivier","Rg"," Schelde","Nete",6]
["VL05_171","LEDE","A0_VL05_171","rivier","Bg"," Schelde","Beneden-Schelde",4]
["VL05_175","MOERVAART","A0_VL05_175","rivier","Rg"," Schelde","Gentse Kanalen",4]
["VL05_177","NIEUWE KALE","A0_VL05_177","rivier","Rk"," Schelde","Gentse Kanalen",4]
["VL05_18","KERKEBEEK","A0_VL05_18","rivier","Bg"," Schelde","Brugse Polders",4]
["VL05_180","ZARRENBEEK","A0_VL05_180","rivier","Bg"," Schelde","Ijzer",6]
["VL05_182","ZUIDLEDE","A0_VL05_182","rivier","Rk"," Schelde","Gentse Kanalen",3]
["VL05_188","BLANKAART Spaarbekken","A0_VL05_188","meer","Ami"," Schelde","Ijzer",4]
["VL05_189","BLOKKERSDIJK","A0_VL05_189","meer","Ami"," Schelde","Beneden-Schelde",4]
["VL05_191","DESSELSE ZANDPUTTEN","A0_VL05_191","meer","Awom"," Schelde","Nete",6]
["VL05_192","DONKMEER","A0_VL05_192","meer","Ami"," Schelde","Beneden-Schelde",4]
["VL05_193","EISDEN MIJN","A0_VL05_193","meer","Awe"," Maas","Maas",1]
["VL05_194","GALGENWEEL","A0_VL05_194","meer","Bzl"," Schelde","Beneden-Schelde",4]
["VL05_195","GAVERS HARELBEKE","A0_VL05_195","meer","Awe"," Schelde","Leie",4]
["VL05_196","GRINDPLAS KESSENICH","A0_VL05_196","meer","Awe"," Maas","Maas",4]
["VL05_197","GROTE VIJVER MECHELEN","A0_VL05_197","meer","Awe"," Schelde","nvt",5]
["VL05_198","HAZEWINKEL","A0_VL05_198","meer","Awe"," Schelde","Beneden-Schelde",4]
["VL05_199","KLUIZEN I + II Spaarbekkens","A0_VL05_199","meer","Ami"," Schelde","nvt",4]
["VL05_2","GROTE KEMMELBEEK","A0_VL05_2","rivier","Bg"," Schelde","Ijzer",4]
["VL05_20","RIVIERBEEK + HERTSBERGEBEEK","A0_VL05_20","rivier","Bg"," Schelde","Brugse Polders",4]
["VL05_200","SCHULENSMEER","A0_VL05_200","meer","Awe"," Schelde","Demer",3]
["VL05_201","SPAANJERD + HEERENLAAK","A0_VL05_201","meer","Awe"," Maas","Maas",4]
["VL05_202","SPUIKOM OOSTENDE","A0_VL05_202","meer","Bs"," Schelde","Brugse Polders",6]
["VL05_21","ZUIDERVAARTJE","A0_VL05_21","rivier","Pz"," Schelde","Brugse Polders",4]
["VL05_22","ZWINNEVAART","A0_VL05_22","rivier","Pb"," Schelde","Brugse Polders",4]
["VL05_24","MEREBEEK + BORISGRACHT + LIEVE","A0_VL05_24","rivier","Bg"," Schelde","Gentse Kanalen",3]
["VL05_25","OUDE KALE","A0_VL05_25","rivier","Bg"," Schelde","Gentse Kanalen",3]
["VL05_28","BENEDENVLIET","A0_VL05_28","rivier","Bg"," Schelde","Beneden-Schelde",3]
["VL05_3","HANDZAMEVAART","A0_VL05_3","rivier","Bg"," Schelde","Ijzer",6]
["VL05_30","GROTE MOLENBEEK - DE VLIET","A0_VL05_30","rivier","Bg"," Schelde","Beneden-Schelde",3]
["VL05_31","KALKENSE VAART","A0_VL05_31","rivier","Bg"," Schelde","Beneden-Schelde",2]
["VL05_32","MOLENBEEK - GROTE BEEK","A0_VL05_32","rivier","Bg"," Schelde","Beneden-Schelde",4]
["VL05_34","NOORD-ZUIDVERBINDING","A0_VL05_34","rivier","Pb"," Schelde","Beneden-Schelde",4]
["VL05_38","ZIELBEEK - BOSBEEK","A0_VL05_38","rivier","Bg"," Schelde","Beneden-Schelde",4]
["VL05_4","HEIDEBEEK","A0_VL05_4","rivier","Bg"," Schelde","Ijzer",6]
["VL05_44","DEVEBEEK","A0_VL05_44","rivier","Bg"," Schelde","Leie",6]
["VL05_45","GAVERBEEK I","A0_VL05_45","rivier","Bg"," Schelde","Leie",4]
["VL05_46","GAVERBEEK II","A0_VL05_46","rivier","Bg"," Schelde","Leie",4]
["VL05_5","IEPERLEE + VERWEZEN KANAAL IEPER-KOMEN","A0_VL05_5","rivier","Bg"," Schelde","Ijzer",5]
["VL05_50","LEIE III","A0_VL05_50","rivier","Rg"," Schelde","Leie",5]
["VL05_51","MANDEL I","A0_VL05_51","rivier","Bg"," Schelde","Leie",6]
["VL05_52","MANDEL II","A0_VL05_52","rivier","Bg"," Schelde","Leie",6]
["VL05_53","OUDE MANDEL","A0_VL05_53","rivier","Bg"," Schelde","Leie",4]
["VL05_58","BOVEN-SCHELDE IV","A0_VL05_58","rivier","Rg"," Schelde","Boven-Schelde",5]
["VL05_6","IEPERLEED","A0_VL05_6","rivier","Pb"," Schelde","Ijzer",6]
["VL05_61","RONE","A0_VL05_61","rivier","Bg"," Schelde","Boven-Schelde",5]
["VL05_62","STAMPKOTBEEK","A0_VL05_62","rivier","Bg"," Schelde","Boven-Schelde",4]
["VL05_64","ZWARTE SPIEREBEEK","A0_VL05_64","rivier","Bg"," Schelde","Boven-Schelde",6]
["VL05_67","DENDER I","A0_VL05_67","rivier","Rg"," Schelde","Dender",5]
["VL05_70","DENDER IV","A0_VL05_70","rivier","Rg"," Schelde","Dender",5]
["VL05_73","MOLENBEEK - PACHTBOSBEEK","A0_VL05_73","rivier","Bg"," Schelde","Dender",3]
["VL05_75","VONDELBEEK","A0_VL05_75","rivier","Bg"," Schelde","Dender",6]
["VL05_77","DIJLE I","A0_VL05_77","rivier","Rg"," Schelde","Dijle Zenne",3]
["VL05_81","DIJLE V","A0_VL05_81","rivier","Rg"," Schelde","Dijle Zenne",4]
["VL05_85","LEIBEEK - LAAKBEEK","A0_VL05_85","rivier","Bg"," Schelde","Dijle Zenne",4]
["VL05_86","NETHEN","A0_VL05_86","rivier","Bg"," Schelde","Dijle Zenne",4]
["VL05_87","VOER (Leuven)","A0_VL05_87","rivier","Bg"," Schelde","Dijle Zenne",3]
["VL05_89","VUNT","A0_VL05_89","rivier","Bg"," Schelde","Dijle Zenne",3]
["VL05_90","WEESBEEK","A0_VL05_90","rivier","Bg"," Schelde","Dijle Zenne",2]
["VL05_93","ZENNE II","A0_VL05_93","rivier","Rg"," Schelde","Dijle Zenne",5]
["VL05_98","DEMER I","A0_VL05_98","rivier","Bg"," Schelde","Demer",3]
["VL05_99","DEMER II","A0_VL05_99","rivier","Bg"," Schelde","Demer",3]
["VL08_125","GROTE NETE III","A0_VL08_125","rivier","BgK"," Schelde","Nete",4]
["VL08_132","GETIJDENETES","A0_VL08_132","rivier","Mlz"," Schelde","Nete",4]
["VL08_157","ISABELLAWATERING","A0_VL08_157","rivier","Rk"," Schelde","Gentse Kanalen",4]
["VL08_16","BLANKENBERGSE VAART + NOORDEDE","A0_VL08_16","rivier","Pb"," Schelde","Brugse Polders",4]
["VL08_162","KANAAL GENT-OOSTENDE I + COUPURE + VERBINDINGSKANAAL","A0_VL08_162","rivier","Rg"," Schelde","Gentse Kanalen",4]
["VL08_164","KANAAL GENT-OOSTENDE III","A0_VL08_164","rivier","Rg"," Schelde","Brugse Polders",5]
["VL08_172","LEOPOLDKANAAL I","A0_VL08_172","rivier","Rk"," Schelde","Gentse Kanalen",4]
["VL08_173","LEOPOLDKANAAL II","A0_VL08_173","rivier","Rk"," Schelde","Brugse Polders",6]
["VL08_176","NETEKANAAL","A0_VL08_176","rivier","Rg"," Schelde","Nete",6]
["VL08_178","NOORDELIJKE RINGVAART","A0_VL08_178","rivier","Rg"," Schelde","Gentse Kanalen",6]
["VL08_179","WESTELIJKE RINGVAART","A0_VL08_179","rivier","Rg"," Schelde","Gentse Kanalen",6]
["VL08_27","ZWARTESLUISBEEK","A0_VL08_27","rivier","Pb"," Schelde","Gentse Kanalen",3]
["VL08_39","GETIJDEDURME","A0_VL08_39","rivier","Mlz"," Schelde","Beneden-Schelde",4]
["VL08_41","ZEESCHELDE II","A0_VL08_41","rivier","Mlz"," Schelde","Beneden-Schelde",5]
["VL08_55","BOVEN-SCHELDE I","A0_VL08_55","rivier","Rg"," Schelde","Boven-Schelde",5]
["VL08_7","IJZER I","A0_VL08_7","rivier","Rk"," Schelde","Ijzer",5]
["VL08_71","DENDER V","A0_VL08_71","rivier","Rg"," Schelde","Dender",5]
["VL08_72","MARK (Denderbekken)","A0_VL08_72","rivier","Bg"," Schelde","Dender",3]
["VL08_80","DIJLE IV","A0_VL08_80","rivier","Rg"," Schelde","Dijle Zenne",4]
["VL08_82","DIJLE VI","A0_VL08_82","rivier","Rg"," Schelde","Dijle Zenne",5]
["VL08_92","ZENNE I","A0_VL08_92","rivier","Rg"," Schelde","Dijle Zenne",4]
["VL08_95","GETIJDEDIJLE & GETIJDEZENNE","A0_VL08_95","rivier","Mlz"," Schelde","Dijle Zenne",5]
["VL09_78","DIJLE II","A0_VL09_78","rivier","Rg"," Schelde","Dijle Zenne",3]
["VL11_10","MARTJEVAART","A0_VL11_10","rivier","Bg"," Schelde","Ijzer",6]
["VL11_109","KLEINE GETE + VLOEDGRACHT","A0_VL11_109","rivier","Bg"," Schelde","Demer",3]
["VL11_11","MOERDIJKVAART","A0_VL11_11","rivier","Bg"," Schelde","Ijzer",5]
["VL11_117","ZWARTEBEEK","A0_VL11_117","rivier","BgK"," Schelde","Demer",2]
["VL11_120","AA I","A0_VL11_120","rivier","BgK"," Schelde","Nete",3]
["VL11_123","GROTE NETE I","A0_VL11_123","rivier","BgK"," Schelde","Nete",2]
["VL11_126","KLEINE NETE I","A0_VL11_126","rivier","BgK"," Schelde","Nete",2]
["VL11_127","KLEINE NETE II","A0_VL11_127","rivier","BgK"," Schelde","Nete",2]
["VL11_128","MOL NEET","A0_VL11_128","rivier","BgK"," Schelde","Nete",3]
["VL11_13","VEURNE AMBACHT POLDER WATERLOPEN","A0_VL11_13","rivier","Pb"," Schelde","Ijzer",6]
["VL11_133","ABEEK","A0_VL11_133","rivier","BgK"," Maas","Maas",3]
["VL11_145","MARK (Maas)","A0_VL11_145","rivier","BgK"," Maas","Maas",3]
["VL11_155","BRUGSE REIEN","A0_VL11_155","meer","Ai"," Schelde","Brugse Polders",6]
["VL11_165","KANAAL GENT-TERNEUZEN + GENTSE HAVENDOKKEN","A0_VL11_165","rivier","Rg"," Schelde","Gentse Kanalen",6]
["VL11_19","OOSTENDS KREKENGEBIED","A0_VL11_19","rivier","Pb"," Schelde","Ijzer",6]
["VL11_203","MAAS I+II+III","A0_VL11_203","rivier","Rzg"," Maas","Maas",4]
["VL11_205","DEMER III+IV","A0_VL11_205","rivier","Rk"," Schelde","Demer",3]
["VL11_207","MELSTERBEEK I+II","A0_VL11_207","rivier","Bg"," Schelde","Demer",4]
["VL11_37","WATERLOOP VAN DE HOGE LANDEN + MELKADER","A0_VL11_37","rivier","Pb"," Schelde","Beneden-Schelde",5]
["VL11_40","ZEESCHELDE I","A0_VL11_40","rivier","Mlz"," Schelde","Beneden-Schelde",5]
["VL11_59","GROTE SPIEREBEEK","A0_VL11_59","rivier","Bg"," Schelde","Boven-Schelde",5]
["VL11_63","ZWALM","A0_VL11_63","rivier","Bg"," Schelde","Boven-Schelde",3]
["VL11_76","BAREBEEK","A0_VL11_76","rivier","Bg"," Schelde","Dijle Zenne",3]
["VL11_83","IJSSE","A0_VL11_83","rivier","Bg"," Schelde","Dijle Zenne",3]
["VL11_84","LAAN","A0_VL11_84","rivier","Bg"," Schelde","Dijle Zenne",2]
["VL11_88","VROUWVLIET","A0_VL11_88","rivier","Bg"," Schelde","Dijle Zenne",3]
["VL11_91","WOLUWE","A0_VL11_91","rivier","Bg"," Schelde","Dijle Zenne",4]
["VL17_147","WARMBEEK","A0_VL17_147","rivier","BgK"," Maas","Maas",2]
["VL17_15","HAVENGEUL IJZER","A0_VL17_15","overgangswater","O2zout"," Schelde","Ijzer",5]
["VL17_154","BRAKELEIKEN + LIEVE","A0_VL17_154","rivier","Rk"," Schelde","Gentse Kanalen",3]
["VL17_156","GENTSE BINNENWATEREN","A0_VL17_156","rivier","Rg"," Schelde","Gentse Kanalen",4]
["VL17_161","KANAAL DUINKERKE-NIEUWPOORT","A0_VL17_161","rivier","Rg"," Schelde","Ijzer",6]
["VL17_168","KANAAL PLASSENDALE-NIEUWPOORT","A0_VL17_168","rivier","Rg"," Schelde","Ijzer",6]
["VL17_169","KANAAL ROESELARE-LEIE","A0_VL17_169","rivier","Rg"," Schelde","Leie",6]
["VL17_174","LOKANAAL","A0_VL17_174","rivier","Rk"," Schelde","Ijzer",6]
["VL17_184","BLANKENBERGSE HAVENGEUL + JACHTHAVENS","A0_VL17_184","overgangswater","O2zout"," Schelde","Brugse Polders",6]
["VL17_185","OOSTENDSE HAVENGEUL + DOKKEN","A0_VL17_185","overgangswater","O2zout"," Schelde","Brugse Polders",6]
["VL17_186","ZEEBRUGGE BUITENHAVEN","A0_VL17_186","overgangswater","O2zout"," Schelde","Brugse Polders",6]
["VL17_187","ANTWERPSE HAVENDOKKEN + SCHELDE-RIJNVERBINDING","A0_VL17_187","meer","Bzl"," Schelde","Beneden-Schelde",5]
["VL17_190","BOUDEWIJNKANAAL + ACHTERHAVEN ZEEBRUGGE","A0_VL17_190","meer","Bs"," Schelde","Brugse Polders",6]
["VL17_204","BOVEN-SCHELDE II+III","A0_VL17_204","rivier","Rg"," Schelde","Boven-Schelde",5]
["VL17_206","DENDER II+III","A0_VL17_206","rivier","Rg"," Schelde","Dender",5]
["VL17_29","GROOT SCHIJN","A0_VL17_29","rivier","BgK"," Schelde","Beneden-Schelde",3]
["VL17_35","VERLEGDE SCHIJN - HOOFDGRACHT","A0_VL17_35","rivier","BgK"," Schelde","Beneden-Schelde",4]
["VL17_42","ZEESCHELDE III + RUPEL","A0_VL17_42","overgangswater","O1o"," Schelde","Beneden-Schelde",5]
["VL17_43","ZEESCHELDE IV","A0_VL17_43","overgangswater","O1brak"," Schelde","Beneden-Schelde",5]
["VL17_48","LEIE I","A0_VL17_48","rivier","Rg"," Schelde","Leie",5]
["VL17_49","LEIE II","A0_VL17_49","rivier","Rg"," Schelde","Leie",5]
["VL17_54","TOERISTISCHE LEIE","A0_VL17_54","rivier","Rg"," Schelde","Leie",5]
["VL17_60","MOLENBEEK - MAARKEBEEK","A0_VL17_60","rivier","Bg"," Schelde","Boven-Schelde",3]
["VL17_66","BELLEBEEK","A0_VL17_66","rivier","Bg"," Schelde","Dender",3]
["VL17_9","IJZER III","A0_VL17_9","rivier","Rg"," Schelde","Ijzer",6]
["VL20_36","VERLEGDE SCHIJN - VOORGRACHT","A0_VL20_36","rivier","BgK"," Schelde","Beneden-Schelde",4]
["VL20_96","BEGIJNENBEEK","A0_VL20_96","rivier","Bg"," Schelde","Demer",3]
["VL21_1","BLANKAART WATERLOPEN","A0_VL21_1","rivier","Pz"," Schelde","Ijzer",3]
["VL21_107","GROTE GETE + BORGGRACHT","A0_VL21_107","rivier","Bg"," Schelde","Demer",3]
["VL21_129","MOLENBEEK - BOLLAAK","A0_VL21_129","rivier","BgK"," Schelde","Nete",2]
["VL21_139","JEKER I","A0_VL21_139","rivier","Bg"," Maas","Maas",5]
["VL21_26","POEKEBEEK","A0_VL21_26","rivier","Bg"," Schelde","Gentse Kanalen",3]
["VL21_33","MOLENBEEK - KOTTEMBEEK","A0_VL21_33","rivier","Bg"," Schelde","Beneden-Schelde",4]
["VL21_47","HEULEBEEK","A0_VL21_47","rivier","Bg"," Schelde","Leie",5]
["VL21_74","MOLENBEEK - TER ERPENBEEK","A0_VL21_74","rivier","Bg"," Schelde","Dender",3]
["VL21_79","DIJLE III","A0_VL21_79","rivier","Rg"," Schelde","Dijle Zenne",4]
["VL21_8","IJZER II","A0_VL21_8","rivier","Rg"," Schelde","Ijzer",6]
["VL21_94","ZUUNBEEK","A0_VL21_94","rivier","Bg"," Schelde","Dijle Zenne",4]
["VL21_97","DE HULPE - ZWART WATER","A0_VL21_97","rivier","BgK"," Schelde","Demer",3]
["VL22_208","ALBERTKANAAL - Maasbekken","A0_VL22_208","rivier","Rg"," Maas","Maas",3]
["VL22_209","ALBERTKANAAL - Demerbekken","A0_VL22_209","rivier","Rg"," Schelde","Demer",3]
["VL22_210","ALBERTKANAAL - Netebekken","A0_VL22_210","rivier","Rg"," Schelde","Nete",3]
["VL22_211","ALBERTKANAAL - Benedenscheldebekken","A0_VL22_211","rivier","Rg"," Schelde","Beneden-Schelde",3]
["VL22_212","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Netebekken","A0_VL22_212","rivier","Rg"," Schelde","Nete",4]
["VL22_213","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Maasbekken","A0_VL22_213","rivier","Rg"," Maas","Maas",4]
["VL22_214","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Benedenscheldebekken","A0_VL22_214","rivier","Rg"," Schelde","Beneden-Schelde",4]
["VL22_215","ZEEKANAAL BRUSSEL-SCHELDE - Dijle-Zennebekken","A0_VL22_215","rivier","Rg"," Schelde","Dijle Zenne",5]
["VL22_216","ZEEKANAAL BRUSSEL-SCHELDE - Benedenscheldebekken","A0_VL22_216","rivier","Rg"," Schelde","Beneden-Schelde",5]
["VL22_217","AFLEIDINGSKANAAL van de LEIE II + KANAAL van EEKLO - Bekken van de Gentse kanalen","A0_VL22_217","rivier","Rg"," Schelde","Gentse Kanalen",5]
["VL22_218","AFLEIDINGSKANAAL van de LEIE II - Bekken van de Brugse polders","A0_VL22_218","rivier","Rg"," Schelde","Brugse Polders",5]
["VL22_219","KANAAL BOSSUIT-KORTRIJK - Bovenscheldebekken","A0_VL22_219","rivier","Rg"," Schelde","Boven-Schelde",5]
["VL22_220","KANAAL BOSSUIT-KORTRIJK - Leiebekken","A0_VL22_220","rivier","Rg"," Schelde","Leie",5]
["VL22_221","ZUID-WILLEMSVAART + KANAAL BOCHOLT-HERENTALS (deels) + KANAAL BRIEGDEN-NEERHAREN","A0_VL22_221","rivier","Rg"," Maas","Maas",6]
["VL22_23","ZWIN","A0_VL22_23","overgangswater","O2zout"," Schelde","Brugse Polders",6]

{"sheet":"Keuzelijst parameters","index":9,"n_rows":194,"n_cols":26,"rows_kept":194,"cut":false,"hidden":true,"merged":[]}
["Parameter ID","Parameter Symbool","Parameter","Parameter ID","Parameter Symbool","Eenheid","Eenheid uniform","Waterrelevante stoffen Vlaanderen","Categorie Stofgroep","MKN - JG","MKN - Max","MKN - WL specifiek","Toetswaarde selectie (JG of Max)","Toetswaarde (G-M","Toetswaarde (M-O)","Toetswaarde (O-S)",null,"Parameter","Afwijkende KE (ja/nee)","KE BBT 2020","KE BBT + 2020",null,"parameter","Afkorting","Meetonzekerheid","Opmerking"]
[252,"MCPA","(4-Chloor-2-methylfenoxy)azijnzuur",252,"MCPA","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B2,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":700},{"$f":"IFERROR(VLOOKUP(B2,'MKN - Max'!B:J,7,FALSE),\"\")","v":20000},null,{"$f":"IF(L2=\"ja\",\"Vul MKN aan\",IF(J2<>\"\",J2,K2))","v":700},{"$f":"M2","v":700},null,{"$f":"N2*5","v":3500},null,{"$f":"C2","v":"(4-Chloor-2-methylfenoxy)azijnzuur"},null,null,null,null,{"$f":"C2","v":"(4-Chloor-2-methylfenoxy)azijnzuur"},{"$f":"B2","v":"MCPA"},1.5]
[308,"111CEa","1,1,1-Trichloorethaan",308,"111CEa","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B3,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":20},{"$f":"IFERROR(VLOOKUP(B3,'MKN - Max'!B:J,7,FALSE),\"\")","v":50},null,20,20,null,100,null,"1,1,1-Trichloorethaan",null,null,null,null,"1,1,1-Trichloorethaan","111CEa",1.5]
[309,"1122CEa","1,1,2,2-Tetrachloorethaan",309,"1122CEa","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B4,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":100},{"$f":"IFERROR(VLOOKUP(B4,'MKN - Max'!B:J,7,FALSE),\"\")","v":900},null,100,100,null,500,null,"1,1,2,2-Tetrachloorethaan",null,null,null,null,"1,1,2,2-Tetrachloorethaan","1122CEa",1.5]
[310,"112CEa","1,1,2-Trichloorethaan",310,"112CEa","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B5,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":20},{"$f":"IFERROR(VLOOKUP(B5,'MKN - Max'!B:J,7,FALSE),\"\")","v":300},null,20,20,null,100,null,"1,1,2-Trichloorethaan",null,null,null,null,"1,1,2-Trichloorethaan","112CEa",1.5]
[502,"112CTFEa","1,1,2-Trichloortrifluorethaan",502,"112CTFEa","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B6,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":7},{"$f":"IFERROR(VLOOKUP(B6,'MKN - Max'!B:J,7,FALSE),\"\")","v":70},null,7,7,null,35,null,"1,1,2-Trichloortrifluorethaan",null,null,null,null,"1,1,2-Trichloortrifluorethaan","112CTFEa",1.5,"MOZ aangevuld"]
[311,"11CEa","1,1-Dichloorethaan",311,"11CEa","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B7,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":100},{"$f":"IFERROR(VLOOKUP(B7,'MKN - Max'!B:J,7,FALSE),\"\")","v":8000},null,100,100,null,500,null,"1,1-Dichloorethaan",null,null,null,null,"1,1-Dichloorethaan","11CEa",1.5]
[312,"11CEe","1,1-Dichlooretheen",312,"11CEe","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B8,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":50},{"$f":"IFERROR(VLOOKUP(B8,'MKN - Max'!B:J,7,FALSE),\"\")","v":500},null,50,50,null,250,null,"1,1-Dichlooretheen",null,null,null,null,"1,1-Dichlooretheen","11CEe",1.5]
[316,"1245CBz","1,2,4,5-Tetrachloorbenzeen",316,"1245CBz","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B9,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":9000},{"$f":"IFERROR(VLOOKUP(B9,'MKN - Max'!B:J,7,FALSE),\"\")","v":30000},null,9000,9000,null,45000,null,"1,2,4,5-Tetrachloorbenzeen",null,null,null,null,"1,2,4,5-Tetrachloorbenzeen","1245CBz",1.5]
[471,"12BEa","1,2-Dibroomethaan",471,"12BEa","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B10,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":3.0000000000000001E-3},{"$f":"IFERROR(VLOOKUP(B10,'MKN - Max'!B:J,7,FALSE),\"\")","v":0.4},null,3.0000000000000001E-3,3.0000000000000001E-3,null,1.4999999999999999E-2,null,"1,2-Dibroomethaan",null,null,null,null,"1,2-Dibroomethaan","12BEa",1.5]
[319,"12CEa","1,2-Dichloorethaan",319,"12CEa","µg/L","µg/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B11,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":10},{"$f":"IFERROR(VLOOKUP(B11,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,10,10,null,50,null,"1,2-Dichloorethaan",null,null,null,null,"1,2-Dichloorethaan","12CEa",1.5]
[320,"12CEe","1,2-Dichlooretheen",320,"12CEe","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B12,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":10},{"$f":"IFERROR(VLOOKUP(B12,'MKN - Max'!B:J,7,FALSE),\"\")","v":100},null,10,10,null,50,null,"1,2-Dichlooretheen",null,null,null,null,"1,2-Dichlooretheen","12CEe",1.5]
[321,"12CPa","1,2-Dichloorpropaan",321,"12CPa","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B13,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":400},{"$f":"IFERROR(VLOOKUP(B13,'MKN - Max'!B:J,7,FALSE),\"\")","v":1000},null,400,400,null,2000,null,"1,2-Dichloorpropaan",null,null,null,null,"1,2-Dichloorpropaan","12CPa",1.5]
[323,"13C2Pol","1,3-Dichloor-2-propanol",323,"13C2Pol","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B14,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":100},{"$f":"IFERROR(VLOOKUP(B14,'MKN - Max'!B:J,7,FALSE),\"\")","v":2000},null,100,100,null,500,null,"1,3-Dichloor-2-propanol",null,null,null,null,"1,3-Dichloor-2-propanol","13C2Pol",1.5,"MOZ aangevuld"]
[895,"ct13CPe","1,3-Dichloorpropeen (cis+trans)",895,"ct13CPe","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B15,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":2},{"$f":"IFERROR(VLOOKUP(B15,'MKN - Max'!B:J,7,FALSE),\"\")","v":20},null,2,2,null,10,null,"1,3-Dichloorpropeen (cis+trans)",null,null,null,null,"1,3-Dichloorpropeen (cis+trans)","ct13CPe",1.5]
[330,"1C24NiBz","1-Chloor-2,4-dinitrobenzeen",330,"1C24NiBz","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B16,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":5},{"$f":"IFERROR(VLOOKUP(B16,'MKN - Max'!B:J,7,FALSE),\"\")","v":20},null,5,5,null,25,null,"1-Chloor-2,4-dinitrobenzeen",null,null,null,null,"1-Chloor-2,4-dinitrobenzeen","1C24NiBz",1.5]
[343,"23CPe","2,3-Dichloorpropeen",343,"23CPe","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B17,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":2},{"$f":"IFERROR(VLOOKUP(B17,'MKN - Max'!B:J,7,FALSE),\"\")","v":20},null,2,2,null,10,null,"2,3-Dichloorpropeen",null,null,null,null,"2,3-Dichloorpropeen","23CPe",1.5,"MOZ aangevuld"]
[229,"245-T","2,4,5-Trichloorfenoxyazijnzuur",229,"245-T","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B18,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":2000},{"$f":"IFERROR(VLOOKUP(B18,'MKN - Max'!B:J,7,FALSE),\"\")","v":20000},null,2000,2000,null,10000,null,"2,4,5-Trichloorfenoxyazijnzuur",null,null,null,null,"2,4,5-Trichloorfenoxyazijnzuur","245-T",1.5]
[473,"246C135Az","2,4,6-Trichloor-1,3,5-triazine",473,"246C135Az","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B19,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.1},{"$f":"IFERROR(VLOOKUP(B19,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,0.1,0.1,null,0.5,null,"2,4,6-Trichloor-1,3,5-triazine",null,null,null,null,"2,4,6-Trichloor-1,3,5-triazine","246C135Az",1.5,"MOZ aangevuld"]
[346,"24CFol","2,4-Dichloorfenol",346,"24CFol","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B20,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":2000},{"$f":"IFERROR(VLOOKUP(B20,'MKN - Max'!B:J,7,FALSE),\"\")","v":70000},null,2000,2000,null,10000,null,"2,4-Dichloorfenol","ja",911,9106,null,"2,4-Dichloorfenol","24CFol",1.5]
[230,"24-D","2,4-Dichloorfenoxyazijnzuur",230,"24-D","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B21,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":20000},{"$f":"IFERROR(VLOOKUP(B21,'MKN - Max'!B:J,7,FALSE),\"\")","v":200000},null,20000,20000,null,100000,null,"2,4-Dichloorfenoxyazijnzuur",null,null,null,null,"2,4-Dichloorfenoxyazijnzuur","24-D",1.5]
[348,"2Am4CFol","2-Amino-4-chloorfenol",348,"2Am4CFol","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B22,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":10},{"$f":"IFERROR(VLOOKUP(B22,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,10,10,null,50,null,"2-Amino-4-chloorfenol","ja",911,9106,null,"2-Amino-4-chloorfenol","2Am4CFol",1.5]
[349,"2C13Bdn","2-Chloor-1,3-butadieen",349,"2C13Bdn","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B23,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":10},{"$f":"IFERROR(VLOOKUP(B23,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,10,10,null,50,null,"2-Chloor-1,3-butadieen",null,null,null,null,"2-Chloor-1,3-butadieen","2C13Bdn",1.5,"MOZ aangevuld"]
[351,"2CEol","2-Chloorethanol",351,"2CEol","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B24,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":30},{"$f":"IFERROR(VLOOKUP(B24,'MKN - Max'!B:J,7,FALSE),\"\")","v":300},null,30,30,null,150,null,"2-Chloorethanol",null,null,null,null,"2-Chloorethanol","2CEol",1.5,"MOZ aangevuld"]
[358,"3CPe","3-Chloorpropeen",358,"3CPe","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B25,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":3},{"$f":"IFERROR(VLOOKUP(B25,'MKN - Max'!B:J,7,FALSE),\"\")","v":30},null,3,3,null,15,null,"3-Chloorpropeen",null,null,null,null,"3-Chloorpropeen","3CPe",1.5,"MOZ aangevuld"]
[361,"4C2NiAn","4-Chloor-2-nitroaniline",361,"4C2NiAn","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B26,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":2},{"$f":"IFERROR(VLOOKUP(B26,'MKN - Max'!B:J,7,FALSE),\"\")","v":20},null,2,2,null,10,null,"4-Chloor-2-nitroaniline",null,null,null,null,"4-Chloor-2-nitroaniline","4C2NiAn",1.5,"MOZ aangevuld"]
[363,"4C3MyFol","4-Chloor-3-methylfenol",363,"4C3MyFol","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B27,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":9000},{"$f":"IFERROR(VLOOKUP(B27,'MKN - Max'!B:J,7,FALSE),\"\")","v":90000},null,9000,9000,null,45000,null,"4-Chloor-3-methylfenol","ja",911,9106,null,"4-Chloor-3-methylfenol","4C3MyFol",1.5]
[418,"Acenaft","Acenafteen",418,"Acenaft","ng/L","ng/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - PAK",{"$f":"IFERROR(VLOOKUP(B28,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":60},{"$f":"IFERROR(VLOOKUP(B28,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,60,60,null,300,null,"Acenafteen","ja",2269,{"$f":"T28*10","v":22690},null,"Acenafteen","Acenaft",1.5]
[511,"Acenaftyl","Acenaftyleen",511,"Acenaftyl","ng/L","ng/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - PAK",{"$f":"IFERROR(VLOOKUP(B29,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":4000},{"$f":"IFERROR(VLOOKUP(B29,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,4000,4000,null,20000,null,"Acenaftyleen","ja",2269,{"$f":"T29*10","v":22690},null,"Acenaftyleen","Acenaftyl",1.5]
[1523,"Aclonifen","Aclonifen",1523,"Aclonifen","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B30,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":120},{"$f":"IFERROR(VLOOKUP(B30,'MKN - Max'!B:J,7,FALSE),\"\")","v":120},null,120,120,null,600,null,"Aclonifen",null,null,null,null,"Aclonifen","Aclonifen",1.5,"MOZ aangevuld"]
[284,"AOX","Adsorbeerbare organohalogenen",284,"AOX","µgCl/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B31,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":40},{"$f":"IFERROR(VLOOKUP(B31,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,40,40,null,200,null,"Adsorbeerbare organohalogenen","nee",1000,10000,null,"Adsorbeerbare organohalogenen","AOX",1.5]
[751,"Alachloor","Alachloor",751,"Alachloor","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B32,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":300},{"$f":"IFERROR(VLOOKUP(B32,'MKN - Max'!B:J,7,FALSE),\"\")","v":700},null,300,300,null,1500,null,"Alachloor",null,null,null,null,"Alachloor","Alachloor",1.5]
[996,"ADEIdrin","Aldrin+Dieldrin+Endrin+Isodrin",996,"ADEIdrin","ng/L","ng/L","Ja","VS",{"$f":"IFERROR(VLOOKUP(B33,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":10},{"$f":"IFERROR(VLOOKUP(B33,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,10,10,null,50,null,"Aldrin+Dieldrin+Endrin+Isodrin",null,null,null,null,"Aldrin+Dieldrin+Endrin+Isodrin","ADEIdrin",1.5]
[1204,"a+bEndoS","alfa+beta Endosulfan",1204,"a+bEndoS","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B34,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":5},{"$f":"IFERROR(VLOOKUP(B34,'MKN - Max'!B:J,7,FALSE),\"\")","v":10},null,{"$f":"IF(L34=\"ja\",\"Vul MKN aan\",IF(J34<>\"\",J34,K34))","v":5},{"$f":"M34","v":5},null,{"$f":"N34*5","v":25},null,{"$f":"C34","v":"alfa+beta Endosulfan"},null,null,null,null,{"$f":"C34","v":"alfa+beta Endosulfan"},{"$f":"B34","v":"a+bEndoS"},1.5]
[1205,"a+b+d+gHCHS","alfa+beta+gamma+delta Hexachloorcyclohexaan",1205,"a+b+d+gHCHS","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B35,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":20},{"$f":"IFERROR(VLOOKUP(B35,'MKN - Max'!B:J,7,FALSE),\"\")","v":40},null,20,20,null,100,null,"alfa+beta+gamma+delta Hexachloorcyclohexaan",null,null,null,null,"alfa+beta+gamma+delta Hexachloorcyclohexaan","a+b+d+gHCHS",1.5]
[770,"aaCTol","alfa-alfa-Dichloortolueen",770,"aaCTol","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B36,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":5},{"$f":"IFERROR(VLOOKUP(B36,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,5,5,null,25,null,"alfa-alfa-Dichloortolueen",null,null,null,null,"alfa-alfa-Dichloortolueen","aaCTol",1.5,"MOZ aangevuld"]
[724,"aCTol","alfa-Chloortolueen",724,"aCTol","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B37,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":1},{"$f":"IFERROR(VLOOKUP(B37,'MKN - Max'!B:J,7,FALSE),\"\")","v":10},null,1,1,null,5,null,"alfa-Chloortolueen",null,null,null,null,"alfa-Chloortolueen","aCTol",1.5,"MOZ aangevuld"]
[949,"Alk c","Alkanen, gechloreerde",949,"Alk c","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B38,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.4},{"$f":"IFERROR(VLOOKUP(B38,'MKN - Max'!B:J,7,FALSE),\"\")","v":1.4},null,0.4,0.4,null,2,null,"Alkanen, gechloreerde",null,null,null,null,"Alkanen, gechloreerde","Alk c",1.5,"MOZ aangevuld"]
[19,"NH3","Ammoniak",19,"NH3","mgN/L","mg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B39,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":2.4670000000000001E-2},{"$f":"IFERROR(VLOOKUP(B39,'MKN - Max'!B:J,7,FALSE),\"\")","v":8.2239999999999994E-2},null,2.4670000000000001E-2,2.4670000000000001E-2,null,0.12335,null,"Ammoniak",null,null,null,null,"Ammoniak","NH3",1.2]
[419,"Ant","Anthraceen",419,"Ant","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B40,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":100},{"$f":"IFERROR(VLOOKUP(B40,'MKN - Max'!B:J,7,FALSE),\"\")","v":100},null,100,100,null,500,null,"Anthraceen",null,null,null,null,"Anthraceen","Ant",1.5]
[134,"Sb t","Antimoon, totaal",134,"Sb t","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B41,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":100},{"$f":"IFERROR(VLOOKUP(B41,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,100,100,null,500,null,"Antimoon, totaal",null,null,null,null,"Antimoon, totaal","Sb t",1.3]
[137,"As t","Arseen, totaal",137,"As t","µg/L","µg/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - >5% OW",{"$f":"IFERROR(VLOOKUP(B42,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":5},{"$f":"IFERROR(VLOOKUP(B42,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,5,5,null,25,null,"Arseen, totaal",null,null,null,null,"Arseen, totaal","As t",1.3]
[268,"Atraz","Atrazine",268,"Atraz","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B43,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":600},{"$f":"IFERROR(VLOOKUP(B43,'MKN - Max'!B:J,7,FALSE),\"\")","v":2000},null,600,600,null,3000,null,"Atrazine",null,null,null,null,"Atrazine","Atraz",1.5]
[393,"AzinfosEy","Azinfos-ethyl",393,"AzinfosEy","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B44,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":10},{"$f":"IFERROR(VLOOKUP(B44,'MKN - Max'!B:J,7,FALSE),\"\")","v":100},null,10,10,null,50,null,"Azinfos-ethyl",null,null,null,null,"Azinfos-ethyl","AzinfosEy",1.5]
[394,"AzinfosMy","Azinfos-methyl",394,"AzinfosMy","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B45,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":2},{"$f":"IFERROR(VLOOKUP(B45,'MKN - Max'!B:J,7,FALSE),\"\")","v":10},null,2,2,null,10,null,"Azinfos-methyl",null,null,null,null,"Azinfos-methyl","AzinfosMy",1.5]
[140,"Ba t","Barium, totaal",140,"Ba t","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B46,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":70},{"$f":"IFERROR(VLOOKUP(B46,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,70,70,null,350,null,"Barium, totaal",null,null,null,null,"Barium, totaal","Ba t",1.3]
[456,"Bentazone","Bentazone",456,"Bentazone","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B47,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":50000},{"$f":"IFERROR(VLOOKUP(B47,'MKN - Max'!B:J,7,FALSE),\"\")","v":500000},null,50000,50000,null,250000,null,"Bentazone",null,null,null,null,"Bentazone","Bentazone",1.5]
[212,"Benzeen","Benzeen",212,"Benzeen","µg/L","µg/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B48,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":10},{"$f":"IFERROR(VLOOKUP(B48,'MKN - Max'!B:J,7,FALSE),\"\")","v":50},null,10,10,null,50,null,"Benzeen","ja",1000,10000,null,"Benzeen","Benzeen",1.5]
[435,"Bzdine","Benzidine",435,"Bzdine","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B49,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.6},{"$f":"IFERROR(VLOOKUP(B49,'MKN - Max'!B:J,7,FALSE),\"\")","v":6},null,0.6,0.6,null,3,null,"Benzidine",null,null,null,null,"Benzidine","Bzdine",1.5,"MOZ aangevuld"]
[420,"B(a)A","Benzo(a)anthraceen",420,"B(a)A","ng/L","ng/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - Toekomstige P(G)S",{"$f":"IFERROR(VLOOKUP(B50,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":300},{"$f":"IFERROR(VLOOKUP(B50,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,300,300,null,1500,null,"Benzo(a)anthraceen","ja",2269,{"$f":"T50*10","v":22690},null,"Benzo(a)anthraceen","B(a)A",1.5]
[421,"B(a)P","Benzo(a)pyreen",421,"B(a)P","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B51,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.17},{"$f":"IFERROR(VLOOKUP(B51,'MKN - Max'!B:J,7,FALSE),\"\")","v":270},null,0.17,0.17,null,0.85000000000000009,null,"Benzo(a)pyreen","ja",2269,{"$f":"T51*10","v":22690},null,"Benzo(a)pyreen","B(a)P",1.5]
[422,"B(b)Flu","Benzo(b)fluorantheen",422,"B(b)Flu","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B52,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(B52,'MKN - Max'!B:J,7,FALSE),\"\")","v":17},null,17,17,null,85,null,"Benzo(b)fluorantheen","ja",2269,{"$f":"T52*10","v":22690},null,"Benzo(b)fluorantheen","B(b)Flu",1.5]
[423,"B(ghi)Pe","Benzo(g,h,i)peryleen",423,"B(ghi)Pe","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B53,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(B53,'MKN - Max'!B:J,7,FALSE),\"\")","v":8.1999999999999993},null,8.1999999999999993,8.1999999999999993,null,41,null,"Benzo(g,h,i)peryleen","ja",2269,{"$f":"T53*10","v":22690},null,"Benzo(g,h,i)peryleen","B(ghi)Pe",1.5]
[424,"B(k)Flu","Benzo(k)fluorantheen",424,"B(k)Flu","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B54,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(B54,'MKN - Max'!B:J,7,FALSE),\"\")","v":17},null,17,17,null,85,null,"Benzo(k)fluorantheen","ja",2269,{"$f":"T54*10","v":22690},null,"Benzo(k)fluorantheen","B(k)Flu",1.5]
[143,"Be t","Berylium, totaal",143,"Be t","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B55,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.1},{"$f":"IFERROR(VLOOKUP(B55,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,0.1,0.1,null,0.5,null,"Berylium, totaal",null,null,null,null,"Berylium, totaal","Be t",1.3]
[1522,"Bifenox","Bifenox",1522,"Bifenox","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B56,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":12},{"$f":"IFERROR(VLOOKUP(B56,'MKN - Max'!B:J,7,FALSE),\"\")","v":40},null,12,12,null,60,null,"Bifenox",null,null,null,null,"Bifenox","Bifenox",1.5,"MOZ aangevuld"]
[287,"BZV5","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","mgO2/L","mg/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - >5% OW",{"$f":"IFERROR(VLOOKUP(B57,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":""},null,"ja",null,null,null,null,null,"Biochemisch zuurstofverbruik na 5d.","nee",5,{"$f":"T57*10","v":50},null,"Biochemisch zuurstofverbruik na 5d.","BZV5",1.4]
[478,"b2CiPyEt","bis-(2-Chloorisopropyl)-ether",478,"b2CiPyEt","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B58,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":10},{"$f":"IFERROR(VLOOKUP(B58,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,{"$f":"IF(L58=\"ja\",\"Vul MKN aan\",IF(J58<>\"\",J58,K58))","v":10},{"$f":"M58","v":10},null,{"$f":"N58*5","v":50},null,"bis-(2-Chloorisopropyl)-ether",null,null,null,null,"bis-(2-Chloorisopropyl)-ether","b2CiPyEt",1.5,"MOZ aangevuld"]
[59,"b2EyHyFt","bis-(2-ethylhexyl)-ftalaat",59,"b2EyHyFt","µg/L","µg/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B59,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":1.3},{"$f":"IFERROR(VLOOKUP(B59,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,{"$f":"IF(L59=\"ja\",\"Vul MKN aan\",IF(J59<>\"\",J59,K59))","v":1.3},{"$f":"M59","v":1.3},null,{"$f":"N59*5","v":6.5},null,"bis-(2-ethylhexyl)-ftalaat",null,null,null,null,"bis-(2-ethylhexyl)-ftalaat","b2EyHyFt",1.5]
[900,"bFol-A","bisfenol A",900,"bFol-A","µg/L","µg/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - Toekomstige P(G)S",{"$f":"IFERROR(VLOOKUP(B60,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":1.5},{"$f":"IFERROR(VLOOKUP(B60,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,{"$f":"IF(L60=\"ja\",\"Vul MKN aan\",IF(J60<>\"\",J60,K60))","v":1.5},{"$f":"M60","v":1.5},null,{"$f":"N60*5","v":7.5},null,"bisfenol A","ja",911,9106,null,"bisfenol A","bFol-A",1.5,"MOZ aangevuld"]
[146,"B t","Boor, totaal",146,"B t","µg/L","µg/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio  - >5% OW",{"$f":"IFERROR(VLOOKUP(B61,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":700},{"$f":"IFERROR(VLOOKUP(B61,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,{"$f":"IF(L61=\"ja\",\"Vul MKN aan\",IF(J61<>\"\",J61,K61))","v":700},{"$f":"M61","v":700},null,{"$f":"N61*5","v":3500},null,"Boor, totaal",null,null,null,null,"Boor, totaal","B t",1.3]
[149,"Cd t","Cadmium, totaal",149,"Cd t","µg/L","µg/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B62,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.8},{"$f":"IFERROR(VLOOKUP(B62,'MKN - Max'!B:J,7,FALSE),\"\")","v":4.5},null,{"$f":"IF(L62=\"ja\",\"Vul MKN aan\",IF(J62<>\"\",J62,K62))","v":0.8},{"$f":"M62","v":0.8},null,{"$f":"N62*5","v":4},null,"Cadmium, totaal","ja",2269,38297,null,"Cadmium, totaal","Cd t",1.3]
[288,"CZV","Chemisch zuurstofverbruik",288,"CZV","mgO2/L","mg/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio  - >5% OW",{"$f":"IFERROR(VLOOKUP(B63,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":""},null,"ja",null,null,null,null,null,"Chemisch zuurstofverbruik","nee",2,20,null,"Chemisch zuurstofverbruik","CZV",1.4]
[1206,"CAnS","Chlooranilines",1206,"CAnS","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B64,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":1},{"$f":"IFERROR(VLOOKUP(B64,'MKN - Max'!B:J,7,FALSE),\"\")","v":5},null,{"$f":"IF(L64=\"ja\",\"Vul MKN aan\",IF(J64<>\"\",J64,K64))","v":1},{"$f":"M64","v":1},null,{"$f":"N64*5","v":5},null,"Chlooranilines",null,null,null,null,"Chlooranilines","CAnS",1.5]
[372,"CHAc","Chloorazijnzuur",372,"CHAc","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B65,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.6},{"$f":"IFERROR(VLOOKUP(B65,'MKN - Max'!B:J,7,FALSE),\"\")","v":3},null,0.6,0.6,null,3,null,"Chloorazijnzuur",null,null,null,null,"Chloorazijnzuur","CHAc",1.5,"MOZ aangevuld"]
[373,"CBz","Chloorbenzeen",373,"CBz","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B66,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":6},{"$f":"IFERROR(VLOOKUP(B66,'MKN - Max'!B:J,7,FALSE),\"\")","v":40},null,6,6,null,30,null,{"$f":"C66","v":"Chloorbenzeen"},null,null,null,null,{"$f":"C66","v":"Chloorbenzeen"},{"$f":"B66","v":"CBz"},1.5]
[233,"Cdaan","Chloordaan",233,"Cdaan","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B67,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":2},{"$f":"IFERROR(VLOOKUP(B67,'MKN - Max'!B:J,7,FALSE),\"\")","v":40},null,2,2,null,10,null,"Chloordaan",null,null,null,null,"Chloordaan","Cdaan",1.5]
[1208,"CFolS","Chloorfenolen",1208,"CFolS","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B68,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":20000},{"$f":"IFERROR(VLOOKUP(B68,'MKN - Max'!B:J,7,FALSE),\"\")","v":120000},null,20000,20000,null,100000,null,"Chloorfenolen","ja",911,9106,null,"Chloorfenolen","CFolS",1.5]
[675,"Cfvinfos","Chloorfenvinfos",675,"Cfvinfos","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B69,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":100},{"$f":"IFERROR(VLOOKUP(B69,'MKN - Max'!B:J,7,FALSE),\"\")","v":300},null,100,100,null,500,null,"Chloorfenvinfos",null,null,null,null,"Chloorfenvinfos","Cfvinfos",1.5]
[481,"CNaft","Chloornaftalenen (technisch)",481,"CNaft","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B70,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":1},{"$f":"IFERROR(VLOOKUP(B70,'MKN - Max'!B:J,7,FALSE),\"\")","v":40},null,1,1,null,5,null,"Chloornaftalenen (technisch)",null,null,null,null,"Chloornaftalenen (technisch)","CNaft",1.5]
[1210,"1C2+3+4NiBzS","Chloornitrobenzenen",1210,"1C2+3+4NiBzS","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B71,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":3},{"$f":"IFERROR(VLOOKUP(B71,'MKN - Max'!B:J,7,FALSE),\"\")","v":60},null,3,3,null,15,null,"Chloornitrobenzenen",null,null,null,null,"Chloornitrobenzenen","1C2+3+4NiBzS",1.5,"MOZ aangevuld"]
[482,"CNiTol","Chloornitrotoluenen",482,"CNiTol","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B72,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":3},{"$f":"IFERROR(VLOOKUP(B72,'MKN - Max'!B:J,7,FALSE),\"\")","v":40},null,3,3,null,15,null,"Chloornitrotoluenen",null,null,null,null,"Chloornitrotoluenen","CNiTol",1.5,"MOZ aangevuld"]
[686,"CpfosEy","Chloorpyrifos-ethyl",686,"CpfosEy","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B73,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":30},{"$f":"IFERROR(VLOOKUP(B73,'MKN - Max'!B:J,7,FALSE),\"\")","v":100},null,30,30,null,150,null,"Chloorpyrifos-ethyl",null,null,null,null,"Chloorpyrifos-ethyl","CpfosEy",1.5]
[1212,"CTolS","Chloortoluenen",1212,"CTolS","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B74,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":3},{"$f":"IFERROR(VLOOKUP(B74,'MKN - Max'!B:J,7,FALSE),\"\")","v":200},null,3,3,null,15,null,"Chloortoluenen",null,null,null,null,"Chloortoluenen","CTolS",1.5]
[484,"CTine","Chloortoluidinen",484,"CTine","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B75,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":8},{"$f":"IFERROR(VLOOKUP(B75,'MKN - Max'!B:J,7,FALSE),\"\")","v":60},null,8,8,null,40,null,"Chloortoluidinen",null,null,null,null,"Chloortoluidinen","CTine",1.5]
[753,"Cdazon","Chloridazon",753,"Cdazon","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B76,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":10000},{"$f":"IFERROR(VLOOKUP(B76,'MKN - Max'!B:J,7,FALSE),\"\")","v":20000},null,10000,10000,null,50000,null,"Chloridazon",null,null,null,null,"Chloridazon","Cdazon",1.5]
[4,"Cl-","Chloride",4,"Cl-","mg/L","mg/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio  - >5% OW",null,null,"ja",null,null,null,null,null,"Chloride",null,null,null,null,"Chloride","Cl-",1.3]
[155,"Cr t","Chroom, totaal",155,"Cr t","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B78,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":50},{"$f":"IFERROR(VLOOKUP(B78,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,{"$f":"IF(L78=\"ja\",\"Vul MKN aan\",IF(J78<>\"\",J78,K78))","v":50},{"$f":"M78","v":50},null,{"$f":"N78*5","v":250},null,"Chroom, totaal",null,null,null,null,"Chroom, totaal","Cr t",1.3]
[425,"Chr","Chryseen",425,"Chr","ng/L","ng/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - Toekomstige P(G)S",{"$f":"IFERROR(VLOOKUP(B79,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":1000},{"$f":"IFERROR(VLOOKUP(B79,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,1000,1000,null,5000,null,"Chryseen","ja",2269,{"$f":"T79*10","v":22690},null,"Chryseen","Chr",1.5]
[486,"Cumafos","Cumafos",486,"Cumafos","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B80,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":1},{"$f":"IFERROR(VLOOKUP(B80,'MKN - Max'!B:J,7,FALSE),\"\")","v":10},null,1,1,null,5,null,"Cumafos",null,null,null,null,"Cumafos","Cumafos",1.5]
[26,"CN- t","Cyaniden, totaal",26,"CN- t","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B81,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":50},{"$f":"IFERROR(VLOOKUP(B81,'MKN - Max'!B:J,7,FALSE),\"\")","v":75},null,50,50,null,250,null,"Cyaniden, totaal",null,null,null,null,"Cyaniden, totaal","CN- t",1.3]
[1506,"Cybutrine","Cybutrine",1506,"Cybutrine","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B82,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":2.5},{"$f":"IFERROR(VLOOKUP(B82,'MKN - Max'!B:J,7,FALSE),\"\")","v":16},null,2.5,2.5,null,12.5,null,"Cybutrine",null,null,null,null,"Cybutrine","Cybutrine",1.5,"MOZ aangevuld"]
[1075,"Cypmethrin","Cypermethrin",1075,"Cypmethrin","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B83,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.08},{"$f":"IFERROR(VLOOKUP(B83,'MKN - Max'!B:J,7,FALSE),\"\")","v":0.6},null,0.08,0.08,null,0.4,null,"Cypermethrin",null,null,null,null,"Cypermethrin","Cypmethrin",1.5,"MOZ aangevuld"]
[907,"DDT t","DDT, totaal",907,"DDT t","ng/L","ng/L","Ja","VS",{"$f":"IFERROR(VLOOKUP(B84,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":25},{"$f":"IFERROR(VLOOKUP(B84,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,25,25,null,125,null,"DDT, totaal",null,null,null,null,"DDT, totaal","DDT t",1.5]
[898,"Demeton","Demeton",898,"Demeton","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B85,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":50},{"$f":"IFERROR(VLOOKUP(B85,'MKN - Max'!B:J,7,FALSE),\"\")","v":500},null,50,50,null,250,null,"Demeton",null,null,null,null,"Demeton","Demeton",1.5]
[426,"dBz(ah)An","Dibenzo(a,h)anthraceen",426,"dBz(ah)An","ng/L","ng/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - Toekomstige P(G)S",{"$f":"IFERROR(VLOOKUP(B86,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":500},{"$f":"IFERROR(VLOOKUP(B86,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,500,500,null,2500,null,"Dibenzo(a,h)anthraceen","ja",2269,{"$f":"T86*10","v":22690},null,"Dibenzo(a,h)anthraceen","dBz(ah)An",1.5]
[1216,"DBySn som","Dibutyltinverbindingen",1216,"DBySn som","ngSn/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B87,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":80},{"$f":"IFERROR(VLOOKUP(B87,'MKN - Max'!B:J,7,FALSE),\"\")","v":700},null,80,80,null,400,null,"Dibutyltinverbindingen",null,null,null,null,"Dibutyltinverbindingen","DBySn som",1.5,"MOZ aangevuld"]
[888,"DCAn t","Dichlooranilines, totaal",888,"DCAn t","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B88,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.2},{"$f":"IFERROR(VLOOKUP(B88,'MKN - Max'!B:J,7,FALSE),\"\")","v":0.6},null,0.2,0.2,null,1,null,"Dichlooranilines, totaal",null,null,null,null,"Dichlooranilines, totaal","DCAn t",1.5,"MOZ aangevuld"]
[1218,"CBzsom","Dichloorbenzenen",1218,"CBzsom","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B89,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":20},{"$f":"IFERROR(VLOOKUP(B89,'MKN - Max'!B:J,7,FALSE),\"\")","v":70},null,20,20,null,100,null,"Dichloorbenzenen",null,null,null,null,"Dichloorbenzenen","CBzsom",1.5]
[886,"DCBzdines","Dichloorbenzidines",886,"DCBzdines","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B90,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.5},{"$f":"IFERROR(VLOOKUP(B90,'MKN - Max'!B:J,7,FALSE),\"\")","v":5},null,0.5,0.5,null,2.5,null,"Dichloorbenzidines",null,null,null,null,"Dichloorbenzidines","DCBzdines",1.5,"MOZ aangevuld"]
[379,"DCMa","Dichloormethaan",379,"DCMa","µg/L","µg/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B91,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":20},{"$f":"IFERROR(VLOOKUP(B91,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,20,20,null,100,null,"Dichloormethaan",null,null,null,null,"Dichloormethaan","DCMa",1.5]
[1219,"diCNiBzsom","Dichloornitrobenzenen",1219,"diCNiBzsom","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B92,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":3},{"$f":"IFERROR(VLOOKUP(B92,'MKN - Max'!B:J,7,FALSE),\"\")","v":60},null,3,3,null,15,null,"Dichloornitrobenzenen",null,null,null,null,"Dichloornitrobenzenen","diCNiBzsom",1.5,"MOZ aangevuld"]
[234,"24-DP","Dichloorprop",234,"24-DP","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B93,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":20000},{"$f":"IFERROR(VLOOKUP(B93,'MKN - Max'!B:J,7,FALSE),\"\")","v":200000},null,20000,20000,null,100000,null,"Dichloorprop",null,null,null,null,"Dichloorprop","24-DP",1.5]
[391,"DCvos","Dichloorvos",391,"DCvos","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B94,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.6},{"$f":"IFERROR(VLOOKUP(B94,'MKN - Max'!B:J,7,FALSE),\"\")","v":0.7},null,0.6,0.6,null,3,null,"Dichloorvos",null,null,null,null,"Dichloorvos","DCvos",1.5]
[1464,"Dicofol","Dicofol",1464,"Dicofol","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B95,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":1.3},{"$f":"IFERROR(VLOOKUP(B95,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,1.3,1.3,null,6.5,null,"Dicofol",null,null,null,null,"Dicofol","Dicofol",1.5,"MOZ aangevuld"]
[496,"DEyAm","Diethylamine",496,"DEyAm","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B96,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":30},{"$f":"IFERROR(VLOOKUP(B96,'MKN - Max'!B:J,7,FALSE),\"\")","v":200},null,30,30,null,150,null,"Diethylamine",null,null,null,null,"Diethylamine","DEyAm",1.5,"MOZ aangevuld"]
[498,"DFy","Difenyl",498,"DFy","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B97,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":2},{"$f":"IFERROR(VLOOKUP(B97,'MKN - Max'!B:J,7,FALSE),\"\")","v":10},null,2,2,null,10,null,"Difenyl",null,null,null,null,"Difenyl","DFy",1.5,"MOZ aangevuld"]
[1020,"Dflucan","Diflufenican",1020,"Dflucan","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B98,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":30},{"$f":"IFERROR(VLOOKUP(B98,'MKN - Max'!B:J,7,FALSE),\"\")","v":50},null,30,30,null,150,null,{"$f":"C98","v":"Diflufenican"},null,null,null,null,{"$f":"C98","v":"Diflufenican"},{"$f":"B98","v":"Dflucan"},1.5,"MOZ aangevuld"]
[1231,"DiMetamid","Dimethenamid",1231,"DiMetamid","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B99,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":1.5},{"$f":"IFERROR(VLOOKUP(B99,'MKN - Max'!B:J,7,FALSE),\"\")","v":6.7},null,1.5,1.5,null,7.5,null,"Dimethenamid",null,null,null,null,"Dimethenamid","DiMetamid",1.5,"MOZ aangevuld"]
[396,"Dmetoat","Dimethoaat",396,"Dmetoat","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B100,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":20},{"$f":"IFERROR(VLOOKUP(B100,'MKN - Max'!B:J,7,FALSE),\"\")","v":200},null,20,20,null,100,null,"Dimethoaat",null,null,null,null,"Dimethoaat","Dmetoat",1.5]
[497,"DMyAm","Dimethylamine",497,"DMyAm","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B101,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":6},{"$f":"IFERROR(VLOOKUP(B101,'MKN - Max'!B:J,7,FALSE),\"\")","v":80},null,6,6,null,30,null,"Dimethylamine",null,null,null,null,"Dimethylamine","DMyAm",1.5,"MOZ aangevuld"]
[397,"Dsulfoton","Disulfoton",397,"Dsulfoton","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B102,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":10},{"$f":"IFERROR(VLOOKUP(B102,'MKN - Max'!B:J,7,FALSE),\"\")","v":70},null,10,10,null,50,null,"Disulfoton",null,null,null,null,"Disulfoton","Dsulfoton",1.5,"MOZ aangevuld"]
[273,"Diuron","Diuron",273,"Diuron","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B103,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":200},{"$f":"IFERROR(VLOOKUP(B103,'MKN - Max'!B:J,7,FALSE),\"\")","v":1800},null,200,200,null,1000,null,"Diuron",null,null,null,null,"Diuron","Diuron",1.5]
[779,"eCHydrine","Epichloorhydrine",779,"eCHydrine","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B104,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":10},{"$f":"IFERROR(VLOOKUP(B104,'MKN - Max'!B:J,7,FALSE),\"\")","v":100},null,10,10,null,50,null,"Epichloorhydrine",null,null,null,null,"Epichloorhydrine","eCHydrine",1.5,"MOZ aangevuld"]
[213,"EyBz","Ethylbenzeen",213,"EyBz","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B105,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":5},{"$f":"IFERROR(VLOOKUP(B105,'MKN - Max'!B:J,7,FALSE),\"\")","v":50},null,5,5,null,25,null,"Ethylbenzeen","ja",1000,10000,null,"Ethylbenzeen","EyBz",1.5]
[428,"Fen","Fenantreen",428,"Fen","ng/L","ng/L","ja","VMM stroomgebiedspecifieke stoffen - VMM prio - PAK",{"$f":"IFERROR(VLOOKUP(B106,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":100},{"$f":"IFERROR(VLOOKUP(B106,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,100,100,null,500,null,"Fenantreen","ja",2269,{"$f":"T106*10","v":22690},null,"Fenantreen","Fen",1.5]
[399,"Fenithion","Fenitrothion",399,"Fenithion","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B107,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.9},{"$f":"IFERROR(VLOOKUP(B107,'MKN - Max'!B:J,7,FALSE),\"\")","v":2},null,0.9,0.9,null,4.5,null,"Fenitrothion",null,null,null,null,"Fenitrothion","Fenithion",1.5]
[500,"Fenthion","Fenthion",500,"Fenthion","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B108,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.2},{"$f":"IFERROR(VLOOKUP(B108,'MKN - Max'!B:J,7,FALSE),\"\")","v":2},null,0.2,0.2,null,1,null,"Fenthion",null,null,null,null,"Fenthion","Fenthion",1.5]
[976,"Flucet","Flufenacet",976,"Flucet","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B109,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":40},{"$f":"IFERROR(VLOOKUP(B109,'MKN - Max'!B:J,7,FALSE),\"\")","v":200},null,40,40,null,200,null,"Flufenacet",null,null,null,null,"Flufenacet","Flucet",1.5,"MOZ aangevuld"]
[429,"Flu","Fluorantheen",429,"Flu","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B110,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":6.3},{"$f":"IFERROR(VLOOKUP(B110,'MKN - Max'!B:J,7,FALSE),\"\")","v":120},null,6.3,6.3,null,31.5,null,"Fluorantheen","ja",2269,{"$f":"T110*10","v":22690},null,"Fluorantheen","Flu",1.5]
[430,"Fluoreen","Fluoreen",430,"Fluoreen","ng/L","ng/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - PAK",{"$f":"IFERROR(VLOOKUP(B111,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":2000},{"$f":"IFERROR(VLOOKUP(B111,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,2000,2000,null,10000,null,"Fluoreen","ja",2269,{"$f":"T111*10","v":22690},null,"Fluoreen","Fluoreen",1.5]
[1328,"F- o","Fluoride, opgelost",1328,"F- o","mg/L","mg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B112,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.9},{"$f":"IFERROR(VLOOKUP(B112,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,0.9,0.9,null,4.5,null,"Fluoride, opgelost",null,null,null,null,"Fluoride, opgelost","F- o",1.3]
[29,"P t","Fosfor, totaal",29,"P t","mgP/L","mg/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - >5% OW",null,null,"ja",null,null,null,null,null,"Fosfor, totaal","ja",20,200,null,"Fosfor, totaal","P t",1.3]
[400,"Foxim","Foxim",400,"Foxim","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B114,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.02},{"$f":"IFERROR(VLOOKUP(B114,'MKN - Max'!B:J,7,FALSE),\"\")","v":0.2},null,{"$f":"IF(L114=\"ja\",\"Vul MKN aan\",IF(J114<>\"\",J114,K114))","v":0.02},{"$f":"M114","v":0.02},null,{"$f":"N114*5","v":0.1},null,"Foxim",null,null,null,null,"Foxim","Foxim",1.5,"MOZ aangevuld"]
[82,"EC 20","Geleidbaarheid (20°C)",82,"EC 20","µS/cm","µS/cm","Nee",null,null,null,"ja",null,null,null,null,null,"Geleidbaarheid (20°C)",null,null,null,null,"Geleidbaarheid (20°C)","EC 20",1.2]
[948,"HpC+Epx","Heptachloor+epoxyde",948,"HpC+Epx","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B116,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":2.0000000000000001E-4},{"$f":"IFERROR(VLOOKUP(B116,'MKN - Max'!B:J,7,FALSE),\"\")","v":0.3},null,{"$f":"IF(L116=\"ja\",\"Vul MKN aan\",IF(J116<>\"\",J116,K116))","v":2.0000000000000001E-4},{"$f":"M116","v":2.0000000000000001E-4},null,{"$f":"N116*5","v":1E-3},null,"Heptachloor+epoxyde",null,null,null,null,"Heptachloor+epoxyde","HpC+Epx",1.5]
[939,"HBCD","Hexabroomcyclododecaan",939,"HBCD","µg/L","µg/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B117,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":1.6000000000000001E-3},{"$f":"IFERROR(VLOOKUP(B117,'MKN - Max'!B:J,7,FALSE),\"\")","v":0.5},null,1.6000000000000001E-3,1.6000000000000001E-3,null,8.0000000000000002E-3,null,"Hexabroomcyclododecaan",null,null,null,null,"Hexabroomcyclododecaan","HBCD",1.5]
[244,"HCBz","Hexachloorbenzeen",244,"HCBz","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B118,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":4.3999999999999997E-2},{"$f":"IFERROR(VLOOKUP(B118,'MKN - Max'!B:J,7,FALSE),\"\")","v":50},null,4.3999999999999997E-2,4.3999999999999997E-2,null,0.21999999999999997,null,"Hexachloorbenzeen",null,null,null,null,"Hexachloorbenzeen","HCBz",1.5]
[245,"HCBdn","Hexachloorbutadieen",245,"HCBdn","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B119,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.55000000000000004},{"$f":"IFERROR(VLOOKUP(B119,'MKN - Max'!B:J,7,FALSE),\"\")","v":600},null,0.55000000000000004,0.55000000000000004,null,2.75,null,"Hexachloorbutadieen",null,null,null,null,"Hexachloorbutadieen","HCBdn",1.5]
[381,"HCEa","Hexachloorethaan",381,"HCEa","µg/L","µg/L",null,null,{"$f":"IFERROR(VLOOKUP(B120,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":3},{"$f":"IFERROR(VLOOKUP(B120,'MKN - Max'!B:J,7,FALSE),\"\")","v":80},null,3,3,null,15,null,"Hexachloorethaan",null,null,null,null,"Hexachloorethaan","HCEa",1.5]
[1440,"Imcloprid","Imidacloprid",1440,"Imcloprid","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B121,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":8.0000000000000002E-3},{"$f":"IFERROR(VLOOKUP(B121,'MKN - Max'!B:J,7,FALSE),\"\")","v":0.2},null,8.0000000000000002E-3,8.0000000000000002E-3,null,0.04,null,"Imidacloprid",null,null,null,null,"Imidacloprid","Imcloprid",1.5,"MOZ aangevuld"]
[221,"iPyBz","Isopropylbenzeen",221,"iPyBz","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B122,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":1},{"$f":"IFERROR(VLOOKUP(B122,'MKN - Max'!B:J,7,FALSE),\"\")","v":10},null,1,1,null,5,null,"Isopropylbenzeen",null,null,null,null,"Isopropylbenzeen","iPyBz",1.5]
[274,"Iproturon","Isoproturon",274,"Iproturon","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B123,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":300},{"$f":"IFERROR(VLOOKUP(B123,'MKN - Max'!B:J,7,FALSE),\"\")","v":1000},null,300,300,null,1500,null,"Isoproturon",null,null,null,null,"Isoproturon","Iproturon",1.5]
[162,"Co t","Kobalt, totaal",162,"Co t","µg/L","µg/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - >5% OW",{"$f":"IFERROR(VLOOKUP(B124,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.6},{"$f":"IFERROR(VLOOKUP(B124,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,0.6,0.6,null,3,null,"Kobalt, totaal","ja",450,4500,null,"Kobalt, totaal","Co t",1.3]
[165,"Cu t","Koper, totaal",165,"Cu t","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B125,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":50},{"$f":"IFERROR(VLOOKUP(B125,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,50,50,null,250,null,"Koper, totaal","ja",450,4500,null,"Koper, totaal","Cu t",1.3]
[168,"Hg t","Kwik, totaal",168,"Hg t","µg/L","µg/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B126,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":6.9999999999999994E-5},{"$f":"IFERROR(VLOOKUP(B126,'MKN - Max'!B:J,7,FALSE),\"\")","v":0.15},null,6.9999999999999994E-5,6.9999999999999994E-5,null,3.4999999999999994E-4,null,"Kwik, totaal","ja",10264,102642,null,"Kwik, totaal","Hg t",1.4]
[275,"Linuron","Linuron",275,"Linuron","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B127,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":300},{"$f":"IFERROR(VLOOKUP(B127,'MKN - Max'!B:J,7,FALSE),\"\")","v":700},null,300,300,null,1500,null,"Linuron",null,null,null,null,"Linuron","Linuron",1.5]
[171,"Pb t","Lood, totaal",171,"Pb t","µg/L","µg/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B128,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":50},{"$f":"IFERROR(VLOOKUP(B128,'MKN - Max'!B:J,7,FALSE),\"\")","v":97.22},null,50,50,null,250,null,"Lood, totaal","ja",800,8000,null,"Lood, totaal","Pb t",1.3]
[401,"Malathion","Malathion",401,"Malathion","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B129,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.8},{"$f":"IFERROR(VLOOKUP(B129,'MKN - Max'!B:J,7,FALSE),\"\")","v":3},null,0.8,0.8,null,4,null,"Malathion",null,null,null,null,"Malathion","Malathion",1.5]
[253,"MCPP","Mecoprop",253,"MCPP","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B130,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":10000},{"$f":"IFERROR(VLOOKUP(B130,'MKN - Max'!B:J,7,FALSE),\"\")","v":40000},null,10000,10000,null,50000,null,{"$f":"C130","v":"Mecoprop"},null,null,null,null,{"$f":"C130","v":"Mecoprop"},{"$f":"B130","v":"MCPP"},1.5]
[402,"Methamfos","Methamidofos",402,"Methamfos","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B131,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.3},{"$f":"IFERROR(VLOOKUP(B131,'MKN - Max'!B:J,7,FALSE),\"\")","v":3},null,0.3,0.3,null,1.5,null,"Methamidofos",null,null,null,null,"Methamidofos","Methamfos",1.5,"MOZ aangevuld"]
[392,"Mevinfos","Mevinfos",392,"Mevinfos","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B132,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":2},{"$f":"IFERROR(VLOOKUP(B132,'MKN - Max'!B:J,7,FALSE),\"\")","v":20},null,2,2,null,10,null,"Mevinfos",null,null,null,null,"Mevinfos","Mevinfos",1.5]
[177,"Mo t","Molybdeen, totaal",177,"Mo t","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B133,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":350},{"$f":"IFERROR(VLOOKUP(B133,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,350,350,null,1750,null,"Molybdeen, totaal",null,null,null,null,"Molybdeen, totaal","Mo t",1.3]
[278,"Mlinuron","Monolinuron",278,"Mlinuron","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B134,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":300},{"$f":"IFERROR(VLOOKUP(B134,'MKN - Max'!B:J,7,FALSE),\"\")","v":10000},null,300,300,null,1500,null,"Monolinuron",null,null,null,null,"Monolinuron","Mlinuron",1.5]
[432,"Naft","Naftaleen",432,"Naft","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B135,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":2000},{"$f":"IFERROR(VLOOKUP(B135,'MKN - Max'!B:J,7,FALSE),\"\")","v":130000},null,2000,2000,null,10000,null,"Naftaleen","ja",3493,34925,null,"Naftaleen","Naft",1.5]
[180,"Ni t","Nikkel, totaal",180,"Ni t","µg/L","µg/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B136,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":30},{"$f":"IFERROR(VLOOKUP(B136,'MKN - Max'!B:J,7,FALSE),\"\")","v":51},null,30,30,null,150,null,"Nikkel, totaal","ja",450,4500,null,"Nikkel, totaal","Ni t",1.3]
[9,"NO2-","Nitriet",9,"NO2-","mgN/L","mg/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - >5% OW",{"$f":"IFERROR(VLOOKUP(B137,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.2},{"$f":"IFERROR(VLOOKUP(B137,'MKN - Max'!B:J,7,FALSE),\"\")","v":0.6},null,0.2,0.2,null,1,null,"Nitriet",null,null,null,null,"Nitriet","NO2-",1.3]
[972,"NyFol","Nonylfenol",972,"NyFol","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B138,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":300},{"$f":"IFERROR(VLOOKUP(B138,'MKN - Max'!B:J,7,FALSE),\"\")","v":2000},null,300,300,null,1500,null,"Nonylfenol","ja",911,9106,null,"Nonylfenol","NyFol",1.5]
[1223,"OyFolsom","Octylfenolen",1223,"OyFolsom","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B139,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":100},{"$f":"IFERROR(VLOOKUP(B139,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,100,100,null,500,null,"Octylfenolen","ja",911,9106,null,"Octylfenolen","OyFolsom",1.5]
[403,"Omethoaat","Omethoaat",403,"Omethoaat","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B140,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.02},{"$f":"IFERROR(VLOOKUP(B140,'MKN - Max'!B:J,7,FALSE),\"\")","v":0.2},null,0.02,0.02,null,0.1,null,"Omethoaat",null,null,null,null,"Omethoaat","Omethoaat",1.5,"MOZ aangevuld"]
[404,"ODemeton-My","Oxydemeton-methyl",404,"ODemeton-My","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B141,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":400},{"$f":"IFERROR(VLOOKUP(B141,'MKN - Max'!B:J,7,FALSE),\"\")","v":4000},null,400,400,null,2000,null,"Oxydemeton-methyl",null,null,null,null,"Oxydemeton-methyl","ODemeton-My",1.5,"MOZ aangevuld"]
[531,"PathionEy","Parathion-ethyl",531,"PathionEy","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B142,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.2},{"$f":"IFERROR(VLOOKUP(B142,'MKN - Max'!B:J,7,FALSE),\"\")","v":4},null,0.2,0.2,null,1,null,"Parathion-ethyl",null,null,null,null,"Parathion-ethyl","PathionEy",1.5]
[508,"PathionMy","Parathion-methyl",508,"PathionMy","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B143,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":10},{"$f":"IFERROR(VLOOKUP(B143,'MKN - Max'!B:J,7,FALSE),\"\")","v":20},null,10,10,null,50,null,"Parathion-methyl",null,null,null,null,"Parathion-methyl","PathionMy",1.5]
[756,"PCBz","Pentachloorbenzeen",756,"PCBz","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B144,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":7},{"$f":"IFERROR(VLOOKUP(B144,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,7,7,null,35,null,"Pentachloorbenzeen",null,null,null,null,"Pentachloorbenzeen","PCBz",1.5]
[259,"PCFol","Pentachloorfenol",259,"PCFol","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B145,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":400},{"$f":"IFERROR(VLOOKUP(B145,'MKN - Max'!B:J,7,FALSE),\"\")","v":1000},null,400,400,null,2000,null,"Pentachloorfenol","ja",911,9106,null,"Pentachloorfenol","PCFol",1.5]
[1044,"PFOS","perfluoroctaansulfonzuur (PFOS)",1044,"PFOS","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B146,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.65},{"$f":"IFERROR(VLOOKUP(B146,'MKN - Max'!B:J,7,FALSE),\"\")","v":36000},null,0.65,0.65,null,3.25,null,"perfluoroctaansulfonzuur (PFOS)",null,null,null,null,"perfluoroctaansulfonzuur (PFOS)","PFOS",1.5]
[1388,"BDE t (6)","Polybroomdifenylether, totaal (6)",1388,"BDE t (6)","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B147,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":4.8999999999999998E-5},{"$f":"IFERROR(VLOOKUP(B147,'MKN - Max'!B:J,7,FALSE),\"\")","v":140},null,4.8999999999999998E-5,4.8999999999999998E-5,null,2.4499999999999999E-4,null,"Polybroomdifenylether, totaal (6)",null,null,null,null,"Polybroomdifenylether, totaal (6)","BDE t (6)",1.5]
[445,"PCB t","Polychloorbifenyl, totaal",445,"PCB t","ng/L","ng/L","Ja","PS - dioxine",{"$f":"IFERROR(VLOOKUP(B148,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":2},{"$f":"IFERROR(VLOOKUP(B148,'MKN - Max'!B:J,7,FALSE),\"\")","v":20},null,2,2,null,10,null,"Polychloorbifenyl, totaal",null,null,null,null,"Polychloorbifenyl, totaal","PCB t",1.5]
[263,"44DDT","pp'Dichloordifenyltrichloorethaan",263,"44DDT","ng/L","ng/L","Ja","VS",{"$f":"IFERROR(VLOOKUP(B149,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":10},{"$f":"IFERROR(VLOOKUP(B149,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,10,10,null,50,null,"pp'Dichloordifenyltrichloorethaan",null,null,null,null,"pp'Dichloordifenyltrichloorethaan","44DDT",1.5]
[231,"Propanil","Propanil",231,"Propanil","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B150,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":200},{"$f":"IFERROR(VLOOKUP(B150,'MKN - Max'!B:J,7,FALSE),\"\")","v":3000},null,200,200,null,1000,null,"Propanil",null,null,null,null,"Propanil","Propanil",1.5]
[434,"Pyr","Pyreen",434,"Pyr","ng/L","ng/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - PAK",{"$f":"IFERROR(VLOOKUP(B151,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":40},{"$f":"IFERROR(VLOOKUP(B151,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,40,40,null,200,null,"Pyreen","ja",2269,{"$f":"T151*10","v":22690},null,"Pyreen","Pyr",1.5]
[1038,"Quinofen","Quinoxyfen",1038,"Quinofen","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B152,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":150},{"$f":"IFERROR(VLOOKUP(B152,'MKN - Max'!B:J,7,FALSE),\"\")","v":2700},null,150,150,null,750,null,"Quinoxyfen",null,null,null,null,"Quinoxyfen","Quinofen",1.5,"MOZ aangevuld"]
[183,"Se t","Seleen, totaal",183,"Se t","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B153,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":3},{"$f":"IFERROR(VLOOKUP(B153,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,3,3,null,15,null,"Seleen, totaal",null,null,null,null,"Seleen, totaal","Se t",1.3]
[280,"Simaz","Simazine",280,"Simaz","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B154,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":1000},{"$f":"IFERROR(VLOOKUP(B154,'MKN - Max'!B:J,7,FALSE),\"\")","v":4000},null,1000,1000,null,5000,null,"Simazine",null,null,null,null,"Simazine","Simaz",1.5]
[31,"N t","Stikstof, totaal",31,"N t","mgN/L","mg/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio  - >5% OW",null,null,"ja",null,null,null,null,null,"Stikstof, totaal","ja",6,60,null,"Stikstof, totaal","N t",1.3]
[14,"SO4=","Sulfaat",14,"SO4=","mg/L","mg/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio  - >5% OW",null,null,"ja",null,null,null,null,null,"Sulfaat","nee",2.1,21,null,"Sulfaat","SO4=",1.3]
[618,"AISurf","Surfactanten, anionische",618,"AISurf","mg/L","mg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B157,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.1},{"$f":"IFERROR(VLOOKUP(B157,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,{"$f":"IF(L157=\"ja\",\"Vul MKN aan\",IF(J157<>\"\",J157,K157))","v":0.1},{"$f":"M157","v":0.1},null,{"$f":"N157*5","v":0.5},null,"Surfactanten, anionische",null,null,null,null,"Surfactanten, anionische","AISurf",1.5]
[1767,"Surf KID+NID","Surfactanten, Kationische + Niet-ionogen",1767,"Surf KID+NID","mg/L","mg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B158,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":1},{"$f":"IFERROR(VLOOKUP(B158,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,1,1,null,5,null,"Surfactanten, Kationische + Niet-ionogen",null,null,null,null,"Surfactanten, Kationische + Niet-ionogen","Surf KID+NID",1.5]
[517,"Te t","Tellurium, totaal",517,"Te t","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B159,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":100},{"$f":"IFERROR(VLOOKUP(B159,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,100,100,null,500,null,"Tellurium, totaal",null,null,null,null,"Tellurium, totaal","Te t",1.3]
[282,"Terbutryn","Terbutryn",282,"Terbutryn","ng/L","ng/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B160,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":65},{"$f":"IFERROR(VLOOKUP(B160,'MKN - Max'!B:J,7,FALSE),\"\")","v":340},null,65,65,null,325,null,"Terbutryn",null,null,null,null,"Terbutryn","Terbutryn",1.5]
[281,"TrByaz","Terbutylazine",281,"TrByaz","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B161,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.32},{"$f":"IFERROR(VLOOKUP(B161,'MKN - Max'!B:J,7,FALSE),\"\")","v":1.8},null,0.32,0.32,null,1.6,null,"Terbutylazine",null,null,null,null,"Terbutylazine","TrByaz",1.5,"MOZ aangevuld"]
[410,"TtBySn","Tetrabutyltin",410,"TtBySn","ngSn/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B162,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":4.0999999999999996},{"$f":"IFERROR(VLOOKUP(B162,'MKN - Max'!B:J,7,FALSE),\"\")","v":41},null,4.0999999999999996,4.0999999999999996,null,20.5,null,{"$f":"C162","v":"Tetrabutyltin"},null,null,null,null,{"$f":"C162","v":"Tetrabutyltin"},{"$f":"B162","v":"TtBySn"},1.5,"MOZ aangevuld"]
[382,"TtCEe","Tetrachlooretheen",382,"TtCEe","µg/L","µg/L","Ja","VS",{"$f":"IFERROR(VLOOKUP(B163,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":10},{"$f":"IFERROR(VLOOKUP(B163,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,10,10,null,50,null,"Tetrachlooretheen",null,null,null,null,"Tetrachlooretheen","TtCEe",1.5]
[383,"TtCMa","Tetrachloormethaan",383,"TtCMa","µg/L","µg/L","Ja","VS",{"$f":"IFERROR(VLOOKUP(B164,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":12},{"$f":"IFERROR(VLOOKUP(B164,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,12,12,null,60,null,"Tetrachloormethaan",null,null,null,null,"Tetrachloormethaan","TtCMa",1.5]
[190,"Tl t","Thallium, totaal",190,"Tl t","µg/L","µg/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - >5% OW",{"$f":"IFERROR(VLOOKUP(B165,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.2},{"$f":"IFERROR(VLOOKUP(B165,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,0.2,0.2,null,1,null,"Thallium, totaal",null,null,null,null,"Thallium, totaal","Tl t",1.3]
[193,"Sn t","Tin, totaal",193,"Sn t","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B166,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":40},{"$f":"IFERROR(VLOOKUP(B166,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,40,40,null,200,null,"Tin, totaal",null,null,null,null,"Tin, totaal","Sn t",1.3]
[196,"Ti t","Titaan, totaal",196,"Ti t","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B167,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":100},{"$f":"IFERROR(VLOOKUP(B167,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,100,100,null,500,null,"Titaan, totaal",null,null,null,null,"Titaan, totaal","Ti t",1.3]
[223,"Tolueen","Tolueen",223,"Tolueen","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B168,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":90},{"$f":"IFERROR(VLOOKUP(B168,'MKN - Max'!B:J,7,FALSE),\"\")","v":700},null,90,90,null,450,null,"Tolueen","ja",1000,10000,null,"Tolueen","Tolueen",1.5]
[406,"Triazofos","Triazofos",406,"Triazofos","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B169,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":30},{"$f":"IFERROR(VLOOKUP(B169,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,30,30,null,150,null,"Triazofos",null,null,null,null,"Triazofos","Triazofos",1.5]
[520,"TBP","Tributylfosfaat",520,"TBP","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B170,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":40000},{"$f":"IFERROR(VLOOKUP(B170,'MKN - Max'!B:J,7,FALSE),\"\")","v":100000},null,40000,40000,null,200000,null,"Tributylfosfaat",null,null,null,null,"Tributylfosfaat","TBP",1.5,"MOZ aangevuld"]
[670,"TBySn","Tributyltin",670,"TBySn","ngSn/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B171,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":8.1000000000000003E-2},{"$f":"IFERROR(VLOOKUP(B171,'MKN - Max'!B:J,7,FALSE),\"\")","v":0.61},null,8.1000000000000003E-2,8.1000000000000003E-2,null,0.40500000000000003,null,"Tributyltin",null,null,null,null,"Tributyltin","TBySn",1.5,"MOZ aangevuld"]
[521,"TCAcyde","Trichlooracetaldehyde-hydraat",521,"TCAcyde","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B172,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":500},{"$f":"IFERROR(VLOOKUP(B172,'MKN - Max'!B:J,7,FALSE),\"\")","v":5000},null,500,500,null,2500,null,"Trichlooracetaldehyde-hydraat",null,null,null,null,"Trichlooracetaldehyde-hydraat","TCAcyde",1.5,"MOZ aangevuld"]
[522,"TCBz","Trichloorbenzenen",522,"TCBz","µg/L","µg/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B173,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.4},{"$f":"IFERROR(VLOOKUP(B173,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,0.4,0.4,null,2,null,"Trichloorbenzenen",null,null,null,null,"Trichloorbenzenen","TCBz",1.5]
[385,"TCEe","Trichlooretheen",385,"TCEe","µg/L","µg/L","Ja","VS",{"$f":"IFERROR(VLOOKUP(B174,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":10},{"$f":"IFERROR(VLOOKUP(B174,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,10,10,null,50,null,"Trichlooretheen",null,null,null,null,"Trichlooretheen","TCEe",1.5]
[1228,"triCFolsom","Trichloorfenolen",1228,"triCFolsom","ng/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B175,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":6000},{"$f":"IFERROR(VLOOKUP(B175,'MKN - Max'!B:J,7,FALSE),\"\")","v":20000},null,6000,6000,null,30000,null,"Trichloorfenolen","ja",911,9106,null,"Trichloorfenolen","triCFolsom",1.5]
[407,"TCfon","Trichloorfon",407,"TCfon","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B176,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":1E-3},{"$f":"IFERROR(VLOOKUP(B176,'MKN - Max'!B:J,7,FALSE),\"\")","v":0.01},null,1E-3,1E-3,null,5.0000000000000001E-3,null,"Trichloorfon",null,null,null,null,"Trichloorfon","TCfon",1.5,"MOZ aangevuld"]
[388,"TCMa","Trichloormethaan",388,"TCMa","µg/L","µg/L","Ja","PS",{"$f":"IFERROR(VLOOKUP(B177,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":2.5},{"$f":"IFERROR(VLOOKUP(B177,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,2.5,2.5,null,12.5,null,"Trichloormethaan",null,null,null,null,"Trichloormethaan","TCMa",1.5]
[1229,"TFySn som","Trifenyltinacetaat, chloride, hydroxide",1229,"TFySn som","ngSn/L","ng/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B178,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.3},{"$f":"IFERROR(VLOOKUP(B178,'MKN - Max'!B:J,7,FALSE),\"\")","v":3},null,0.3,0.3,null,1.5,null,"Trifenyltinacetaat, chloride, hydroxide",null,null,null,null,"Trifenyltinacetaat, chloride, hydroxide","TFySn som",1.5,"MOZ aangevuld"]
[417,"Tfluralin","Trifluralin",417,"Tfluralin","ng/L","ng/L","Ja","PGS",{"$f":"IFERROR(VLOOKUP(B179,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":30},{"$f":"IFERROR(VLOOKUP(B179,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,30,30,null,150,null,"Trifluralin",null,null,null,null,"Trifluralin","Tfluralin",1.5]
[525,"U t","Uranium, totaal",525,"U t","µg/L","µg/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - >5% OW",{"$f":"IFERROR(VLOOKUP(B180,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":1},{"$f":"IFERROR(VLOOKUP(B180,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,1,1,null,5,null,"Uranium, totaal",null,null,null,null,"Uranium, totaal","U t",1.3]
[199,"V t","Vanadium, totaal",199,"V t","µg/L","µg/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - >5% OW",{"$f":"IFERROR(VLOOKUP(B181,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":5},{"$f":"IFERROR(VLOOKUP(B181,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,5,5,null,25,null,"Vanadium, totaal",null,null,null,null,"Vanadium, totaal","V t",1.3]
[570,"VinCl","Vinylchloride",570,"VinCl","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B182,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.09},{"$f":"IFERROR(VLOOKUP(B182,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,0.09,0.09,null,0.44999999999999996,null,"Vinylchloride",null,null,null,null,"Vinylchloride","VinCl",1.5]
[526,"ompXyl","Xylenen (o+m+p)",526,"ompXyl","µg/L","µg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B183,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":4},{"$f":"IFERROR(VLOOKUP(B183,'MKN - Max'!B:J,7,FALSE),\"\")","v":40},null,4,4,null,20,null,"Xylenen (o+m+p)","ja",1000,10000,null,"Xylenen (o+m+p)","ompXyl",1.5]
[202,"Ag t","Zilver, totaal",202,"Ag t","µg/L","µg/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - Toekomstige P(G)S",{"$f":"IFERROR(VLOOKUP(B184,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":0.4},{"$f":"IFERROR(VLOOKUP(B184,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,0.4,0.4,null,2,null,"Zilver, totaal",null,null,null,null,"Zilver, totaal","Ag t",1.3]
[205,"Zn t","Zink, totaal",205,"Zn t","µg/L","µg/L","Ja","VMM stroomgebiedspecifieke stoffen - VMM prio - >5% OW",{"$f":"IFERROR(VLOOKUP(B185,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":200},{"$f":"IFERROR(VLOOKUP(B185,'MKN - Max'!B:J,7,FALSE),\"\")","v":""},null,200,200,null,1000,null,"Zink, totaal","ja",450,4500,null,"Zink, totaal","Zn t",1.3]
[113,"ZS","Zwevende stoffen",113,"ZS","mg/L","mg/L","Nee",null,{"$f":"IFERROR(VLOOKUP(B186,'MKN - JG'!$B:$J,7,FALSE),\"\")","v":""},null,"ja",null,null,null,null,null,"Zwevende stoffen",null,null,null,null,"Zwevende stoffen","ZS",1.4]
[2000,"IP","Indeno(1,2,3-cd)Pyreen",2000,"IP","ng/L","ng/L","ja","PGS",null,null,null,null,null,null,null,null,"Indeno(1,2,3-cd)Pyreen",null,null,null,null,"Indeno(1,2,3-cd)Pyreen","IP"]
[{"$f":"IF(ISBLANK('Input impactbeoordeing'!A37)=TRUE,\"\",'Input impactbeoordeing'!A37)","v":"E1"},{"$f":"C188","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B37)=TRUE,\"\",'Input impactbeoordeing'!B37)","v":""},null,{"$f":"C188","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!D37)=TRUE,\"\",'Input impactbeoordeing'!D37)","v":""},{"$f":"F188","v":""},{"$f":"IF(C188=\"\",\"\",\"Nee\")","v":""},null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!C37)=TRUE,\"\",'Input impactbeoordeing'!C37)","v":""},null,null,null,null,"",null,null,null,null,"",""]
[{"$f":"IF(ISBLANK('Input impactbeoordeing'!A38)=TRUE,\"\",'Input impactbeoordeing'!A38)","v":"E2"},{"$f":"C189","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B38)=TRUE,\"\",'Input impactbeoordeing'!B38)","v":""},null,{"$f":"C189","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!D38)=TRUE,\"\",'Input impactbeoordeing'!D38)","v":""},{"$f":"F189","v":""},{"$f":"IF(C189=\"\",\"\",\"Nee\")","v":""},null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!C38)=TRUE,\"\",'Input impactbeoordeing'!C38)","v":""},null,null,null,null,"",null,null,null,null,"",""]
[{"$f":"IF(ISBLANK('Input impactbeoordeing'!A39)=TRUE,\"\",'Input impactbeoordeing'!A39)","v":"E3"},"",{"$f":"IF(ISBLANK('Input impactbeoordeing'!B39)=TRUE,\"\",'Input impactbeoordeing'!B39)","v":""},null,"",{"$f":"IF(ISBLANK('Input impactbeoordeing'!D39)=TRUE,\"\",'Input impactbeoordeing'!D39)","v":""},"","",null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!C39)=TRUE,\"\",'Input impactbeoordeing'!C39)","v":""},null,null,null,null,"",null,null,null,null,"",""]
[{"$f":"IF(ISBLANK('Input impactbeoordeing'!A40)=TRUE,\"\",'Input impactbeoordeing'!A40)","v":"E4"},"",{"$f":"IF(ISBLANK('Input impactbeoordeing'!B40)=TRUE,\"\",'Input impactbeoordeing'!B40)","v":""},null,"",{"$f":"IF(ISBLANK('Input impactbeoordeing'!D40)=TRUE,\"\",'Input impactbeoordeing'!D40)","v":""},"","",null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!C40)=TRUE,\"\",'Input impactbeoordeing'!C40)","v":""},null,null,null,null,"",null,null,null,null,"",""]
[{"$f":"IF(ISBLANK('Input impactbeoordeing'!A41)=TRUE,\"\",'Input impactbeoordeing'!A41)","v":"E5"},"",{"$f":"IF(ISBLANK('Input impactbeoordeing'!B41)=TRUE,\"\",'Input impactbeoordeing'!B41)","v":""},null,"",{"$f":"IF(ISBLANK('Input impactbeoordeing'!D41)=TRUE,\"\",'Input impactbeoordeing'!D41)","v":""},"","",null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!C41)=TRUE,\"\",'Input impactbeoordeing'!C41)","v":""},null,null,null,null,"",null,null,null,null,"",""]
[{"$f":"IF(ISBLANK('Input impactbeoordeing'!A42)=TRUE,\"\",'Input impactbeoordeing'!A42)","v":"E6"},"",{"$f":"IF(ISBLANK('Input impactbeoordeing'!B42)=TRUE,\"\",'Input impactbeoordeing'!B42)","v":""},null,"",{"$f":"IF(ISBLANK('Input impactbeoordeing'!D42)=TRUE,\"\",'Input impactbeoordeing'!D42)","v":""},"","",null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!C42)=TRUE,\"\",'Input impactbeoordeing'!C42)","v":""},null,null,null,null,"",null,null,null,null,"",""]
[{"$f":"IF(ISBLANK('Input impactbeoordeing'!A43)=TRUE,\"\",'Input impactbeoordeing'!A43)","v":"E7"},"",{"$f":"IF(ISBLANK('Input impactbeoordeing'!B43)=TRUE,\"\",'Input impactbeoordeing'!B43)","v":""},null,"",{"$f":"IF(ISBLANK('Input impactbeoordeing'!D43)=TRUE,\"\",'Input impactbeoordeing'!D43)","v":""},"","",null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!C43)=TRUE,\"\",'Input impactbeoordeing'!C43)","v":""},null,null,null,null,"",null,null,null,null,"",""]

{"sheet":"Toetswaarden spec wl","index":10,"n_rows":3996,"n_cols":14,"rows_kept":3996,"cut":false,"hidden":true,"merged":[]}
["Code","Naam waterlichaam","Parameter","Parameter ID","Parameter Symbool","WL + PAR combo","Toets","Eenheid","toetswaarde stap 4","toetscriterium stap 5","toetswaarde stap 5 - halen doelstellingen","toetswaarde stap 5 - achteruitgang (goed-matig)","toetswaarde stap 5 - achteruitgang (matig-ontoereikend)","toetswaarde stap 5 - achteruitgang (ontoereikend-slecht)"]
["L107_10","KEMMELBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5",{"$f":"_xlfn.CONCAT(A2,E2)","v":"L107_10BZV5"},"90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_104","NEERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5",{"$f":"_xlfn.CONCAT(A3,E3)","v":"L107_104BZV5"},"90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_105","PALINGBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_105BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_11","WANEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_11BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_112","LA HAUTE PLANCHE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_112BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_113","DOUVEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_113BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_116","GROTE SPIERE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_116BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_12","VLETERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_12BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_120","SCHEEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_120BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_122","HET GELEED","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_122BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_123","KANAAL VAN BRUGGE NAAR SLUIS","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_123BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_124","RONSELAREBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_124BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_130","KLEINE GEUL","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_130BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_131","LISSEWEEGSEVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_131BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_133","BLANKENBERGSEVAART L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_133BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_135","JABBEEKSE BEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_135BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_136","HOGE WATERING","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_136BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_140","SCHELLEVLIET","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_140BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_143","GROOT ZWIN - NOORDGELEED","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_143BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_149","PROVINCIEGELEED","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_149BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_150","GRANINGATEVLIET","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_150BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_16","HARINGEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_16BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_202","OOSTPOLDERKREEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_202BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_209","ZWARTESLUISBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_209BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_213","EEKLOSE WATERGANG","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_213BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_218","SLEIDINGSVAARDEKEN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_218BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_225","KEUTELBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_225BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_234","POEKEBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_234BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_235","REIGERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_235BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_236","NEERSCHUURBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_236BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_237","SPEIBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_237BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_239","OUDE MANDEL L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_239BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_240","ZOUBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_240BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_241","KATTEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_241BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_242","DUIVEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_242BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_246","STAMPKOTBEEK - MOLENBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_246BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_247","STAMPKOTBEEK - WALLEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_247BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_253","STAMPKOTBEEK - MUNKBOSBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_253BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_254","MOLENBEEK - BEIAARDBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_254BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_266","PEERDESTOKBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_266BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_272","OPHASSELTBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_272BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_273","MOLENBEEK - PACHTBOSBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_273BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_274","MOLENBEEK - KALSTERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_274BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_275","TER ERPENBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_275BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_276","MOLENBEEK - GRAADBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_276BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_277","WILDEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_277BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_279","MOLENBEEK - VOGELENZANGBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_279BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_282","MOLENBEEK - GONDEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_282BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_287","MOLENBEEK - GROTE BEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_287BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_289","DAMSLOOT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_289BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_296","VOORSTESLOOT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_296BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_299","VONDELBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_299BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_3","BROENBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_3BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_305","ZELEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_305BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_325","GROTE ASTBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_325BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_328","ZUIDELIJKE WATERGANG","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_328BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_329","BLOKSTRAATBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_329BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_33","BOMMELAREVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_33BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_330","WATERLOOP VAN DE HOGE LANDEN L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_330BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_333","DOORLOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_333BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_335","MOLENBEEK - BEVERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_335BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_336","DE RIJT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_336BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_34","RINGSLOT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_34BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_37","LANGGELEED","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_37BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_4","KORVERSBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_4BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_40","STENENSLUISVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5",{"$f":"_xlfn.CONCAT(A67,E67)","v":"L107_40BZV5"},"90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_403","MOLENBEEK - NEERPEDEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_403BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_404","LOTBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_404BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_407","GROEBENGRACHT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_407BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_409","KLEINE MAALBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_409BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_411","MOLENBEEK - PARKBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_411BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_413","TANGEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_413BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_417","DE GROTE LAAK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_417BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_418","MENE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_418BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_421","GENOVEVABEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_421BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_422","'S HERTOGENGRACHT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_422BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_423","BEGIJNEBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_423BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_424","VIJVERSLOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_424BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_431","ST-ODULPHUSBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_431BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_432","DORMAALBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_432BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_433","BEVERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_433BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_434","SCHEIBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_434BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_435","AREBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_435BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_439","IJSE L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_439BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_441","LANGEGRACHT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_441BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_449","VOER (BERTEM)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_449BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_451","GROTE LAAK - GROTE LOOP - MESTENLOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_451BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_452","LAARBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_452BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_453","ZWARTEBEEK (SCHERPENHEUVEL-ZICHEM)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_453BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_454","KLEINEBEEK - RIJSELSESTRAATVLIET","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_454BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_462","LEMINGSBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_462BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_463","AABEEK (MECHELEN)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_463BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_464","LEYBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_464BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_47","ZARRENBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_47BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_48","KANAAL VAN ESEN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_48BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_5","BOLLAERTBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_5BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_56","REYGAERTSVLIET","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_56BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_6","DIKKEBUSBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_6BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_60","GROOTGELEED","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_60BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_600","LEYLOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_600BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_601","DE AA (RAVELS)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_601BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_602","BLAUWPUTTEN EN LEILOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_602BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_603","HEERLESE LOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_603BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_607","MERKSKE L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_607BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_609","KLEINE MARK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_609BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_61","VAARTDIJKGELEED","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_61BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_610","MARK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_610BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_613","SLUISKENSVIJVER","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_613BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_614","WEERIJSEBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_614BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_615","KLEINE BEEK (WUUSTWEZEL)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_615BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_629","KLEIN WILBOEREBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_629BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_63","BOERGONJEVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_63BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_631","MOLENBEEK - BOLLAAK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_631BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_632","DE DELFTE BEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_632BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_633","BOSBEEK - DIEPTELOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_633BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_638","GROTE CALIE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_638BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_640","DE AA - NATTENLOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_640BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_644","ITTERBEEK (DUFFEL)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_644BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_648","BRUINBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_648BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_650","REEHAGENBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_650BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_654","LARUMSE LOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_654BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_655","DALEMANSLOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_655BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_656","BEGGELBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_656BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_66","KERKBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_66BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_664","MOLENBEEK - ZIJP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_664BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_665","BOUWBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_665BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_67","LIJSTERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_67BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_677","DIEPE BEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_677BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_681","KOUDE BEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_681BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_684","SCHOON SCHIJN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5",{"$f":"_xlfn.CONCAT(A131,E131)","v":"L107_684BZV5"},"90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_688","LAARSE BEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_688BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_695","VARENDONKSE BEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_695BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_702","MILLEGEMLOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_702BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_705","SCHEPPELIJKE NETE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_705BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_706","MOLSE NETE L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_706BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_708","GROTE NETE L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_708BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_722","WAMP L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_722BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_723","RODE LOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_723BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_729","STAPKENSLOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_729BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_735","GESTELBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_735BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_740","BERGEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_740BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_741","SPILLEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_741BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_742","PLATTE BEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_742BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_78","DEVEBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_78BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_8","IEPERLEE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_8BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_809","KLEINE HERK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_809BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_810","WINTERBEEK (KORTESSEM)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_810BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_812","MOMBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_812BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_814","STEENLAAK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_814BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_82","BABILLEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_82BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_824","ROELBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_824BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_83","ROOBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_83BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_836","LAAMBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_836BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_839","ZONDERIKBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_839BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_84","KROMMEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_84BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_846","KAATSBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_846BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_847","WINTERBEEK (BILZEN)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_847BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_848","DEMER L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_848BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_852","MUNSTERBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_852BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_853","ZUTENDAALBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_853BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_854","BOLLISENBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_854BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_855","DOMMEL L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_855BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_856","HOLVENLOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_856BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_857","EINDERGATLOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_857BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_858","WARMBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_858BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_859","PRINSENLOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_859BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_861","ABEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_861BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_866","LOSSING L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_866BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_869","SOERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_869BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_876","BOSBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_876BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_879","VRIETSELBEEK - OUDE MAAS (DILSEN)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_879BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_883","ZIEPBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_883BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_885","HEESWATER","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_885BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_890","BEEK - DE BUTH (TONGEREN)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_890BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_891","VOER (VOEREN)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_891BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_892","BEEK (VOEREN)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_892BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_893","GULP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_893BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_91","PLAATSBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_91BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_92","MAALBEEK (LEIEBEKKEN)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_92BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_97","KASSELRIJBEEK - WEST","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_97BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_98","GAVERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L107_98BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L110_1100","ZILVERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L110_1100BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1001","MARTJEVAART - LEKKERBOTERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1001BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1003","GELUWEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1003BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1004","RIJTGRACHT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1004BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1005","KALSIJDEADER","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1005BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1006","HOOFDSLOOT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1006BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1007","STEGERSZWIN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1007BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1010","OOSTKERKEVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1010BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1011","BOEREKREEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1011BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1014","MEREBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1014BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1015","OUDE AVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1015BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1016","WANTEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1016BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1018","LEEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5",{"$f":"_xlfn.CONCAT(A195,E195)","v":"L111_1018BZV5"},"90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1019","MOLENBEEK - MARKEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1019BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1020","OOSSEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1020BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1021","ZWALMBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1021BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1022","MOLENBEEK (RONSE)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1022BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1024","BAVEGEMSE BEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1024BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1025","MAANBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1025BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1027","GROOTEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1027BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1028","LANGELEDE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1028BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1029","KLEINE WATERGANG","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1029BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1030","WATERGANG VAN DE MOERBEKEPOLDER","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1030BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1031","KANAAL VAN STEKENE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1031BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1032","DIJKGRACHT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1032BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1033","PAPENMEERSBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1033BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1034","NIEUWE GRACHT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1034BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1035","KOEVAARDEKEN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1035BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1037","MOLENBEEK - LAKEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1037BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1038","MAALBEEK - AMELVONNEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1038BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1039","STEENVOORDBEEK (TERNAT)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1039BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1040","BELLEBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1040BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1041","WINGE L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1041BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1042","LEIBEEK - LIPSEBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1042BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1043","WEESBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1043BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1044","KASTEELBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1044BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1046","GROTE MOTTE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1046BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1047","BAREBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1047BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1048","ZIJDELINGSGELEED","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1048BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1049","MUNTLOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1049BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1050","WEHAGENBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1050BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1052","LAAKBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1052BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1053","MOUBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1053BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1054","GOORBOSBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1054BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1056","VROUWVLIET L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1056BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1057","GROTE MOLENBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1057BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1058","ZWARTE BEEK (WILLEBROEK)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1058BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1059","ZIELBEEK - BOSBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1059BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1060","GROOT SCHIJN L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1060BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1062","HERSELTSELOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1062BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1063","STEENKENSBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1063BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1064","ST. TRUDOLEKEN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1064BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1065","ASBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1065BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1066","LOEIJENS NEETJE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1066BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1067","KLEINE NETE L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1067BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1069","AFWATERINGSGRACHT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1069BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1070","WIMP L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1070BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1071","GOORLOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1071BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1072","POVERSBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1072BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1075","MELSTERBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1075BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1076","CICINDRIA","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1076BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1077","MOLENBEEK (SINT-TRUIDEN)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1077BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1078","GRONDBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1078BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1079","HELDERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1079BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1080","ZWARTEBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1080BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1081","MANGELBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1081BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1082","SLANGBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1082BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1083","MISERIKBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1083BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1084","MANDEL L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1084BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1086","LOZERBROEKBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1086BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1087","HORSTGATERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1087BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1088","ITTERBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1088BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1089","WITBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1089BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1090","ZANDERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1090BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1091","KIKBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1091BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1092","ZOUW","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1092BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1093","EZELSBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5",{"$f":"_xlfn.CONCAT(A259,E259)","v":"L111_1093BZV5"},"90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1094","HEULEBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1094BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1095","KLEINE LAAK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1095BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1096","GROTE LAAK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1096BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1098","KEIBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1098BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1099","GAVERSE BEEK (BECQUE DE NEUVILLE)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1099BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1101","GROTE KEIGNAERT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1101BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1102","KLEINE A - WILDERTSE BEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1102BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1104","DESPIERREBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1104BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1105","MELSENBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1105BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1106","DONKSE BEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1106BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1107","SLIJKVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1107BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1108","STEENGRACHT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1108BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1109","MOERDIJKVAART L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1109BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1110","EDE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1110BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1111","GELEEDBEEK - PASSENDALEGELEED","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1111BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1112","ISABELLASTROOM","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1112BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1113","LACHENEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1113BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1114","ANTITANKGRACHT ZUID","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1114BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_1201","S HERTOGENDIJKSE BEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_1201BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_15","HEIDEBEEK (VLETEREN)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_15BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_18","ST-MACHUITSBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_18BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_298","OUDE DENDER","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_298BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_315","FONDATIEGRACHT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_315BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_326","BARBIERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_326BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_419","SCHOORBROEKBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_419BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_436","VELPE L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_436BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_624","TAPPELBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_624BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_627","KLEINE BEEK (ZANDHOVEN)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_627BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_639","VISBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_639BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_674","BENEDENVLIET L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_674BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_676","WEZELSE BEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_676BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_699","SCHERPENBERGLOOP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_699BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_707","KLEINE HOOFDGRACHT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_707BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_717","DESSELSE NEET","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_717BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_724","ANTITANKGRACHT NOORD","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_724BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L111_844","STIEMER","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L111_844BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L117_1036","ZUUNBEEK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L117_1036BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L117_1068","HERTSBERGEBEEK - GETEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L117_1068BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L117_1073","RIVIERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L117_1073BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L117_1074","HERK L1","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L117_1074BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L117_1085","WILDERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L117_1085BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L117_17","STEENVOORDEBEEK (WATOU)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L117_17BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L117_219","BURGGRAVENSTROOM","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L117_219BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L117_232","JOBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L117_232BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L117_233","RINGBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L117_233BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L117_402","MOLENBEEK - SLAGVIJVERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L117_402BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L117_659","KREKELBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L117_659BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L117_673","KLEIN SCHIJN (NOORDELIJK DEEL)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L117_673BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L117_813","HERKEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L117_813BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L118_238","KROMMEDIJKBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L118_238BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L119_675","KLEIN SCHIJN (ZUIDELIJK DEEL)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L119_675BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L120_1097","KASSELRIJBEEK - OOST","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L120_1097BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L121_1045","GROTEBEEK - WINTERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L121_1045BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L2 Bk","L2 Kleine Beek","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L2 BkBZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L2 Bk","L2 kleine beek","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","L2 BkBZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_102","DEMER V","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_102BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_103","DEMER VI","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_103BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_104","DEMER VII","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_104BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_105","GETE I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_105BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_106","GETE II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_106BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_108","HERK + KLEINE HERK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_108BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_110","MANGELBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_110BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_113","MOMBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_113BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_114","MUNSTERBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5",{"$f":"_xlfn.CONCAT(A323,E323)","v":"VL05_114BZV5"},"90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_115","VELPE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_115BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_116","WINGE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_116BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_118","ZWARTWATER","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_118BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_119","VINNE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_119BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_12","POPERINGEVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_12BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_121","AA II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_121BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_122","GROTE LAAK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_122BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_124","GROTE NETE II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_124BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_130","WAMP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_130BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_131","WIMP","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_131BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_134","BERWIJN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_134BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_135","BOSBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_135BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_136","DOMMEL","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_136BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_137","ITTERBEEK I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_137BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_138","ITTERBEEK II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_138BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_14","VLADSLOVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_14BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_140","JEKER II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_140BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_141","LOSSING","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_141BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_146","MERKSKE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_146BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_148","WEERIJSEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_148BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_150","AFLEIDINGSKANAAL van de LEIE/SCHIPDONKKANAAL I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_150BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_152","AVRIJEVAART + SLEIDINGSVAARDEKE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_152BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_153","BERGENVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_153BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_159","KANAAL CHARLEROI-BRUSSEL","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_159BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_163","KANAAL GENT-OOSTENDE II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_163BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_166","KANAAL IEPER-IJZER","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_166BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_167","KANAAL LEUVEN-DIJLE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_167BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_17","ISABELLAVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_17BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_170","KANAAL VAN BEVERLO","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_170BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_171","LEDE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_171BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_175","MOERVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_175BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_177","NIEUWE KALE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_177BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_18","KERKEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_18BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_180","ZARRENBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_180BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_182","ZUIDLEDE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_182BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_191","DESSELSE ZANDPUTTEN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_191BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_192","DONKMEER","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_192BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_195","GAVERS HARELBEKE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_195BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_196","GRINDPLAS KESSENICH","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_196BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_2","GROTE KEMMELBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_2BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_20","RIVIERBEEK + HERTSBERGEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_20BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_200","SCHULENSMEER","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_200BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_201","SPAANJERD + HEERENLAAK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_201BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_202","SPUIKOM OOSTENDE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_202BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_21","ZUIDERVAARTJE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_21BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_22","ZWINNEVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_22BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_24","MEREBEEK + BORISGRACHT + LIEVE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_24BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_25","OUDE KALE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_25BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_28","BENEDENVLIET","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_28BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_3","HANDZAMEVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_3BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_30","GROTE MOLENBEEK - DE VLIET","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_30BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_31","KALKENSE VAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_31BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_32","MOLENBEEK - GROTE BEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_32BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_34","NOORD-ZUIDVERBINDING","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_34BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_38","ZIELBEEK - BOSBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_38BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_4","HEIDEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_4BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_44","DEVEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_44BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_45","GAVERBEEK I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_45BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_46","GAVERBEEK II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_46BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_5","IEPERLEE + VERWEZEN KANAAL IEPER-KOMEN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_5BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_50","LEIE III","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_50BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_51","MANDEL I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_51BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_52","MANDEL II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_52BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_53","OUDE MANDEL","Biochemisch zuurstofverbruik na 5d.",287,"BZV5",{"$f":"_xlfn.CONCAT(A387,E387)","v":"VL05_53BZV5"},"90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_58","BOVEN-SCHELDE IV","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_58BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_6","IEPERLEED","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_6BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_61","RONE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_61BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_62","STAMPKOTBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_62BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_64","ZWARTE SPIEREBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_64BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_67","DENDER I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_67BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_70","DENDER IV","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_70BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_73","MOLENBEEK - PACHTBOSBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_73BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_75","VONDELBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_75BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_77","DIJLE I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_77BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_81","DIJLE V","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_81BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_85","LEIBEEK - LAAKBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_85BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_86","NETHEN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_86BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_87","VOER (Leuven)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_87BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_89","VUNT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_89BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_90","WEESBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_90BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_93","ZENNE II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_93BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_98","DEMER I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_98BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL05_99","DEMER II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL05_99BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_125","GROTE NETE III","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_125BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_132","GETIJDENETES","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_132BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_157","ISABELLAWATERING","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_157BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_16","BLANKENBERGSE VAART + NOORDEDE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_16BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_162","KANAAL GENT-OOSTENDE I + COUPURE + VERBINDINGSKANAAL","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_162BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_164","KANAAL GENT-OOSTENDE III","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_164BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_172","LEOPOLDKANAAL I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_172BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_173","LEOPOLDKANAAL II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_173BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_176","NETEKANAAL","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_176BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_178","NOORDELIJKE RINGVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_178BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_179","WESTELIJKE RINGVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_179BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_27","ZWARTESLUISBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_27BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_39","GETIJDEDURME","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_39BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_41","ZEESCHELDE II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_41BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_55","BOVEN-SCHELDE I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_55BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_7","IJZER I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_7BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_71","DENDER V","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_71BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_72","MARK (Denderbekken)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_72BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_80","DIJLE IV","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_80BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_82","DIJLE VI","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_82BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_92","ZENNE I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_92BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL08_95","GETIJDEDIJLE & GETIJDEZENNE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL08_95BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL09_78","DIJLE II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL09_78BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_10","MARTJEVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_10BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_109","KLEINE GETE + VLOEDGRACHT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_109BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_11","MOERDIJKVAART","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_11BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_117","ZWARTEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_117BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_120","AA I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_120BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_123","GROTE NETE I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_123BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_126","KLEINE NETE I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_126BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_127","KLEINE NETE II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_127BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_128","MOL NEET","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_128BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_13","VEURNE AMBACHT POLDER WATERLOPEN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_13BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_133","ABEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_133BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_145","MARK (Maas)","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_145BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_155","BRUGSE REIEN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_155BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_165","KANAAL GENT-TERNEUZEN + GENTSE HAVENDOKKEN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_165BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_19","OOSTENDS KREKENGEBIED","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_19BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_203","MAAS I+II+III","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_203BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_205","DEMER III+IV","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_205BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_207","MELSTERBEEK I+II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_207BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_37","WATERLOOP VAN DE HOGE LANDEN + MELKADER","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_37BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_40","ZEESCHELDE I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_40BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_59","GROTE SPIEREBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_59BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_63","ZWALM","Biochemisch zuurstofverbruik na 5d.",287,"BZV5",{"$f":"_xlfn.CONCAT(A451,E451)","v":"VL11_63BZV5"},"90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_76","BAREBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_76BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_83","IJSSE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_83BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_84","LAAN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_84BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_88","VROUWVLIET","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_88BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL11_91","WOLUWE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL11_91BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_147","WARMBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_147BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_15","HAVENGEUL IJZER","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_15BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_154","BRAKELEIKEN + LIEVE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_154BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_156","GENTSE BINNENWATEREN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_156BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_161","KANAAL DUINKERKE-NIEUWPOORT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_161BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_168","KANAAL PLASSENDALE-NIEUWPOORT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_168BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_169","KANAAL ROESELARE-LEIE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_169BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_174","LOKANAAL","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_174BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_184","BLANKENBERGSE HAVENGEUL + JACHTHAVENS","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_184BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_185","OOSTENDSE HAVENGEUL + DOKKEN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_185BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_186","ZEEBRUGGE BUITENHAVEN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_186BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_187","ANTWERPSE HAVENDOKKEN + SCHELDE-RIJNVERBINDING","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_187BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_190","BOUDEWIJNKANAAL + ACHTERHAVEN ZEEBRUGGE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_190BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_204","BOVEN-SCHELDE II+III","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_204BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_206","DENDER II+III","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_206BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_29","GROOT SCHIJN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_29BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_35","VERLEGDE SCHIJN - HOOFDGRACHT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_35BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_42","ZEESCHELDE III + RUPEL","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_42BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_43","ZEESCHELDE IV","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_43BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_48","LEIE I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_48BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_49","LEIE II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_49BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_54","TOERISTISCHE LEIE","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_54BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_60","MOLENBEEK - MAARKEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_60BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_66","BELLEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_66BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL17_9","IJZER III","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL17_9BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL20_36","VERLEGDE SCHIJN - VOORGRACHT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL20_36BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL20_96","BEGIJNENBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL20_96BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL21_1","BLANKAART WATERLOPEN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL21_1BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL21_107","GROTE GETE + BORGGRACHT","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL21_107BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL21_129","MOLENBEEK - BOLLAAK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL21_129BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL21_139","JEKER I","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL21_139BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL21_26","POEKEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL21_26BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL21_33","MOLENBEEK - KOTTEMBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL21_33BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL21_47","HEULEBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL21_47BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL21_74","MOLENBEEK - TER ERPENBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL21_74BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL21_79","DIJLE III","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL21_79BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL21_8","IJZER II","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL21_8BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL21_94","ZUUNBEEK","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL21_94BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL21_97","DE HULPE - ZWART WATER","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL21_97BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL22_208","ALBERTKANAAL - Maasbekken","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL22_208BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL22_209","ALBERTKANAAL - Demerbekken","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL22_209BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL22_210","ALBERTKANAAL - Netebekken","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL22_210BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL22_211","ALBERTKANAAL - Benedenscheldebekken","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL22_211BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL22_212","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Netebekken","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL22_212BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL22_213","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Maasbekken","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL22_213BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL22_214","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Benedenscheldebekken","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL22_214BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL22_215","ZEEKANAAL BRUSSEL-SCHELDE - Dijle-Zennebekken","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL22_215BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL22_216","ZEEKANAAL BRUSSEL-SCHELDE - Benedenscheldebekken","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL22_216BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL22_217","AFLEIDINGSKANAAL van de LEIE II + KANAAL van EEKLO - Bekken van de Gentse kanalen","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL22_217BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL22_218","AFLEIDINGSKANAAL van de LEIE II - Bekken van de Brugse polders","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL22_218BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL22_219","KANAAL BOSSUIT-KORTRIJK - Bovenscheldebekken","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL22_219BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL22_220","KANAAL BOSSUIT-KORTRIJK - Leiebekken","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL22_220BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["VL22_221","ZUID-WILLEMSVAART + KANAAL BOCHOLT-HERENTALS (deels) + KANAAL BRIEGDEN-NEERHAREN","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","VL22_221BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_10","KEMMELBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_10CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_104","NEERBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_104CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_105","PALINGBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_105CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_11","WANEBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_11CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_112","LA HAUTE PLANCHE","Chemisch zuurstofverbruik",288,"CZV","L107_112CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_113","DOUVEBEEK","Chemisch zuurstofverbruik",288,"CZV",{"$f":"_xlfn.CONCAT(A515,E515)","v":"L107_113CZV"},"90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_116","GROTE SPIERE","Chemisch zuurstofverbruik",288,"CZV","L107_116CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_12","VLETERBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_12CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_120","SCHEEBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_120CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_122","HET GELEED","Chemisch zuurstofverbruik",288,"CZV","L107_122CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_123","KANAAL VAN BRUGGE NAAR SLUIS","Chemisch zuurstofverbruik",288,"CZV","L107_123CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_124","RONSELAREBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_124CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_130","KLEINE GEUL","Chemisch zuurstofverbruik",288,"CZV","L107_130CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_131","LISSEWEEGSEVAART","Chemisch zuurstofverbruik",288,"CZV","L107_131CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_133","BLANKENBERGSEVAART L1","Chemisch zuurstofverbruik",288,"CZV","L107_133CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_135","JABBEEKSE BEEK","Chemisch zuurstofverbruik",288,"CZV","L107_135CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_136","HOGE WATERING","Chemisch zuurstofverbruik",288,"CZV","L107_136CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_140","SCHELLEVLIET","Chemisch zuurstofverbruik",288,"CZV","L107_140CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_143","GROOT ZWIN - NOORDGELEED","Chemisch zuurstofverbruik",288,"CZV","L107_143CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_149","PROVINCIEGELEED","Chemisch zuurstofverbruik",288,"CZV","L107_149CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_150","GRANINGATEVLIET","Chemisch zuurstofverbruik",288,"CZV","L107_150CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_16","HARINGEBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_16CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_202","OOSTPOLDERKREEK","Chemisch zuurstofverbruik",288,"CZV","L107_202CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_209","ZWARTESLUISBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L107_209CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_213","EEKLOSE WATERGANG","Chemisch zuurstofverbruik",288,"CZV","L107_213CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_218","SLEIDINGSVAARDEKEN","Chemisch zuurstofverbruik",288,"CZV","L107_218CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_225","KEUTELBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_225CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_234","POEKEBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L107_234CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_235","REIGERBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_235CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_236","NEERSCHUURBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_236CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_237","SPEIBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_237CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_239","OUDE MANDEL L1","Chemisch zuurstofverbruik",288,"CZV","L107_239CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_240","ZOUBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_240CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_241","KATTEBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_241CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_242","DUIVEBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_242CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_246","STAMPKOTBEEK - MOLENBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_246CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_247","STAMPKOTBEEK - WALLEBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_247CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_253","STAMPKOTBEEK - MUNKBOSBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_253CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_254","MOLENBEEK - BEIAARDBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_254CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_266","PEERDESTOKBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_266CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_272","OPHASSELTBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_272CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_273","MOLENBEEK - PACHTBOSBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L107_273CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_274","MOLENBEEK - KALSTERBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_274CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_275","TER ERPENBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_275CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_276","MOLENBEEK - GRAADBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_276CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_277","WILDEBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_277CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_279","MOLENBEEK - VOGELENZANGBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_279CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_282","MOLENBEEK - GONDEBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_282CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_287","MOLENBEEK - GROTE BEEK","Chemisch zuurstofverbruik",288,"CZV","L107_287CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_289","DAMSLOOT","Chemisch zuurstofverbruik",288,"CZV","L107_289CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_296","VOORSTESLOOT","Chemisch zuurstofverbruik",288,"CZV","L107_296CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_299","VONDELBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L107_299CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_3","BROENBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_3CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_305","ZELEBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_305CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_325","GROTE ASTBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_325CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_328","ZUIDELIJKE WATERGANG","Chemisch zuurstofverbruik",288,"CZV","L107_328CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_329","BLOKSTRAATBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_329CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_33","BOMMELAREVAART","Chemisch zuurstofverbruik",288,"CZV","L107_33CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_330","WATERLOOP VAN DE HOGE LANDEN L1","Chemisch zuurstofverbruik",288,"CZV","L107_330CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_333","DOORLOOP","Chemisch zuurstofverbruik",288,"CZV","L107_333CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_335","MOLENBEEK - BEVERBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_335CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_336","DE RIJT","Chemisch zuurstofverbruik",288,"CZV","L107_336CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_34","RINGSLOT","Chemisch zuurstofverbruik",288,"CZV","L107_34CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_37","LANGGELEED","Chemisch zuurstofverbruik",288,"CZV","L107_37CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_4","KORVERSBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_4CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_40","STENENSLUISVAART","Chemisch zuurstofverbruik",288,"CZV","L107_40CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_403","MOLENBEEK - NEERPEDEBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_403CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_404","LOTBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_404CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_407","GROEBENGRACHT","Chemisch zuurstofverbruik",288,"CZV","L107_407CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_409","KLEINE MAALBEEK","Chemisch zuurstofverbruik",288,"CZV",{"$f":"_xlfn.CONCAT(A579,E579)","v":"L107_409CZV"},"90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_411","MOLENBEEK - PARKBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_411CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_413","TANGEBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_413CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_417","DE GROTE LAAK","Chemisch zuurstofverbruik",288,"CZV","L107_417CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_418","MENE","Chemisch zuurstofverbruik",288,"CZV","L107_418CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_421","GENOVEVABEEK","Chemisch zuurstofverbruik",288,"CZV","L107_421CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_422","'S HERTOGENGRACHT","Chemisch zuurstofverbruik",288,"CZV","L107_422CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_423","BEGIJNEBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L107_423CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_424","VIJVERSLOOP","Chemisch zuurstofverbruik",288,"CZV","L107_424CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_431","ST-ODULPHUSBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_431CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_432","DORMAALBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_432CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_433","BEVERBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_433CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_434","SCHEIBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_434CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_435","AREBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_435CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_439","IJSE L1","Chemisch zuurstofverbruik",288,"CZV","L107_439CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_441","LANGEGRACHT","Chemisch zuurstofverbruik",288,"CZV","L107_441CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_449","VOER (BERTEM)","Chemisch zuurstofverbruik",288,"CZV","L107_449CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_451","GROTE LAAK - GROTE LOOP - MESTENLOOP","Chemisch zuurstofverbruik",288,"CZV","L107_451CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_452","LAARBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_452CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_453","ZWARTEBEEK (SCHERPENHEUVEL-ZICHEM)","Chemisch zuurstofverbruik",288,"CZV","L107_453CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_454","KLEINEBEEK - RIJSELSESTRAATVLIET","Chemisch zuurstofverbruik",288,"CZV","L107_454CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_462","LEMINGSBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_462CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_463","AABEEK (MECHELEN)","Chemisch zuurstofverbruik",288,"CZV","L107_463CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_464","LEYBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_464CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_47","ZARRENBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L107_47CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_48","KANAAL VAN ESEN","Chemisch zuurstofverbruik",288,"CZV","L107_48CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_5","BOLLAERTBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_5CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_56","REYGAERTSVLIET","Chemisch zuurstofverbruik",288,"CZV","L107_56CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_6","DIKKEBUSBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_6CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_60","GROOTGELEED","Chemisch zuurstofverbruik",288,"CZV","L107_60CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_600","LEYLOOP","Chemisch zuurstofverbruik",288,"CZV","L107_600CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_601","DE AA (RAVELS)","Chemisch zuurstofverbruik",288,"CZV","L107_601CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_602","BLAUWPUTTEN EN LEILOOP","Chemisch zuurstofverbruik",288,"CZV","L107_602CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_603","HEERLESE LOOP","Chemisch zuurstofverbruik",288,"CZV","L107_603CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_607","MERKSKE L1","Chemisch zuurstofverbruik",288,"CZV","L107_607CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_609","KLEINE MARK","Chemisch zuurstofverbruik",288,"CZV","L107_609CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_61","VAARTDIJKGELEED","Chemisch zuurstofverbruik",288,"CZV","L107_61CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_610","MARK L1","Chemisch zuurstofverbruik",288,"CZV","L107_610CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_613","SLUISKENSVIJVER","Chemisch zuurstofverbruik",288,"CZV","L107_613CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_614","WEERIJSEBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L107_614CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_615","KLEINE BEEK (WUUSTWEZEL)","Chemisch zuurstofverbruik",288,"CZV","L107_615CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_629","KLEIN WILBOEREBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_629CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_63","BOERGONJEVAART","Chemisch zuurstofverbruik",288,"CZV","L107_63CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_631","MOLENBEEK - BOLLAAK L1","Chemisch zuurstofverbruik",288,"CZV","L107_631CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_632","DE DELFTE BEEK","Chemisch zuurstofverbruik",288,"CZV","L107_632CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_633","BOSBEEK - DIEPTELOOP","Chemisch zuurstofverbruik",288,"CZV","L107_633CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_638","GROTE CALIE","Chemisch zuurstofverbruik",288,"CZV","L107_638CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_640","DE AA - NATTENLOOP","Chemisch zuurstofverbruik",288,"CZV","L107_640CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_644","ITTERBEEK (DUFFEL)","Chemisch zuurstofverbruik",288,"CZV","L107_644CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_648","BRUINBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_648CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_650","REEHAGENBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_650CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_654","LARUMSE LOOP","Chemisch zuurstofverbruik",288,"CZV","L107_654CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_655","DALEMANSLOOP","Chemisch zuurstofverbruik",288,"CZV","L107_655CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_656","BEGGELBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_656CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_66","KERKBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_66CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_664","MOLENBEEK - ZIJP","Chemisch zuurstofverbruik",288,"CZV","L107_664CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_665","BOUWBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_665CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_67","LIJSTERBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_67CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_677","DIEPE BEEK","Chemisch zuurstofverbruik",288,"CZV","L107_677CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_681","KOUDE BEEK","Chemisch zuurstofverbruik",288,"CZV","L107_681CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_684","SCHOON SCHIJN","Chemisch zuurstofverbruik",288,"CZV","L107_684CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_688","LAARSE BEEK","Chemisch zuurstofverbruik",288,"CZV","L107_688CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_695","VARENDONKSE BEEK","Chemisch zuurstofverbruik",288,"CZV","L107_695CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_702","MILLEGEMLOOP","Chemisch zuurstofverbruik",288,"CZV","L107_702CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_705","SCHEPPELIJKE NETE","Chemisch zuurstofverbruik",288,"CZV",{"$f":"_xlfn.CONCAT(A643,E643)","v":"L107_705CZV"},"90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_706","MOLSE NETE L1","Chemisch zuurstofverbruik",288,"CZV","L107_706CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_708","GROTE NETE L1","Chemisch zuurstofverbruik",288,"CZV","L107_708CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_722","WAMP L1","Chemisch zuurstofverbruik",288,"CZV","L107_722CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_723","RODE LOOP","Chemisch zuurstofverbruik",288,"CZV","L107_723CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_729","STAPKENSLOOP","Chemisch zuurstofverbruik",288,"CZV","L107_729CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_735","GESTELBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_735CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_740","BERGEBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_740CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_741","SPILLEBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_741CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_742","PLATTE BEEK","Chemisch zuurstofverbruik",288,"CZV","L107_742CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_78","DEVEBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L107_78CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_8","IEPERLEE","Chemisch zuurstofverbruik",288,"CZV","L107_8CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_809","KLEINE HERK L1","Chemisch zuurstofverbruik",288,"CZV","L107_809CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_810","WINTERBEEK (KORTESSEM)","Chemisch zuurstofverbruik",288,"CZV","L107_810CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_812","MOMBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L107_812CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_814","STEENLAAK","Chemisch zuurstofverbruik",288,"CZV","L107_814CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_82","BABILLEBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_82CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_824","ROELBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_824CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_83","ROOBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_83CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_836","LAAMBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_836CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_839","ZONDERIKBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_839CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_84","KROMMEBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_84CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_846","KAATSBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_846CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_847","WINTERBEEK (BILZEN)","Chemisch zuurstofverbruik",288,"CZV","L107_847CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_848","DEMER L1","Chemisch zuurstofverbruik",288,"CZV","L107_848CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_852","MUNSTERBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L107_852CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_853","ZUTENDAALBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_853CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_854","BOLLISENBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_854CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_855","DOMMEL L1","Chemisch zuurstofverbruik",288,"CZV","L107_855CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_856","HOLVENLOOP","Chemisch zuurstofverbruik",288,"CZV","L107_856CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_857","EINDERGATLOOP","Chemisch zuurstofverbruik",288,"CZV","L107_857CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_858","WARMBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L107_858CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_859","PRINSENLOOP","Chemisch zuurstofverbruik",288,"CZV","L107_859CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_861","ABEEK L1","Chemisch zuurstofverbruik",288,"CZV","L107_861CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_866","LOSSING L1","Chemisch zuurstofverbruik",288,"CZV","L107_866CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_869","SOERBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_869CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_876","BOSBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L107_876CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_879","VRIETSELBEEK - OUDE MAAS (DILSEN)","Chemisch zuurstofverbruik",288,"CZV","L107_879CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_883","ZIEPBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_883CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_885","HEESWATER","Chemisch zuurstofverbruik",288,"CZV","L107_885CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_890","BEEK - DE BUTH (TONGEREN)","Chemisch zuurstofverbruik",288,"CZV","L107_890CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_891","VOER (VOEREN)","Chemisch zuurstofverbruik",288,"CZV","L107_891CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_892","BEEK (VOEREN)","Chemisch zuurstofverbruik",288,"CZV","L107_892CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_893","GULP","Chemisch zuurstofverbruik",288,"CZV","L107_893CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_91","PLAATSBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_91CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_92","MAALBEEK (LEIEBEKKEN)","Chemisch zuurstofverbruik",288,"CZV","L107_92CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_97","KASSELRIJBEEK - WEST","Chemisch zuurstofverbruik",288,"CZV","L107_97CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_98","GAVERBEEK","Chemisch zuurstofverbruik",288,"CZV","L107_98CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L110_1100","ZILVERBEEK","Chemisch zuurstofverbruik",288,"CZV","L110_1100CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1001","MARTJEVAART - LEKKERBOTERBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1001CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1003","GELUWEBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1003CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1004","RIJTGRACHT","Chemisch zuurstofverbruik",288,"CZV","L111_1004CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1005","KALSIJDEADER","Chemisch zuurstofverbruik",288,"CZV","L111_1005CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1006","HOOFDSLOOT","Chemisch zuurstofverbruik",288,"CZV","L111_1006CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1007","STEGERSZWIN","Chemisch zuurstofverbruik",288,"CZV","L111_1007CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1010","OOSTKERKEVAART","Chemisch zuurstofverbruik",288,"CZV","L111_1010CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1011","BOEREKREEK","Chemisch zuurstofverbruik",288,"CZV","L111_1011CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1014","MEREBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1014CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1015","OUDE AVAART","Chemisch zuurstofverbruik",288,"CZV","L111_1015CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1016","WANTEBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1016CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1018","LEEBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1018CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1019","MOLENBEEK - MARKEBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1019CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1020","OOSSEBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1020CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1021","ZWALMBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1021CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1022","MOLENBEEK (RONSE)","Chemisch zuurstofverbruik",288,"CZV",{"$f":"_xlfn.CONCAT(A707,E707)","v":"L111_1022CZV"},"90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1024","BAVEGEMSE BEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1024CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1025","MAANBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1025CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1027","GROOTEBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1027CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1028","LANGELEDE","Chemisch zuurstofverbruik",288,"CZV","L111_1028CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1029","KLEINE WATERGANG","Chemisch zuurstofverbruik",288,"CZV","L111_1029CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1030","WATERGANG VAN DE MOERBEKEPOLDER","Chemisch zuurstofverbruik",288,"CZV","L111_1030CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1031","KANAAL VAN STEKENE","Chemisch zuurstofverbruik",288,"CZV","L111_1031CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1032","DIJKGRACHT","Chemisch zuurstofverbruik",288,"CZV","L111_1032CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1033","PAPENMEERSBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1033CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1034","NIEUWE GRACHT","Chemisch zuurstofverbruik",288,"CZV","L111_1034CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1035","KOEVAARDEKEN","Chemisch zuurstofverbruik",288,"CZV","L111_1035CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1037","MOLENBEEK - LAKEBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1037CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1038","MAALBEEK - AMELVONNEBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1038CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1039","STEENVOORDBEEK (TERNAT)","Chemisch zuurstofverbruik",288,"CZV","L111_1039CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1040","BELLEBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L111_1040CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1041","WINGE L1","Chemisch zuurstofverbruik",288,"CZV","L111_1041CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1042","LEIBEEK - LIPSEBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L111_1042CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1043","WEESBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L111_1043CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1044","KASTEELBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1044CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1046","GROTE MOTTE","Chemisch zuurstofverbruik",288,"CZV","L111_1046CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1047","BAREBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L111_1047CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1048","ZIJDELINGSGELEED","Chemisch zuurstofverbruik",288,"CZV","L111_1048CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1049","MUNTLOOP","Chemisch zuurstofverbruik",288,"CZV","L111_1049CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1050","WEHAGENBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1050CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1052","LAAKBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1052CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1053","MOUBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1053CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1054","GOORBOSBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1054CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1056","VROUWVLIET L1","Chemisch zuurstofverbruik",288,"CZV","L111_1056CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1057","GROTE MOLENBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L111_1057CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1058","ZWARTE BEEK (WILLEBROEK)","Chemisch zuurstofverbruik",288,"CZV","L111_1058CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1059","ZIELBEEK - BOSBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L111_1059CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1060","GROOT SCHIJN L1","Chemisch zuurstofverbruik",288,"CZV","L111_1060CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1062","HERSELTSELOOP","Chemisch zuurstofverbruik",288,"CZV","L111_1062CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1063","STEENKENSBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1063CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1064","ST. TRUDOLEKEN","Chemisch zuurstofverbruik",288,"CZV","L111_1064CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1065","ASBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1065CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1066","LOEIJENS NEETJE","Chemisch zuurstofverbruik",288,"CZV","L111_1066CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1067","KLEINE NETE L1","Chemisch zuurstofverbruik",288,"CZV","L111_1067CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1069","AFWATERINGSGRACHT","Chemisch zuurstofverbruik",288,"CZV","L111_1069CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1070","WIMP L1","Chemisch zuurstofverbruik",288,"CZV","L111_1070CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1071","GOORLOOP","Chemisch zuurstofverbruik",288,"CZV","L111_1071CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1072","POVERSBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1072CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1075","MELSTERBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L111_1075CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1076","CICINDRIA","Chemisch zuurstofverbruik",288,"CZV","L111_1076CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1077","MOLENBEEK (SINT-TRUIDEN)","Chemisch zuurstofverbruik",288,"CZV","L111_1077CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1078","GRONDBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1078CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1079","HELDERBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1079CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1080","ZWARTEBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L111_1080CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1081","MANGELBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L111_1081CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1082","SLANGBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1082CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1083","MISERIKBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1083CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1084","MANDEL L1","Chemisch zuurstofverbruik",288,"CZV","L111_1084CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1086","LOZERBROEKBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1086CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1087","HORSTGATERBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1087CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1088","ITTERBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L111_1088CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1089","WITBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1089CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1090","ZANDERBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1090CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1091","KIKBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1091CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1092","ZOUW","Chemisch zuurstofverbruik",288,"CZV","L111_1092CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1093","EZELSBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1093CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1094","HEULEBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L111_1094CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1095","KLEINE LAAK","Chemisch zuurstofverbruik",288,"CZV","L111_1095CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1096","GROTE LAAK L1","Chemisch zuurstofverbruik",288,"CZV","L111_1096CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1098","KEIBEEK","Chemisch zuurstofverbruik",288,"CZV",{"$f":"_xlfn.CONCAT(A771,E771)","v":"L111_1098CZV"},"90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1099","GAVERSE BEEK (BECQUE DE NEUVILLE)","Chemisch zuurstofverbruik",288,"CZV","L111_1099CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1101","GROTE KEIGNAERT","Chemisch zuurstofverbruik",288,"CZV","L111_1101CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1102","KLEINE A - WILDERTSE BEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1102CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1104","DESPIERREBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1104CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1105","MELSENBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1105CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1106","DONKSE BEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1106CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1107","SLIJKVAART","Chemisch zuurstofverbruik",288,"CZV","L111_1107CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1108","STEENGRACHT","Chemisch zuurstofverbruik",288,"CZV","L111_1108CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1109","MOERDIJKVAART L1","Chemisch zuurstofverbruik",288,"CZV","L111_1109CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1110","EDE","Chemisch zuurstofverbruik",288,"CZV","L111_1110CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1111","GELEEDBEEK - PASSENDALEGELEED","Chemisch zuurstofverbruik",288,"CZV","L111_1111CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1112","ISABELLASTROOM","Chemisch zuurstofverbruik",288,"CZV","L111_1112CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1113","LACHENEBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1113CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1114","ANTITANKGRACHT ZUID","Chemisch zuurstofverbruik",288,"CZV","L111_1114CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_1201","S HERTOGENDIJKSE BEEK","Chemisch zuurstofverbruik",288,"CZV","L111_1201CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_15","HEIDEBEEK (VLETEREN)","Chemisch zuurstofverbruik",288,"CZV","L111_15CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_18","ST-MACHUITSBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_18CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_298","OUDE DENDER","Chemisch zuurstofverbruik",288,"CZV","L111_298CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_315","FONDATIEGRACHT","Chemisch zuurstofverbruik",288,"CZV","L111_315CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_326","BARBIERBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_326CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_419","SCHOORBROEKBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_419CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_436","VELPE L1","Chemisch zuurstofverbruik",288,"CZV","L111_436CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_624","TAPPELBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_624CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_627","KLEINE BEEK (ZANDHOVEN)","Chemisch zuurstofverbruik",288,"CZV","L111_627CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_639","VISBEEK","Chemisch zuurstofverbruik",288,"CZV","L111_639CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_674","BENEDENVLIET L1","Chemisch zuurstofverbruik",288,"CZV","L111_674CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_676","WEZELSE BEEK","Chemisch zuurstofverbruik",288,"CZV","L111_676CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_699","SCHERPENBERGLOOP","Chemisch zuurstofverbruik",288,"CZV","L111_699CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_707","KLEINE HOOFDGRACHT","Chemisch zuurstofverbruik",288,"CZV","L111_707CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_717","DESSELSE NEET","Chemisch zuurstofverbruik",288,"CZV","L111_717CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_724","ANTITANKGRACHT NOORD","Chemisch zuurstofverbruik",288,"CZV","L111_724CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L111_844","STIEMER","Chemisch zuurstofverbruik",288,"CZV","L111_844CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L117_1036","ZUUNBEEK L1","Chemisch zuurstofverbruik",288,"CZV","L117_1036CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L117_1068","HERTSBERGEBEEK - GETEBEEK","Chemisch zuurstofverbruik",288,"CZV","L117_1068CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L117_1073","RIVIERBEEK","Chemisch zuurstofverbruik",288,"CZV","L117_1073CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L117_1074","HERK L1","Chemisch zuurstofverbruik",288,"CZV","L117_1074CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L117_1085","WILDERBEEK","Chemisch zuurstofverbruik",288,"CZV","L117_1085CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L117_17","STEENVOORDEBEEK (WATOU)","Chemisch zuurstofverbruik",288,"CZV","L117_17CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L117_219","BURGGRAVENSTROOM","Chemisch zuurstofverbruik",288,"CZV","L117_219CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L117_232","JOBEEK","Chemisch zuurstofverbruik",288,"CZV","L117_232CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L117_233","RINGBEEK","Chemisch zuurstofverbruik",288,"CZV","L117_233CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L117_402","MOLENBEEK - SLAGVIJVERBEEK","Chemisch zuurstofverbruik",288,"CZV","L117_402CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L117_659","KREKELBEEK","Chemisch zuurstofverbruik",288,"CZV","L117_659CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L117_673","KLEIN SCHIJN (NOORDELIJK DEEL)","Chemisch zuurstofverbruik",288,"CZV","L117_673CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L117_813","HERKEBEEK","Chemisch zuurstofverbruik",288,"CZV","L117_813CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L118_238","KROMMEDIJKBEEK","Chemisch zuurstofverbruik",288,"CZV","L118_238CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L119_675","KLEIN SCHIJN (ZUIDELIJK DEEL)","Chemisch zuurstofverbruik",288,"CZV","L119_675CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L120_1097","KASSELRIJBEEK - OOST","Chemisch zuurstofverbruik",288,"CZV","L120_1097CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L121_1045","GROTEBEEK - WINTERBEEK","Chemisch zuurstofverbruik",288,"CZV","L121_1045CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L2 Bk","L2 Kleine Beek","Chemisch zuurstofverbruik",288,"CZV","L2 BkCZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L2 Bk","L2 kleine beek","Chemisch zuurstofverbruik",288,"CZV","L2 BkCZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_102","DEMER V","Chemisch zuurstofverbruik",288,"CZV","VL05_102CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_103","DEMER VI","Chemisch zuurstofverbruik",288,"CZV","VL05_103CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_104","DEMER VII","Chemisch zuurstofverbruik",288,"CZV","VL05_104CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_105","GETE I","Chemisch zuurstofverbruik",288,"CZV","VL05_105CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_106","GETE II","Chemisch zuurstofverbruik",288,"CZV","VL05_106CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_108","HERK + KLEINE HERK","Chemisch zuurstofverbruik",288,"CZV","VL05_108CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_110","MANGELBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_110CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_113","MOMBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_113CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_114","MUNSTERBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_114CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_115","VELPE","Chemisch zuurstofverbruik",288,"CZV","VL05_115CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_116","WINGE","Chemisch zuurstofverbruik",288,"CZV","VL05_116CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_118","ZWARTWATER","Chemisch zuurstofverbruik",288,"CZV","VL05_118CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_119","VINNE","Chemisch zuurstofverbruik",288,"CZV",{"$f":"_xlfn.CONCAT(A835,E835)","v":"VL05_119CZV"},"90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_12","POPERINGEVAART","Chemisch zuurstofverbruik",288,"CZV","VL05_12CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_121","AA II","Chemisch zuurstofverbruik",288,"CZV","VL05_121CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_122","GROTE LAAK","Chemisch zuurstofverbruik",288,"CZV","VL05_122CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_124","GROTE NETE II","Chemisch zuurstofverbruik",288,"CZV","VL05_124CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_130","WAMP","Chemisch zuurstofverbruik",288,"CZV","VL05_130CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_131","WIMP","Chemisch zuurstofverbruik",288,"CZV","VL05_131CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_134","BERWIJN","Chemisch zuurstofverbruik",288,"CZV","VL05_134CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_135","BOSBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_135CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_136","DOMMEL","Chemisch zuurstofverbruik",288,"CZV","VL05_136CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_137","ITTERBEEK I","Chemisch zuurstofverbruik",288,"CZV","VL05_137CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_138","ITTERBEEK II","Chemisch zuurstofverbruik",288,"CZV","VL05_138CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_14","VLADSLOVAART","Chemisch zuurstofverbruik",288,"CZV","VL05_14CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_140","JEKER II","Chemisch zuurstofverbruik",288,"CZV","VL05_140CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_141","LOSSING","Chemisch zuurstofverbruik",288,"CZV","VL05_141CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_146","MERKSKE","Chemisch zuurstofverbruik",288,"CZV","VL05_146CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_148","WEERIJSEBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_148CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_150","AFLEIDINGSKANAAL van de LEIE/SCHIPDONKKANAAL I","Chemisch zuurstofverbruik",288,"CZV","VL05_150CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_152","AVRIJEVAART + SLEIDINGSVAARDEKE","Chemisch zuurstofverbruik",288,"CZV","VL05_152CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_153","BERGENVAART","Chemisch zuurstofverbruik",288,"CZV","VL05_153CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_159","KANAAL CHARLEROI-BRUSSEL","Chemisch zuurstofverbruik",288,"CZV","VL05_159CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_163","KANAAL GENT-OOSTENDE II","Chemisch zuurstofverbruik",288,"CZV","VL05_163CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_166","KANAAL IEPER-IJZER","Chemisch zuurstofverbruik",288,"CZV","VL05_166CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_167","KANAAL LEUVEN-DIJLE","Chemisch zuurstofverbruik",288,"CZV","VL05_167CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_17","ISABELLAVAART","Chemisch zuurstofverbruik",288,"CZV","VL05_17CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_170","KANAAL VAN BEVERLO","Chemisch zuurstofverbruik",288,"CZV","VL05_170CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_171","LEDE","Chemisch zuurstofverbruik",288,"CZV","VL05_171CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_175","MOERVAART","Chemisch zuurstofverbruik",288,"CZV","VL05_175CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_177","NIEUWE KALE","Chemisch zuurstofverbruik",288,"CZV","VL05_177CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_18","KERKEBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_18CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_180","ZARRENBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_180CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_182","ZUIDLEDE","Chemisch zuurstofverbruik",288,"CZV","VL05_182CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_191","DESSELSE ZANDPUTTEN","Chemisch zuurstofverbruik",288,"CZV","VL05_191CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_192","DONKMEER","Chemisch zuurstofverbruik",288,"CZV","VL05_192CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_195","GAVERS HARELBEKE","Chemisch zuurstofverbruik",288,"CZV","VL05_195CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_196","GRINDPLAS KESSENICH","Chemisch zuurstofverbruik",288,"CZV","VL05_196CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_2","GROTE KEMMELBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_2CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_20","RIVIERBEEK + HERTSBERGEBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_20CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_200","SCHULENSMEER","Chemisch zuurstofverbruik",288,"CZV","VL05_200CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_201","SPAANJERD + HEERENLAAK","Chemisch zuurstofverbruik",288,"CZV","VL05_201CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_202","SPUIKOM OOSTENDE","Chemisch zuurstofverbruik",288,"CZV","VL05_202CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_21","ZUIDERVAARTJE","Chemisch zuurstofverbruik",288,"CZV","VL05_21CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_22","ZWINNEVAART","Chemisch zuurstofverbruik",288,"CZV","VL05_22CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_24","MEREBEEK + BORISGRACHT + LIEVE","Chemisch zuurstofverbruik",288,"CZV","VL05_24CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_25","OUDE KALE","Chemisch zuurstofverbruik",288,"CZV","VL05_25CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_28","BENEDENVLIET","Chemisch zuurstofverbruik",288,"CZV","VL05_28CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_3","HANDZAMEVAART","Chemisch zuurstofverbruik",288,"CZV","VL05_3CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_30","GROTE MOLENBEEK - DE VLIET","Chemisch zuurstofverbruik",288,"CZV","VL05_30CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_31","KALKENSE VAART","Chemisch zuurstofverbruik",288,"CZV","VL05_31CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_32","MOLENBEEK - GROTE BEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_32CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_34","NOORD-ZUIDVERBINDING","Chemisch zuurstofverbruik",288,"CZV","VL05_34CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_38","ZIELBEEK - BOSBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_38CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_4","HEIDEBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_4CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_44","DEVEBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_44CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_45","GAVERBEEK I","Chemisch zuurstofverbruik",288,"CZV","VL05_45CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_46","GAVERBEEK II","Chemisch zuurstofverbruik",288,"CZV","VL05_46CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_5","IEPERLEE + VERWEZEN KANAAL IEPER-KOMEN","Chemisch zuurstofverbruik",288,"CZV","VL05_5CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_50","LEIE III","Chemisch zuurstofverbruik",288,"CZV","VL05_50CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_51","MANDEL I","Chemisch zuurstofverbruik",288,"CZV","VL05_51CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_52","MANDEL II","Chemisch zuurstofverbruik",288,"CZV","VL05_52CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_53","OUDE MANDEL","Chemisch zuurstofverbruik",288,"CZV","VL05_53CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_58","BOVEN-SCHELDE IV","Chemisch zuurstofverbruik",288,"CZV","VL05_58CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_6","IEPERLEED","Chemisch zuurstofverbruik",288,"CZV","VL05_6CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_61","RONE","Chemisch zuurstofverbruik",288,"CZV","VL05_61CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_62","STAMPKOTBEEK","Chemisch zuurstofverbruik",288,"CZV",{"$f":"_xlfn.CONCAT(A899,E899)","v":"VL05_62CZV"},"90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_64","ZWARTE SPIEREBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_64CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_67","DENDER I","Chemisch zuurstofverbruik",288,"CZV","VL05_67CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_70","DENDER IV","Chemisch zuurstofverbruik",288,"CZV","VL05_70CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_73","MOLENBEEK - PACHTBOSBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_73CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_75","VONDELBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_75CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_77","DIJLE I","Chemisch zuurstofverbruik",288,"CZV","VL05_77CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_81","DIJLE V","Chemisch zuurstofverbruik",288,"CZV","VL05_81CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_85","LEIBEEK - LAAKBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_85CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_86","NETHEN","Chemisch zuurstofverbruik",288,"CZV","VL05_86CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_87","VOER (Leuven)","Chemisch zuurstofverbruik",288,"CZV","VL05_87CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_89","VUNT","Chemisch zuurstofverbruik",288,"CZV","VL05_89CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_90","WEESBEEK","Chemisch zuurstofverbruik",288,"CZV","VL05_90CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_93","ZENNE II","Chemisch zuurstofverbruik",288,"CZV","VL05_93CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_98","DEMER I","Chemisch zuurstofverbruik",288,"CZV","VL05_98CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL05_99","DEMER II","Chemisch zuurstofverbruik",288,"CZV","VL05_99CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_125","GROTE NETE III","Chemisch zuurstofverbruik",288,"CZV","VL08_125CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_132","GETIJDENETES","Chemisch zuurstofverbruik",288,"CZV","VL08_132CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_157","ISABELLAWATERING","Chemisch zuurstofverbruik",288,"CZV","VL08_157CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_16","BLANKENBERGSE VAART + NOORDEDE","Chemisch zuurstofverbruik",288,"CZV","VL08_16CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_162","KANAAL GENT-OOSTENDE I + COUPURE + VERBINDINGSKANAAL","Chemisch zuurstofverbruik",288,"CZV","VL08_162CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_164","KANAAL GENT-OOSTENDE III","Chemisch zuurstofverbruik",288,"CZV","VL08_164CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_172","LEOPOLDKANAAL I","Chemisch zuurstofverbruik",288,"CZV","VL08_172CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_173","LEOPOLDKANAAL II","Chemisch zuurstofverbruik",288,"CZV","VL08_173CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_176","NETEKANAAL","Chemisch zuurstofverbruik",288,"CZV","VL08_176CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_178","NOORDELIJKE RINGVAART","Chemisch zuurstofverbruik",288,"CZV","VL08_178CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_179","WESTELIJKE RINGVAART","Chemisch zuurstofverbruik",288,"CZV","VL08_179CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_27","ZWARTESLUISBEEK","Chemisch zuurstofverbruik",288,"CZV","VL08_27CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_39","GETIJDEDURME","Chemisch zuurstofverbruik",288,"CZV","VL08_39CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_41","ZEESCHELDE II","Chemisch zuurstofverbruik",288,"CZV","VL08_41CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_55","BOVEN-SCHELDE I","Chemisch zuurstofverbruik",288,"CZV","VL08_55CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_7","IJZER I","Chemisch zuurstofverbruik",288,"CZV","VL08_7CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_71","DENDER V","Chemisch zuurstofverbruik",288,"CZV","VL08_71CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_72","MARK (Denderbekken)","Chemisch zuurstofverbruik",288,"CZV","VL08_72CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_80","DIJLE IV","Chemisch zuurstofverbruik",288,"CZV","VL08_80CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_82","DIJLE VI","Chemisch zuurstofverbruik",288,"CZV","VL08_82CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_92","ZENNE I","Chemisch zuurstofverbruik",288,"CZV","VL08_92CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL08_95","GETIJDEDIJLE & GETIJDEZENNE","Chemisch zuurstofverbruik",288,"CZV","VL08_95CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL09_78","DIJLE II","Chemisch zuurstofverbruik",288,"CZV","VL09_78CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_10","MARTJEVAART","Chemisch zuurstofverbruik",288,"CZV","VL11_10CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_109","KLEINE GETE + VLOEDGRACHT","Chemisch zuurstofverbruik",288,"CZV","VL11_109CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_11","MOERDIJKVAART","Chemisch zuurstofverbruik",288,"CZV","VL11_11CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_117","ZWARTEBEEK","Chemisch zuurstofverbruik",288,"CZV","VL11_117CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_120","AA I","Chemisch zuurstofverbruik",288,"CZV","VL11_120CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_123","GROTE NETE I","Chemisch zuurstofverbruik",288,"CZV","VL11_123CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_126","KLEINE NETE I","Chemisch zuurstofverbruik",288,"CZV","VL11_126CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_127","KLEINE NETE II","Chemisch zuurstofverbruik",288,"CZV","VL11_127CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_128","MOL NEET","Chemisch zuurstofverbruik",288,"CZV","VL11_128CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_13","VEURNE AMBACHT POLDER WATERLOPEN","Chemisch zuurstofverbruik",288,"CZV","VL11_13CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_133","ABEEK","Chemisch zuurstofverbruik",288,"CZV","VL11_133CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_145","MARK (Maas)","Chemisch zuurstofverbruik",288,"CZV","VL11_145CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_155","BRUGSE REIEN","Chemisch zuurstofverbruik",288,"CZV","VL11_155CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_165","KANAAL GENT-TERNEUZEN + GENTSE HAVENDOKKEN","Chemisch zuurstofverbruik",288,"CZV","VL11_165CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_19","OOSTENDS KREKENGEBIED","Chemisch zuurstofverbruik",288,"CZV","VL11_19CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_203","MAAS I+II+III","Chemisch zuurstofverbruik",288,"CZV","VL11_203CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_205","DEMER III+IV","Chemisch zuurstofverbruik",288,"CZV","VL11_205CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_207","MELSTERBEEK I+II","Chemisch zuurstofverbruik",288,"CZV","VL11_207CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_37","WATERLOOP VAN DE HOGE LANDEN + MELKADER","Chemisch zuurstofverbruik",288,"CZV","VL11_37CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_40","ZEESCHELDE I","Chemisch zuurstofverbruik",288,"CZV","VL11_40CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_59","GROTE SPIEREBEEK","Chemisch zuurstofverbruik",288,"CZV","VL11_59CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_63","ZWALM","Chemisch zuurstofverbruik",288,"CZV","VL11_63CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_76","BAREBEEK","Chemisch zuurstofverbruik",288,"CZV","VL11_76CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_83","IJSSE","Chemisch zuurstofverbruik",288,"CZV","VL11_83CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_84","LAAN","Chemisch zuurstofverbruik",288,"CZV","VL11_84CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_88","VROUWVLIET","Chemisch zuurstofverbruik",288,"CZV",{"$f":"_xlfn.CONCAT(A963,E963)","v":"VL11_88CZV"},"90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL11_91","WOLUWE","Chemisch zuurstofverbruik",288,"CZV","VL11_91CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_147","WARMBEEK","Chemisch zuurstofverbruik",288,"CZV","VL17_147CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_15","HAVENGEUL IJZER","Chemisch zuurstofverbruik",288,"CZV","VL17_15CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_154","BRAKELEIKEN + LIEVE","Chemisch zuurstofverbruik",288,"CZV","VL17_154CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_156","GENTSE BINNENWATEREN","Chemisch zuurstofverbruik",288,"CZV","VL17_156CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_161","KANAAL DUINKERKE-NIEUWPOORT","Chemisch zuurstofverbruik",288,"CZV","VL17_161CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_168","KANAAL PLASSENDALE-NIEUWPOORT","Chemisch zuurstofverbruik",288,"CZV","VL17_168CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_169","KANAAL ROESELARE-LEIE","Chemisch zuurstofverbruik",288,"CZV","VL17_169CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_174","LOKANAAL","Chemisch zuurstofverbruik",288,"CZV","VL17_174CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_184","BLANKENBERGSE HAVENGEUL + JACHTHAVENS","Chemisch zuurstofverbruik",288,"CZV","VL17_184CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_185","OOSTENDSE HAVENGEUL + DOKKEN","Chemisch zuurstofverbruik",288,"CZV","VL17_185CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_186","ZEEBRUGGE BUITENHAVEN","Chemisch zuurstofverbruik",288,"CZV","VL17_186CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_187","ANTWERPSE HAVENDOKKEN + SCHELDE-RIJNVERBINDING","Chemisch zuurstofverbruik",288,"CZV","VL17_187CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_190","BOUDEWIJNKANAAL + ACHTERHAVEN ZEEBRUGGE","Chemisch zuurstofverbruik",288,"CZV","VL17_190CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_204","BOVEN-SCHELDE II+III","Chemisch zuurstofverbruik",288,"CZV","VL17_204CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_206","DENDER II+III","Chemisch zuurstofverbruik",288,"CZV","VL17_206CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_29","GROOT SCHIJN","Chemisch zuurstofverbruik",288,"CZV","VL17_29CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_35","VERLEGDE SCHIJN - HOOFDGRACHT","Chemisch zuurstofverbruik",288,"CZV","VL17_35CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_42","ZEESCHELDE III + RUPEL","Chemisch zuurstofverbruik",288,"CZV","VL17_42CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_43","ZEESCHELDE IV","Chemisch zuurstofverbruik",288,"CZV","VL17_43CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_48","LEIE I","Chemisch zuurstofverbruik",288,"CZV","VL17_48CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_49","LEIE II","Chemisch zuurstofverbruik",288,"CZV","VL17_49CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_54","TOERISTISCHE LEIE","Chemisch zuurstofverbruik",288,"CZV","VL17_54CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_60","MOLENBEEK - MAARKEBEEK","Chemisch zuurstofverbruik",288,"CZV","VL17_60CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_66","BELLEBEEK","Chemisch zuurstofverbruik",288,"CZV","VL17_66CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL17_9","IJZER III","Chemisch zuurstofverbruik",288,"CZV","VL17_9CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL20_36","VERLEGDE SCHIJN - VOORGRACHT","Chemisch zuurstofverbruik",288,"CZV","VL20_36CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL20_96","BEGIJNENBEEK","Chemisch zuurstofverbruik",288,"CZV","VL20_96CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL21_1","BLANKAART WATERLOPEN","Chemisch zuurstofverbruik",288,"CZV","VL21_1CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL21_107","GROTE GETE + BORGGRACHT","Chemisch zuurstofverbruik",288,"CZV","VL21_107CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL21_129","MOLENBEEK - BOLLAAK","Chemisch zuurstofverbruik",288,"CZV","VL21_129CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL21_139","JEKER I","Chemisch zuurstofverbruik",288,"CZV","VL21_139CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL21_26","POEKEBEEK","Chemisch zuurstofverbruik",288,"CZV","VL21_26CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL21_33","MOLENBEEK - KOTTEMBEEK","Chemisch zuurstofverbruik",288,"CZV","VL21_33CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL21_47","HEULEBEEK","Chemisch zuurstofverbruik",288,"CZV","VL21_47CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL21_74","MOLENBEEK - TER ERPENBEEK","Chemisch zuurstofverbruik",288,"CZV","VL21_74CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL21_79","DIJLE III","Chemisch zuurstofverbruik",288,"CZV","VL21_79CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL21_8","IJZER II","Chemisch zuurstofverbruik",288,"CZV","VL21_8CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL21_94","ZUUNBEEK","Chemisch zuurstofverbruik",288,"CZV","VL21_94CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL21_97","DE HULPE - ZWART WATER","Chemisch zuurstofverbruik",288,"CZV","VL21_97CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL22_208","ALBERTKANAAL - Maasbekken","Chemisch zuurstofverbruik",288,"CZV","VL22_208CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL22_209","ALBERTKANAAL - Demerbekken","Chemisch zuurstofverbruik",288,"CZV","VL22_209CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL22_210","ALBERTKANAAL - Netebekken","Chemisch zuurstofverbruik",288,"CZV","VL22_210CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL22_211","ALBERTKANAAL - Benedenscheldebekken","Chemisch zuurstofverbruik",288,"CZV","VL22_211CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL22_212","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Netebekken","Chemisch zuurstofverbruik",288,"CZV","VL22_212CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL22_213","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Maasbekken","Chemisch zuurstofverbruik",288,"CZV","VL22_213CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL22_214","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Benedenscheldebekken","Chemisch zuurstofverbruik",288,"CZV","VL22_214CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL22_215","ZEEKANAAL BRUSSEL-SCHELDE - Dijle-Zennebekken","Chemisch zuurstofverbruik",288,"CZV","VL22_215CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL22_216","ZEEKANAAL BRUSSEL-SCHELDE - Benedenscheldebekken","Chemisch zuurstofverbruik",288,"CZV","VL22_216CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL22_217","AFLEIDINGSKANAAL van de LEIE II + KANAAL van EEKLO - Bekken van de Gentse kanalen","Chemisch zuurstofverbruik",288,"CZV","VL22_217CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL22_218","AFLEIDINGSKANAAL van de LEIE II - Bekken van de Brugse polders","Chemisch zuurstofverbruik",288,"CZV","VL22_218CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL22_219","KANAAL BOSSUIT-KORTRIJK - Bovenscheldebekken","Chemisch zuurstofverbruik",288,"CZV","VL22_219CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL22_220","KANAAL BOSSUIT-KORTRIJK - Leiebekken","Chemisch zuurstofverbruik",288,"CZV","VL22_220CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["VL22_221","ZUID-WILLEMSVAART + KANAAL BOCHOLT-HERENTALS (deels) + KANAAL BRIEGDEN-NEERHAREN","Chemisch zuurstofverbruik",288,"CZV","VL22_221CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_10","KEMMELBEEK","Chloride",4,"Cl-","L107_10Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_104","NEERBEEK","Chloride",4,"Cl-","L107_104Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_105","PALINGBEEK","Chloride",4,"Cl-","L107_105Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_11","WANEBEEK","Chloride",4,"Cl-","L107_11Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_112","LA HAUTE PLANCHE","Chloride",4,"Cl-","L107_112Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_113","DOUVEBEEK","Chloride",4,"Cl-","L107_113Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_116","GROTE SPIERE","Chloride",4,"Cl-","L107_116Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_12","VLETERBEEK","Chloride",4,"Cl-","L107_12Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_120","SCHEEBEEK","Chloride",4,"Cl-","L107_120Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_123","KANAAL VAN BRUGGE NAAR SLUIS","Chloride",4,"Cl-",{"$f":"_xlfn.CONCAT(A1027,E1027)","v":"L107_123Cl-"},"90 percentiel","mg/L",200,"maximum",300,300,375,450]
["L107_135","JABBEEKSE BEEK","Chloride",4,"Cl-","L107_135Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_136","HOGE WATERING","Chloride",4,"Cl-","L107_136Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["L107_16","HARINGEBEEK","Chloride",4,"Cl-","L107_16Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_209","ZWARTESLUISBEEK L1","Chloride",4,"Cl-","L107_209Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["L107_218","SLEIDINGSVAARDEKEN","Chloride",4,"Cl-","L107_218Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_225","KEUTELBEEK","Chloride",4,"Cl-","L107_225Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_234","POEKEBEEK L1","Chloride",4,"Cl-","L107_234Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_235","REIGERBEEK","Chloride",4,"Cl-","L107_235Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_236","NEERSCHUURBEEK","Chloride",4,"Cl-","L107_236Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_237","SPEIBEEK","Chloride",4,"Cl-","L107_237Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_239","OUDE MANDEL L1","Chloride",4,"Cl-","L107_239Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_240","ZOUBEEK","Chloride",4,"Cl-","L107_240Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_241","KATTEBEEK","Chloride",4,"Cl-","L107_241Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_242","DUIVEBEEK","Chloride",4,"Cl-","L107_242Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_246","STAMPKOTBEEK - MOLENBEEK","Chloride",4,"Cl-","L107_246Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_247","STAMPKOTBEEK - WALLEBEEK","Chloride",4,"Cl-","L107_247Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_253","STAMPKOTBEEK - MUNKBOSBEEK","Chloride",4,"Cl-","L107_253Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_254","MOLENBEEK - BEIAARDBEEK","Chloride",4,"Cl-","L107_254Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_266","PEERDESTOKBEEK","Chloride",4,"Cl-","L107_266Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_272","OPHASSELTBEEK","Chloride",4,"Cl-","L107_272Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_273","MOLENBEEK - PACHTBOSBEEK L1","Chloride",4,"Cl-","L107_273Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_274","MOLENBEEK - KALSTERBEEK","Chloride",4,"Cl-","L107_274Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_275","TER ERPENBEEK","Chloride",4,"Cl-","L107_275Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_276","MOLENBEEK - GRAADBEEK","Chloride",4,"Cl-","L107_276Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_277","WILDEBEEK","Chloride",4,"Cl-","L107_277Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_279","MOLENBEEK - VOGELENZANGBEEK","Chloride",4,"Cl-","L107_279Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_282","MOLENBEEK - GONDEBEEK","Chloride",4,"Cl-","L107_282Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_287","MOLENBEEK - GROTE BEEK","Chloride",4,"Cl-","L107_287Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_289","DAMSLOOT","Chloride",4,"Cl-","L107_289Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_296","VOORSTESLOOT","Chloride",4,"Cl-","L107_296Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_299","VONDELBEEK L1","Chloride",4,"Cl-","L107_299Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_3","BROENBEEK","Chloride",4,"Cl-","L107_3Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_305","ZELEBEEK","Chloride",4,"Cl-","L107_305Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_325","GROTE ASTBEEK","Chloride",4,"Cl-","L107_325Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_329","BLOKSTRAATBEEK","Chloride",4,"Cl-","L107_329Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["L107_330","WATERLOOP VAN DE HOGE LANDEN L1","Chloride",4,"Cl-","L107_330Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_335","MOLENBEEK - BEVERBEEK","Chloride",4,"Cl-","L107_335Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_336","DE RIJT","Chloride",4,"Cl-","L107_336Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_4","KORVERSBEEK","Chloride",4,"Cl-","L107_4Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_40","STENENSLUISVAART","Chloride",4,"Cl-","L107_40Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["L107_403","MOLENBEEK - NEERPEDEBEEK","Chloride",4,"Cl-","L107_403Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_404","LOTBEEK","Chloride",4,"Cl-","L107_404Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_407","GROEBENGRACHT","Chloride",4,"Cl-","L107_407Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_409","KLEINE MAALBEEK","Chloride",4,"Cl-","L107_409Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_411","MOLENBEEK - PARKBEEK","Chloride",4,"Cl-","L107_411Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_413","TANGEBEEK","Chloride",4,"Cl-","L107_413Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_417","DE GROTE LAAK","Chloride",4,"Cl-","L107_417Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_418","MENE","Chloride",4,"Cl-","L107_418Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_421","GENOVEVABEEK","Chloride",4,"Cl-","L107_421Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_422","'S HERTOGENGRACHT","Chloride",4,"Cl-","L107_422Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_423","BEGIJNEBEEK L1","Chloride",4,"Cl-","L107_423Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_424","VIJVERSLOOP","Chloride",4,"Cl-","L107_424Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_431","ST-ODULPHUSBEEK","Chloride",4,"Cl-","L107_431Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_432","DORMAALBEEK","Chloride",4,"Cl-","L107_432Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_433","BEVERBEEK","Chloride",4,"Cl-","L107_433Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_434","SCHEIBEEK","Chloride",4,"Cl-","L107_434Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_435","AREBEEK","Chloride",4,"Cl-","L107_435Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_439","IJSE L1","Chloride",4,"Cl-","L107_439Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_441","LANGEGRACHT","Chloride",4,"Cl-","L107_441Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_449","VOER (BERTEM)","Chloride",4,"Cl-","L107_449Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_451","GROTE LAAK - GROTE LOOP - MESTENLOOP","Chloride",4,"Cl-","L107_451Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_452","LAARBEEK","Chloride",4,"Cl-","L107_452Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_453","ZWARTEBEEK (SCHERPENHEUVEL-ZICHEM)","Chloride",4,"Cl-","L107_453Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_454","KLEINEBEEK - RIJSELSESTRAATVLIET","Chloride",4,"Cl-",{"$f":"_xlfn.CONCAT(A1091,E1091)","v":"L107_454Cl-"},"90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_462","LEMINGSBEEK","Chloride",4,"Cl-","L107_462Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_463","AABEEK (MECHELEN)","Chloride",4,"Cl-","L107_463Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_464","LEYBEEK","Chloride",4,"Cl-","L107_464Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_47","ZARRENBEEK L1","Chloride",4,"Cl-","L107_47Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_48","KANAAL VAN ESEN","Chloride",4,"Cl-","L107_48Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["L107_5","BOLLAERTBEEK","Chloride",4,"Cl-","L107_5Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_6","DIKKEBUSBEEK","Chloride",4,"Cl-","L107_6Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_600","LEYLOOP","Chloride",4,"Cl-","L107_600Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_601","DE AA (RAVELS)","Chloride",4,"Cl-","L107_601Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_602","BLAUWPUTTEN EN LEILOOP","Chloride",4,"Cl-","L107_602Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_603","HEERLESE LOOP","Chloride",4,"Cl-","L107_603Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_607","MERKSKE L1","Chloride",4,"Cl-","L107_607Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_609","KLEINE MARK","Chloride",4,"Cl-","L107_609Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_61","VAARTDIJKGELEED","Chloride",4,"Cl-","L107_61Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["L107_610","MARK L1","Chloride",4,"Cl-","L107_610Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_613","SLUISKENSVIJVER","Chloride",4,"Cl-","L107_613Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_614","WEERIJSEBEEK L1","Chloride",4,"Cl-","L107_614Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_615","KLEINE BEEK (WUUSTWEZEL)","Chloride",4,"Cl-","L107_615Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_629","KLEIN WILBOEREBEEK","Chloride",4,"Cl-","L107_629Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_63","BOERGONJEVAART","Chloride",4,"Cl-","L107_63Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["L107_631","MOLENBEEK - BOLLAAK L1","Chloride",4,"Cl-","L107_631Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_632","DE DELFTE BEEK","Chloride",4,"Cl-","L107_632Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_633","BOSBEEK - DIEPTELOOP","Chloride",4,"Cl-","L107_633Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_638","GROTE CALIE","Chloride",4,"Cl-","L107_638Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_640","DE AA - NATTENLOOP","Chloride",4,"Cl-","L107_640Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_644","ITTERBEEK (DUFFEL)","Chloride",4,"Cl-","L107_644Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_648","BRUINBEEK","Chloride",4,"Cl-","L107_648Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_650","REEHAGENBEEK","Chloride",4,"Cl-","L107_650Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_654","LARUMSE LOOP","Chloride",4,"Cl-","L107_654Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_655","DALEMANSLOOP","Chloride",4,"Cl-","L107_655Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_656","BEGGELBEEK","Chloride",4,"Cl-","L107_656Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_66","KERKBEEK","Chloride",4,"Cl-","L107_66Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_664","MOLENBEEK - ZIJP","Chloride",4,"Cl-","L107_664Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_665","BOUWBEEK","Chloride",4,"Cl-","L107_665Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_67","LIJSTERBEEK","Chloride",4,"Cl-","L107_67Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_677","DIEPE BEEK","Chloride",4,"Cl-","L107_677Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_681","KOUDE BEEK","Chloride",4,"Cl-","L107_681Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_684","SCHOON SCHIJN","Chloride",4,"Cl-","L107_684Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["L107_688","LAARSE BEEK","Chloride",4,"Cl-","L107_688Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_695","VARENDONKSE BEEK","Chloride",4,"Cl-","L107_695Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_702","MILLEGEMLOOP","Chloride",4,"Cl-","L107_702Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_705","SCHEPPELIJKE NETE","Chloride",4,"Cl-","L107_705Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_706","MOLSE NETE L1","Chloride",4,"Cl-","L107_706Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_708","GROTE NETE L1","Chloride",4,"Cl-","L107_708Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_722","WAMP L1","Chloride",4,"Cl-","L107_722Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_723","RODE LOOP","Chloride",4,"Cl-","L107_723Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_729","STAPKENSLOOP","Chloride",4,"Cl-","L107_729Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_735","GESTELBEEK","Chloride",4,"Cl-","L107_735Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_740","BERGEBEEK","Chloride",4,"Cl-","L107_740Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_741","SPILLEBEEK","Chloride",4,"Cl-","L107_741Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_742","PLATTE BEEK","Chloride",4,"Cl-","L107_742Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_78","DEVEBEEK L1","Chloride",4,"Cl-","L107_78Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_8","IEPERLEE","Chloride",4,"Cl-","L107_8Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_809","KLEINE HERK L1","Chloride",4,"Cl-","L107_809Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_810","WINTERBEEK (KORTESSEM)","Chloride",4,"Cl-","L107_810Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_812","MOMBEEK L1","Chloride",4,"Cl-","L107_812Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_814","STEENLAAK","Chloride",4,"Cl-","L107_814Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_82","BABILLEBEEK","Chloride",4,"Cl-","L107_82Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_824","ROELBEEK","Chloride",4,"Cl-","L107_824Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_83","ROOBEEK","Chloride",4,"Cl-","L107_83Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_836","LAAMBEEK","Chloride",4,"Cl-","L107_836Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_839","ZONDERIKBEEK","Chloride",4,"Cl-","L107_839Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_84","KROMMEBEEK","Chloride",4,"Cl-","L107_84Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_846","KAATSBEEK","Chloride",4,"Cl-",{"$f":"_xlfn.CONCAT(A1155,E1155)","v":"L107_846Cl-"},"90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_847","WINTERBEEK (BILZEN)","Chloride",4,"Cl-","L107_847Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_848","DEMER L1","Chloride",4,"Cl-","L107_848Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_852","MUNSTERBEEK L1","Chloride",4,"Cl-","L107_852Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_853","ZUTENDAALBEEK","Chloride",4,"Cl-","L107_853Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_854","BOLLISENBEEK","Chloride",4,"Cl-","L107_854Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_855","DOMMEL L1","Chloride",4,"Cl-","L107_855Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_856","HOLVENLOOP","Chloride",4,"Cl-","L107_856Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_857","EINDERGATLOOP","Chloride",4,"Cl-","L107_857Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_858","WARMBEEK L1","Chloride",4,"Cl-","L107_858Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_859","PRINSENLOOP","Chloride",4,"Cl-","L107_859Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_861","ABEEK L1","Chloride",4,"Cl-","L107_861Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_866","LOSSING L1","Chloride",4,"Cl-","L107_866Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_869","SOERBEEK","Chloride",4,"Cl-","L107_869Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_876","BOSBEEK L1","Chloride",4,"Cl-","L107_876Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_879","VRIETSELBEEK - OUDE MAAS (DILSEN)","Chloride",4,"Cl-","L107_879Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_883","ZIEPBEEK","Chloride",4,"Cl-","L107_883Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_885","HEESWATER","Chloride",4,"Cl-","L107_885Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_890","BEEK - DE BUTH (TONGEREN)","Chloride",4,"Cl-","L107_890Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_891","VOER (VOEREN)","Chloride",4,"Cl-","L107_891Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_892","BEEK (VOEREN)","Chloride",4,"Cl-","L107_892Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_893","GULP","Chloride",4,"Cl-","L107_893Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_91","PLAATSBEEK","Chloride",4,"Cl-","L107_91Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_92","MAALBEEK (LEIEBEKKEN)","Chloride",4,"Cl-","L107_92Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_97","KASSELRIJBEEK - WEST","Chloride",4,"Cl-","L107_97Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L107_98","GAVERBEEK","Chloride",4,"Cl-","L107_98Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L110_1100","ZILVERBEEK","Chloride",4,"Cl-","L110_1100Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1001","MARTJEVAART - LEKKERBOTERBEEK","Chloride",4,"Cl-","L111_1001Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1003","GELUWEBEEK","Chloride",4,"Cl-","L111_1003Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1004","RIJTGRACHT","Chloride",4,"Cl-","L111_1004Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1006","HOOFDSLOOT","Chloride",4,"Cl-","L111_1006Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1014","MEREBEEK","Chloride",4,"Cl-","L111_1014Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1016","WANTEBEEK","Chloride",4,"Cl-","L111_1016Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1018","LEEBEEK","Chloride",4,"Cl-","L111_1018Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1019","MOLENBEEK - MARKEBEEK","Chloride",4,"Cl-","L111_1019Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1020","OOSSEBEEK","Chloride",4,"Cl-","L111_1020Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1021","ZWALMBEEK","Chloride",4,"Cl-","L111_1021Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1022","MOLENBEEK (RONSE)","Chloride",4,"Cl-","L111_1022Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1024","BAVEGEMSE BEEK","Chloride",4,"Cl-","L111_1024Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1025","MAANBEEK","Chloride",4,"Cl-","L111_1025Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1027","GROOTEBEEK","Chloride",4,"Cl-","L111_1027Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1028","LANGELEDE","Chloride",4,"Cl-","L111_1028Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1029","KLEINE WATERGANG","Chloride",4,"Cl-","L111_1029Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1030","WATERGANG VAN DE MOERBEKEPOLDER","Chloride",4,"Cl-","L111_1030Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1031","KANAAL VAN STEKENE","Chloride",4,"Cl-","L111_1031Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1032","DIJKGRACHT","Chloride",4,"Cl-","L111_1032Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["L111_1033","PAPENMEERSBEEK","Chloride",4,"Cl-","L111_1033Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1035","KOEVAARDEKEN","Chloride",4,"Cl-","L111_1035Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["L111_1037","MOLENBEEK - LAKEBEEK","Chloride",4,"Cl-","L111_1037Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1038","MAALBEEK - AMELVONNEBEEK","Chloride",4,"Cl-","L111_1038Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1039","STEENVOORDBEEK (TERNAT)","Chloride",4,"Cl-","L111_1039Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1040","BELLEBEEK L1","Chloride",4,"Cl-","L111_1040Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1041","WINGE L1","Chloride",4,"Cl-","L111_1041Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1042","LEIBEEK - LIPSEBEEK L1","Chloride",4,"Cl-","L111_1042Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1043","WEESBEEK L1","Chloride",4,"Cl-","L111_1043Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1044","KASTEELBEEK","Chloride",4,"Cl-","L111_1044Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1046","GROTE MOTTE","Chloride",4,"Cl-","L111_1046Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1047","BAREBEEK L1","Chloride",4,"Cl-","L111_1047Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1049","MUNTLOOP","Chloride",4,"Cl-","L111_1049Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1050","WEHAGENBEEK","Chloride",4,"Cl-","L111_1050Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1052","LAAKBEEK","Chloride",4,"Cl-","L111_1052Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1053","MOUBEEK","Chloride",4,"Cl-","L111_1053Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1054","GOORBOSBEEK","Chloride",4,"Cl-","L111_1054Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1056","VROUWVLIET L1","Chloride",4,"Cl-","L111_1056Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1057","GROTE MOLENBEEK L1","Chloride",4,"Cl-",{"$f":"_xlfn.CONCAT(A1219,E1219)","v":"L111_1057Cl-"},"90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1058","ZWARTE BEEK (WILLEBROEK)","Chloride",4,"Cl-","L111_1058Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1059","ZIELBEEK - BOSBEEK L1","Chloride",4,"Cl-","L111_1059Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1060","GROOT SCHIJN L1","Chloride",4,"Cl-","L111_1060Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1062","HERSELTSELOOP","Chloride",4,"Cl-","L111_1062Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1063","STEENKENSBEEK","Chloride",4,"Cl-","L111_1063Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1064","ST. TRUDOLEKEN","Chloride",4,"Cl-","L111_1064Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1065","ASBEEK","Chloride",4,"Cl-","L111_1065Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1066","LOEIJENS NEETJE","Chloride",4,"Cl-","L111_1066Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1067","KLEINE NETE L1","Chloride",4,"Cl-","L111_1067Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1070","WIMP L1","Chloride",4,"Cl-","L111_1070Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1071","GOORLOOP","Chloride",4,"Cl-","L111_1071Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1072","POVERSBEEK","Chloride",4,"Cl-","L111_1072Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1075","MELSTERBEEK L1","Chloride",4,"Cl-","L111_1075Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1076","CICINDRIA","Chloride",4,"Cl-","L111_1076Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1077","MOLENBEEK (SINT-TRUIDEN)","Chloride",4,"Cl-","L111_1077Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1078","GRONDBEEK","Chloride",4,"Cl-","L111_1078Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1079","HELDERBEEK","Chloride",4,"Cl-","L111_1079Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1080","ZWARTEBEEK L1","Chloride",4,"Cl-","L111_1080Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1081","MANGELBEEK L1","Chloride",4,"Cl-","L111_1081Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1082","SLANGBEEK","Chloride",4,"Cl-","L111_1082Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1083","MISERIKBEEK","Chloride",4,"Cl-","L111_1083Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1084","MANDEL L1","Chloride",4,"Cl-","L111_1084Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1086","LOZERBROEKBEEK","Chloride",4,"Cl-","L111_1086Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1087","HORSTGATERBEEK","Chloride",4,"Cl-","L111_1087Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1088","ITTERBEEK L1","Chloride",4,"Cl-","L111_1088Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1089","WITBEEK","Chloride",4,"Cl-","L111_1089Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1090","ZANDERBEEK","Chloride",4,"Cl-","L111_1090Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1091","KIKBEEK","Chloride",4,"Cl-","L111_1091Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1092","ZOUW","Chloride",4,"Cl-","L111_1092Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1093","EZELSBEEK","Chloride",4,"Cl-","L111_1093Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1094","HEULEBEEK L1","Chloride",4,"Cl-","L111_1094Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1095","KLEINE LAAK","Chloride",4,"Cl-","L111_1095Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1096","GROTE LAAK L1","Chloride",4,"Cl-","L111_1096Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1098","KEIBEEK","Chloride",4,"Cl-","L111_1098Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1099","GAVERSE BEEK (BECQUE DE NEUVILLE)","Chloride",4,"Cl-","L111_1099Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1102","KLEINE A - WILDERTSE BEEK","Chloride",4,"Cl-","L111_1102Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1104","DESPIERREBEEK","Chloride",4,"Cl-","L111_1104Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1105","MELSENBEEK","Chloride",4,"Cl-","L111_1105Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1106","DONKSE BEEK","Chloride",4,"Cl-","L111_1106Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["L111_1109","MOERDIJKVAART L1","Chloride",4,"Cl-","L111_1109Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1110","EDE","Chloride",4,"Cl-","L111_1110Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1112","ISABELLASTROOM","Chloride",4,"Cl-","L111_1112Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1113","LACHENEBEEK","Chloride",4,"Cl-","L111_1113Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1114","ANTITANKGRACHT ZUID","Chloride",4,"Cl-","L111_1114Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_1201","S HERTOGENDIJKSE BEEK","Chloride",4,"Cl-","L111_1201Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["L111_15","HEIDEBEEK (VLETEREN)","Chloride",4,"Cl-","L111_15Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["L111_298","OUDE DENDER","Chloride",4,"Cl-","L111_298Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_315","FONDATIEGRACHT","Chloride",4,"Cl-","L111_315Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_326","BARBIERBEEK","Chloride",4,"Cl-","L111_326Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_419","SCHOORBROEKBEEK","Chloride",4,"Cl-","L111_419Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_436","VELPE L1","Chloride",4,"Cl-","L111_436Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_624","TAPPELBEEK","Chloride",4,"Cl-","L111_624Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_627","KLEINE BEEK (ZANDHOVEN)","Chloride",4,"Cl-","L111_627Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_639","VISBEEK","Chloride",4,"Cl-","L111_639Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_674","BENEDENVLIET L1","Chloride",4,"Cl-","L111_674Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_676","WEZELSE BEEK","Chloride",4,"Cl-","L111_676Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_699","SCHERPENBERGLOOP","Chloride",4,"Cl-","L111_699Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_707","KLEINE HOOFDGRACHT","Chloride",4,"Cl-","L111_707Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_717","DESSELSE NEET","Chloride",4,"Cl-","L111_717Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_724","ANTITANKGRACHT NOORD","Chloride",4,"Cl-","L111_724Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L111_844","STIEMER","Chloride",4,"Cl-","L111_844Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L117_1036","ZUUNBEEK L1","Chloride",4,"Cl-","L117_1036Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L117_1068","HERTSBERGEBEEK - GETEBEEK","Chloride",4,"Cl-","L117_1068Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L117_1073","RIVIERBEEK","Chloride",4,"Cl-",{"$f":"_xlfn.CONCAT(A1283,E1283)","v":"L117_1073Cl-"},"90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L117_1074","HERK L1","Chloride",4,"Cl-","L117_1074Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L117_1085","WILDERBEEK","Chloride",4,"Cl-","L117_1085Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L117_17","STEENVOORDEBEEK (WATOU)","Chloride",4,"Cl-","L117_17Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L117_219","BURGGRAVENSTROOM","Chloride",4,"Cl-","L117_219Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L117_232","JOBEEK","Chloride",4,"Cl-","L117_232Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L117_233","RINGBEEK","Chloride",4,"Cl-","L117_233Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L117_402","MOLENBEEK - SLAGVIJVERBEEK","Chloride",4,"Cl-","L117_402Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L117_659","KREKELBEEK","Chloride",4,"Cl-","L117_659Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L117_673","KLEIN SCHIJN (NOORDELIJK DEEL)","Chloride",4,"Cl-","L117_673Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L117_813","HERKEBEEK","Chloride",4,"Cl-","L117_813Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L118_238","KROMMEDIJKBEEK","Chloride",4,"Cl-","L118_238Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L119_675","KLEIN SCHIJN (ZUIDELIJK DEEL)","Chloride",4,"Cl-","L119_675Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L120_1097","KASSELRIJBEEK - OOST","Chloride",4,"Cl-","L120_1097Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L121_1045","GROTEBEEK - WINTERBEEK","Chloride",4,"Cl-","L121_1045Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L2 Bk","L2 Kleine Beek","Chloride",4,"Cl-","L2 BkCl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["L2 Bk","L2 kleine beek","Chloride",4,"Cl-","L2 BkCl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_102","DEMER V","Chloride",4,"Cl-","VL05_102Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_103","DEMER VI","Chloride",4,"Cl-","VL05_103Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_104","DEMER VII","Chloride",4,"Cl-","VL05_104Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_105","GETE I","Chloride",4,"Cl-","VL05_105Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_106","GETE II","Chloride",4,"Cl-","VL05_106Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_108","HERK + KLEINE HERK","Chloride",4,"Cl-","VL05_108Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,0]
["VL05_110","MANGELBEEK","Chloride",4,"Cl-","VL05_110Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_113","MOMBEEK","Chloride",4,"Cl-","VL05_113Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,0]
["VL05_114","MUNSTERBEEK","Chloride",4,"Cl-","VL05_114Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_115","VELPE","Chloride",4,"Cl-","VL05_115Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,0]
["VL05_116","WINGE","Chloride",4,"Cl-","VL05_116Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,0]
["VL05_118","ZWARTWATER","Chloride",4,"Cl-","VL05_118Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_119","VINNE","Chloride",4,"Cl-","VL05_119Cl-","90 percentiel","mg/L",140,"maximum",210,210,315,450]
["VL05_12","POPERINGEVAART","Chloride",4,"Cl-","VL05_12Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_121","AA II","Chloride",4,"Cl-","VL05_121Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_122","GROTE LAAK","Chloride",4,"Cl-","VL05_122Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_124","GROTE NETE II","Chloride",4,"Cl-","VL05_124Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_130","WAMP","Chloride",4,"Cl-","VL05_130Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_131","WIMP","Chloride",4,"Cl-","VL05_131Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_134","BERWIJN","Chloride",4,"Cl-","VL05_134Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,0]
["VL05_135","BOSBEEK","Chloride",4,"Cl-","VL05_135Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_136","DOMMEL","Chloride",4,"Cl-","VL05_136Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_137","ITTERBEEK I","Chloride",4,"Cl-","VL05_137Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_138","ITTERBEEK II","Chloride",4,"Cl-","VL05_138Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_140","JEKER II","Chloride",4,"Cl-","VL05_140Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_141","LOSSING","Chloride",4,"Cl-","VL05_141Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_146","MERKSKE","Chloride",4,"Cl-","VL05_146Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_148","WEERIJSEBEEK","Chloride",4,"Cl-","VL05_148Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_150","AFLEIDINGSKANAAL van de LEIE/SCHIPDONKKANAAL I","Chloride",4,"Cl-","VL05_150Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_152","AVRIJEVAART + SLEIDINGSVAARDEKE","Chloride",4,"Cl-","VL05_152Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_159","KANAAL CHARLEROI-BRUSSEL","Chloride",4,"Cl-","VL05_159Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_163","KANAAL GENT-OOSTENDE II","Chloride",4,"Cl-","VL05_163Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_166","KANAAL IEPER-IJZER","Chloride",4,"Cl-","VL05_166Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_167","KANAAL LEUVEN-DIJLE","Chloride",4,"Cl-","VL05_167Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_170","KANAAL VAN BEVERLO","Chloride",4,"Cl-","VL05_170Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_171","LEDE","Chloride",4,"Cl-","VL05_171Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_175","MOERVAART","Chloride",4,"Cl-","VL05_175Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_177","NIEUWE KALE","Chloride",4,"Cl-","VL05_177Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_18","KERKEBEEK","Chloride",4,"Cl-","VL05_18Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_180","ZARRENBEEK","Chloride",4,"Cl-","VL05_180Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_182","ZUIDLEDE","Chloride",4,"Cl-","VL05_182Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_191","DESSELSE ZANDPUTTEN","Chloride",4,"Cl-","VL05_191Cl-","90 percentiel","mg/L",140,"maximum",210,210,315,450]
["VL05_192","DONKMEER","Chloride",4,"Cl-","VL05_192Cl-","90 percentiel","mg/L",140,"maximum",210,210,315,450]
["VL05_195","GAVERS HARELBEKE","Chloride",4,"Cl-","VL05_195Cl-","90 percentiel","mg/L",140,"maximum",210,210,315,450]
["VL05_196","GRINDPLAS KESSENICH","Chloride",4,"Cl-","VL05_196Cl-","90 percentiel","mg/L",140,"maximum",210,210,315,450]
["VL05_2","GROTE KEMMELBEEK","Chloride",4,"Cl-","VL05_2Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_20","RIVIERBEEK + HERTSBERGEBEEK","Chloride",4,"Cl-","VL05_20Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,0]
["VL05_200","SCHULENSMEER","Chloride",4,"Cl-",{"$f":"_xlfn.CONCAT(A1347,E1347)","v":"VL05_200Cl-"},"90 percentiel","mg/L",140,"maximum",210,210,315,450]
["VL05_201","SPAANJERD + HEERENLAAK","Chloride",4,"Cl-","VL05_201Cl-","90 percentiel","mg/L",140,"maximum",210,210,315,450]
["VL05_21","ZUIDERVAARTJE","Chloride",4,"Cl-","VL05_21Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_24","MEREBEEK + BORISGRACHT + LIEVE","Chloride",4,"Cl-","VL05_24Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_25","OUDE KALE","Chloride",4,"Cl-","VL05_25Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_28","BENEDENVLIET","Chloride",4,"Cl-","VL05_28Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_3","HANDZAMEVAART","Chloride",4,"Cl-","VL05_3Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_30","GROTE MOLENBEEK - DE VLIET","Chloride",4,"Cl-","VL05_30Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_31","KALKENSE VAART","Chloride",4,"Cl-","VL05_31Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_32","MOLENBEEK - GROTE BEEK","Chloride",4,"Cl-","VL05_32Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_38","ZIELBEEK - BOSBEEK","Chloride",4,"Cl-","VL05_38Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_4","HEIDEBEEK","Chloride",4,"Cl-","VL05_4Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,0]
["VL05_44","DEVEBEEK","Chloride",4,"Cl-","VL05_44Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_45","GAVERBEEK I","Chloride",4,"Cl-","VL05_45Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_46","GAVERBEEK II","Chloride",4,"Cl-","VL05_46Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_5","IEPERLEE + VERWEZEN KANAAL IEPER-KOMEN","Chloride",4,"Cl-","VL05_5Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_50","LEIE III","Chloride",4,"Cl-","VL05_50Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_51","MANDEL I","Chloride",4,"Cl-","VL05_51Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_52","MANDEL II","Chloride",4,"Cl-","VL05_52Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_53","OUDE MANDEL","Chloride",4,"Cl-","VL05_53Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,0]
["VL05_58","BOVEN-SCHELDE IV","Chloride",4,"Cl-","VL05_58Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_61","RONE","Chloride",4,"Cl-","VL05_61Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_62","STAMPKOTBEEK","Chloride",4,"Cl-","VL05_62Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_64","ZWARTE SPIEREBEEK","Chloride",4,"Cl-","VL05_64Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_67","DENDER I","Chloride",4,"Cl-","VL05_67Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_70","DENDER IV","Chloride",4,"Cl-","VL05_70Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_73","MOLENBEEK - PACHTBOSBEEK","Chloride",4,"Cl-","VL05_73Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_75","VONDELBEEK","Chloride",4,"Cl-","VL05_75Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_77","DIJLE I","Chloride",4,"Cl-","VL05_77Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_81","DIJLE V","Chloride",4,"Cl-","VL05_81Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_85","LEIBEEK - LAAKBEEK","Chloride",4,"Cl-","VL05_85Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,0]
["VL05_86","NETHEN","Chloride",4,"Cl-","VL05_86Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,0]
["VL05_87","VOER (Leuven)","Chloride",4,"Cl-","VL05_87Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_89","VUNT","Chloride",4,"Cl-","VL05_89Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_90","WEESBEEK","Chloride",4,"Cl-","VL05_90Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_93","ZENNE II","Chloride",4,"Cl-","VL05_93Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL05_98","DEMER I","Chloride",4,"Cl-","VL05_98Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL05_99","DEMER II","Chloride",4,"Cl-","VL05_99Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL08_125","GROTE NETE III","Chloride",4,"Cl-","VL08_125Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL08_132","GETIJDENETES","Chloride",4,"Cl-","VL08_132Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL08_157","ISABELLAWATERING","Chloride",4,"Cl-","VL08_157Cl-","90 percentiel","mg/L",400,"maximum",600,600,990,1237.5]
["VL08_162","KANAAL GENT-OOSTENDE I + COUPURE + VERBINDINGSKANAAL","Chloride",4,"Cl-","VL08_162Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL08_164","KANAAL GENT-OOSTENDE III","Chloride",4,"Cl-","VL08_164Cl-","90 percentiel","mg/L",800,"maximum",1200,1200,1500,1800]
["VL08_172","LEOPOLDKANAAL I","Chloride",4,"Cl-","VL08_172Cl-","90 percentiel","mg/L",1200,"maximum",1800,1800,2400,3000]
["VL08_173","LEOPOLDKANAAL II","Chloride",4,"Cl-","VL08_173Cl-","90 percentiel","mg/L",1500,"maximum",2250,2250,3000,3750]
["VL08_176","NETEKANAAL","Chloride",4,"Cl-","VL08_176Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL08_178","NOORDELIJKE RINGVAART","Chloride",4,"Cl-","VL08_178Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL08_179","WESTELIJKE RINGVAART","Chloride",4,"Cl-","VL08_179Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL08_39","GETIJDEDURME","Chloride",4,"Cl-","VL08_39Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL08_41","ZEESCHELDE II","Chloride",4,"Cl-","VL08_41Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL08_55","BOVEN-SCHELDE I","Chloride",4,"Cl-","VL08_55Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL08_7","IJZER I","Chloride",4,"Cl-","VL08_7Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL08_71","DENDER V","Chloride",4,"Cl-","VL08_71Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL08_72","MARK (Denderbekken)","Chloride",4,"Cl-","VL08_72Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL08_80","DIJLE IV","Chloride",4,"Cl-","VL08_80Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL08_82","DIJLE VI","Chloride",4,"Cl-","VL08_82Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL08_92","ZENNE I","Chloride",4,"Cl-","VL08_92Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL08_95","GETIJDEDIJLE & GETIJDEZENNE","Chloride",4,"Cl-","VL08_95Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL09_78","DIJLE II","Chloride",4,"Cl-","VL09_78Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL11_10","MARTJEVAART","Chloride",4,"Cl-","VL11_10Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL11_109","KLEINE GETE + VLOEDGRACHT","Chloride",4,"Cl-","VL11_109Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL11_11","MOERDIJKVAART","Chloride",4,"Cl-","VL11_11Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL11_117","ZWARTEBEEK","Chloride",4,"Cl-","VL11_117Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL11_120","AA I","Chloride",4,"Cl-","VL11_120Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL11_123","GROTE NETE I","Chloride",4,"Cl-",{"$f":"_xlfn.CONCAT(A1411,E1411)","v":"VL11_123Cl-"},"90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL11_126","KLEINE NETE I","Chloride",4,"Cl-","VL11_126Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL11_127","KLEINE NETE II","Chloride",4,"Cl-","VL11_127Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL11_128","MOL NEET","Chloride",4,"Cl-","VL11_128Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL11_133","ABEEK","Chloride",4,"Cl-","VL11_133Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL11_145","MARK (Maas)","Chloride",4,"Cl-","VL11_145Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL11_155","BRUGSE REIEN","Chloride",4,"Cl-","VL11_155Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL11_203","MAAS I+II+III","Chloride",4,"Cl-","VL11_203Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL11_205","DEMER III+IV","Chloride",4,"Cl-","VL11_205Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL11_207","MELSTERBEEK I+II","Chloride",4,"Cl-","VL11_207Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL11_40","ZEESCHELDE I","Chloride",4,"Cl-","VL11_40Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL11_59","GROTE SPIEREBEEK","Chloride",4,"Cl-","VL11_59Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL11_63","ZWALM","Chloride",4,"Cl-","VL11_63Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,0]
["VL11_76","BAREBEEK","Chloride",4,"Cl-","VL11_76Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,0]
["VL11_83","IJSSE","Chloride",4,"Cl-","VL11_83Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL11_84","LAAN","Chloride",4,"Cl-","VL11_84Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,0]
["VL11_88","VROUWVLIET","Chloride",4,"Cl-","VL11_88Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL11_91","WOLUWE","Chloride",4,"Cl-","VL11_91Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL17_147","WARMBEEK","Chloride",4,"Cl-","VL17_147Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL17_154","BRAKELEIKEN + LIEVE","Chloride",4,"Cl-","VL17_154Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL17_156","GENTSE BINNENWATEREN","Chloride",4,"Cl-","VL17_156Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL17_161","KANAAL DUINKERKE-NIEUWPOORT","Chloride",4,"Cl-","VL17_161Cl-","90 percentiel","mg/L",3000,"maximum",4500,4500,5625,6750]
["VL17_168","KANAAL PLASSENDALE-NIEUWPOORT","Chloride",4,"Cl-","VL17_168Cl-","90 percentiel","mg/L",800,"maximum",1200,1200,1500,1800]
["VL17_169","KANAAL ROESELARE-LEIE","Chloride",4,"Cl-","VL17_169Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL17_174","LOKANAAL","Chloride",4,"Cl-","VL17_174Cl-","90 percentiel","mg/L",400,"maximum",600,600,990,1237.5]
["VL17_187","ANTWERPSE HAVENDOKKEN + SCHELDE-RIJNVERBINDING","Chloride",4,"Cl-","VL17_187Cl-","90 percentiel","mg/L",6000,"maximum",9000,9000,13500,27000]
["VL17_204","BOVEN-SCHELDE II+III","Chloride",4,"Cl-","VL17_204Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL17_206","DENDER II+III","Chloride",4,"Cl-","VL17_206Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL17_29","GROOT SCHIJN","Chloride",4,"Cl-","VL17_29Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL17_35","VERLEGDE SCHIJN - HOOFDGRACHT","Chloride",4,"Cl-","VL17_35Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL17_48","LEIE I","Chloride",4,"Cl-","VL17_48Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL17_49","LEIE II","Chloride",4,"Cl-","VL17_49Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL17_54","TOERISTISCHE LEIE","Chloride",4,"Cl-","VL17_54Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL17_60","MOLENBEEK - MAARKEBEEK","Chloride",4,"Cl-","VL17_60Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL17_66","BELLEBEEK","Chloride",4,"Cl-","VL17_66Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,0]
["VL17_9","IJZER III","Chloride",4,"Cl-","VL17_9Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL20_36","VERLEGDE SCHIJN - VOORGRACHT","Chloride",4,"Cl-","VL20_36Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL20_96","BEGIJNENBEEK","Chloride",4,"Cl-","VL20_96Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL21_1","BLANKAART WATERLOPEN","Chloride",4,"Cl-","VL21_1Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL21_107","GROTE GETE + BORGGRACHT","Chloride",4,"Cl-","VL21_107Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL21_129","MOLENBEEK - BOLLAAK","Chloride",4,"Cl-","VL21_129Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL21_139","JEKER I","Chloride",4,"Cl-","VL21_139Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,0]
["VL21_26","POEKEBEEK","Chloride",4,"Cl-","VL21_26Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL21_33","MOLENBEEK - KOTTEMBEEK","Chloride",4,"Cl-","VL21_33Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL21_47","HEULEBEEK","Chloride",4,"Cl-","VL21_47Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL21_74","MOLENBEEK - TER ERPENBEEK","Chloride",4,"Cl-","VL21_74Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL21_79","DIJLE III","Chloride",4,"Cl-","VL21_79Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL21_8","IJZER II","Chloride",4,"Cl-","VL21_8Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL21_94","ZUUNBEEK","Chloride",4,"Cl-","VL21_94Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL21_97","DE HULPE - ZWART WATER","Chloride",4,"Cl-","VL21_97Cl-","90 percentiel","mg/L",120,"maximum",180,180,300,375]
["VL22_208","ALBERTKANAAL - Maasbekken","Chloride",4,"Cl-","VL22_208Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL22_209","ALBERTKANAAL - Demerbekken","Chloride",4,"Cl-","VL22_209Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL22_210","ALBERTKANAAL - Netebekken","Chloride",4,"Cl-","VL22_210Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL22_211","ALBERTKANAAL - Benedenscheldebekken","Chloride",4,"Cl-","VL22_211Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL22_212","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Netebekken","Chloride",4,"Cl-","VL22_212Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL22_213","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Maasbekken","Chloride",4,"Cl-","VL22_213Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL22_214","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Benedenscheldebekken","Chloride",4,"Cl-","VL22_214Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL22_215","ZEEKANAAL BRUSSEL-SCHELDE - Dijle-Zennebekken","Chloride",4,"Cl-","VL22_215Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL22_216","ZEEKANAAL BRUSSEL-SCHELDE - Benedenscheldebekken","Chloride",4,"Cl-","VL22_216Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL22_217","AFLEIDINGSKANAAL van de LEIE II + KANAAL van EEKLO - Bekken van de Gentse kanalen","Chloride",4,"Cl-","VL22_217Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL22_218","AFLEIDINGSKANAAL van de LEIE II - Bekken van de Brugse polders","Chloride",4,"Cl-","VL22_218Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL22_219","KANAAL BOSSUIT-KORTRIJK - Bovenscheldebekken","Chloride",4,"Cl-","VL22_219Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL22_220","KANAAL BOSSUIT-KORTRIJK - Leiebekken","Chloride",4,"Cl-","VL22_220Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["VL22_221","ZUID-WILLEMSVAART + KANAAL BOCHOLT-HERENTALS (deels) + KANAAL BRIEGDEN-NEERHAREN","Chloride",4,"Cl-","VL22_221Cl-","90 percentiel","mg/L",200,"maximum",300,300,375,450]
["L107_122","HET GELEED","Chloride",4,"Cl-",{"$f":"_xlfn.CONCAT(A1475,E1475)","v":"L107_122Cl-"},"zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L107_130","KLEINE GEUL","Chloride",4,"Cl-","L107_130Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L107_133","BLANKENBERGSEVAART L1","Chloride",4,"Cl-","L107_133Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L107_143","GROOT ZWIN - NOORDGELEED","Chloride",4,"Cl-","L107_143Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L107_149","PROVINCIEGELEED","Chloride",4,"Cl-","L107_149Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L107_150","GRANINGATEVLIET","Chloride",4,"Cl-","L107_150Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L107_202","OOSTPOLDERKREEK","Chloride",4,"Cl-","L107_202Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L107_213","EEKLOSE WATERGANG","Chloride",4,"Cl-","L107_213Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L107_328","ZUIDELIJKE WATERGANG","Chloride",4,"Cl-","L107_328Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L107_33","BOMMELAREVAART","Chloride",4,"Cl-","L107_33Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L107_333","DOORLOOP","Chloride",4,"Cl-","L107_333Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L107_34","RINGSLOT","Chloride",4,"Cl-","L107_34Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L107_37","LANGGELEED","Chloride",4,"Cl-","L107_37Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L107_56","REYGAERTSVLIET","Chloride",4,"Cl-","L107_56Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L107_60","GROOTGELEED","Chloride",4,"Cl-","L107_60Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L111_1005","KALSIJDEADER","Chloride",4,"Cl-","L111_1005Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L111_1007","STEGERSZWIN","Chloride",4,"Cl-","L111_1007Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L111_1010","OOSTKERKEVAART","Chloride",4,"Cl-","L111_1010Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L111_1011","BOEREKREEK","Chloride",4,"Cl-","L111_1011Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L111_1015","OUDE AVAART","Chloride",4,"Cl-","L111_1015Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L111_1034","NIEUWE GRACHT","Chloride",4,"Cl-","L111_1034Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L111_1048","ZIJDELINGSGELEED","Chloride",4,"Cl-","L111_1048Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L111_1069","AFWATERINGSGRACHT","Chloride",4,"Cl-","L111_1069Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L111_1101","GROTE KEIGNAERT","Chloride",4,"Cl-","L111_1101Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L111_1107","SLIJKVAART","Chloride",4,"Cl-","L111_1107Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L111_1108","STEENGRACHT","Chloride",4,"Cl-","L111_1108Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L111_18","ST-MACHUITSBEEK","Chloride",4,"Cl-","L111_18Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["VL05_14","VLADSLOVAART","Chloride",4,"Cl-","VL05_14Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["VL05_153","BERGENVAART","Chloride",4,"Cl-","VL05_153Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["VL05_17","ISABELLAVAART","Chloride",4,"Cl-","VL05_17Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["VL05_22","ZWINNEVAART","Chloride",4,"Cl-","VL05_22Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["VL05_34","NOORD-ZUIDVERBINDING","Chloride",4,"Cl-","VL05_34Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["VL05_6","IEPERLEED","Chloride",4,"Cl-","VL05_6Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["VL08_16","BLANKENBERGSE VAART + NOORDEDE","Chloride",4,"Cl-","VL08_16Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["VL08_27","ZWARTESLUISBEEK","Chloride",4,"Cl-","VL08_27Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["VL11_13","VEURNE AMBACHT POLDER WATERLOPEN","Chloride",4,"Cl-","VL11_13Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["VL11_19","OOSTENDS KREKENGEBIED","Chloride",4,"Cl-","VL11_19Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["VL11_37","WATERLOOP VAN DE HOGE LANDEN + MELKADER","Chloride",4,"Cl-","VL11_37Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L107_10","KEMMELBEEK","Fosfor, totaal",29,"P t","L107_10P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_104","NEERBEEK","Fosfor, totaal",29,"P t","L107_104P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_105","PALINGBEEK","Fosfor, totaal",29,"P t","L107_105P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_11","WANEBEEK","Fosfor, totaal",29,"P t","L107_11P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_112","LA HAUTE PLANCHE","Fosfor, totaal",29,"P t","L107_112P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_113","DOUVEBEEK","Fosfor, totaal",29,"P t","L107_113P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_116","GROTE SPIERE","Fosfor, totaal",29,"P t","L107_116P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_12","VLETERBEEK","Fosfor, totaal",29,"P t","L107_12P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_120","SCHEEBEEK","Fosfor, totaal",29,"P t","L107_120P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_122","HET GELEED","Fosfor, totaal",29,"P t","L107_122P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_123","KANAAL VAN BRUGGE NAAR SLUIS","Fosfor, totaal",29,"P t","L107_123P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_124","RONSELAREBEEK","Fosfor, totaal",29,"P t","L107_124P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_130","KLEINE GEUL","Fosfor, totaal",29,"P t","L107_130P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_131","LISSEWEEGSEVAART","Fosfor, totaal",29,"P t","L107_131P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_133","BLANKENBERGSEVAART L1","Fosfor, totaal",29,"P t","L107_133P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_135","JABBEEKSE BEEK","Fosfor, totaal",29,"P t","L107_135P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_136","HOGE WATERING","Fosfor, totaal",29,"P t","L107_136P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_140","SCHELLEVLIET","Fosfor, totaal",29,"P t","L107_140P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_143","GROOT ZWIN - NOORDGELEED","Fosfor, totaal",29,"P t","L107_143P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_149","PROVINCIEGELEED","Fosfor, totaal",29,"P t","L107_149P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_150","GRANINGATEVLIET","Fosfor, totaal",29,"P t","L107_150P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_16","HARINGEBEEK","Fosfor, totaal",29,"P t","L107_16P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_202","OOSTPOLDERKREEK","Fosfor, totaal",29,"P t","L107_202P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_209","ZWARTESLUISBEEK L1","Fosfor, totaal",29,"P t","L107_209P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_213","EEKLOSE WATERGANG","Fosfor, totaal",29,"P t","L107_213P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_218","SLEIDINGSVAARDEKEN","Fosfor, totaal",29,"P t","L107_218P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_225","KEUTELBEEK","Fosfor, totaal",29,"P t",{"$f":"_xlfn.CONCAT(A1539,E1539)","v":"L107_225P t"},"zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_234","POEKEBEEK L1","Fosfor, totaal",29,"P t","L107_234P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_235","REIGERBEEK","Fosfor, totaal",29,"P t","L107_235P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_236","NEERSCHUURBEEK","Fosfor, totaal",29,"P t","L107_236P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_237","SPEIBEEK","Fosfor, totaal",29,"P t","L107_237P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_239","OUDE MANDEL L1","Fosfor, totaal",29,"P t","L107_239P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_240","ZOUBEEK","Fosfor, totaal",29,"P t","L107_240P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_241","KATTEBEEK","Fosfor, totaal",29,"P t","L107_241P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_242","DUIVEBEEK","Fosfor, totaal",29,"P t","L107_242P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_246","STAMPKOTBEEK - MOLENBEEK","Fosfor, totaal",29,"P t","L107_246P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_247","STAMPKOTBEEK - WALLEBEEK","Fosfor, totaal",29,"P t","L107_247P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_253","STAMPKOTBEEK - MUNKBOSBEEK","Fosfor, totaal",29,"P t","L107_253P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_254","MOLENBEEK - BEIAARDBEEK","Fosfor, totaal",29,"P t","L107_254P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_266","PEERDESTOKBEEK","Fosfor, totaal",29,"P t","L107_266P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_272","OPHASSELTBEEK","Fosfor, totaal",29,"P t","L107_272P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_273","MOLENBEEK - PACHTBOSBEEK L1","Fosfor, totaal",29,"P t","L107_273P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_274","MOLENBEEK - KALSTERBEEK","Fosfor, totaal",29,"P t","L107_274P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_275","TER ERPENBEEK","Fosfor, totaal",29,"P t","L107_275P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_276","MOLENBEEK - GRAADBEEK","Fosfor, totaal",29,"P t","L107_276P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_277","WILDEBEEK","Fosfor, totaal",29,"P t","L107_277P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_279","MOLENBEEK - VOGELENZANGBEEK","Fosfor, totaal",29,"P t","L107_279P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_282","MOLENBEEK - GONDEBEEK","Fosfor, totaal",29,"P t","L107_282P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_287","MOLENBEEK - GROTE BEEK","Fosfor, totaal",29,"P t","L107_287P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_289","DAMSLOOT","Fosfor, totaal",29,"P t","L107_289P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_296","VOORSTESLOOT","Fosfor, totaal",29,"P t","L107_296P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_299","VONDELBEEK L1","Fosfor, totaal",29,"P t","L107_299P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_3","BROENBEEK","Fosfor, totaal",29,"P t","L107_3P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_305","ZELEBEEK","Fosfor, totaal",29,"P t","L107_305P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_325","GROTE ASTBEEK","Fosfor, totaal",29,"P t","L107_325P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_328","ZUIDELIJKE WATERGANG","Fosfor, totaal",29,"P t","L107_328P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_329","BLOKSTRAATBEEK","Fosfor, totaal",29,"P t","L107_329P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_33","BOMMELAREVAART","Fosfor, totaal",29,"P t","L107_33P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_330","WATERLOOP VAN DE HOGE LANDEN L1","Fosfor, totaal",29,"P t","L107_330P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_333","DOORLOOP","Fosfor, totaal",29,"P t","L107_333P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_335","MOLENBEEK - BEVERBEEK","Fosfor, totaal",29,"P t","L107_335P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_336","DE RIJT","Fosfor, totaal",29,"P t","L107_336P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_34","RINGSLOT","Fosfor, totaal",29,"P t","L107_34P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_37","LANGGELEED","Fosfor, totaal",29,"P t","L107_37P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_4","KORVERSBEEK","Fosfor, totaal",29,"P t","L107_4P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_40","STENENSLUISVAART","Fosfor, totaal",29,"P t","L107_40P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_403","MOLENBEEK - NEERPEDEBEEK","Fosfor, totaal",29,"P t","L107_403P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_404","LOTBEEK","Fosfor, totaal",29,"P t","L107_404P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_407","GROEBENGRACHT","Fosfor, totaal",29,"P t","L107_407P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_409","KLEINE MAALBEEK","Fosfor, totaal",29,"P t","L107_409P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_411","MOLENBEEK - PARKBEEK","Fosfor, totaal",29,"P t","L107_411P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_413","TANGEBEEK","Fosfor, totaal",29,"P t","L107_413P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_417","DE GROTE LAAK","Fosfor, totaal",29,"P t","L107_417P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_418","MENE","Fosfor, totaal",29,"P t","L107_418P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_421","GENOVEVABEEK","Fosfor, totaal",29,"P t","L107_421P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_422","'S HERTOGENGRACHT","Fosfor, totaal",29,"P t","L107_422P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_423","BEGIJNEBEEK L1","Fosfor, totaal",29,"P t","L107_423P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_424","VIJVERSLOOP","Fosfor, totaal",29,"P t","L107_424P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_431","ST-ODULPHUSBEEK","Fosfor, totaal",29,"P t","L107_431P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_432","DORMAALBEEK","Fosfor, totaal",29,"P t","L107_432P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_433","BEVERBEEK","Fosfor, totaal",29,"P t","L107_433P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_434","SCHEIBEEK","Fosfor, totaal",29,"P t","L107_434P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_435","AREBEEK","Fosfor, totaal",29,"P t","L107_435P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_439","IJSE L1","Fosfor, totaal",29,"P t","L107_439P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_441","LANGEGRACHT","Fosfor, totaal",29,"P t","L107_441P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_449","VOER (BERTEM)","Fosfor, totaal",29,"P t","L107_449P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_451","GROTE LAAK - GROTE LOOP - MESTENLOOP","Fosfor, totaal",29,"P t","L107_451P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_452","LAARBEEK","Fosfor, totaal",29,"P t","L107_452P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_453","ZWARTEBEEK (SCHERPENHEUVEL-ZICHEM)","Fosfor, totaal",29,"P t","L107_453P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_454","KLEINEBEEK - RIJSELSESTRAATVLIET","Fosfor, totaal",29,"P t","L107_454P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_462","LEMINGSBEEK","Fosfor, totaal",29,"P t",{"$f":"_xlfn.CONCAT(A1603,E1603)","v":"L107_462P t"},"zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_463","AABEEK (MECHELEN)","Fosfor, totaal",29,"P t","L107_463P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_464","LEYBEEK","Fosfor, totaal",29,"P t","L107_464P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_47","ZARRENBEEK L1","Fosfor, totaal",29,"P t","L107_47P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_48","KANAAL VAN ESEN","Fosfor, totaal",29,"P t","L107_48P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_5","BOLLAERTBEEK","Fosfor, totaal",29,"P t","L107_5P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_56","REYGAERTSVLIET","Fosfor, totaal",29,"P t","L107_56P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_6","DIKKEBUSBEEK","Fosfor, totaal",29,"P t","L107_6P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_60","GROOTGELEED","Fosfor, totaal",29,"P t","L107_60P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_600","LEYLOOP","Fosfor, totaal",29,"P t","L107_600P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_601","DE AA (RAVELS)","Fosfor, totaal",29,"P t","L107_601P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_602","BLAUWPUTTEN EN LEILOOP","Fosfor, totaal",29,"P t","L107_602P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_603","HEERLESE LOOP","Fosfor, totaal",29,"P t","L107_603P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_607","MERKSKE L1","Fosfor, totaal",29,"P t","L107_607P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_609","KLEINE MARK","Fosfor, totaal",29,"P t","L107_609P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_61","VAARTDIJKGELEED","Fosfor, totaal",29,"P t","L107_61P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_610","MARK L1","Fosfor, totaal",29,"P t","L107_610P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_613","SLUISKENSVIJVER","Fosfor, totaal",29,"P t","L107_613P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_614","WEERIJSEBEEK L1","Fosfor, totaal",29,"P t","L107_614P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_615","KLEINE BEEK (WUUSTWEZEL)","Fosfor, totaal",29,"P t","L107_615P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_629","KLEIN WILBOEREBEEK","Fosfor, totaal",29,"P t","L107_629P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_63","BOERGONJEVAART","Fosfor, totaal",29,"P t","L107_63P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_631","MOLENBEEK - BOLLAAK L1","Fosfor, totaal",29,"P t","L107_631P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_632","DE DELFTE BEEK","Fosfor, totaal",29,"P t","L107_632P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_633","BOSBEEK - DIEPTELOOP","Fosfor, totaal",29,"P t","L107_633P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_638","GROTE CALIE","Fosfor, totaal",29,"P t","L107_638P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_640","DE AA - NATTENLOOP","Fosfor, totaal",29,"P t","L107_640P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_644","ITTERBEEK (DUFFEL)","Fosfor, totaal",29,"P t","L107_644P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_648","BRUINBEEK","Fosfor, totaal",29,"P t","L107_648P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_650","REEHAGENBEEK","Fosfor, totaal",29,"P t","L107_650P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_654","LARUMSE LOOP","Fosfor, totaal",29,"P t","L107_654P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_655","DALEMANSLOOP","Fosfor, totaal",29,"P t","L107_655P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_656","BEGGELBEEK","Fosfor, totaal",29,"P t","L107_656P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_66","KERKBEEK","Fosfor, totaal",29,"P t","L107_66P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_664","MOLENBEEK - ZIJP","Fosfor, totaal",29,"P t","L107_664P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_665","BOUWBEEK","Fosfor, totaal",29,"P t","L107_665P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_67","LIJSTERBEEK","Fosfor, totaal",29,"P t","L107_67P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_677","DIEPE BEEK","Fosfor, totaal",29,"P t","L107_677P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_681","KOUDE BEEK","Fosfor, totaal",29,"P t","L107_681P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_684","SCHOON SCHIJN","Fosfor, totaal",29,"P t","L107_684P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_688","LAARSE BEEK","Fosfor, totaal",29,"P t","L107_688P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_695","VARENDONKSE BEEK","Fosfor, totaal",29,"P t","L107_695P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_702","MILLEGEMLOOP","Fosfor, totaal",29,"P t","L107_702P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_705","SCHEPPELIJKE NETE","Fosfor, totaal",29,"P t","L107_705P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_706","MOLSE NETE L1","Fosfor, totaal",29,"P t","L107_706P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_708","GROTE NETE L1","Fosfor, totaal",29,"P t","L107_708P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_722","WAMP L1","Fosfor, totaal",29,"P t","L107_722P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_723","RODE LOOP","Fosfor, totaal",29,"P t","L107_723P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_729","STAPKENSLOOP","Fosfor, totaal",29,"P t","L107_729P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_735","GESTELBEEK","Fosfor, totaal",29,"P t","L107_735P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_740","BERGEBEEK","Fosfor, totaal",29,"P t","L107_740P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_741","SPILLEBEEK","Fosfor, totaal",29,"P t","L107_741P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_742","PLATTE BEEK","Fosfor, totaal",29,"P t","L107_742P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_78","DEVEBEEK L1","Fosfor, totaal",29,"P t","L107_78P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_8","IEPERLEE","Fosfor, totaal",29,"P t","L107_8P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_809","KLEINE HERK L1","Fosfor, totaal",29,"P t","L107_809P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_810","WINTERBEEK (KORTESSEM)","Fosfor, totaal",29,"P t","L107_810P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_812","MOMBEEK L1","Fosfor, totaal",29,"P t","L107_812P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_814","STEENLAAK","Fosfor, totaal",29,"P t","L107_814P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_82","BABILLEBEEK","Fosfor, totaal",29,"P t","L107_82P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_824","ROELBEEK","Fosfor, totaal",29,"P t","L107_824P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_83","ROOBEEK","Fosfor, totaal",29,"P t","L107_83P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_836","LAAMBEEK","Fosfor, totaal",29,"P t","L107_836P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_839","ZONDERIKBEEK","Fosfor, totaal",29,"P t","L107_839P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_84","KROMMEBEEK","Fosfor, totaal",29,"P t",{"$f":"_xlfn.CONCAT(A1667,E1667)","v":"L107_84P t"},"zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_846","KAATSBEEK","Fosfor, totaal",29,"P t","L107_846P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_847","WINTERBEEK (BILZEN)","Fosfor, totaal",29,"P t","L107_847P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_848","DEMER L1","Fosfor, totaal",29,"P t","L107_848P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_852","MUNSTERBEEK L1","Fosfor, totaal",29,"P t","L107_852P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_853","ZUTENDAALBEEK","Fosfor, totaal",29,"P t","L107_853P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_854","BOLLISENBEEK","Fosfor, totaal",29,"P t","L107_854P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_855","DOMMEL L1","Fosfor, totaal",29,"P t","L107_855P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_856","HOLVENLOOP","Fosfor, totaal",29,"P t","L107_856P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_857","EINDERGATLOOP","Fosfor, totaal",29,"P t","L107_857P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_858","WARMBEEK L1","Fosfor, totaal",29,"P t","L107_858P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_859","PRINSENLOOP","Fosfor, totaal",29,"P t","L107_859P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_861","ABEEK L1","Fosfor, totaal",29,"P t","L107_861P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_866","LOSSING L1","Fosfor, totaal",29,"P t","L107_866P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_869","SOERBEEK","Fosfor, totaal",29,"P t","L107_869P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_876","BOSBEEK L1","Fosfor, totaal",29,"P t","L107_876P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_879","VRIETSELBEEK - OUDE MAAS (DILSEN)","Fosfor, totaal",29,"P t","L107_879P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_883","ZIEPBEEK","Fosfor, totaal",29,"P t","L107_883P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_885","HEESWATER","Fosfor, totaal",29,"P t","L107_885P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_890","BEEK - DE BUTH (TONGEREN)","Fosfor, totaal",29,"P t","L107_890P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_891","VOER (VOEREN)","Fosfor, totaal",29,"P t","L107_891P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_892","BEEK (VOEREN)","Fosfor, totaal",29,"P t","L107_892P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_893","GULP","Fosfor, totaal",29,"P t","L107_893P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_91","PLAATSBEEK","Fosfor, totaal",29,"P t","L107_91P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_92","MAALBEEK (LEIEBEKKEN)","Fosfor, totaal",29,"P t","L107_92P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_97","KASSELRIJBEEK - WEST","Fosfor, totaal",29,"P t","L107_97P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_98","GAVERBEEK","Fosfor, totaal",29,"P t","L107_98P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L110_1100","ZILVERBEEK","Fosfor, totaal",29,"P t","L110_1100P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1001","MARTJEVAART - LEKKERBOTERBEEK","Fosfor, totaal",29,"P t","L111_1001P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1003","GELUWEBEEK","Fosfor, totaal",29,"P t","L111_1003P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1004","RIJTGRACHT","Fosfor, totaal",29,"P t","L111_1004P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1005","KALSIJDEADER","Fosfor, totaal",29,"P t","L111_1005P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1006","HOOFDSLOOT","Fosfor, totaal",29,"P t","L111_1006P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1007","STEGERSZWIN","Fosfor, totaal",29,"P t","L111_1007P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1010","OOSTKERKEVAART","Fosfor, totaal",29,"P t","L111_1010P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1011","BOEREKREEK","Fosfor, totaal",29,"P t","L111_1011P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1014","MEREBEEK","Fosfor, totaal",29,"P t","L111_1014P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1015","OUDE AVAART","Fosfor, totaal",29,"P t","L111_1015P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1016","WANTEBEEK","Fosfor, totaal",29,"P t","L111_1016P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1018","LEEBEEK","Fosfor, totaal",29,"P t","L111_1018P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1019","MOLENBEEK - MARKEBEEK","Fosfor, totaal",29,"P t","L111_1019P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1020","OOSSEBEEK","Fosfor, totaal",29,"P t","L111_1020P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1021","ZWALMBEEK","Fosfor, totaal",29,"P t","L111_1021P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1022","MOLENBEEK (RONSE)","Fosfor, totaal",29,"P t","L111_1022P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1024","BAVEGEMSE BEEK","Fosfor, totaal",29,"P t","L111_1024P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1025","MAANBEEK","Fosfor, totaal",29,"P t","L111_1025P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1027","GROOTEBEEK","Fosfor, totaal",29,"P t","L111_1027P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1028","LANGELEDE","Fosfor, totaal",29,"P t","L111_1028P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1029","KLEINE WATERGANG","Fosfor, totaal",29,"P t","L111_1029P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1030","WATERGANG VAN DE MOERBEKEPOLDER","Fosfor, totaal",29,"P t","L111_1030P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1031","KANAAL VAN STEKENE","Fosfor, totaal",29,"P t","L111_1031P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1032","DIJKGRACHT","Fosfor, totaal",29,"P t","L111_1032P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1033","PAPENMEERSBEEK","Fosfor, totaal",29,"P t","L111_1033P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1034","NIEUWE GRACHT","Fosfor, totaal",29,"P t","L111_1034P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1035","KOEVAARDEKEN","Fosfor, totaal",29,"P t","L111_1035P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1037","MOLENBEEK - LAKEBEEK","Fosfor, totaal",29,"P t","L111_1037P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1038","MAALBEEK - AMELVONNEBEEK","Fosfor, totaal",29,"P t","L111_1038P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1039","STEENVOORDBEEK (TERNAT)","Fosfor, totaal",29,"P t","L111_1039P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1040","BELLEBEEK L1","Fosfor, totaal",29,"P t","L111_1040P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1041","WINGE L1","Fosfor, totaal",29,"P t","L111_1041P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1042","LEIBEEK - LIPSEBEEK L1","Fosfor, totaal",29,"P t","L111_1042P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1043","WEESBEEK L1","Fosfor, totaal",29,"P t","L111_1043P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1044","KASTEELBEEK","Fosfor, totaal",29,"P t","L111_1044P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1046","GROTE MOTTE","Fosfor, totaal",29,"P t","L111_1046P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1047","BAREBEEK L1","Fosfor, totaal",29,"P t",{"$f":"_xlfn.CONCAT(A1731,E1731)","v":"L111_1047P t"},"zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1048","ZIJDELINGSGELEED","Fosfor, totaal",29,"P t","L111_1048P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1049","MUNTLOOP","Fosfor, totaal",29,"P t","L111_1049P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1050","WEHAGENBEEK","Fosfor, totaal",29,"P t","L111_1050P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1052","LAAKBEEK","Fosfor, totaal",29,"P t","L111_1052P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1053","MOUBEEK","Fosfor, totaal",29,"P t","L111_1053P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1054","GOORBOSBEEK","Fosfor, totaal",29,"P t","L111_1054P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1056","VROUWVLIET L1","Fosfor, totaal",29,"P t","L111_1056P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1057","GROTE MOLENBEEK L1","Fosfor, totaal",29,"P t","L111_1057P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1058","ZWARTE BEEK (WILLEBROEK)","Fosfor, totaal",29,"P t","L111_1058P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1059","ZIELBEEK - BOSBEEK L1","Fosfor, totaal",29,"P t","L111_1059P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1060","GROOT SCHIJN L1","Fosfor, totaal",29,"P t","L111_1060P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1062","HERSELTSELOOP","Fosfor, totaal",29,"P t","L111_1062P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1063","STEENKENSBEEK","Fosfor, totaal",29,"P t","L111_1063P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1064","ST. TRUDOLEKEN","Fosfor, totaal",29,"P t","L111_1064P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1065","ASBEEK","Fosfor, totaal",29,"P t","L111_1065P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1066","LOEIJENS NEETJE","Fosfor, totaal",29,"P t","L111_1066P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1067","KLEINE NETE L1","Fosfor, totaal",29,"P t","L111_1067P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1069","AFWATERINGSGRACHT","Fosfor, totaal",29,"P t","L111_1069P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1070","WIMP L1","Fosfor, totaal",29,"P t","L111_1070P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1071","GOORLOOP","Fosfor, totaal",29,"P t","L111_1071P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1072","POVERSBEEK","Fosfor, totaal",29,"P t","L111_1072P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1075","MELSTERBEEK L1","Fosfor, totaal",29,"P t","L111_1075P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1076","CICINDRIA","Fosfor, totaal",29,"P t","L111_1076P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1077","MOLENBEEK (SINT-TRUIDEN)","Fosfor, totaal",29,"P t","L111_1077P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1078","GRONDBEEK","Fosfor, totaal",29,"P t","L111_1078P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1079","HELDERBEEK","Fosfor, totaal",29,"P t","L111_1079P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1080","ZWARTEBEEK L1","Fosfor, totaal",29,"P t","L111_1080P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1081","MANGELBEEK L1","Fosfor, totaal",29,"P t","L111_1081P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1082","SLANGBEEK","Fosfor, totaal",29,"P t","L111_1082P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1083","MISERIKBEEK","Fosfor, totaal",29,"P t","L111_1083P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1084","MANDEL L1","Fosfor, totaal",29,"P t","L111_1084P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1086","LOZERBROEKBEEK","Fosfor, totaal",29,"P t","L111_1086P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1087","HORSTGATERBEEK","Fosfor, totaal",29,"P t","L111_1087P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1088","ITTERBEEK L1","Fosfor, totaal",29,"P t","L111_1088P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1089","WITBEEK","Fosfor, totaal",29,"P t","L111_1089P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1090","ZANDERBEEK","Fosfor, totaal",29,"P t","L111_1090P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1091","KIKBEEK","Fosfor, totaal",29,"P t","L111_1091P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1092","ZOUW","Fosfor, totaal",29,"P t","L111_1092P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1093","EZELSBEEK","Fosfor, totaal",29,"P t","L111_1093P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1094","HEULEBEEK L1","Fosfor, totaal",29,"P t","L111_1094P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1095","KLEINE LAAK","Fosfor, totaal",29,"P t","L111_1095P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1096","GROTE LAAK L1","Fosfor, totaal",29,"P t","L111_1096P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1098","KEIBEEK","Fosfor, totaal",29,"P t","L111_1098P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1099","GAVERSE BEEK (BECQUE DE NEUVILLE)","Fosfor, totaal",29,"P t","L111_1099P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1101","GROTE KEIGNAERT","Fosfor, totaal",29,"P t","L111_1101P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1102","KLEINE A - WILDERTSE BEEK","Fosfor, totaal",29,"P t","L111_1102P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1104","DESPIERREBEEK","Fosfor, totaal",29,"P t","L111_1104P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1105","MELSENBEEK","Fosfor, totaal",29,"P t","L111_1105P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1106","DONKSE BEEK","Fosfor, totaal",29,"P t","L111_1106P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1107","SLIJKVAART","Fosfor, totaal",29,"P t","L111_1107P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1108","STEENGRACHT","Fosfor, totaal",29,"P t","L111_1108P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1109","MOERDIJKVAART L1","Fosfor, totaal",29,"P t","L111_1109P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1110","EDE","Fosfor, totaal",29,"P t","L111_1110P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1111","GELEEDBEEK - PASSENDALEGELEED","Fosfor, totaal",29,"P t","L111_1111P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1112","ISABELLASTROOM","Fosfor, totaal",29,"P t","L111_1112P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1113","LACHENEBEEK","Fosfor, totaal",29,"P t","L111_1113P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1114","ANTITANKGRACHT ZUID","Fosfor, totaal",29,"P t","L111_1114P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_1201","S HERTOGENDIJKSE BEEK","Fosfor, totaal",29,"P t","L111_1201P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_15","HEIDEBEEK (VLETEREN)","Fosfor, totaal",29,"P t","L111_15P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_18","ST-MACHUITSBEEK","Fosfor, totaal",29,"P t","L111_18P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_298","OUDE DENDER","Fosfor, totaal",29,"P t","L111_298P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_315","FONDATIEGRACHT","Fosfor, totaal",29,"P t","L111_315P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_326","BARBIERBEEK","Fosfor, totaal",29,"P t","L111_326P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_419","SCHOORBROEKBEEK","Fosfor, totaal",29,"P t",{"$f":"_xlfn.CONCAT(A1795,E1795)","v":"L111_419P t"},"zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_436","VELPE L1","Fosfor, totaal",29,"P t","L111_436P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_624","TAPPELBEEK","Fosfor, totaal",29,"P t","L111_624P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_627","KLEINE BEEK (ZANDHOVEN)","Fosfor, totaal",29,"P t","L111_627P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_639","VISBEEK","Fosfor, totaal",29,"P t","L111_639P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_674","BENEDENVLIET L1","Fosfor, totaal",29,"P t","L111_674P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_676","WEZELSE BEEK","Fosfor, totaal",29,"P t","L111_676P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_699","SCHERPENBERGLOOP","Fosfor, totaal",29,"P t","L111_699P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_707","KLEINE HOOFDGRACHT","Fosfor, totaal",29,"P t","L111_707P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_717","DESSELSE NEET","Fosfor, totaal",29,"P t","L111_717P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_724","ANTITANKGRACHT NOORD","Fosfor, totaal",29,"P t","L111_724P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L111_844","STIEMER","Fosfor, totaal",29,"P t","L111_844P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L117_1036","ZUUNBEEK L1","Fosfor, totaal",29,"P t","L117_1036P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L117_1068","HERTSBERGEBEEK - GETEBEEK","Fosfor, totaal",29,"P t","L117_1068P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L117_1073","RIVIERBEEK","Fosfor, totaal",29,"P t","L117_1073P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L117_1074","HERK L1","Fosfor, totaal",29,"P t","L117_1074P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L117_1085","WILDERBEEK","Fosfor, totaal",29,"P t","L117_1085P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L117_17","STEENVOORDEBEEK (WATOU)","Fosfor, totaal",29,"P t","L117_17P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L117_219","BURGGRAVENSTROOM","Fosfor, totaal",29,"P t","L117_219P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L117_232","JOBEEK","Fosfor, totaal",29,"P t","L117_232P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L117_233","RINGBEEK","Fosfor, totaal",29,"P t","L117_233P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L117_402","MOLENBEEK - SLAGVIJVERBEEK","Fosfor, totaal",29,"P t","L117_402P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L117_659","KREKELBEEK","Fosfor, totaal",29,"P t","L117_659P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L117_673","KLEIN SCHIJN (NOORDELIJK DEEL)","Fosfor, totaal",29,"P t","L117_673P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L117_813","HERKEBEEK","Fosfor, totaal",29,"P t","L117_813P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L118_238","KROMMEDIJKBEEK","Fosfor, totaal",29,"P t","L118_238P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L119_675","KLEIN SCHIJN (ZUIDELIJK DEEL)","Fosfor, totaal",29,"P t","L119_675P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L120_1097","KASSELRIJBEEK - OOST","Fosfor, totaal",29,"P t","L120_1097P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L121_1045","GROTEBEEK - WINTERBEEK","Fosfor, totaal",29,"P t","L121_1045P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L2 Bk","L2 Kleine Beek","Fosfor, totaal",29,"P t","L2 BkP t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L2 Bk","L2 kleine beek","Fosfor, totaal",29,"P t","L2 BkP t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_102","DEMER V","Fosfor, totaal",29,"P t","VL05_102P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_103","DEMER VI","Fosfor, totaal",29,"P t","VL05_103P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_104","DEMER VII","Fosfor, totaal",29,"P t","VL05_104P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_105","GETE I","Fosfor, totaal",29,"P t","VL05_105P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_106","GETE II","Fosfor, totaal",29,"P t","VL05_106P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_108","HERK + KLEINE HERK","Fosfor, totaal",29,"P t","VL05_108P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_110","MANGELBEEK","Fosfor, totaal",29,"P t","VL05_110P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_113","MOMBEEK","Fosfor, totaal",29,"P t","VL05_113P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_114","MUNSTERBEEK","Fosfor, totaal",29,"P t","VL05_114P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_115","VELPE","Fosfor, totaal",29,"P t","VL05_115P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_116","WINGE","Fosfor, totaal",29,"P t","VL05_116P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_118","ZWARTWATER","Fosfor, totaal",29,"P t","VL05_118P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_119","VINNE","Fosfor, totaal",29,"P t","VL05_119P t","zomergemiddelde (apr-sept)","mgP/L",7.0000000000000007E-2,"jaargemiddelde",7.0000000000000007E-2,7.0000000000000007E-2,0.14000000000000001,0.28000000000000003]
["VL05_12","POPERINGEVAART","Fosfor, totaal",29,"P t","VL05_12P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_121","AA II","Fosfor, totaal",29,"P t","VL05_121P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_122","GROTE LAAK","Fosfor, totaal",29,"P t","VL05_122P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_124","GROTE NETE II","Fosfor, totaal",29,"P t","VL05_124P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_130","WAMP","Fosfor, totaal",29,"P t","VL05_130P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_131","WIMP","Fosfor, totaal",29,"P t","VL05_131P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_134","BERWIJN","Fosfor, totaal",29,"P t","VL05_134P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_135","BOSBEEK","Fosfor, totaal",29,"P t","VL05_135P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_136","DOMMEL","Fosfor, totaal",29,"P t","VL05_136P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_137","ITTERBEEK I","Fosfor, totaal",29,"P t","VL05_137P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_138","ITTERBEEK II","Fosfor, totaal",29,"P t","VL05_138P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_14","VLADSLOVAART","Fosfor, totaal",29,"P t","VL05_14P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_140","JEKER II","Fosfor, totaal",29,"P t","VL05_140P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_141","LOSSING","Fosfor, totaal",29,"P t","VL05_141P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_146","MERKSKE","Fosfor, totaal",29,"P t","VL05_146P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_148","WEERIJSEBEEK","Fosfor, totaal",29,"P t","VL05_148P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_150","AFLEIDINGSKANAAL van de LEIE/SCHIPDONKKANAAL I","Fosfor, totaal",29,"P t","VL05_150P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_152","AVRIJEVAART + SLEIDINGSVAARDEKE","Fosfor, totaal",29,"P t","VL05_152P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_153","BERGENVAART","Fosfor, totaal",29,"P t","VL05_153P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_159","KANAAL CHARLEROI-BRUSSEL","Fosfor, totaal",29,"P t","VL05_159P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_163","KANAAL GENT-OOSTENDE II","Fosfor, totaal",29,"P t",{"$f":"_xlfn.CONCAT(A1859,E1859)","v":"VL05_163P t"},"zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_166","KANAAL IEPER-IJZER","Fosfor, totaal",29,"P t","VL05_166P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_167","KANAAL LEUVEN-DIJLE","Fosfor, totaal",29,"P t","VL05_167P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_17","ISABELLAVAART","Fosfor, totaal",29,"P t","VL05_17P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_170","KANAAL VAN BEVERLO","Fosfor, totaal",29,"P t","VL05_170P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_171","LEDE","Fosfor, totaal",29,"P t","VL05_171P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_175","MOERVAART","Fosfor, totaal",29,"P t","VL05_175P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_177","NIEUWE KALE","Fosfor, totaal",29,"P t","VL05_177P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_18","KERKEBEEK","Fosfor, totaal",29,"P t","VL05_18P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_180","ZARRENBEEK","Fosfor, totaal",29,"P t","VL05_180P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_182","ZUIDLEDE","Fosfor, totaal",29,"P t","VL05_182P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_191","DESSELSE ZANDPUTTEN","Fosfor, totaal",29,"P t","VL05_191P t","zomergemiddelde (apr-sept)","mgP/L",0.04,"jaargemiddelde",0.04,0.04,0.06,0.13]
["VL05_192","DONKMEER","Fosfor, totaal",29,"P t","VL05_192P t","zomergemiddelde (apr-sept)","mgP/L",7.0000000000000007E-2,"jaargemiddelde",7.0000000000000007E-2,7.0000000000000007E-2,0.14000000000000001,0.28000000000000003]
["VL05_195","GAVERS HARELBEKE","Fosfor, totaal",29,"P t","VL05_195P t","zomergemiddelde (apr-sept)","mgP/L",5.5E-2,"jaargemiddelde",5.5E-2,5.5E-2,0.14000000000000001,0.28000000000000003]
["VL05_196","GRINDPLAS KESSENICH","Fosfor, totaal",29,"P t","VL05_196P t","zomergemiddelde (apr-sept)","mgP/L",5.5E-2,"jaargemiddelde",5.5E-2,5.5E-2,0.14000000000000001,0.28000000000000003]
["VL05_2","GROTE KEMMELBEEK","Fosfor, totaal",29,"P t","VL05_2P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_20","RIVIERBEEK + HERTSBERGEBEEK","Fosfor, totaal",29,"P t","VL05_20P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_200","SCHULENSMEER","Fosfor, totaal",29,"P t","VL05_200P t","zomergemiddelde (apr-sept)","mgP/L",5.5E-2,"jaargemiddelde",5.5E-2,5.5E-2,0.14000000000000001,0.28000000000000003]
["VL05_201","SPAANJERD + HEERENLAAK","Fosfor, totaal",29,"P t","VL05_201P t","zomergemiddelde (apr-sept)","mgP/L",5.5E-2,"jaargemiddelde",5.5E-2,5.5E-2,0.14000000000000001,0.28000000000000003]
["VL05_202","SPUIKOM OOSTENDE","Fosfor, totaal",29,"P t","VL05_202P t","zomergemiddelde (apr-sept)","mgP/L",0.11,"jaargemiddelde",0.11,0.11,0.22,0.33]
["VL05_21","ZUIDERVAARTJE","Fosfor, totaal",29,"P t","VL05_21P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_22","ZWINNEVAART","Fosfor, totaal",29,"P t","VL05_22P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_24","MEREBEEK + BORISGRACHT + LIEVE","Fosfor, totaal",29,"P t","VL05_24P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_25","OUDE KALE","Fosfor, totaal",29,"P t","VL05_25P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_28","BENEDENVLIET","Fosfor, totaal",29,"P t","VL05_28P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_3","HANDZAMEVAART","Fosfor, totaal",29,"P t","VL05_3P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_30","GROTE MOLENBEEK - DE VLIET","Fosfor, totaal",29,"P t","VL05_30P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_31","KALKENSE VAART","Fosfor, totaal",29,"P t","VL05_31P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_32","MOLENBEEK - GROTE BEEK","Fosfor, totaal",29,"P t","VL05_32P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_34","NOORD-ZUIDVERBINDING","Fosfor, totaal",29,"P t","VL05_34P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_38","ZIELBEEK - BOSBEEK","Fosfor, totaal",29,"P t","VL05_38P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_4","HEIDEBEEK","Fosfor, totaal",29,"P t","VL05_4P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_44","DEVEBEEK","Fosfor, totaal",29,"P t","VL05_44P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_45","GAVERBEEK I","Fosfor, totaal",29,"P t","VL05_45P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_46","GAVERBEEK II","Fosfor, totaal",29,"P t","VL05_46P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_5","IEPERLEE + VERWEZEN KANAAL IEPER-KOMEN","Fosfor, totaal",29,"P t","VL05_5P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_50","LEIE III","Fosfor, totaal",29,"P t","VL05_50P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_51","MANDEL I","Fosfor, totaal",29,"P t","VL05_51P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_52","MANDEL II","Fosfor, totaal",29,"P t","VL05_52P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_53","OUDE MANDEL","Fosfor, totaal",29,"P t","VL05_53P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_58","BOVEN-SCHELDE IV","Fosfor, totaal",29,"P t","VL05_58P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_6","IEPERLEED","Fosfor, totaal",29,"P t","VL05_6P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_61","RONE","Fosfor, totaal",29,"P t","VL05_61P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_62","STAMPKOTBEEK","Fosfor, totaal",29,"P t","VL05_62P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_64","ZWARTE SPIEREBEEK","Fosfor, totaal",29,"P t","VL05_64P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_67","DENDER I","Fosfor, totaal",29,"P t","VL05_67P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_70","DENDER IV","Fosfor, totaal",29,"P t","VL05_70P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_73","MOLENBEEK - PACHTBOSBEEK","Fosfor, totaal",29,"P t","VL05_73P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_75","VONDELBEEK","Fosfor, totaal",29,"P t","VL05_75P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_77","DIJLE I","Fosfor, totaal",29,"P t","VL05_77P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_81","DIJLE V","Fosfor, totaal",29,"P t","VL05_81P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_85","LEIBEEK - LAAKBEEK","Fosfor, totaal",29,"P t","VL05_85P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_86","NETHEN","Fosfor, totaal",29,"P t","VL05_86P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_87","VOER (Leuven)","Fosfor, totaal",29,"P t","VL05_87P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_89","VUNT","Fosfor, totaal",29,"P t","VL05_89P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_90","WEESBEEK","Fosfor, totaal",29,"P t","VL05_90P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_93","ZENNE II","Fosfor, totaal",29,"P t","VL05_93P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_98","DEMER I","Fosfor, totaal",29,"P t","VL05_98P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL05_99","DEMER II","Fosfor, totaal",29,"P t","VL05_99P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_125","GROTE NETE III","Fosfor, totaal",29,"P t","VL08_125P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_132","GETIJDENETES","Fosfor, totaal",29,"P t","VL08_132P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.19,0.42]
["VL08_157","ISABELLAWATERING","Fosfor, totaal",29,"P t","VL08_157P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_16","BLANKENBERGSE VAART + NOORDEDE","Fosfor, totaal",29,"P t","VL08_16P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_162","KANAAL GENT-OOSTENDE I + COUPURE + VERBINDINGSKANAAL","Fosfor, totaal",29,"P t","VL08_162P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_164","KANAAL GENT-OOSTENDE III","Fosfor, totaal",29,"P t",{"$f":"_xlfn.CONCAT(A1923,E1923)","v":"VL08_164P t"},"zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_172","LEOPOLDKANAAL I","Fosfor, totaal",29,"P t","VL08_172P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_173","LEOPOLDKANAAL II","Fosfor, totaal",29,"P t","VL08_173P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_176","NETEKANAAL","Fosfor, totaal",29,"P t","VL08_176P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_178","NOORDELIJKE RINGVAART","Fosfor, totaal",29,"P t","VL08_178P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_179","WESTELIJKE RINGVAART","Fosfor, totaal",29,"P t","VL08_179P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_27","ZWARTESLUISBEEK","Fosfor, totaal",29,"P t","VL08_27P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_39","GETIJDEDURME","Fosfor, totaal",29,"P t","VL08_39P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.19,0.42]
["VL08_41","ZEESCHELDE II","Fosfor, totaal",29,"P t","VL08_41P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.19,0.42]
["VL08_55","BOVEN-SCHELDE I","Fosfor, totaal",29,"P t","VL08_55P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_7","IJZER I","Fosfor, totaal",29,"P t","VL08_7P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_71","DENDER V","Fosfor, totaal",29,"P t","VL08_71P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_72","MARK (Denderbekken)","Fosfor, totaal",29,"P t","VL08_72P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_80","DIJLE IV","Fosfor, totaal",29,"P t","VL08_80P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_82","DIJLE VI","Fosfor, totaal",29,"P t","VL08_82P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_92","ZENNE I","Fosfor, totaal",29,"P t","VL08_92P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL08_95","GETIJDEDIJLE & GETIJDEZENNE","Fosfor, totaal",29,"P t","VL08_95P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.19,0.42]
["VL09_78","DIJLE II","Fosfor, totaal",29,"P t","VL09_78P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_10","MARTJEVAART","Fosfor, totaal",29,"P t","VL11_10P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_109","KLEINE GETE + VLOEDGRACHT","Fosfor, totaal",29,"P t","VL11_109P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_11","MOERDIJKVAART","Fosfor, totaal",29,"P t","VL11_11P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_117","ZWARTEBEEK","Fosfor, totaal",29,"P t","VL11_117P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_120","AA I","Fosfor, totaal",29,"P t","VL11_120P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_123","GROTE NETE I","Fosfor, totaal",29,"P t","VL11_123P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_126","KLEINE NETE I","Fosfor, totaal",29,"P t","VL11_126P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_127","KLEINE NETE II","Fosfor, totaal",29,"P t","VL11_127P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_128","MOL NEET","Fosfor, totaal",29,"P t","VL11_128P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_13","VEURNE AMBACHT POLDER WATERLOPEN","Fosfor, totaal",29,"P t","VL11_13P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_133","ABEEK","Fosfor, totaal",29,"P t","VL11_133P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_145","MARK (Maas)","Fosfor, totaal",29,"P t","VL11_145P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_155","BRUGSE REIEN","Fosfor, totaal",29,"P t","VL11_155P t","zomergemiddelde (apr-sept)","mgP/L",0.105,"jaargemiddelde",0.105,0.105,0.2,0.3]
["VL11_165","KANAAL GENT-TERNEUZEN + GENTSE HAVENDOKKEN","Fosfor, totaal",29,"P t","VL11_165P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_19","OOSTENDS KREKENGEBIED","Fosfor, totaal",29,"P t","VL11_19P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_203","MAAS I+II+III","Fosfor, totaal",29,"P t","VL11_203P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_205","DEMER III+IV","Fosfor, totaal",29,"P t","VL11_205P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_207","MELSTERBEEK I+II","Fosfor, totaal",29,"P t","VL11_207P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_37","WATERLOOP VAN DE HOGE LANDEN + MELKADER","Fosfor, totaal",29,"P t","VL11_37P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_40","ZEESCHELDE I","Fosfor, totaal",29,"P t","VL11_40P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.19,0.42]
["VL11_59","GROTE SPIEREBEEK","Fosfor, totaal",29,"P t","VL11_59P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_63","ZWALM","Fosfor, totaal",29,"P t","VL11_63P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_76","BAREBEEK","Fosfor, totaal",29,"P t","VL11_76P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_83","IJSSE","Fosfor, totaal",29,"P t","VL11_83P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_84","LAAN","Fosfor, totaal",29,"P t","VL11_84P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_88","VROUWVLIET","Fosfor, totaal",29,"P t","VL11_88P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL11_91","WOLUWE","Fosfor, totaal",29,"P t","VL11_91P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_147","WARMBEEK","Fosfor, totaal",29,"P t","VL17_147P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_154","BRAKELEIKEN + LIEVE","Fosfor, totaal",29,"P t","VL17_154P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_156","GENTSE BINNENWATEREN","Fosfor, totaal",29,"P t","VL17_156P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_161","KANAAL DUINKERKE-NIEUWPOORT","Fosfor, totaal",29,"P t","VL17_161P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_168","KANAAL PLASSENDALE-NIEUWPOORT","Fosfor, totaal",29,"P t","VL17_168P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_169","KANAAL ROESELARE-LEIE","Fosfor, totaal",29,"P t","VL17_169P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_174","LOKANAAL","Fosfor, totaal",29,"P t","VL17_174P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_187","ANTWERPSE HAVENDOKKEN + SCHELDE-RIJNVERBINDING","Fosfor, totaal",29,"P t","VL17_187P t","zomergemiddelde (apr-sept)","mgP/L",0.11,"jaargemiddelde",0.11,0.11,0.22,0.33]
["VL17_190","BOUDEWIJNKANAAL + ACHTERHAVEN ZEEBRUGGE","Fosfor, totaal",29,"P t","VL17_190P t","zomergemiddelde (apr-sept)","mgP/L",0.11,"jaargemiddelde",0.11,0.11,0.22,0.33]
["VL17_204","BOVEN-SCHELDE II+III","Fosfor, totaal",29,"P t","VL17_204P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_206","DENDER II+III","Fosfor, totaal",29,"P t","VL17_206P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_29","GROOT SCHIJN","Fosfor, totaal",29,"P t","VL17_29P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_35","VERLEGDE SCHIJN - HOOFDGRACHT","Fosfor, totaal",29,"P t","VL17_35P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_42","ZEESCHELDE III + RUPEL","Fosfor, totaal",29,"P t","VL17_42P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.19,0.42]
["VL17_43","ZEESCHELDE IV","Fosfor, totaal",29,"P t","VL17_43P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.19,0.42]
["VL17_48","LEIE I","Fosfor, totaal",29,"P t","VL17_48P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_49","LEIE II","Fosfor, totaal",29,"P t","VL17_49P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_54","TOERISTISCHE LEIE","Fosfor, totaal",29,"P t","VL17_54P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_60","MOLENBEEK - MAARKEBEEK","Fosfor, totaal",29,"P t","VL17_60P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_66","BELLEBEEK","Fosfor, totaal",29,"P t",{"$f":"_xlfn.CONCAT(A1987,E1987)","v":"VL17_66P t"},"zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL17_9","IJZER III","Fosfor, totaal",29,"P t","VL17_9P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL20_36","VERLEGDE SCHIJN - VOORGRACHT","Fosfor, totaal",29,"P t","VL20_36P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL20_96","BEGIJNENBEEK","Fosfor, totaal",29,"P t","VL20_96P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL21_1","BLANKAART WATERLOPEN","Fosfor, totaal",29,"P t","VL21_1P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL21_107","GROTE GETE + BORGGRACHT","Fosfor, totaal",29,"P t","VL21_107P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL21_129","MOLENBEEK - BOLLAAK","Fosfor, totaal",29,"P t","VL21_129P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL21_139","JEKER I","Fosfor, totaal",29,"P t","VL21_139P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL21_26","POEKEBEEK","Fosfor, totaal",29,"P t","VL21_26P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL21_33","MOLENBEEK - KOTTEMBEEK","Fosfor, totaal",29,"P t","VL21_33P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL21_47","HEULEBEEK","Fosfor, totaal",29,"P t","VL21_47P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL21_74","MOLENBEEK - TER ERPENBEEK","Fosfor, totaal",29,"P t","VL21_74P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL21_79","DIJLE III","Fosfor, totaal",29,"P t","VL21_79P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL21_8","IJZER II","Fosfor, totaal",29,"P t","VL21_8P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL21_94","ZUUNBEEK","Fosfor, totaal",29,"P t","VL21_94P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL21_97","DE HULPE - ZWART WATER","Fosfor, totaal",29,"P t","VL21_97P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL22_208","ALBERTKANAAL - Maasbekken","Fosfor, totaal",29,"P t","VL22_208P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL22_209","ALBERTKANAAL - Demerbekken","Fosfor, totaal",29,"P t","VL22_209P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL22_210","ALBERTKANAAL - Netebekken","Fosfor, totaal",29,"P t","VL22_210P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL22_211","ALBERTKANAAL - Benedenscheldebekken","Fosfor, totaal",29,"P t","VL22_211P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL22_212","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Netebekken","Fosfor, totaal",29,"P t","VL22_212P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL22_213","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Maasbekken","Fosfor, totaal",29,"P t","VL22_213P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL22_214","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Benedenscheldebekken","Fosfor, totaal",29,"P t","VL22_214P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL22_215","ZEEKANAAL BRUSSEL-SCHELDE - Dijle-Zennebekken","Fosfor, totaal",29,"P t","VL22_215P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL22_216","ZEEKANAAL BRUSSEL-SCHELDE - Benedenscheldebekken","Fosfor, totaal",29,"P t","VL22_216P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL22_217","AFLEIDINGSKANAAL van de LEIE II + KANAAL van EEKLO - Bekken van de Gentse kanalen","Fosfor, totaal",29,"P t","VL22_217P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL22_218","AFLEIDINGSKANAAL van de LEIE II - Bekken van de Brugse polders","Fosfor, totaal",29,"P t","VL22_218P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL22_219","KANAAL BOSSUIT-KORTRIJK - Bovenscheldebekken","Fosfor, totaal",29,"P t","VL22_219P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL22_220","KANAAL BOSSUIT-KORTRIJK - Leiebekken","Fosfor, totaal",29,"P t","VL22_220P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["VL22_221","ZUID-WILLEMSVAART + KANAAL BOCHOLT-HERENTALS (deels) + KANAAL BRIEGDEN-NEERHAREN","Fosfor, totaal",29,"P t","VL22_221P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_10","KEMMELBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_10EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_104","NEERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_104EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_105","PALINGBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_105EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_11","WANEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_11EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_112","LA HAUTE PLANCHE","Geleidbaarheid (20°C)",82,"EC 20","L107_112EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_113","DOUVEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_113EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_116","GROTE SPIERE","Geleidbaarheid (20°C)",82,"EC 20","L107_116EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_12","VLETERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_12EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_120","SCHEEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_120EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_123","KANAAL VAN BRUGGE NAAR SLUIS","Geleidbaarheid (20°C)",82,"EC 20","L107_123EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["L107_135","JABBEEKSE BEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_135EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_136","HOGE WATERING","Geleidbaarheid (20°C)",82,"EC 20","L107_136EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["L107_16","HARINGEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_16EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_209","ZWARTESLUISBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L107_209EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["L107_218","SLEIDINGSVAARDEKEN","Geleidbaarheid (20°C)",82,"EC 20","L107_218EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_225","KEUTELBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_225EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_234","POEKEBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L107_234EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_235","REIGERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_235EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_236","NEERSCHUURBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_236EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_237","SPEIBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_237EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_239","OUDE MANDEL L1","Geleidbaarheid (20°C)",82,"EC 20","L107_239EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_240","ZOUBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_240EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_241","KATTEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_241EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_242","DUIVEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_242EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_246","STAMPKOTBEEK - MOLENBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_246EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_247","STAMPKOTBEEK - WALLEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_247EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_253","STAMPKOTBEEK - MUNKBOSBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_253EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_254","MOLENBEEK - BEIAARDBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_254EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_266","PEERDESTOKBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_266EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_272","OPHASSELTBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_272EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_273","MOLENBEEK - PACHTBOSBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L107_273EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_274","MOLENBEEK - KALSTERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_274EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_275","TER ERPENBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_275EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_276","MOLENBEEK - GRAADBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_276EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_277","WILDEBEEK","Geleidbaarheid (20°C)",82,"EC 20",{"$f":"_xlfn.CONCAT(A2051,E2051)","v":"L107_277EC 20"},"90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_279","MOLENBEEK - VOGELENZANGBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_279EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_282","MOLENBEEK - GONDEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_282EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_287","MOLENBEEK - GROTE BEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_287EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_289","DAMSLOOT","Geleidbaarheid (20°C)",82,"EC 20","L107_289EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_296","VOORSTESLOOT","Geleidbaarheid (20°C)",82,"EC 20","L107_296EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_299","VONDELBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L107_299EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_3","BROENBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_3EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_305","ZELEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_305EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_325","GROTE ASTBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_325EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_329","BLOKSTRAATBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_329EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["L107_330","WATERLOOP VAN DE HOGE LANDEN L1","Geleidbaarheid (20°C)",82,"EC 20","L107_330EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_335","MOLENBEEK - BEVERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_335EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_336","DE RIJT","Geleidbaarheid (20°C)",82,"EC 20","L107_336EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_4","KORVERSBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_4EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_40","STENENSLUISVAART","Geleidbaarheid (20°C)",82,"EC 20","L107_40EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["L107_403","MOLENBEEK - NEERPEDEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_403EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_404","LOTBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_404EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_407","GROEBENGRACHT","Geleidbaarheid (20°C)",82,"EC 20","L107_407EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_409","KLEINE MAALBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_409EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_411","MOLENBEEK - PARKBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_411EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_413","TANGEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_413EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_417","DE GROTE LAAK","Geleidbaarheid (20°C)",82,"EC 20","L107_417EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_418","MENE","Geleidbaarheid (20°C)",82,"EC 20","L107_418EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_421","GENOVEVABEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_421EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_422","'S HERTOGENGRACHT","Geleidbaarheid (20°C)",82,"EC 20","L107_422EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_423","BEGIJNEBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L107_423EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_424","VIJVERSLOOP","Geleidbaarheid (20°C)",82,"EC 20","L107_424EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_431","ST-ODULPHUSBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_431EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_432","DORMAALBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_432EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_433","BEVERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_433EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_434","SCHEIBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_434EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_435","AREBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_435EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_439","IJSE L1","Geleidbaarheid (20°C)",82,"EC 20","L107_439EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_441","LANGEGRACHT","Geleidbaarheid (20°C)",82,"EC 20","L107_441EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_449","VOER (BERTEM)","Geleidbaarheid (20°C)",82,"EC 20","L107_449EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_451","GROTE LAAK - GROTE LOOP - MESTENLOOP","Geleidbaarheid (20°C)",82,"EC 20","L107_451EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_452","LAARBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_452EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_453","ZWARTEBEEK (SCHERPENHEUVEL-ZICHEM)","Geleidbaarheid (20°C)",82,"EC 20","L107_453EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_454","KLEINEBEEK - RIJSELSESTRAATVLIET","Geleidbaarheid (20°C)",82,"EC 20","L107_454EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_462","LEMINGSBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_462EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_463","AABEEK (MECHELEN)","Geleidbaarheid (20°C)",82,"EC 20","L107_463EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_464","LEYBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_464EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_47","ZARRENBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L107_47EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_48","KANAAL VAN ESEN","Geleidbaarheid (20°C)",82,"EC 20","L107_48EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["L107_5","BOLLAERTBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_5EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_6","DIKKEBUSBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_6EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_600","LEYLOOP","Geleidbaarheid (20°C)",82,"EC 20","L107_600EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_601","DE AA (RAVELS)","Geleidbaarheid (20°C)",82,"EC 20","L107_601EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_602","BLAUWPUTTEN EN LEILOOP","Geleidbaarheid (20°C)",82,"EC 20","L107_602EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_603","HEERLESE LOOP","Geleidbaarheid (20°C)",82,"EC 20","L107_603EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_607","MERKSKE L1","Geleidbaarheid (20°C)",82,"EC 20","L107_607EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_609","KLEINE MARK","Geleidbaarheid (20°C)",82,"EC 20","L107_609EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_61","VAARTDIJKGELEED","Geleidbaarheid (20°C)",82,"EC 20","L107_61EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["L107_610","MARK L1","Geleidbaarheid (20°C)",82,"EC 20","L107_610EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_613","SLUISKENSVIJVER","Geleidbaarheid (20°C)",82,"EC 20","L107_613EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_614","WEERIJSEBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L107_614EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_615","KLEINE BEEK (WUUSTWEZEL)","Geleidbaarheid (20°C)",82,"EC 20","L107_615EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_629","KLEIN WILBOEREBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_629EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_63","BOERGONJEVAART","Geleidbaarheid (20°C)",82,"EC 20","L107_63EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["L107_631","MOLENBEEK - BOLLAAK L1","Geleidbaarheid (20°C)",82,"EC 20","L107_631EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_632","DE DELFTE BEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_632EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_633","BOSBEEK - DIEPTELOOP","Geleidbaarheid (20°C)",82,"EC 20","L107_633EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_638","GROTE CALIE","Geleidbaarheid (20°C)",82,"EC 20","L107_638EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_640","DE AA - NATTENLOOP","Geleidbaarheid (20°C)",82,"EC 20",{"$f":"_xlfn.CONCAT(A2115,E2115)","v":"L107_640EC 20"},"90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_644","ITTERBEEK (DUFFEL)","Geleidbaarheid (20°C)",82,"EC 20","L107_644EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_648","BRUINBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_648EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_650","REEHAGENBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_650EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_654","LARUMSE LOOP","Geleidbaarheid (20°C)",82,"EC 20","L107_654EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_655","DALEMANSLOOP","Geleidbaarheid (20°C)",82,"EC 20","L107_655EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_656","BEGGELBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_656EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_66","KERKBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_66EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_664","MOLENBEEK - ZIJP","Geleidbaarheid (20°C)",82,"EC 20","L107_664EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_665","BOUWBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_665EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_67","LIJSTERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_67EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_677","DIEPE BEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_677EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_681","KOUDE BEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_681EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_684","SCHOON SCHIJN","Geleidbaarheid (20°C)",82,"EC 20","L107_684EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["L107_688","LAARSE BEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_688EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_695","VARENDONKSE BEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_695EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_702","MILLEGEMLOOP","Geleidbaarheid (20°C)",82,"EC 20","L107_702EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_705","SCHEPPELIJKE NETE","Geleidbaarheid (20°C)",82,"EC 20","L107_705EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_706","MOLSE NETE L1","Geleidbaarheid (20°C)",82,"EC 20","L107_706EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_708","GROTE NETE L1","Geleidbaarheid (20°C)",82,"EC 20","L107_708EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_722","WAMP L1","Geleidbaarheid (20°C)",82,"EC 20","L107_722EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_723","RODE LOOP","Geleidbaarheid (20°C)",82,"EC 20","L107_723EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_729","STAPKENSLOOP","Geleidbaarheid (20°C)",82,"EC 20","L107_729EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_735","GESTELBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_735EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_740","BERGEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_740EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_741","SPILLEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_741EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_742","PLATTE BEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_742EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_78","DEVEBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L107_78EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_8","IEPERLEE","Geleidbaarheid (20°C)",82,"EC 20","L107_8EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_809","KLEINE HERK L1","Geleidbaarheid (20°C)",82,"EC 20","L107_809EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_810","WINTERBEEK (KORTESSEM)","Geleidbaarheid (20°C)",82,"EC 20","L107_810EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_812","MOMBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L107_812EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_814","STEENLAAK","Geleidbaarheid (20°C)",82,"EC 20","L107_814EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_82","BABILLEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_82EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_824","ROELBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_824EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_83","ROOBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_83EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_836","LAAMBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_836EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_839","ZONDERIKBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_839EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_84","KROMMEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_84EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_846","KAATSBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_846EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_847","WINTERBEEK (BILZEN)","Geleidbaarheid (20°C)",82,"EC 20","L107_847EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_848","DEMER L1","Geleidbaarheid (20°C)",82,"EC 20","L107_848EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_852","MUNSTERBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L107_852EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_853","ZUTENDAALBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_853EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_854","BOLLISENBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_854EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_855","DOMMEL L1","Geleidbaarheid (20°C)",82,"EC 20","L107_855EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_856","HOLVENLOOP","Geleidbaarheid (20°C)",82,"EC 20","L107_856EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_857","EINDERGATLOOP","Geleidbaarheid (20°C)",82,"EC 20","L107_857EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_858","WARMBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L107_858EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_859","PRINSENLOOP","Geleidbaarheid (20°C)",82,"EC 20","L107_859EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_861","ABEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L107_861EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_866","LOSSING L1","Geleidbaarheid (20°C)",82,"EC 20","L107_866EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_869","SOERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_869EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_876","BOSBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L107_876EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_879","VRIETSELBEEK - OUDE MAAS (DILSEN)","Geleidbaarheid (20°C)",82,"EC 20","L107_879EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_883","ZIEPBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_883EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_885","HEESWATER","Geleidbaarheid (20°C)",82,"EC 20","L107_885EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_890","BEEK - DE BUTH (TONGEREN)","Geleidbaarheid (20°C)",82,"EC 20","L107_890EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_891","VOER (VOEREN)","Geleidbaarheid (20°C)",82,"EC 20","L107_891EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_892","BEEK (VOEREN)","Geleidbaarheid (20°C)",82,"EC 20","L107_892EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_893","GULP","Geleidbaarheid (20°C)",82,"EC 20","L107_893EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_91","PLAATSBEEK","Geleidbaarheid (20°C)",82,"EC 20","L107_91EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_92","MAALBEEK (LEIEBEKKEN)","Geleidbaarheid (20°C)",82,"EC 20","L107_92EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_97","KASSELRIJBEEK - WEST","Geleidbaarheid (20°C)",82,"EC 20","L107_97EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L107_98","GAVERBEEK","Geleidbaarheid (20°C)",82,"EC 20",{"$f":"_xlfn.CONCAT(A2179,E2179)","v":"L107_98EC 20"},"90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L110_1100","ZILVERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L110_1100EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1001","MARTJEVAART - LEKKERBOTERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1001EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1003","GELUWEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1003EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1004","RIJTGRACHT","Geleidbaarheid (20°C)",82,"EC 20","L111_1004EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1006","HOOFDSLOOT","Geleidbaarheid (20°C)",82,"EC 20","L111_1006EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1014","MEREBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1014EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1016","WANTEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1016EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1018","LEEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1018EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1019","MOLENBEEK - MARKEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1019EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1020","OOSSEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1020EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1021","ZWALMBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1021EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1022","MOLENBEEK (RONSE)","Geleidbaarheid (20°C)",82,"EC 20","L111_1022EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1024","BAVEGEMSE BEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1024EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1025","MAANBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1025EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1027","GROOTEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1027EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1028","LANGELEDE","Geleidbaarheid (20°C)",82,"EC 20","L111_1028EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1029","KLEINE WATERGANG","Geleidbaarheid (20°C)",82,"EC 20","L111_1029EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1030","WATERGANG VAN DE MOERBEKEPOLDER","Geleidbaarheid (20°C)",82,"EC 20","L111_1030EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1031","KANAAL VAN STEKENE","Geleidbaarheid (20°C)",82,"EC 20","L111_1031EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1032","DIJKGRACHT","Geleidbaarheid (20°C)",82,"EC 20","L111_1032EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["L111_1033","PAPENMEERSBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1033EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1035","KOEVAARDEKEN","Geleidbaarheid (20°C)",82,"EC 20","L111_1035EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["L111_1037","MOLENBEEK - LAKEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1037EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1038","MAALBEEK - AMELVONNEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1038EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1039","STEENVOORDBEEK (TERNAT)","Geleidbaarheid (20°C)",82,"EC 20","L111_1039EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1040","BELLEBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1040EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1041","WINGE L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1041EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1042","LEIBEEK - LIPSEBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1042EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1043","WEESBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1043EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1044","KASTEELBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1044EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1046","GROTE MOTTE","Geleidbaarheid (20°C)",82,"EC 20","L111_1046EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1047","BAREBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1047EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1049","MUNTLOOP","Geleidbaarheid (20°C)",82,"EC 20","L111_1049EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1050","WEHAGENBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1050EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1052","LAAKBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1052EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1053","MOUBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1053EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1054","GOORBOSBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1054EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1056","VROUWVLIET L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1056EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1057","GROTE MOLENBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1057EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1058","ZWARTE BEEK (WILLEBROEK)","Geleidbaarheid (20°C)",82,"EC 20","L111_1058EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1059","ZIELBEEK - BOSBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1059EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1060","GROOT SCHIJN L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1060EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1062","HERSELTSELOOP","Geleidbaarheid (20°C)",82,"EC 20","L111_1062EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1063","STEENKENSBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1063EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1064","ST. TRUDOLEKEN","Geleidbaarheid (20°C)",82,"EC 20","L111_1064EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1065","ASBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1065EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1066","LOEIJENS NEETJE","Geleidbaarheid (20°C)",82,"EC 20","L111_1066EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1067","KLEINE NETE L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1067EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1070","WIMP L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1070EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1071","GOORLOOP","Geleidbaarheid (20°C)",82,"EC 20","L111_1071EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1072","POVERSBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1072EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1075","MELSTERBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1075EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1076","CICINDRIA","Geleidbaarheid (20°C)",82,"EC 20","L111_1076EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1077","MOLENBEEK (SINT-TRUIDEN)","Geleidbaarheid (20°C)",82,"EC 20","L111_1077EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1078","GRONDBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1078EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1079","HELDERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1079EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1080","ZWARTEBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1080EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1081","MANGELBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1081EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1082","SLANGBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1082EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1083","MISERIKBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1083EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1084","MANDEL L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1084EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1086","LOZERBROEKBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1086EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1087","HORSTGATERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1087EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1088","ITTERBEEK L1","Geleidbaarheid (20°C)",82,"EC 20",{"$f":"_xlfn.CONCAT(A2243,E2243)","v":"L111_1088EC 20"},"90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1089","WITBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1089EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1090","ZANDERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1090EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1091","KIKBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1091EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1092","ZOUW","Geleidbaarheid (20°C)",82,"EC 20","L111_1092EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1093","EZELSBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1093EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1094","HEULEBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1094EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1095","KLEINE LAAK","Geleidbaarheid (20°C)",82,"EC 20","L111_1095EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1096","GROTE LAAK L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1096EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1098","KEIBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1098EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1099","GAVERSE BEEK (BECQUE DE NEUVILLE)","Geleidbaarheid (20°C)",82,"EC 20","L111_1099EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1102","KLEINE A - WILDERTSE BEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1102EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1104","DESPIERREBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1104EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1105","MELSENBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1105EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1106","DONKSE BEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1106EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["L111_1109","MOERDIJKVAART L1","Geleidbaarheid (20°C)",82,"EC 20","L111_1109EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1110","EDE","Geleidbaarheid (20°C)",82,"EC 20","L111_1110EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1112","ISABELLASTROOM","Geleidbaarheid (20°C)",82,"EC 20","L111_1112EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1113","LACHENEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1113EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1114","ANTITANKGRACHT ZUID","Geleidbaarheid (20°C)",82,"EC 20","L111_1114EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_1201","S HERTOGENDIJKSE BEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1201EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["L111_15","HEIDEBEEK (VLETEREN)","Geleidbaarheid (20°C)",82,"EC 20","L111_15EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["L111_298","OUDE DENDER","Geleidbaarheid (20°C)",82,"EC 20","L111_298EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_315","FONDATIEGRACHT","Geleidbaarheid (20°C)",82,"EC 20","L111_315EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_326","BARBIERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_326EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_419","SCHOORBROEKBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_419EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_436","VELPE L1","Geleidbaarheid (20°C)",82,"EC 20","L111_436EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_624","TAPPELBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_624EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_627","KLEINE BEEK (ZANDHOVEN)","Geleidbaarheid (20°C)",82,"EC 20","L111_627EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_639","VISBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_639EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_674","BENEDENVLIET L1","Geleidbaarheid (20°C)",82,"EC 20","L111_674EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_676","WEZELSE BEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_676EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_699","SCHERPENBERGLOOP","Geleidbaarheid (20°C)",82,"EC 20","L111_699EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_707","KLEINE HOOFDGRACHT","Geleidbaarheid (20°C)",82,"EC 20","L111_707EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_717","DESSELSE NEET","Geleidbaarheid (20°C)",82,"EC 20","L111_717EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_724","ANTITANKGRACHT NOORD","Geleidbaarheid (20°C)",82,"EC 20","L111_724EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L111_844","STIEMER","Geleidbaarheid (20°C)",82,"EC 20","L111_844EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L117_1036","ZUUNBEEK L1","Geleidbaarheid (20°C)",82,"EC 20","L117_1036EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L117_1068","HERTSBERGEBEEK - GETEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L117_1068EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L117_1073","RIVIERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L117_1073EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L117_1074","HERK L1","Geleidbaarheid (20°C)",82,"EC 20","L117_1074EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L117_1085","WILDERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L117_1085EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L117_17","STEENVOORDEBEEK (WATOU)","Geleidbaarheid (20°C)",82,"EC 20","L117_17EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L117_219","BURGGRAVENSTROOM","Geleidbaarheid (20°C)",82,"EC 20","L117_219EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L117_232","JOBEEK","Geleidbaarheid (20°C)",82,"EC 20","L117_232EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L117_233","RINGBEEK","Geleidbaarheid (20°C)",82,"EC 20","L117_233EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L117_402","MOLENBEEK - SLAGVIJVERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L117_402EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L117_659","KREKELBEEK","Geleidbaarheid (20°C)",82,"EC 20","L117_659EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L117_673","KLEIN SCHIJN (NOORDELIJK DEEL)","Geleidbaarheid (20°C)",82,"EC 20","L117_673EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L117_813","HERKEBEEK","Geleidbaarheid (20°C)",82,"EC 20","L117_813EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L118_238","KROMMEDIJKBEEK","Geleidbaarheid (20°C)",82,"EC 20","L118_238EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L119_675","KLEIN SCHIJN (ZUIDELIJK DEEL)","Geleidbaarheid (20°C)",82,"EC 20","L119_675EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L120_1097","KASSELRIJBEEK - OOST","Geleidbaarheid (20°C)",82,"EC 20","L120_1097EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L121_1045","GROTEBEEK - WINTERBEEK","Geleidbaarheid (20°C)",82,"EC 20","L121_1045EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L2 Bk","L2 Kleine Beek","Geleidbaarheid (20°C)",82,"EC 20","L2 BkEC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["L2 Bk","L2 kleine beek","Geleidbaarheid (20°C)",82,"EC 20","L2 BkEC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_102","DEMER V","Geleidbaarheid (20°C)",82,"EC 20","VL05_102EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_103","DEMER VI","Geleidbaarheid (20°C)",82,"EC 20","VL05_103EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_104","DEMER VII","Geleidbaarheid (20°C)",82,"EC 20","VL05_104EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_105","GETE I","Geleidbaarheid (20°C)",82,"EC 20","VL05_105EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_106","GETE II","Geleidbaarheid (20°C)",82,"EC 20","VL05_106EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_108","HERK + KLEINE HERK","Geleidbaarheid (20°C)",82,"EC 20","VL05_108EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_110","MANGELBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_110EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_113","MOMBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_113EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_114","MUNSTERBEEK","Geleidbaarheid (20°C)",82,"EC 20",{"$f":"_xlfn.CONCAT(A2307,E2307)","v":"VL05_114EC 20"},"90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_115","VELPE","Geleidbaarheid (20°C)",82,"EC 20","VL05_115EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_116","WINGE","Geleidbaarheid (20°C)",82,"EC 20","VL05_116EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_118","ZWARTWATER","Geleidbaarheid (20°C)",82,"EC 20","VL05_118EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_119","VINNE","Geleidbaarheid (20°C)",82,"EC 20","VL05_119EC 20","90 percentiel","µS/cm",750,"maximum",1125,1125,1687.5,3375]
["VL05_12","POPERINGEVAART","Geleidbaarheid (20°C)",82,"EC 20","VL05_12EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_121","AA II","Geleidbaarheid (20°C)",82,"EC 20","VL05_121EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_122","GROTE LAAK","Geleidbaarheid (20°C)",82,"EC 20","VL05_122EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_124","GROTE NETE II","Geleidbaarheid (20°C)",82,"EC 20","VL05_124EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_130","WAMP","Geleidbaarheid (20°C)",82,"EC 20","VL05_130EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_131","WIMP","Geleidbaarheid (20°C)",82,"EC 20","VL05_131EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_134","BERWIJN","Geleidbaarheid (20°C)",82,"EC 20","VL05_134EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_135","BOSBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_135EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_136","DOMMEL","Geleidbaarheid (20°C)",82,"EC 20","VL05_136EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_137","ITTERBEEK I","Geleidbaarheid (20°C)",82,"EC 20","VL05_137EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_138","ITTERBEEK II","Geleidbaarheid (20°C)",82,"EC 20","VL05_138EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_140","JEKER II","Geleidbaarheid (20°C)",82,"EC 20","VL05_140EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_141","LOSSING","Geleidbaarheid (20°C)",82,"EC 20","VL05_141EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_146","MERKSKE","Geleidbaarheid (20°C)",82,"EC 20","VL05_146EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_148","WEERIJSEBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_148EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_150","AFLEIDINGSKANAAL van de LEIE/SCHIPDONKKANAAL I","Geleidbaarheid (20°C)",82,"EC 20","VL05_150EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_152","AVRIJEVAART + SLEIDINGSVAARDEKE","Geleidbaarheid (20°C)",82,"EC 20","VL05_152EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_159","KANAAL CHARLEROI-BRUSSEL","Geleidbaarheid (20°C)",82,"EC 20","VL05_159EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_163","KANAAL GENT-OOSTENDE II","Geleidbaarheid (20°C)",82,"EC 20","VL05_163EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_166","KANAAL IEPER-IJZER","Geleidbaarheid (20°C)",82,"EC 20","VL05_166EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_167","KANAAL LEUVEN-DIJLE","Geleidbaarheid (20°C)",82,"EC 20","VL05_167EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_170","KANAAL VAN BEVERLO","Geleidbaarheid (20°C)",82,"EC 20","VL05_170EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_171","LEDE","Geleidbaarheid (20°C)",82,"EC 20","VL05_171EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_175","MOERVAART","Geleidbaarheid (20°C)",82,"EC 20","VL05_175EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_177","NIEUWE KALE","Geleidbaarheid (20°C)",82,"EC 20","VL05_177EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_18","KERKEBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_18EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_180","ZARRENBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_180EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_182","ZUIDLEDE","Geleidbaarheid (20°C)",82,"EC 20","VL05_182EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_191","DESSELSE ZANDPUTTEN","Geleidbaarheid (20°C)",82,"EC 20","VL05_191EC 20","90 percentiel","µS/cm",750,"maximum",1125,1125,1687.5,3375]
["VL05_192","DONKMEER","Geleidbaarheid (20°C)",82,"EC 20","VL05_192EC 20","90 percentiel","µS/cm",750,"maximum",1125,1125,1687.5,3375]
["VL05_195","GAVERS HARELBEKE","Geleidbaarheid (20°C)",82,"EC 20","VL05_195EC 20","90 percentiel","µS/cm",750,"maximum",1125,1125,1687.5,3375]
["VL05_196","GRINDPLAS KESSENICH","Geleidbaarheid (20°C)",82,"EC 20","VL05_196EC 20","90 percentiel","µS/cm",750,"maximum",1125,1125,1687.5,3375]
["VL05_2","GROTE KEMMELBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_2EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_20","RIVIERBEEK + HERTSBERGEBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_20EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_200","SCHULENSMEER","Geleidbaarheid (20°C)",82,"EC 20","VL05_200EC 20","90 percentiel","µS/cm",750,"maximum",1125,1125,1687.5,3375]
["VL05_201","SPAANJERD + HEERENLAAK","Geleidbaarheid (20°C)",82,"EC 20","VL05_201EC 20","90 percentiel","µS/cm",750,"maximum",1125,1125,1687.5,3375]
["VL05_21","ZUIDERVAARTJE","Geleidbaarheid (20°C)",82,"EC 20","VL05_21EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_24","MEREBEEK + BORISGRACHT + LIEVE","Geleidbaarheid (20°C)",82,"EC 20","VL05_24EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_25","OUDE KALE","Geleidbaarheid (20°C)",82,"EC 20","VL05_25EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_28","BENEDENVLIET","Geleidbaarheid (20°C)",82,"EC 20","VL05_28EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_3","HANDZAMEVAART","Geleidbaarheid (20°C)",82,"EC 20","VL05_3EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_30","GROTE MOLENBEEK - DE VLIET","Geleidbaarheid (20°C)",82,"EC 20","VL05_30EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_31","KALKENSE VAART","Geleidbaarheid (20°C)",82,"EC 20","VL05_31EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_32","MOLENBEEK - GROTE BEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_32EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_38","ZIELBEEK - BOSBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_38EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_4","HEIDEBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_4EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_44","DEVEBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_44EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_45","GAVERBEEK I","Geleidbaarheid (20°C)",82,"EC 20","VL05_45EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_46","GAVERBEEK II","Geleidbaarheid (20°C)",82,"EC 20","VL05_46EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_5","IEPERLEE + VERWEZEN KANAAL IEPER-KOMEN","Geleidbaarheid (20°C)",82,"EC 20","VL05_5EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_50","LEIE III","Geleidbaarheid (20°C)",82,"EC 20","VL05_50EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_51","MANDEL I","Geleidbaarheid (20°C)",82,"EC 20","VL05_51EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_52","MANDEL II","Geleidbaarheid (20°C)",82,"EC 20","VL05_52EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_53","OUDE MANDEL","Geleidbaarheid (20°C)",82,"EC 20","VL05_53EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_58","BOVEN-SCHELDE IV","Geleidbaarheid (20°C)",82,"EC 20","VL05_58EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_61","RONE","Geleidbaarheid (20°C)",82,"EC 20","VL05_61EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_62","STAMPKOTBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_62EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_64","ZWARTE SPIEREBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_64EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_67","DENDER I","Geleidbaarheid (20°C)",82,"EC 20","VL05_67EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_70","DENDER IV","Geleidbaarheid (20°C)",82,"EC 20",{"$f":"_xlfn.CONCAT(A2371,E2371)","v":"VL05_70EC 20"},"90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_73","MOLENBEEK - PACHTBOSBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_73EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_75","VONDELBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_75EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_77","DIJLE I","Geleidbaarheid (20°C)",82,"EC 20","VL05_77EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_81","DIJLE V","Geleidbaarheid (20°C)",82,"EC 20","VL05_81EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_85","LEIBEEK - LAAKBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_85EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_86","NETHEN","Geleidbaarheid (20°C)",82,"EC 20","VL05_86EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_87","VOER (Leuven)","Geleidbaarheid (20°C)",82,"EC 20","VL05_87EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_89","VUNT","Geleidbaarheid (20°C)",82,"EC 20","VL05_89EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_90","WEESBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL05_90EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_93","ZENNE II","Geleidbaarheid (20°C)",82,"EC 20","VL05_93EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL05_98","DEMER I","Geleidbaarheid (20°C)",82,"EC 20","VL05_98EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL05_99","DEMER II","Geleidbaarheid (20°C)",82,"EC 20","VL05_99EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL08_125","GROTE NETE III","Geleidbaarheid (20°C)",82,"EC 20","VL08_125EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL08_132","GETIJDENETES","Geleidbaarheid (20°C)",82,"EC 20","VL08_132EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL08_157","ISABELLAWATERING","Geleidbaarheid (20°C)",82,"EC 20","VL08_157EC 20","90 percentiel","µS/cm",1200,"maximum",1800,1800,3000,3750]
["VL08_162","KANAAL GENT-OOSTENDE I + COUPURE + VERBINDINGSKANAAL","Geleidbaarheid (20°C)",82,"EC 20","VL08_162EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL08_164","KANAAL GENT-OOSTENDE III","Geleidbaarheid (20°C)",82,"EC 20","VL08_164EC 20","90 percentiel","µS/cm",3200,"maximum",4800,4800,7200,8700]
["VL08_172","LEOPOLDKANAAL I","Geleidbaarheid (20°C)",82,"EC 20","VL08_172EC 20","90 percentiel","µS/cm",6000,"maximum",9000,9000,12000,15000]
["VL08_173","LEOPOLDKANAAL II","Geleidbaarheid (20°C)",82,"EC 20","VL08_173EC 20","90 percentiel","µS/cm",6000,"maximum",9000,9000,12000,15000]
["VL08_176","NETEKANAAL","Geleidbaarheid (20°C)",82,"EC 20","VL08_176EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL08_178","NOORDELIJKE RINGVAART","Geleidbaarheid (20°C)",82,"EC 20","VL08_178EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL08_179","WESTELIJKE RINGVAART","Geleidbaarheid (20°C)",82,"EC 20","VL08_179EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL08_39","GETIJDEDURME","Geleidbaarheid (20°C)",82,"EC 20","VL08_39EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL08_41","ZEESCHELDE II","Geleidbaarheid (20°C)",82,"EC 20","VL08_41EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL08_55","BOVEN-SCHELDE I","Geleidbaarheid (20°C)",82,"EC 20","VL08_55EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL08_7","IJZER I","Geleidbaarheid (20°C)",82,"EC 20","VL08_7EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL08_71","DENDER V","Geleidbaarheid (20°C)",82,"EC 20","VL08_71EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL08_72","MARK (Denderbekken)","Geleidbaarheid (20°C)",82,"EC 20","VL08_72EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL08_80","DIJLE IV","Geleidbaarheid (20°C)",82,"EC 20","VL08_80EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL08_82","DIJLE VI","Geleidbaarheid (20°C)",82,"EC 20","VL08_82EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL08_92","ZENNE I","Geleidbaarheid (20°C)",82,"EC 20","VL08_92EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL08_95","GETIJDEDIJLE & GETIJDEZENNE","Geleidbaarheid (20°C)",82,"EC 20","VL08_95EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL09_78","DIJLE II","Geleidbaarheid (20°C)",82,"EC 20","VL09_78EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL11_10","MARTJEVAART","Geleidbaarheid (20°C)",82,"EC 20","VL11_10EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_109","KLEINE GETE + VLOEDGRACHT","Geleidbaarheid (20°C)",82,"EC 20","VL11_109EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_11","MOERDIJKVAART","Geleidbaarheid (20°C)",82,"EC 20","VL11_11EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_117","ZWARTEBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL11_117EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_120","AA I","Geleidbaarheid (20°C)",82,"EC 20","VL11_120EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_123","GROTE NETE I","Geleidbaarheid (20°C)",82,"EC 20","VL11_123EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_126","KLEINE NETE I","Geleidbaarheid (20°C)",82,"EC 20","VL11_126EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_127","KLEINE NETE II","Geleidbaarheid (20°C)",82,"EC 20","VL11_127EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_128","MOL NEET","Geleidbaarheid (20°C)",82,"EC 20","VL11_128EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_133","ABEEK","Geleidbaarheid (20°C)",82,"EC 20","VL11_133EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_145","MARK (Maas)","Geleidbaarheid (20°C)",82,"EC 20","VL11_145EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_155","BRUGSE REIEN","Geleidbaarheid (20°C)",82,"EC 20","VL11_155EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,2250,4500]
["VL11_203","MAAS I+II+III","Geleidbaarheid (20°C)",82,"EC 20","VL11_203EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL11_205","DEMER III+IV","Geleidbaarheid (20°C)",82,"EC 20","VL11_205EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_207","MELSTERBEEK I+II","Geleidbaarheid (20°C)",82,"EC 20","VL11_207EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_40","ZEESCHELDE I","Geleidbaarheid (20°C)",82,"EC 20","VL11_40EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL11_59","GROTE SPIEREBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL11_59EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_63","ZWALM","Geleidbaarheid (20°C)",82,"EC 20","VL11_63EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_76","BAREBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL11_76EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_83","IJSSE","Geleidbaarheid (20°C)",82,"EC 20","VL11_83EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_84","LAAN","Geleidbaarheid (20°C)",82,"EC 20","VL11_84EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_88","VROUWVLIET","Geleidbaarheid (20°C)",82,"EC 20","VL11_88EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL11_91","WOLUWE","Geleidbaarheid (20°C)",82,"EC 20","VL11_91EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL17_147","WARMBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL17_147EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL17_154","BRAKELEIKEN + LIEVE","Geleidbaarheid (20°C)",82,"EC 20","VL17_154EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL17_156","GENTSE BINNENWATEREN","Geleidbaarheid (20°C)",82,"EC 20","VL17_156EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL17_161","KANAAL DUINKERKE-NIEUWPOORT","Geleidbaarheid (20°C)",82,"EC 20","VL17_161EC 20","90 percentiel","µS/cm",9000,"maximum",13500,13500,18000,22500]
["VL17_168","KANAAL PLASSENDALE-NIEUWPOORT","Geleidbaarheid (20°C)",82,"EC 20","VL17_168EC 20","90 percentiel","µS/cm",3200,"maximum",4800,4800,7200,8700]
["VL17_169","KANAAL ROESELARE-LEIE","Geleidbaarheid (20°C)",82,"EC 20","VL17_169EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL17_174","LOKANAAL","Geleidbaarheid (20°C)",82,"EC 20","VL17_174EC 20","90 percentiel","µS/cm",2000,"maximum",3000,3000,5250,6450]
["VL17_187","ANTWERPSE HAVENDOKKEN + SCHELDE-RIJNVERBINDING","Geleidbaarheid (20°C)",82,"EC 20",{"$f":"_xlfn.CONCAT(A2435,E2435)","v":"VL17_187EC 20"},"90 percentiel","µS/cm",18000,"maximum",27000,27000,40500,81000]
["VL17_204","BOVEN-SCHELDE II+III","Geleidbaarheid (20°C)",82,"EC 20","VL17_204EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL17_206","DENDER II+III","Geleidbaarheid (20°C)",82,"EC 20","VL17_206EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL17_29","GROOT SCHIJN","Geleidbaarheid (20°C)",82,"EC 20","VL17_29EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL17_35","VERLEGDE SCHIJN - HOOFDGRACHT","Geleidbaarheid (20°C)",82,"EC 20","VL17_35EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL17_48","LEIE I","Geleidbaarheid (20°C)",82,"EC 20","VL17_48EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL17_49","LEIE II","Geleidbaarheid (20°C)",82,"EC 20","VL17_49EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL17_54","TOERISTISCHE LEIE","Geleidbaarheid (20°C)",82,"EC 20","VL17_54EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL17_60","MOLENBEEK - MAARKEBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL17_60EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL17_66","BELLEBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL17_66EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL17_9","IJZER III","Geleidbaarheid (20°C)",82,"EC 20","VL17_9EC 20","90 percentiel","µS/cm",1250,"maximum",1875,1875,2250,2700]
["VL20_36","VERLEGDE SCHIJN - VOORGRACHT","Geleidbaarheid (20°C)",82,"EC 20","VL20_36EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL20_96","BEGIJNENBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL20_96EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL21_1","BLANKAART WATERLOPEN","Geleidbaarheid (20°C)",82,"EC 20","VL21_1EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL21_107","GROTE GETE + BORGGRACHT","Geleidbaarheid (20°C)",82,"EC 20","VL21_107EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL21_129","MOLENBEEK - BOLLAAK","Geleidbaarheid (20°C)",82,"EC 20","VL21_129EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL21_139","JEKER I","Geleidbaarheid (20°C)",82,"EC 20","VL21_139EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL21_26","POEKEBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL21_26EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL21_33","MOLENBEEK - KOTTEMBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL21_33EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL21_47","HEULEBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL21_47EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL21_74","MOLENBEEK - TER ERPENBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL21_74EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL21_79","DIJLE III","Geleidbaarheid (20°C)",82,"EC 20","VL21_79EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL21_8","IJZER II","Geleidbaarheid (20°C)",82,"EC 20","VL21_8EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL21_94","ZUUNBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL21_94EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL21_97","DE HULPE - ZWART WATER","Geleidbaarheid (20°C)",82,"EC 20","VL21_97EC 20","90 percentiel","µS/cm",600,"maximum",900,900,1500,1875]
["VL22_208","ALBERTKANAAL - Maasbekken","Geleidbaarheid (20°C)",82,"EC 20","VL22_208EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL22_209","ALBERTKANAAL - Demerbekken","Geleidbaarheid (20°C)",82,"EC 20","VL22_209EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL22_210","ALBERTKANAAL - Netebekken","Geleidbaarheid (20°C)",82,"EC 20","VL22_210EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL22_211","ALBERTKANAAL - Benedenscheldebekken","Geleidbaarheid (20°C)",82,"EC 20","VL22_211EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL22_212","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Netebekken","Geleidbaarheid (20°C)",82,"EC 20","VL22_212EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL22_213","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Maasbekken","Geleidbaarheid (20°C)",82,"EC 20","VL22_213EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL22_214","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Benedenscheldebekken","Geleidbaarheid (20°C)",82,"EC 20","VL22_214EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL22_215","ZEEKANAAL BRUSSEL-SCHELDE - Dijle-Zennebekken","Geleidbaarheid (20°C)",82,"EC 20","VL22_215EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL22_216","ZEEKANAAL BRUSSEL-SCHELDE - Benedenscheldebekken","Geleidbaarheid (20°C)",82,"EC 20","VL22_216EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL22_217","AFLEIDINGSKANAAL van de LEIE II + KANAAL van EEKLO - Bekken van de Gentse kanalen","Geleidbaarheid (20°C)",82,"EC 20","VL22_217EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL22_218","AFLEIDINGSKANAAL van de LEIE II - Bekken van de Brugse polders","Geleidbaarheid (20°C)",82,"EC 20","VL22_218EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL22_219","KANAAL BOSSUIT-KORTRIJK - Bovenscheldebekken","Geleidbaarheid (20°C)",82,"EC 20","VL22_219EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL22_220","KANAAL BOSSUIT-KORTRIJK - Leiebekken","Geleidbaarheid (20°C)",82,"EC 20","VL22_220EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["VL22_221","ZUID-WILLEMSVAART + KANAAL BOCHOLT-HERENTALS (deels) + KANAAL BRIEGDEN-NEERHAREN","Geleidbaarheid (20°C)",82,"EC 20","VL22_221EC 20","90 percentiel","µS/cm",1000,"maximum",1500,1500,1875,2250]
["L107_122","HET GELEED","Geleidbaarheid (20°C)",82,"EC 20","L107_122EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L107_130","KLEINE GEUL","Geleidbaarheid (20°C)",82,"EC 20","L107_130EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L107_133","BLANKENBERGSEVAART L1","Geleidbaarheid (20°C)",82,"EC 20","L107_133EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L107_143","GROOT ZWIN - NOORDGELEED","Geleidbaarheid (20°C)",82,"EC 20","L107_143EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L107_149","PROVINCIEGELEED","Geleidbaarheid (20°C)",82,"EC 20","L107_149EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L107_150","GRANINGATEVLIET","Geleidbaarheid (20°C)",82,"EC 20","L107_150EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L107_202","OOSTPOLDERKREEK","Geleidbaarheid (20°C)",82,"EC 20","L107_202EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L107_213","EEKLOSE WATERGANG","Geleidbaarheid (20°C)",82,"EC 20","L107_213EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L107_328","ZUIDELIJKE WATERGANG","Geleidbaarheid (20°C)",82,"EC 20","L107_328EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L107_33","BOMMELAREVAART","Geleidbaarheid (20°C)",82,"EC 20","L107_33EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L107_333","DOORLOOP","Geleidbaarheid (20°C)",82,"EC 20","L107_333EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L107_34","RINGSLOT","Geleidbaarheid (20°C)",82,"EC 20","L107_34EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L107_37","LANGGELEED","Geleidbaarheid (20°C)",82,"EC 20","L107_37EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L107_56","REYGAERTSVLIET","Geleidbaarheid (20°C)",82,"EC 20","L107_56EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L107_60","GROOTGELEED","Geleidbaarheid (20°C)",82,"EC 20","L107_60EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L111_1005","KALSIJDEADER","Geleidbaarheid (20°C)",82,"EC 20","L111_1005EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L111_1007","STEGERSZWIN","Geleidbaarheid (20°C)",82,"EC 20","L111_1007EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L111_1010","OOSTKERKEVAART","Geleidbaarheid (20°C)",82,"EC 20","L111_1010EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L111_1011","BOEREKREEK","Geleidbaarheid (20°C)",82,"EC 20","L111_1011EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L111_1015","OUDE AVAART","Geleidbaarheid (20°C)",82,"EC 20","L111_1015EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L111_1034","NIEUWE GRACHT","Geleidbaarheid (20°C)",82,"EC 20","L111_1034EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L111_1048","ZIJDELINGSGELEED","Geleidbaarheid (20°C)",82,"EC 20","L111_1048EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L111_1069","AFWATERINGSGRACHT","Geleidbaarheid (20°C)",82,"EC 20","L111_1069EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L111_1101","GROTE KEIGNAERT","Geleidbaarheid (20°C)",82,"EC 20","L111_1101EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L111_1107","SLIJKVAART","Geleidbaarheid (20°C)",82,"EC 20","L111_1107EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L111_1108","STEENGRACHT","Geleidbaarheid (20°C)",82,"EC 20",{"$f":"_xlfn.CONCAT(A2499,E2499)","v":"L111_1108EC 20"},"zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L111_18","ST-MACHUITSBEEK","Geleidbaarheid (20°C)",82,"EC 20","L111_18EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["VL05_14","VLADSLOVAART","Geleidbaarheid (20°C)",82,"EC 20","VL05_14EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["VL05_153","BERGENVAART","Geleidbaarheid (20°C)",82,"EC 20","VL05_153EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["VL05_17","ISABELLAVAART","Geleidbaarheid (20°C)",82,"EC 20","VL05_17EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["VL05_22","ZWINNEVAART","Geleidbaarheid (20°C)",82,"EC 20","VL05_22EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["VL05_34","NOORD-ZUIDVERBINDING","Geleidbaarheid (20°C)",82,"EC 20","VL05_34EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["VL05_6","IEPERLEED","Geleidbaarheid (20°C)",82,"EC 20","VL05_6EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["VL08_16","BLANKENBERGSE VAART + NOORDEDE","Geleidbaarheid (20°C)",82,"EC 20","VL08_16EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["VL08_27","ZWARTESLUISBEEK","Geleidbaarheid (20°C)",82,"EC 20","VL08_27EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["VL11_13","VEURNE AMBACHT POLDER WATERLOPEN","Geleidbaarheid (20°C)",82,"EC 20","VL11_13EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["VL11_19","OOSTENDS KREKENGEBIED","Geleidbaarheid (20°C)",82,"EC 20","VL11_19EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["VL11_37","WATERLOOP VAN DE HOGE LANDEN + MELKADER","Geleidbaarheid (20°C)",82,"EC 20","VL11_37EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L107_10","KEMMELBEEK","Stikstof, totaal",31,"N t","L107_10N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_104","NEERBEEK","Stikstof, totaal",31,"N t","L107_104N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_105","PALINGBEEK","Stikstof, totaal",31,"N t","L107_105N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_11","WANEBEEK","Stikstof, totaal",31,"N t","L107_11N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_112","LA HAUTE PLANCHE","Stikstof, totaal",31,"N t","L107_112N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_113","DOUVEBEEK","Stikstof, totaal",31,"N t","L107_113N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_116","GROTE SPIERE","Stikstof, totaal",31,"N t","L107_116N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_12","VLETERBEEK","Stikstof, totaal",31,"N t","L107_12N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_120","SCHEEBEEK","Stikstof, totaal",31,"N t","L107_120N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_122","HET GELEED","Stikstof, totaal",31,"N t","L107_122N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_123","KANAAL VAN BRUGGE NAAR SLUIS","Stikstof, totaal",31,"N t","L107_123N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_124","RONSELAREBEEK","Stikstof, totaal",31,"N t","L107_124N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_130","KLEINE GEUL","Stikstof, totaal",31,"N t","L107_130N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_131","LISSEWEEGSEVAART","Stikstof, totaal",31,"N t","L107_131N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_133","BLANKENBERGSEVAART L1","Stikstof, totaal",31,"N t","L107_133N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_135","JABBEEKSE BEEK","Stikstof, totaal",31,"N t","L107_135N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_136","HOGE WATERING","Stikstof, totaal",31,"N t","L107_136N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_140","SCHELLEVLIET","Stikstof, totaal",31,"N t","L107_140N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_143","GROOT ZWIN - NOORDGELEED","Stikstof, totaal",31,"N t","L107_143N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_149","PROVINCIEGELEED","Stikstof, totaal",31,"N t","L107_149N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_150","GRANINGATEVLIET","Stikstof, totaal",31,"N t","L107_150N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_16","HARINGEBEEK","Stikstof, totaal",31,"N t","L107_16N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_202","OOSTPOLDERKREEK","Stikstof, totaal",31,"N t","L107_202N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_209","ZWARTESLUISBEEK L1","Stikstof, totaal",31,"N t","L107_209N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_213","EEKLOSE WATERGANG","Stikstof, totaal",31,"N t","L107_213N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_218","SLEIDINGSVAARDEKEN","Stikstof, totaal",31,"N t","L107_218N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_225","KEUTELBEEK","Stikstof, totaal",31,"N t","L107_225N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_234","POEKEBEEK L1","Stikstof, totaal",31,"N t","L107_234N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_235","REIGERBEEK","Stikstof, totaal",31,"N t","L107_235N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_236","NEERSCHUURBEEK","Stikstof, totaal",31,"N t","L107_236N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_237","SPEIBEEK","Stikstof, totaal",31,"N t","L107_237N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_239","OUDE MANDEL L1","Stikstof, totaal",31,"N t","L107_239N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_240","ZOUBEEK","Stikstof, totaal",31,"N t","L107_240N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_241","KATTEBEEK","Stikstof, totaal",31,"N t","L107_241N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_242","DUIVEBEEK","Stikstof, totaal",31,"N t","L107_242N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_246","STAMPKOTBEEK - MOLENBEEK","Stikstof, totaal",31,"N t","L107_246N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_247","STAMPKOTBEEK - WALLEBEEK","Stikstof, totaal",31,"N t","L107_247N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_253","STAMPKOTBEEK - MUNKBOSBEEK","Stikstof, totaal",31,"N t","L107_253N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_254","MOLENBEEK - BEIAARDBEEK","Stikstof, totaal",31,"N t","L107_254N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_266","PEERDESTOKBEEK","Stikstof, totaal",31,"N t","L107_266N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_272","OPHASSELTBEEK","Stikstof, totaal",31,"N t","L107_272N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_273","MOLENBEEK - PACHTBOSBEEK L1","Stikstof, totaal",31,"N t","L107_273N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_274","MOLENBEEK - KALSTERBEEK","Stikstof, totaal",31,"N t","L107_274N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_275","TER ERPENBEEK","Stikstof, totaal",31,"N t","L107_275N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_276","MOLENBEEK - GRAADBEEK","Stikstof, totaal",31,"N t","L107_276N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_277","WILDEBEEK","Stikstof, totaal",31,"N t","L107_277N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_279","MOLENBEEK - VOGELENZANGBEEK","Stikstof, totaal",31,"N t","L107_279N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_282","MOLENBEEK - GONDEBEEK","Stikstof, totaal",31,"N t","L107_282N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_287","MOLENBEEK - GROTE BEEK","Stikstof, totaal",31,"N t","L107_287N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_289","DAMSLOOT","Stikstof, totaal",31,"N t","L107_289N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_296","VOORSTESLOOT","Stikstof, totaal",31,"N t","L107_296N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_299","VONDELBEEK L1","Stikstof, totaal",31,"N t",{"$f":"_xlfn.CONCAT(A2563,E2563)","v":"L107_299N t"},"zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_3","BROENBEEK","Stikstof, totaal",31,"N t","L107_3N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_305","ZELEBEEK","Stikstof, totaal",31,"N t","L107_305N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_325","GROTE ASTBEEK","Stikstof, totaal",31,"N t","L107_325N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_328","ZUIDELIJKE WATERGANG","Stikstof, totaal",31,"N t","L107_328N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_329","BLOKSTRAATBEEK","Stikstof, totaal",31,"N t","L107_329N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_33","BOMMELAREVAART","Stikstof, totaal",31,"N t","L107_33N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_330","WATERLOOP VAN DE HOGE LANDEN L1","Stikstof, totaal",31,"N t","L107_330N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_333","DOORLOOP","Stikstof, totaal",31,"N t","L107_333N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_335","MOLENBEEK - BEVERBEEK","Stikstof, totaal",31,"N t","L107_335N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_336","DE RIJT","Stikstof, totaal",31,"N t","L107_336N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_34","RINGSLOT","Stikstof, totaal",31,"N t","L107_34N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_37","LANGGELEED","Stikstof, totaal",31,"N t","L107_37N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_4","KORVERSBEEK","Stikstof, totaal",31,"N t","L107_4N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_40","STENENSLUISVAART","Stikstof, totaal",31,"N t","L107_40N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_403","MOLENBEEK - NEERPEDEBEEK","Stikstof, totaal",31,"N t","L107_403N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_404","LOTBEEK","Stikstof, totaal",31,"N t","L107_404N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_407","GROEBENGRACHT","Stikstof, totaal",31,"N t","L107_407N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_409","KLEINE MAALBEEK","Stikstof, totaal",31,"N t","L107_409N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_411","MOLENBEEK - PARKBEEK","Stikstof, totaal",31,"N t","L107_411N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_413","TANGEBEEK","Stikstof, totaal",31,"N t","L107_413N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_417","DE GROTE LAAK","Stikstof, totaal",31,"N t","L107_417N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_418","MENE","Stikstof, totaal",31,"N t","L107_418N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_421","GENOVEVABEEK","Stikstof, totaal",31,"N t","L107_421N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_422","'S HERTOGENGRACHT","Stikstof, totaal",31,"N t","L107_422N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_423","BEGIJNEBEEK L1","Stikstof, totaal",31,"N t","L107_423N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_424","VIJVERSLOOP","Stikstof, totaal",31,"N t","L107_424N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_431","ST-ODULPHUSBEEK","Stikstof, totaal",31,"N t","L107_431N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_432","DORMAALBEEK","Stikstof, totaal",31,"N t","L107_432N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_433","BEVERBEEK","Stikstof, totaal",31,"N t","L107_433N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_434","SCHEIBEEK","Stikstof, totaal",31,"N t","L107_434N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_435","AREBEEK","Stikstof, totaal",31,"N t","L107_435N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_439","IJSE L1","Stikstof, totaal",31,"N t","L107_439N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_441","LANGEGRACHT","Stikstof, totaal",31,"N t","L107_441N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_449","VOER (BERTEM)","Stikstof, totaal",31,"N t","L107_449N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_451","GROTE LAAK - GROTE LOOP - MESTENLOOP","Stikstof, totaal",31,"N t","L107_451N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_452","LAARBEEK","Stikstof, totaal",31,"N t","L107_452N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_453","ZWARTEBEEK (SCHERPENHEUVEL-ZICHEM)","Stikstof, totaal",31,"N t","L107_453N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_454","KLEINEBEEK - RIJSELSESTRAATVLIET","Stikstof, totaal",31,"N t","L107_454N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_462","LEMINGSBEEK","Stikstof, totaal",31,"N t","L107_462N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_463","AABEEK (MECHELEN)","Stikstof, totaal",31,"N t","L107_463N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_464","LEYBEEK","Stikstof, totaal",31,"N t","L107_464N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_47","ZARRENBEEK L1","Stikstof, totaal",31,"N t","L107_47N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_48","KANAAL VAN ESEN","Stikstof, totaal",31,"N t","L107_48N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_5","BOLLAERTBEEK","Stikstof, totaal",31,"N t","L107_5N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_56","REYGAERTSVLIET","Stikstof, totaal",31,"N t","L107_56N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_6","DIKKEBUSBEEK","Stikstof, totaal",31,"N t","L107_6N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_60","GROOTGELEED","Stikstof, totaal",31,"N t","L107_60N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_600","LEYLOOP","Stikstof, totaal",31,"N t","L107_600N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_601","DE AA (RAVELS)","Stikstof, totaal",31,"N t","L107_601N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_602","BLAUWPUTTEN EN LEILOOP","Stikstof, totaal",31,"N t","L107_602N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_603","HEERLESE LOOP","Stikstof, totaal",31,"N t","L107_603N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_607","MERKSKE L1","Stikstof, totaal",31,"N t","L107_607N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_609","KLEINE MARK","Stikstof, totaal",31,"N t","L107_609N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_61","VAARTDIJKGELEED","Stikstof, totaal",31,"N t","L107_61N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_610","MARK L1","Stikstof, totaal",31,"N t","L107_610N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_613","SLUISKENSVIJVER","Stikstof, totaal",31,"N t","L107_613N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_614","WEERIJSEBEEK L1","Stikstof, totaal",31,"N t","L107_614N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_615","KLEINE BEEK (WUUSTWEZEL)","Stikstof, totaal",31,"N t","L107_615N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_629","KLEIN WILBOEREBEEK","Stikstof, totaal",31,"N t","L107_629N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_63","BOERGONJEVAART","Stikstof, totaal",31,"N t","L107_63N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_631","MOLENBEEK - BOLLAAK L1","Stikstof, totaal",31,"N t","L107_631N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_632","DE DELFTE BEEK","Stikstof, totaal",31,"N t","L107_632N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_633","BOSBEEK - DIEPTELOOP","Stikstof, totaal",31,"N t","L107_633N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_638","GROTE CALIE","Stikstof, totaal",31,"N t",{"$f":"_xlfn.CONCAT(A2627,E2627)","v":"L107_638N t"},"zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_640","DE AA - NATTENLOOP","Stikstof, totaal",31,"N t","L107_640N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_644","ITTERBEEK (DUFFEL)","Stikstof, totaal",31,"N t","L107_644N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_648","BRUINBEEK","Stikstof, totaal",31,"N t","L107_648N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_650","REEHAGENBEEK","Stikstof, totaal",31,"N t","L107_650N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_654","LARUMSE LOOP","Stikstof, totaal",31,"N t","L107_654N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_655","DALEMANSLOOP","Stikstof, totaal",31,"N t","L107_655N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_656","BEGGELBEEK","Stikstof, totaal",31,"N t","L107_656N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_66","KERKBEEK","Stikstof, totaal",31,"N t","L107_66N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_664","MOLENBEEK - ZIJP","Stikstof, totaal",31,"N t","L107_664N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_665","BOUWBEEK","Stikstof, totaal",31,"N t","L107_665N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_67","LIJSTERBEEK","Stikstof, totaal",31,"N t","L107_67N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_677","DIEPE BEEK","Stikstof, totaal",31,"N t","L107_677N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_681","KOUDE BEEK","Stikstof, totaal",31,"N t","L107_681N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_684","SCHOON SCHIJN","Stikstof, totaal",31,"N t","L107_684N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_688","LAARSE BEEK","Stikstof, totaal",31,"N t","L107_688N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_695","VARENDONKSE BEEK","Stikstof, totaal",31,"N t","L107_695N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_702","MILLEGEMLOOP","Stikstof, totaal",31,"N t","L107_702N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_705","SCHEPPELIJKE NETE","Stikstof, totaal",31,"N t","L107_705N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_706","MOLSE NETE L1","Stikstof, totaal",31,"N t","L107_706N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_708","GROTE NETE L1","Stikstof, totaal",31,"N t","L107_708N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_722","WAMP L1","Stikstof, totaal",31,"N t","L107_722N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_723","RODE LOOP","Stikstof, totaal",31,"N t","L107_723N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_729","STAPKENSLOOP","Stikstof, totaal",31,"N t","L107_729N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_735","GESTELBEEK","Stikstof, totaal",31,"N t","L107_735N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_740","BERGEBEEK","Stikstof, totaal",31,"N t","L107_740N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_741","SPILLEBEEK","Stikstof, totaal",31,"N t","L107_741N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_742","PLATTE BEEK","Stikstof, totaal",31,"N t","L107_742N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_78","DEVEBEEK L1","Stikstof, totaal",31,"N t","L107_78N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_8","IEPERLEE","Stikstof, totaal",31,"N t","L107_8N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_809","KLEINE HERK L1","Stikstof, totaal",31,"N t","L107_809N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_810","WINTERBEEK (KORTESSEM)","Stikstof, totaal",31,"N t","L107_810N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_812","MOMBEEK L1","Stikstof, totaal",31,"N t","L107_812N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_814","STEENLAAK","Stikstof, totaal",31,"N t","L107_814N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_82","BABILLEBEEK","Stikstof, totaal",31,"N t","L107_82N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_824","ROELBEEK","Stikstof, totaal",31,"N t","L107_824N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_83","ROOBEEK","Stikstof, totaal",31,"N t","L107_83N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_836","LAAMBEEK","Stikstof, totaal",31,"N t","L107_836N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_839","ZONDERIKBEEK","Stikstof, totaal",31,"N t","L107_839N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_84","KROMMEBEEK","Stikstof, totaal",31,"N t","L107_84N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_846","KAATSBEEK","Stikstof, totaal",31,"N t","L107_846N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_847","WINTERBEEK (BILZEN)","Stikstof, totaal",31,"N t","L107_847N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_848","DEMER L1","Stikstof, totaal",31,"N t","L107_848N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_852","MUNSTERBEEK L1","Stikstof, totaal",31,"N t","L107_852N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_853","ZUTENDAALBEEK","Stikstof, totaal",31,"N t","L107_853N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_854","BOLLISENBEEK","Stikstof, totaal",31,"N t","L107_854N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_855","DOMMEL L1","Stikstof, totaal",31,"N t","L107_855N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_856","HOLVENLOOP","Stikstof, totaal",31,"N t","L107_856N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_857","EINDERGATLOOP","Stikstof, totaal",31,"N t","L107_857N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_858","WARMBEEK L1","Stikstof, totaal",31,"N t","L107_858N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_859","PRINSENLOOP","Stikstof, totaal",31,"N t","L107_859N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_861","ABEEK L1","Stikstof, totaal",31,"N t","L107_861N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_866","LOSSING L1","Stikstof, totaal",31,"N t","L107_866N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_869","SOERBEEK","Stikstof, totaal",31,"N t","L107_869N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_876","BOSBEEK L1","Stikstof, totaal",31,"N t","L107_876N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_879","VRIETSELBEEK - OUDE MAAS (DILSEN)","Stikstof, totaal",31,"N t","L107_879N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_883","ZIEPBEEK","Stikstof, totaal",31,"N t","L107_883N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_885","HEESWATER","Stikstof, totaal",31,"N t","L107_885N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_890","BEEK - DE BUTH (TONGEREN)","Stikstof, totaal",31,"N t","L107_890N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_891","VOER (VOEREN)","Stikstof, totaal",31,"N t","L107_891N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_892","BEEK (VOEREN)","Stikstof, totaal",31,"N t","L107_892N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_893","GULP","Stikstof, totaal",31,"N t","L107_893N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_91","PLAATSBEEK","Stikstof, totaal",31,"N t","L107_91N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_92","MAALBEEK (LEIEBEKKEN)","Stikstof, totaal",31,"N t","L107_92N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_97","KASSELRIJBEEK - WEST","Stikstof, totaal",31,"N t",{"$f":"_xlfn.CONCAT(A2691,E2691)","v":"L107_97N t"},"zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_98","GAVERBEEK","Stikstof, totaal",31,"N t","L107_98N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L110_1100","ZILVERBEEK","Stikstof, totaal",31,"N t","L110_1100N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1001","MARTJEVAART - LEKKERBOTERBEEK","Stikstof, totaal",31,"N t","L111_1001N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1003","GELUWEBEEK","Stikstof, totaal",31,"N t","L111_1003N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1004","RIJTGRACHT","Stikstof, totaal",31,"N t","L111_1004N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1005","KALSIJDEADER","Stikstof, totaal",31,"N t","L111_1005N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1006","HOOFDSLOOT","Stikstof, totaal",31,"N t","L111_1006N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1007","STEGERSZWIN","Stikstof, totaal",31,"N t","L111_1007N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1010","OOSTKERKEVAART","Stikstof, totaal",31,"N t","L111_1010N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1011","BOEREKREEK","Stikstof, totaal",31,"N t","L111_1011N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1014","MEREBEEK","Stikstof, totaal",31,"N t","L111_1014N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1015","OUDE AVAART","Stikstof, totaal",31,"N t","L111_1015N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1016","WANTEBEEK","Stikstof, totaal",31,"N t","L111_1016N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1018","LEEBEEK","Stikstof, totaal",31,"N t","L111_1018N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1019","MOLENBEEK - MARKEBEEK","Stikstof, totaal",31,"N t","L111_1019N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1020","OOSSEBEEK","Stikstof, totaal",31,"N t","L111_1020N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1021","ZWALMBEEK","Stikstof, totaal",31,"N t","L111_1021N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1022","MOLENBEEK (RONSE)","Stikstof, totaal",31,"N t","L111_1022N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1024","BAVEGEMSE BEEK","Stikstof, totaal",31,"N t","L111_1024N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1025","MAANBEEK","Stikstof, totaal",31,"N t","L111_1025N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1027","GROOTEBEEK","Stikstof, totaal",31,"N t","L111_1027N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1028","LANGELEDE","Stikstof, totaal",31,"N t","L111_1028N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1029","KLEINE WATERGANG","Stikstof, totaal",31,"N t","L111_1029N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1030","WATERGANG VAN DE MOERBEKEPOLDER","Stikstof, totaal",31,"N t","L111_1030N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1031","KANAAL VAN STEKENE","Stikstof, totaal",31,"N t","L111_1031N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1032","DIJKGRACHT","Stikstof, totaal",31,"N t","L111_1032N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1033","PAPENMEERSBEEK","Stikstof, totaal",31,"N t","L111_1033N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1034","NIEUWE GRACHT","Stikstof, totaal",31,"N t","L111_1034N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1035","KOEVAARDEKEN","Stikstof, totaal",31,"N t","L111_1035N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1037","MOLENBEEK - LAKEBEEK","Stikstof, totaal",31,"N t","L111_1037N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1038","MAALBEEK - AMELVONNEBEEK","Stikstof, totaal",31,"N t","L111_1038N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1039","STEENVOORDBEEK (TERNAT)","Stikstof, totaal",31,"N t","L111_1039N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1040","BELLEBEEK L1","Stikstof, totaal",31,"N t","L111_1040N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1041","WINGE L1","Stikstof, totaal",31,"N t","L111_1041N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1042","LEIBEEK - LIPSEBEEK L1","Stikstof, totaal",31,"N t","L111_1042N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1043","WEESBEEK L1","Stikstof, totaal",31,"N t","L111_1043N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1044","KASTEELBEEK","Stikstof, totaal",31,"N t","L111_1044N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1046","GROTE MOTTE","Stikstof, totaal",31,"N t","L111_1046N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1047","BAREBEEK L1","Stikstof, totaal",31,"N t","L111_1047N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1048","ZIJDELINGSGELEED","Stikstof, totaal",31,"N t","L111_1048N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1049","MUNTLOOP","Stikstof, totaal",31,"N t","L111_1049N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1050","WEHAGENBEEK","Stikstof, totaal",31,"N t","L111_1050N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1052","LAAKBEEK","Stikstof, totaal",31,"N t","L111_1052N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1053","MOUBEEK","Stikstof, totaal",31,"N t","L111_1053N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1054","GOORBOSBEEK","Stikstof, totaal",31,"N t","L111_1054N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1056","VROUWVLIET L1","Stikstof, totaal",31,"N t","L111_1056N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1057","GROTE MOLENBEEK L1","Stikstof, totaal",31,"N t","L111_1057N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1058","ZWARTE BEEK (WILLEBROEK)","Stikstof, totaal",31,"N t","L111_1058N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1059","ZIELBEEK - BOSBEEK L1","Stikstof, totaal",31,"N t","L111_1059N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1060","GROOT SCHIJN L1","Stikstof, totaal",31,"N t","L111_1060N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1062","HERSELTSELOOP","Stikstof, totaal",31,"N t","L111_1062N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1063","STEENKENSBEEK","Stikstof, totaal",31,"N t","L111_1063N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1064","ST. TRUDOLEKEN","Stikstof, totaal",31,"N t","L111_1064N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1065","ASBEEK","Stikstof, totaal",31,"N t","L111_1065N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1066","LOEIJENS NEETJE","Stikstof, totaal",31,"N t","L111_1066N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1067","KLEINE NETE L1","Stikstof, totaal",31,"N t","L111_1067N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1069","AFWATERINGSGRACHT","Stikstof, totaal",31,"N t","L111_1069N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1070","WIMP L1","Stikstof, totaal",31,"N t","L111_1070N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1071","GOORLOOP","Stikstof, totaal",31,"N t","L111_1071N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1072","POVERSBEEK","Stikstof, totaal",31,"N t","L111_1072N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1075","MELSTERBEEK L1","Stikstof, totaal",31,"N t","L111_1075N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1076","CICINDRIA","Stikstof, totaal",31,"N t","L111_1076N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1077","MOLENBEEK (SINT-TRUIDEN)","Stikstof, totaal",31,"N t","L111_1077N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1078","GRONDBEEK","Stikstof, totaal",31,"N t",{"$f":"_xlfn.CONCAT(A2755,E2755)","v":"L111_1078N t"},"zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1079","HELDERBEEK","Stikstof, totaal",31,"N t","L111_1079N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1080","ZWARTEBEEK L1","Stikstof, totaal",31,"N t","L111_1080N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1081","MANGELBEEK L1","Stikstof, totaal",31,"N t","L111_1081N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1082","SLANGBEEK","Stikstof, totaal",31,"N t","L111_1082N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1083","MISERIKBEEK","Stikstof, totaal",31,"N t","L111_1083N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1084","MANDEL L1","Stikstof, totaal",31,"N t","L111_1084N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1086","LOZERBROEKBEEK","Stikstof, totaal",31,"N t","L111_1086N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1087","HORSTGATERBEEK","Stikstof, totaal",31,"N t","L111_1087N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1088","ITTERBEEK L1","Stikstof, totaal",31,"N t","L111_1088N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1089","WITBEEK","Stikstof, totaal",31,"N t","L111_1089N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1090","ZANDERBEEK","Stikstof, totaal",31,"N t","L111_1090N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1091","KIKBEEK","Stikstof, totaal",31,"N t","L111_1091N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1092","ZOUW","Stikstof, totaal",31,"N t","L111_1092N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1093","EZELSBEEK","Stikstof, totaal",31,"N t","L111_1093N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1094","HEULEBEEK L1","Stikstof, totaal",31,"N t","L111_1094N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1095","KLEINE LAAK","Stikstof, totaal",31,"N t","L111_1095N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1096","GROTE LAAK L1","Stikstof, totaal",31,"N t","L111_1096N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1098","KEIBEEK","Stikstof, totaal",31,"N t","L111_1098N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1099","GAVERSE BEEK (BECQUE DE NEUVILLE)","Stikstof, totaal",31,"N t","L111_1099N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1101","GROTE KEIGNAERT","Stikstof, totaal",31,"N t","L111_1101N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1102","KLEINE A - WILDERTSE BEEK","Stikstof, totaal",31,"N t","L111_1102N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1104","DESPIERREBEEK","Stikstof, totaal",31,"N t","L111_1104N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1105","MELSENBEEK","Stikstof, totaal",31,"N t","L111_1105N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1106","DONKSE BEEK","Stikstof, totaal",31,"N t","L111_1106N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1107","SLIJKVAART","Stikstof, totaal",31,"N t","L111_1107N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1108","STEENGRACHT","Stikstof, totaal",31,"N t","L111_1108N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1109","MOERDIJKVAART L1","Stikstof, totaal",31,"N t","L111_1109N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1110","EDE","Stikstof, totaal",31,"N t","L111_1110N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1111","GELEEDBEEK - PASSENDALEGELEED","Stikstof, totaal",31,"N t","L111_1111N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1112","ISABELLASTROOM","Stikstof, totaal",31,"N t","L111_1112N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1113","LACHENEBEEK","Stikstof, totaal",31,"N t","L111_1113N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1114","ANTITANKGRACHT ZUID","Stikstof, totaal",31,"N t","L111_1114N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_1201","S HERTOGENDIJKSE BEEK","Stikstof, totaal",31,"N t","L111_1201N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_15","HEIDEBEEK (VLETEREN)","Stikstof, totaal",31,"N t","L111_15N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_18","ST-MACHUITSBEEK","Stikstof, totaal",31,"N t","L111_18N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_298","OUDE DENDER","Stikstof, totaal",31,"N t","L111_298N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_315","FONDATIEGRACHT","Stikstof, totaal",31,"N t","L111_315N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_326","BARBIERBEEK","Stikstof, totaal",31,"N t","L111_326N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_419","SCHOORBROEKBEEK","Stikstof, totaal",31,"N t","L111_419N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_436","VELPE L1","Stikstof, totaal",31,"N t","L111_436N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_624","TAPPELBEEK","Stikstof, totaal",31,"N t","L111_624N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_627","KLEINE BEEK (ZANDHOVEN)","Stikstof, totaal",31,"N t","L111_627N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_639","VISBEEK","Stikstof, totaal",31,"N t","L111_639N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_674","BENEDENVLIET L1","Stikstof, totaal",31,"N t","L111_674N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_676","WEZELSE BEEK","Stikstof, totaal",31,"N t","L111_676N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_699","SCHERPENBERGLOOP","Stikstof, totaal",31,"N t","L111_699N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_707","KLEINE HOOFDGRACHT","Stikstof, totaal",31,"N t","L111_707N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_717","DESSELSE NEET","Stikstof, totaal",31,"N t","L111_717N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_724","ANTITANKGRACHT NOORD","Stikstof, totaal",31,"N t","L111_724N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L111_844","STIEMER","Stikstof, totaal",31,"N t","L111_844N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L117_1036","ZUUNBEEK L1","Stikstof, totaal",31,"N t","L117_1036N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L117_1068","HERTSBERGEBEEK - GETEBEEK","Stikstof, totaal",31,"N t","L117_1068N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L117_1073","RIVIERBEEK","Stikstof, totaal",31,"N t","L117_1073N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L117_1074","HERK L1","Stikstof, totaal",31,"N t","L117_1074N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L117_1085","WILDERBEEK","Stikstof, totaal",31,"N t","L117_1085N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L117_17","STEENVOORDEBEEK (WATOU)","Stikstof, totaal",31,"N t","L117_17N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L117_219","BURGGRAVENSTROOM","Stikstof, totaal",31,"N t","L117_219N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L117_232","JOBEEK","Stikstof, totaal",31,"N t","L117_232N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L117_233","RINGBEEK","Stikstof, totaal",31,"N t","L117_233N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L117_402","MOLENBEEK - SLAGVIJVERBEEK","Stikstof, totaal",31,"N t","L117_402N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L117_659","KREKELBEEK","Stikstof, totaal",31,"N t","L117_659N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L117_673","KLEIN SCHIJN (NOORDELIJK DEEL)","Stikstof, totaal",31,"N t","L117_673N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L117_813","HERKEBEEK","Stikstof, totaal",31,"N t","L117_813N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L118_238","KROMMEDIJKBEEK","Stikstof, totaal",31,"N t",{"$f":"_xlfn.CONCAT(A2819,E2819)","v":"L118_238N t"},"zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L119_675","KLEIN SCHIJN (ZUIDELIJK DEEL)","Stikstof, totaal",31,"N t","L119_675N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L120_1097","KASSELRIJBEEK - OOST","Stikstof, totaal",31,"N t","L120_1097N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L121_1045","GROTEBEEK - WINTERBEEK","Stikstof, totaal",31,"N t","L121_1045N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L2 Bk","L2 Kleine Beek","Stikstof, totaal",31,"N t","L2 BkN t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L2 Bk","L2 kleine beek","Stikstof, totaal",31,"N t","L2 BkN t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_102","DEMER V","Stikstof, totaal",31,"N t","VL05_102N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_103","DEMER VI","Stikstof, totaal",31,"N t","VL05_103N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_104","DEMER VII","Stikstof, totaal",31,"N t","VL05_104N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_105","GETE I","Stikstof, totaal",31,"N t","VL05_105N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_106","GETE II","Stikstof, totaal",31,"N t","VL05_106N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_108","HERK + KLEINE HERK","Stikstof, totaal",31,"N t","VL05_108N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_110","MANGELBEEK","Stikstof, totaal",31,"N t","VL05_110N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_113","MOMBEEK","Stikstof, totaal",31,"N t","VL05_113N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_114","MUNSTERBEEK","Stikstof, totaal",31,"N t","VL05_114N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_115","VELPE","Stikstof, totaal",31,"N t","VL05_115N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_116","WINGE","Stikstof, totaal",31,"N t","VL05_116N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_118","ZWARTWATER","Stikstof, totaal",31,"N t","VL05_118N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_119","VINNE","Stikstof, totaal",31,"N t","VL05_119N t","zomergemiddelde (apr-sept)","mgN/L",1.3,"jaargemiddelde",1.3,1.3,1.9,2.6]
["VL05_12","POPERINGEVAART","Stikstof, totaal",31,"N t","VL05_12N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_121","AA II","Stikstof, totaal",31,"N t","VL05_121N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_122","GROTE LAAK","Stikstof, totaal",31,"N t","VL05_122N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_124","GROTE NETE II","Stikstof, totaal",31,"N t","VL05_124N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_130","WAMP","Stikstof, totaal",31,"N t","VL05_130N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_131","WIMP","Stikstof, totaal",31,"N t","VL05_131N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_134","BERWIJN","Stikstof, totaal",31,"N t","VL05_134N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_135","BOSBEEK","Stikstof, totaal",31,"N t","VL05_135N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_136","DOMMEL","Stikstof, totaal",31,"N t","VL05_136N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_137","ITTERBEEK I","Stikstof, totaal",31,"N t","VL05_137N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_138","ITTERBEEK II","Stikstof, totaal",31,"N t","VL05_138N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_14","VLADSLOVAART","Stikstof, totaal",31,"N t","VL05_14N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_140","JEKER II","Stikstof, totaal",31,"N t","VL05_140N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_141","LOSSING","Stikstof, totaal",31,"N t","VL05_141N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_146","MERKSKE","Stikstof, totaal",31,"N t","VL05_146N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_148","WEERIJSEBEEK","Stikstof, totaal",31,"N t","VL05_148N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_150","AFLEIDINGSKANAAL van de LEIE/SCHIPDONKKANAAL I","Stikstof, totaal",31,"N t","VL05_150N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_152","AVRIJEVAART + SLEIDINGSVAARDEKE","Stikstof, totaal",31,"N t","VL05_152N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_153","BERGENVAART","Stikstof, totaal",31,"N t","VL05_153N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_159","KANAAL CHARLEROI-BRUSSEL","Stikstof, totaal",31,"N t","VL05_159N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_163","KANAAL GENT-OOSTENDE II","Stikstof, totaal",31,"N t","VL05_163N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_166","KANAAL IEPER-IJZER","Stikstof, totaal",31,"N t","VL05_166N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_167","KANAAL LEUVEN-DIJLE","Stikstof, totaal",31,"N t","VL05_167N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_17","ISABELLAVAART","Stikstof, totaal",31,"N t","VL05_17N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_170","KANAAL VAN BEVERLO","Stikstof, totaal",31,"N t","VL05_170N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_171","LEDE","Stikstof, totaal",31,"N t","VL05_171N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_175","MOERVAART","Stikstof, totaal",31,"N t","VL05_175N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_177","NIEUWE KALE","Stikstof, totaal",31,"N t","VL05_177N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_18","KERKEBEEK","Stikstof, totaal",31,"N t","VL05_18N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_180","ZARRENBEEK","Stikstof, totaal",31,"N t","VL05_180N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_182","ZUIDLEDE","Stikstof, totaal",31,"N t","VL05_182N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_191","DESSELSE ZANDPUTTEN","Stikstof, totaal",31,"N t","VL05_191N t","zomergemiddelde (apr-sept)","mgN/L",1,"jaargemiddelde",1,1,1.1000000000000001,1.4]
["VL05_192","DONKMEER","Stikstof, totaal",31,"N t","VL05_192N t","zomergemiddelde (apr-sept)","mgN/L",1.3,"jaargemiddelde",1.3,1.3,1.9,2.6]
["VL05_195","GAVERS HARELBEKE","Stikstof, totaal",31,"N t","VL05_195N t","zomergemiddelde (apr-sept)","mgN/L",1.3,"jaargemiddelde",1.3,1.3,1.9,2.6]
["VL05_196","GRINDPLAS KESSENICH","Stikstof, totaal",31,"N t","VL05_196N t","zomergemiddelde (apr-sept)","mgN/L",1.3,"jaargemiddelde",1.3,1.3,1.9,2.6]
["VL05_2","GROTE KEMMELBEEK","Stikstof, totaal",31,"N t","VL05_2N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_20","RIVIERBEEK + HERTSBERGEBEEK","Stikstof, totaal",31,"N t","VL05_20N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_200","SCHULENSMEER","Stikstof, totaal",31,"N t","VL05_200N t","zomergemiddelde (apr-sept)","mgN/L",1.3,"jaargemiddelde",1.3,1.3,1.9,2.6]
["VL05_201","SPAANJERD + HEERENLAAK","Stikstof, totaal",31,"N t","VL05_201N t","zomergemiddelde (apr-sept)","mgN/L",1.3,"jaargemiddelde",1.3,1.3,1.9,2.6]
["VL05_202","SPUIKOM OOSTENDE","Stikstof, totaal",31,"N t","VL05_202N t","zomergemiddelde (apr-sept)","mgN/L",1.8,"jaargemiddelde",1.8,1.8,2.9,4.0999999999999996]
["VL05_21","ZUIDERVAARTJE","Stikstof, totaal",31,"N t","VL05_21N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_22","ZWINNEVAART","Stikstof, totaal",31,"N t","VL05_22N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_24","MEREBEEK + BORISGRACHT + LIEVE","Stikstof, totaal",31,"N t","VL05_24N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_25","OUDE KALE","Stikstof, totaal",31,"N t","VL05_25N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_28","BENEDENVLIET","Stikstof, totaal",31,"N t","VL05_28N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_3","HANDZAMEVAART","Stikstof, totaal",31,"N t",{"$f":"_xlfn.CONCAT(A2883,E2883)","v":"VL05_3N t"},"zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_30","GROTE MOLENBEEK - DE VLIET","Stikstof, totaal",31,"N t","VL05_30N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_31","KALKENSE VAART","Stikstof, totaal",31,"N t","VL05_31N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_32","MOLENBEEK - GROTE BEEK","Stikstof, totaal",31,"N t","VL05_32N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_34","NOORD-ZUIDVERBINDING","Stikstof, totaal",31,"N t","VL05_34N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_38","ZIELBEEK - BOSBEEK","Stikstof, totaal",31,"N t","VL05_38N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_4","HEIDEBEEK","Stikstof, totaal",31,"N t","VL05_4N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_44","DEVEBEEK","Stikstof, totaal",31,"N t","VL05_44N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_45","GAVERBEEK I","Stikstof, totaal",31,"N t","VL05_45N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_46","GAVERBEEK II","Stikstof, totaal",31,"N t","VL05_46N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_5","IEPERLEE + VERWEZEN KANAAL IEPER-KOMEN","Stikstof, totaal",31,"N t","VL05_5N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_50","LEIE III","Stikstof, totaal",31,"N t","VL05_50N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_51","MANDEL I","Stikstof, totaal",31,"N t","VL05_51N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_52","MANDEL II","Stikstof, totaal",31,"N t","VL05_52N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_53","OUDE MANDEL","Stikstof, totaal",31,"N t","VL05_53N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_58","BOVEN-SCHELDE IV","Stikstof, totaal",31,"N t","VL05_58N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_6","IEPERLEED","Stikstof, totaal",31,"N t","VL05_6N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_61","RONE","Stikstof, totaal",31,"N t","VL05_61N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_62","STAMPKOTBEEK","Stikstof, totaal",31,"N t","VL05_62N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_64","ZWARTE SPIEREBEEK","Stikstof, totaal",31,"N t","VL05_64N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_67","DENDER I","Stikstof, totaal",31,"N t","VL05_67N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_70","DENDER IV","Stikstof, totaal",31,"N t","VL05_70N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_73","MOLENBEEK - PACHTBOSBEEK","Stikstof, totaal",31,"N t","VL05_73N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_75","VONDELBEEK","Stikstof, totaal",31,"N t","VL05_75N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_77","DIJLE I","Stikstof, totaal",31,"N t","VL05_77N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_81","DIJLE V","Stikstof, totaal",31,"N t","VL05_81N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_85","LEIBEEK - LAAKBEEK","Stikstof, totaal",31,"N t","VL05_85N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_86","NETHEN","Stikstof, totaal",31,"N t","VL05_86N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_87","VOER (Leuven)","Stikstof, totaal",31,"N t","VL05_87N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_89","VUNT","Stikstof, totaal",31,"N t","VL05_89N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_90","WEESBEEK","Stikstof, totaal",31,"N t","VL05_90N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_93","ZENNE II","Stikstof, totaal",31,"N t","VL05_93N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL05_98","DEMER I","Stikstof, totaal",31,"N t","VL05_98N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL05_99","DEMER II","Stikstof, totaal",31,"N t","VL05_99N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL08_125","GROTE NETE III","Stikstof, totaal",31,"N t","VL08_125N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL08_132","GETIJDENETES","Stikstof, totaal",31,"N t","VL08_132N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL08_157","ISABELLAWATERING","Stikstof, totaal",31,"N t","VL08_157N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL08_16","BLANKENBERGSE VAART + NOORDEDE","Stikstof, totaal",31,"N t","VL08_16N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL08_162","KANAAL GENT-OOSTENDE I + COUPURE + VERBINDINGSKANAAL","Stikstof, totaal",31,"N t","VL08_162N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL08_164","KANAAL GENT-OOSTENDE III","Stikstof, totaal",31,"N t","VL08_164N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL08_172","LEOPOLDKANAAL I","Stikstof, totaal",31,"N t","VL08_172N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL08_173","LEOPOLDKANAAL II","Stikstof, totaal",31,"N t","VL08_173N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL08_176","NETEKANAAL","Stikstof, totaal",31,"N t","VL08_176N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL08_178","NOORDELIJKE RINGVAART","Stikstof, totaal",31,"N t","VL08_178N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL08_179","WESTELIJKE RINGVAART","Stikstof, totaal",31,"N t","VL08_179N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL08_27","ZWARTESLUISBEEK","Stikstof, totaal",31,"N t","VL08_27N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL08_39","GETIJDEDURME","Stikstof, totaal",31,"N t","VL08_39N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL08_41","ZEESCHELDE II","Stikstof, totaal",31,"N t","VL08_41N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL08_55","BOVEN-SCHELDE I","Stikstof, totaal",31,"N t","VL08_55N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL08_7","IJZER I","Stikstof, totaal",31,"N t","VL08_7N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL08_71","DENDER V","Stikstof, totaal",31,"N t","VL08_71N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL08_72","MARK (Denderbekken)","Stikstof, totaal",31,"N t","VL08_72N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL08_80","DIJLE IV","Stikstof, totaal",31,"N t","VL08_80N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL08_82","DIJLE VI","Stikstof, totaal",31,"N t","VL08_82N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL08_92","ZENNE I","Stikstof, totaal",31,"N t","VL08_92N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL08_95","GETIJDEDIJLE & GETIJDEZENNE","Stikstof, totaal",31,"N t","VL08_95N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL09_78","DIJLE II","Stikstof, totaal",31,"N t","VL09_78N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL11_10","MARTJEVAART","Stikstof, totaal",31,"N t","VL11_10N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_109","KLEINE GETE + VLOEDGRACHT","Stikstof, totaal",31,"N t","VL11_109N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_11","MOERDIJKVAART","Stikstof, totaal",31,"N t","VL11_11N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_117","ZWARTEBEEK","Stikstof, totaal",31,"N t","VL11_117N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_120","AA I","Stikstof, totaal",31,"N t","VL11_120N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_123","GROTE NETE I","Stikstof, totaal",31,"N t","VL11_123N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_126","KLEINE NETE I","Stikstof, totaal",31,"N t","VL11_126N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_127","KLEINE NETE II","Stikstof, totaal",31,"N t",{"$f":"_xlfn.CONCAT(A2947,E2947)","v":"VL11_127N t"},"zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_128","MOL NEET","Stikstof, totaal",31,"N t","VL11_128N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_13","VEURNE AMBACHT POLDER WATERLOPEN","Stikstof, totaal",31,"N t","VL11_13N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_133","ABEEK","Stikstof, totaal",31,"N t","VL11_133N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_145","MARK (Maas)","Stikstof, totaal",31,"N t","VL11_145N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_155","BRUGSE REIEN","Stikstof, totaal",31,"N t","VL11_155N t","zomergemiddelde (apr-sept)","mgN/L",1.3,"jaargemiddelde",1.3,1.3,1.9,2.6]
["VL11_165","KANAAL GENT-TERNEUZEN + GENTSE HAVENDOKKEN","Stikstof, totaal",31,"N t","VL11_165N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL11_19","OOSTENDS KREKENGEBIED","Stikstof, totaal",31,"N t","VL11_19N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_203","MAAS I+II+III","Stikstof, totaal",31,"N t","VL11_203N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL11_205","DEMER III+IV","Stikstof, totaal",31,"N t","VL11_205N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_207","MELSTERBEEK I+II","Stikstof, totaal",31,"N t","VL11_207N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_37","WATERLOOP VAN DE HOGE LANDEN + MELKADER","Stikstof, totaal",31,"N t","VL11_37N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_40","ZEESCHELDE I","Stikstof, totaal",31,"N t","VL11_40N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL11_59","GROTE SPIEREBEEK","Stikstof, totaal",31,"N t","VL11_59N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_63","ZWALM","Stikstof, totaal",31,"N t","VL11_63N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_76","BAREBEEK","Stikstof, totaal",31,"N t","VL11_76N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_83","IJSSE","Stikstof, totaal",31,"N t","VL11_83N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_84","LAAN","Stikstof, totaal",31,"N t","VL11_84N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_88","VROUWVLIET","Stikstof, totaal",31,"N t","VL11_88N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL11_91","WOLUWE","Stikstof, totaal",31,"N t","VL11_91N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL17_147","WARMBEEK","Stikstof, totaal",31,"N t","VL17_147N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL17_154","BRAKELEIKEN + LIEVE","Stikstof, totaal",31,"N t","VL17_154N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL17_156","GENTSE BINNENWATEREN","Stikstof, totaal",31,"N t","VL17_156N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL17_161","KANAAL DUINKERKE-NIEUWPOORT","Stikstof, totaal",31,"N t","VL17_161N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL17_168","KANAAL PLASSENDALE-NIEUWPOORT","Stikstof, totaal",31,"N t","VL17_168N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL17_169","KANAAL ROESELARE-LEIE","Stikstof, totaal",31,"N t","VL17_169N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL17_174","LOKANAAL","Stikstof, totaal",31,"N t","VL17_174N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL17_187","ANTWERPSE HAVENDOKKEN + SCHELDE-RIJNVERBINDING","Stikstof, totaal",31,"N t","VL17_187N t","zomergemiddelde (apr-sept)","mgN/L",1.8,"jaargemiddelde",1.8,1.8,2.9,4.0999999999999996]
["VL17_190","BOUDEWIJNKANAAL + ACHTERHAVEN ZEEBRUGGE","Stikstof, totaal",31,"N t","VL17_190N t","zomergemiddelde (apr-sept)","mgN/L",1.8,"jaargemiddelde",1.8,1.8,2.9,4.0999999999999996]
["VL17_204","BOVEN-SCHELDE II+III","Stikstof, totaal",31,"N t","VL17_204N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL17_206","DENDER II+III","Stikstof, totaal",31,"N t","VL17_206N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL17_29","GROOT SCHIJN","Stikstof, totaal",31,"N t","VL17_29N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL17_35","VERLEGDE SCHIJN - HOOFDGRACHT","Stikstof, totaal",31,"N t","VL17_35N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL17_42","ZEESCHELDE III + RUPEL","Stikstof, totaal",31,"N t","VL17_42N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL17_43","ZEESCHELDE IV","Stikstof, totaal",31,"N t","VL17_43N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL17_48","LEIE I","Stikstof, totaal",31,"N t","VL17_48N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL17_49","LEIE II","Stikstof, totaal",31,"N t","VL17_49N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL17_54","TOERISTISCHE LEIE","Stikstof, totaal",31,"N t","VL17_54N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL17_60","MOLENBEEK - MAARKEBEEK","Stikstof, totaal",31,"N t","VL17_60N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL17_66","BELLEBEEK","Stikstof, totaal",31,"N t","VL17_66N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL17_9","IJZER III","Stikstof, totaal",31,"N t","VL17_9N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL20_36","VERLEGDE SCHIJN - VOORGRACHT","Stikstof, totaal",31,"N t","VL20_36N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL20_96","BEGIJNENBEEK","Stikstof, totaal",31,"N t","VL20_96N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL21_1","BLANKAART WATERLOPEN","Stikstof, totaal",31,"N t","VL21_1N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL21_107","GROTE GETE + BORGGRACHT","Stikstof, totaal",31,"N t","VL21_107N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL21_129","MOLENBEEK - BOLLAAK","Stikstof, totaal",31,"N t","VL21_129N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL21_139","JEKER I","Stikstof, totaal",31,"N t","VL21_139N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL21_26","POEKEBEEK","Stikstof, totaal",31,"N t","VL21_26N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL21_33","MOLENBEEK - KOTTEMBEEK","Stikstof, totaal",31,"N t","VL21_33N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL21_47","HEULEBEEK","Stikstof, totaal",31,"N t","VL21_47N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL21_74","MOLENBEEK - TER ERPENBEEK","Stikstof, totaal",31,"N t","VL21_74N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL21_79","DIJLE III","Stikstof, totaal",31,"N t","VL21_79N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL21_8","IJZER II","Stikstof, totaal",31,"N t","VL21_8N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL21_94","ZUUNBEEK","Stikstof, totaal",31,"N t","VL21_94N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL21_97","DE HULPE - ZWART WATER","Stikstof, totaal",31,"N t","VL21_97N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["VL22_208","ALBERTKANAAL - Maasbekken","Stikstof, totaal",31,"N t","VL22_208N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL22_209","ALBERTKANAAL - Demerbekken","Stikstof, totaal",31,"N t","VL22_209N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL22_210","ALBERTKANAAL - Netebekken","Stikstof, totaal",31,"N t","VL22_210N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL22_211","ALBERTKANAAL - Benedenscheldebekken","Stikstof, totaal",31,"N t","VL22_211N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL22_212","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Netebekken","Stikstof, totaal",31,"N t","VL22_212N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL22_213","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Maasbekken","Stikstof, totaal",31,"N t","VL22_213N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL22_214","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Benedenscheldebekken","Stikstof, totaal",31,"N t","VL22_214N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL22_215","ZEEKANAAL BRUSSEL-SCHELDE - Dijle-Zennebekken","Stikstof, totaal",31,"N t","VL22_215N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL22_216","ZEEKANAAL BRUSSEL-SCHELDE - Benedenscheldebekken","Stikstof, totaal",31,"N t","VL22_216N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL22_217","AFLEIDINGSKANAAL van de LEIE II + KANAAL van EEKLO - Bekken van de Gentse kanalen","Stikstof, totaal",31,"N t",{"$f":"_xlfn.CONCAT(A3011,E3011)","v":"VL22_217N t"},"zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL22_218","AFLEIDINGSKANAAL van de LEIE II - Bekken van de Brugse polders","Stikstof, totaal",31,"N t","VL22_218N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL22_219","KANAAL BOSSUIT-KORTRIJK - Bovenscheldebekken","Stikstof, totaal",31,"N t","VL22_219N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL22_220","KANAAL BOSSUIT-KORTRIJK - Leiebekken","Stikstof, totaal",31,"N t","VL22_220N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["VL22_221","ZUID-WILLEMSVAART + KANAAL BOCHOLT-HERENTALS (deels) + KANAAL BRIEGDEN-NEERHAREN","Stikstof, totaal",31,"N t","VL22_221N t","zomergemiddelde (apr-sept)","mgN/L",2.5,"jaargemiddelde",2.5,2.5,5,7.5]
["L107_10","KEMMELBEEK","Sulfaat",14,"SO4=","L107_10SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_104","NEERBEEK","Sulfaat",14,"SO4=","L107_104SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_105","PALINGBEEK","Sulfaat",14,"SO4=","L107_105SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_11","WANEBEEK","Sulfaat",14,"SO4=","L107_11SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_112","LA HAUTE PLANCHE","Sulfaat",14,"SO4=","L107_112SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_113","DOUVEBEEK","Sulfaat",14,"SO4=","L107_113SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_116","GROTE SPIERE","Sulfaat",14,"SO4=","L107_116SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_12","VLETERBEEK","Sulfaat",14,"SO4=","L107_12SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_120","SCHEEBEEK","Sulfaat",14,"SO4=","L107_120SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_123","KANAAL VAN BRUGGE NAAR SLUIS","Sulfaat",14,"SO4=","L107_123SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["L107_135","JABBEEKSE BEEK","Sulfaat",14,"SO4=","L107_135SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_136","HOGE WATERING","Sulfaat",14,"SO4=","L107_136SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["L107_16","HARINGEBEEK","Sulfaat",14,"SO4=","L107_16SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_209","ZWARTESLUISBEEK L1","Sulfaat",14,"SO4=","L107_209SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["L107_218","SLEIDINGSVAARDEKEN","Sulfaat",14,"SO4=","L107_218SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_225","KEUTELBEEK","Sulfaat",14,"SO4=","L107_225SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_234","POEKEBEEK L1","Sulfaat",14,"SO4=","L107_234SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_235","REIGERBEEK","Sulfaat",14,"SO4=","L107_235SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_236","NEERSCHUURBEEK","Sulfaat",14,"SO4=","L107_236SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_237","SPEIBEEK","Sulfaat",14,"SO4=","L107_237SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_239","OUDE MANDEL L1","Sulfaat",14,"SO4=","L107_239SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_240","ZOUBEEK","Sulfaat",14,"SO4=","L107_240SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_241","KATTEBEEK","Sulfaat",14,"SO4=","L107_241SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_242","DUIVEBEEK","Sulfaat",14,"SO4=","L107_242SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_246","STAMPKOTBEEK - MOLENBEEK","Sulfaat",14,"SO4=","L107_246SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_247","STAMPKOTBEEK - WALLEBEEK","Sulfaat",14,"SO4=","L107_247SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_253","STAMPKOTBEEK - MUNKBOSBEEK","Sulfaat",14,"SO4=","L107_253SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_254","MOLENBEEK - BEIAARDBEEK","Sulfaat",14,"SO4=","L107_254SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_266","PEERDESTOKBEEK","Sulfaat",14,"SO4=","L107_266SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_272","OPHASSELTBEEK","Sulfaat",14,"SO4=","L107_272SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_273","MOLENBEEK - PACHTBOSBEEK L1","Sulfaat",14,"SO4=","L107_273SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_274","MOLENBEEK - KALSTERBEEK","Sulfaat",14,"SO4=","L107_274SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_275","TER ERPENBEEK","Sulfaat",14,"SO4=","L107_275SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_276","MOLENBEEK - GRAADBEEK","Sulfaat",14,"SO4=","L107_276SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_277","WILDEBEEK","Sulfaat",14,"SO4=","L107_277SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_279","MOLENBEEK - VOGELENZANGBEEK","Sulfaat",14,"SO4=","L107_279SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_282","MOLENBEEK - GONDEBEEK","Sulfaat",14,"SO4=","L107_282SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_287","MOLENBEEK - GROTE BEEK","Sulfaat",14,"SO4=","L107_287SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_289","DAMSLOOT","Sulfaat",14,"SO4=","L107_289SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_296","VOORSTESLOOT","Sulfaat",14,"SO4=","L107_296SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_299","VONDELBEEK L1","Sulfaat",14,"SO4=","L107_299SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_3","BROENBEEK","Sulfaat",14,"SO4=","L107_3SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_305","ZELEBEEK","Sulfaat",14,"SO4=","L107_305SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_325","GROTE ASTBEEK","Sulfaat",14,"SO4=","L107_325SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_329","BLOKSTRAATBEEK","Sulfaat",14,"SO4=","L107_329SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["L107_330","WATERLOOP VAN DE HOGE LANDEN L1","Sulfaat",14,"SO4=","L107_330SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_335","MOLENBEEK - BEVERBEEK","Sulfaat",14,"SO4=","L107_335SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_336","DE RIJT","Sulfaat",14,"SO4=","L107_336SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_4","KORVERSBEEK","Sulfaat",14,"SO4=","L107_4SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_40","STENENSLUISVAART","Sulfaat",14,"SO4=","L107_40SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["L107_403","MOLENBEEK - NEERPEDEBEEK","Sulfaat",14,"SO4=","L107_403SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_404","LOTBEEK","Sulfaat",14,"SO4=","L107_404SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_407","GROEBENGRACHT","Sulfaat",14,"SO4=","L107_407SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_409","KLEINE MAALBEEK","Sulfaat",14,"SO4=","L107_409SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_411","MOLENBEEK - PARKBEEK","Sulfaat",14,"SO4=","L107_411SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_413","TANGEBEEK","Sulfaat",14,"SO4=","L107_413SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_417","DE GROTE LAAK","Sulfaat",14,"SO4=","L107_417SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_418","MENE","Sulfaat",14,"SO4=","L107_418SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_421","GENOVEVABEEK","Sulfaat",14,"SO4=","L107_421SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_422","'S HERTOGENGRACHT","Sulfaat",14,"SO4=",{"$f":"_xlfn.CONCAT(A3075,E3075)","v":"L107_422SO4="},"jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_423","BEGIJNEBEEK L1","Sulfaat",14,"SO4=","L107_423SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_424","VIJVERSLOOP","Sulfaat",14,"SO4=","L107_424SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_431","ST-ODULPHUSBEEK","Sulfaat",14,"SO4=","L107_431SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_432","DORMAALBEEK","Sulfaat",14,"SO4=","L107_432SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_433","BEVERBEEK","Sulfaat",14,"SO4=","L107_433SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_434","SCHEIBEEK","Sulfaat",14,"SO4=","L107_434SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_435","AREBEEK","Sulfaat",14,"SO4=","L107_435SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_439","IJSE L1","Sulfaat",14,"SO4=","L107_439SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_441","LANGEGRACHT","Sulfaat",14,"SO4=","L107_441SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_449","VOER (BERTEM)","Sulfaat",14,"SO4=","L107_449SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_451","GROTE LAAK - GROTE LOOP - MESTENLOOP","Sulfaat",14,"SO4=","L107_451SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_452","LAARBEEK","Sulfaat",14,"SO4=","L107_452SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_453","ZWARTEBEEK (SCHERPENHEUVEL-ZICHEM)","Sulfaat",14,"SO4=","L107_453SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_454","KLEINEBEEK - RIJSELSESTRAATVLIET","Sulfaat",14,"SO4=","L107_454SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_462","LEMINGSBEEK","Sulfaat",14,"SO4=","L107_462SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_463","AABEEK (MECHELEN)","Sulfaat",14,"SO4=","L107_463SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_464","LEYBEEK","Sulfaat",14,"SO4=","L107_464SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_47","ZARRENBEEK L1","Sulfaat",14,"SO4=","L107_47SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_48","KANAAL VAN ESEN","Sulfaat",14,"SO4=","L107_48SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["L107_5","BOLLAERTBEEK","Sulfaat",14,"SO4=","L107_5SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_6","DIKKEBUSBEEK","Sulfaat",14,"SO4=","L107_6SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_600","LEYLOOP","Sulfaat",14,"SO4=","L107_600SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_601","DE AA (RAVELS)","Sulfaat",14,"SO4=","L107_601SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_602","BLAUWPUTTEN EN LEILOOP","Sulfaat",14,"SO4=","L107_602SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_603","HEERLESE LOOP","Sulfaat",14,"SO4=","L107_603SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_607","MERKSKE L1","Sulfaat",14,"SO4=","L107_607SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_609","KLEINE MARK","Sulfaat",14,"SO4=","L107_609SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_61","VAARTDIJKGELEED","Sulfaat",14,"SO4=","L107_61SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["L107_610","MARK L1","Sulfaat",14,"SO4=","L107_610SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_613","SLUISKENSVIJVER","Sulfaat",14,"SO4=","L107_613SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_614","WEERIJSEBEEK L1","Sulfaat",14,"SO4=","L107_614SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_615","KLEINE BEEK (WUUSTWEZEL)","Sulfaat",14,"SO4=","L107_615SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_629","KLEIN WILBOEREBEEK","Sulfaat",14,"SO4=","L107_629SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_63","BOERGONJEVAART","Sulfaat",14,"SO4=","L107_63SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["L107_631","MOLENBEEK - BOLLAAK L1","Sulfaat",14,"SO4=","L107_631SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_632","DE DELFTE BEEK","Sulfaat",14,"SO4=","L107_632SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_633","BOSBEEK - DIEPTELOOP","Sulfaat",14,"SO4=","L107_633SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_638","GROTE CALIE","Sulfaat",14,"SO4=","L107_638SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_640","DE AA - NATTENLOOP","Sulfaat",14,"SO4=","L107_640SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_644","ITTERBEEK (DUFFEL)","Sulfaat",14,"SO4=","L107_644SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_648","BRUINBEEK","Sulfaat",14,"SO4=","L107_648SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_650","REEHAGENBEEK","Sulfaat",14,"SO4=","L107_650SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_654","LARUMSE LOOP","Sulfaat",14,"SO4=","L107_654SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_655","DALEMANSLOOP","Sulfaat",14,"SO4=","L107_655SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_656","BEGGELBEEK","Sulfaat",14,"SO4=","L107_656SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_66","KERKBEEK","Sulfaat",14,"SO4=","L107_66SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_664","MOLENBEEK - ZIJP","Sulfaat",14,"SO4=","L107_664SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_665","BOUWBEEK","Sulfaat",14,"SO4=","L107_665SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_67","LIJSTERBEEK","Sulfaat",14,"SO4=","L107_67SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_677","DIEPE BEEK","Sulfaat",14,"SO4=","L107_677SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_681","KOUDE BEEK","Sulfaat",14,"SO4=","L107_681SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_684","SCHOON SCHIJN","Sulfaat",14,"SO4=","L107_684SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["L107_688","LAARSE BEEK","Sulfaat",14,"SO4=","L107_688SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_695","VARENDONKSE BEEK","Sulfaat",14,"SO4=","L107_695SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_702","MILLEGEMLOOP","Sulfaat",14,"SO4=","L107_702SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_705","SCHEPPELIJKE NETE","Sulfaat",14,"SO4=","L107_705SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_706","MOLSE NETE L1","Sulfaat",14,"SO4=","L107_706SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_708","GROTE NETE L1","Sulfaat",14,"SO4=","L107_708SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_722","WAMP L1","Sulfaat",14,"SO4=","L107_722SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_723","RODE LOOP","Sulfaat",14,"SO4=","L107_723SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_729","STAPKENSLOOP","Sulfaat",14,"SO4=","L107_729SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_735","GESTELBEEK","Sulfaat",14,"SO4=","L107_735SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_740","BERGEBEEK","Sulfaat",14,"SO4=","L107_740SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_741","SPILLEBEEK","Sulfaat",14,"SO4=",{"$f":"_xlfn.CONCAT(A3139,E3139)","v":"L107_741SO4="},"jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_742","PLATTE BEEK","Sulfaat",14,"SO4=","L107_742SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_78","DEVEBEEK L1","Sulfaat",14,"SO4=","L107_78SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_8","IEPERLEE","Sulfaat",14,"SO4=","L107_8SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_809","KLEINE HERK L1","Sulfaat",14,"SO4=","L107_809SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_810","WINTERBEEK (KORTESSEM)","Sulfaat",14,"SO4=","L107_810SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_812","MOMBEEK L1","Sulfaat",14,"SO4=","L107_812SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_814","STEENLAAK","Sulfaat",14,"SO4=","L107_814SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_82","BABILLEBEEK","Sulfaat",14,"SO4=","L107_82SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_824","ROELBEEK","Sulfaat",14,"SO4=","L107_824SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_83","ROOBEEK","Sulfaat",14,"SO4=","L107_83SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_836","LAAMBEEK","Sulfaat",14,"SO4=","L107_836SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_839","ZONDERIKBEEK","Sulfaat",14,"SO4=","L107_839SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_84","KROMMEBEEK","Sulfaat",14,"SO4=","L107_84SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_846","KAATSBEEK","Sulfaat",14,"SO4=","L107_846SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_847","WINTERBEEK (BILZEN)","Sulfaat",14,"SO4=","L107_847SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_848","DEMER L1","Sulfaat",14,"SO4=","L107_848SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_852","MUNSTERBEEK L1","Sulfaat",14,"SO4=","L107_852SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_853","ZUTENDAALBEEK","Sulfaat",14,"SO4=","L107_853SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_854","BOLLISENBEEK","Sulfaat",14,"SO4=","L107_854SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_855","DOMMEL L1","Sulfaat",14,"SO4=","L107_855SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_856","HOLVENLOOP","Sulfaat",14,"SO4=","L107_856SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_857","EINDERGATLOOP","Sulfaat",14,"SO4=","L107_857SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_858","WARMBEEK L1","Sulfaat",14,"SO4=","L107_858SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_859","PRINSENLOOP","Sulfaat",14,"SO4=","L107_859SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_861","ABEEK L1","Sulfaat",14,"SO4=","L107_861SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_866","LOSSING L1","Sulfaat",14,"SO4=","L107_866SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_869","SOERBEEK","Sulfaat",14,"SO4=","L107_869SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_876","BOSBEEK L1","Sulfaat",14,"SO4=","L107_876SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_879","VRIETSELBEEK - OUDE MAAS (DILSEN)","Sulfaat",14,"SO4=","L107_879SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_883","ZIEPBEEK","Sulfaat",14,"SO4=","L107_883SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_885","HEESWATER","Sulfaat",14,"SO4=","L107_885SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_890","BEEK - DE BUTH (TONGEREN)","Sulfaat",14,"SO4=","L107_890SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_891","VOER (VOEREN)","Sulfaat",14,"SO4=","L107_891SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_892","BEEK (VOEREN)","Sulfaat",14,"SO4=","L107_892SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_893","GULP","Sulfaat",14,"SO4=","L107_893SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_91","PLAATSBEEK","Sulfaat",14,"SO4=","L107_91SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_92","MAALBEEK (LEIEBEKKEN)","Sulfaat",14,"SO4=","L107_92SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_97","KASSELRIJBEEK - WEST","Sulfaat",14,"SO4=","L107_97SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L107_98","GAVERBEEK","Sulfaat",14,"SO4=","L107_98SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L110_1100","ZILVERBEEK","Sulfaat",14,"SO4=","L110_1100SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1001","MARTJEVAART - LEKKERBOTERBEEK","Sulfaat",14,"SO4=","L111_1001SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1003","GELUWEBEEK","Sulfaat",14,"SO4=","L111_1003SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1004","RIJTGRACHT","Sulfaat",14,"SO4=","L111_1004SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1006","HOOFDSLOOT","Sulfaat",14,"SO4=","L111_1006SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1014","MEREBEEK","Sulfaat",14,"SO4=","L111_1014SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1016","WANTEBEEK","Sulfaat",14,"SO4=","L111_1016SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1018","LEEBEEK","Sulfaat",14,"SO4=","L111_1018SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1019","MOLENBEEK - MARKEBEEK","Sulfaat",14,"SO4=","L111_1019SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1020","OOSSEBEEK","Sulfaat",14,"SO4=","L111_1020SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1021","ZWALMBEEK","Sulfaat",14,"SO4=","L111_1021SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1022","MOLENBEEK (RONSE)","Sulfaat",14,"SO4=","L111_1022SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1024","BAVEGEMSE BEEK","Sulfaat",14,"SO4=","L111_1024SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1025","MAANBEEK","Sulfaat",14,"SO4=","L111_1025SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1027","GROOTEBEEK","Sulfaat",14,"SO4=","L111_1027SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1028","LANGELEDE","Sulfaat",14,"SO4=","L111_1028SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1029","KLEINE WATERGANG","Sulfaat",14,"SO4=","L111_1029SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1030","WATERGANG VAN DE MOERBEKEPOLDER","Sulfaat",14,"SO4=","L111_1030SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1031","KANAAL VAN STEKENE","Sulfaat",14,"SO4=","L111_1031SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1032","DIJKGRACHT","Sulfaat",14,"SO4=","L111_1032SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["L111_1033","PAPENMEERSBEEK","Sulfaat",14,"SO4=","L111_1033SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1035","KOEVAARDEKEN","Sulfaat",14,"SO4=","L111_1035SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["L111_1037","MOLENBEEK - LAKEBEEK","Sulfaat",14,"SO4=","L111_1037SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1038","MAALBEEK - AMELVONNEBEEK","Sulfaat",14,"SO4=","L111_1038SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1039","STEENVOORDBEEK (TERNAT)","Sulfaat",14,"SO4=",{"$f":"_xlfn.CONCAT(A3203,E3203)","v":"L111_1039SO4="},"jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1040","BELLEBEEK L1","Sulfaat",14,"SO4=","L111_1040SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1041","WINGE L1","Sulfaat",14,"SO4=","L111_1041SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1042","LEIBEEK - LIPSEBEEK L1","Sulfaat",14,"SO4=","L111_1042SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1043","WEESBEEK L1","Sulfaat",14,"SO4=","L111_1043SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1044","KASTEELBEEK","Sulfaat",14,"SO4=","L111_1044SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1046","GROTE MOTTE","Sulfaat",14,"SO4=","L111_1046SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1047","BAREBEEK L1","Sulfaat",14,"SO4=","L111_1047SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1049","MUNTLOOP","Sulfaat",14,"SO4=","L111_1049SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1050","WEHAGENBEEK","Sulfaat",14,"SO4=","L111_1050SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1052","LAAKBEEK","Sulfaat",14,"SO4=","L111_1052SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1053","MOUBEEK","Sulfaat",14,"SO4=","L111_1053SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1054","GOORBOSBEEK","Sulfaat",14,"SO4=","L111_1054SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1056","VROUWVLIET L1","Sulfaat",14,"SO4=","L111_1056SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1057","GROTE MOLENBEEK L1","Sulfaat",14,"SO4=","L111_1057SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1058","ZWARTE BEEK (WILLEBROEK)","Sulfaat",14,"SO4=","L111_1058SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1059","ZIELBEEK - BOSBEEK L1","Sulfaat",14,"SO4=","L111_1059SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1060","GROOT SCHIJN L1","Sulfaat",14,"SO4=","L111_1060SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1062","HERSELTSELOOP","Sulfaat",14,"SO4=","L111_1062SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1063","STEENKENSBEEK","Sulfaat",14,"SO4=","L111_1063SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1064","ST. TRUDOLEKEN","Sulfaat",14,"SO4=","L111_1064SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1065","ASBEEK","Sulfaat",14,"SO4=","L111_1065SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1066","LOEIJENS NEETJE","Sulfaat",14,"SO4=","L111_1066SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1067","KLEINE NETE L1","Sulfaat",14,"SO4=","L111_1067SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1070","WIMP L1","Sulfaat",14,"SO4=","L111_1070SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1071","GOORLOOP","Sulfaat",14,"SO4=","L111_1071SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1072","POVERSBEEK","Sulfaat",14,"SO4=","L111_1072SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1075","MELSTERBEEK L1","Sulfaat",14,"SO4=","L111_1075SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1076","CICINDRIA","Sulfaat",14,"SO4=","L111_1076SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1077","MOLENBEEK (SINT-TRUIDEN)","Sulfaat",14,"SO4=","L111_1077SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1078","GRONDBEEK","Sulfaat",14,"SO4=","L111_1078SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1079","HELDERBEEK","Sulfaat",14,"SO4=","L111_1079SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1080","ZWARTEBEEK L1","Sulfaat",14,"SO4=","L111_1080SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1081","MANGELBEEK L1","Sulfaat",14,"SO4=","L111_1081SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1082","SLANGBEEK","Sulfaat",14,"SO4=","L111_1082SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1083","MISERIKBEEK","Sulfaat",14,"SO4=","L111_1083SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1084","MANDEL L1","Sulfaat",14,"SO4=","L111_1084SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1086","LOZERBROEKBEEK","Sulfaat",14,"SO4=","L111_1086SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1087","HORSTGATERBEEK","Sulfaat",14,"SO4=","L111_1087SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1088","ITTERBEEK L1","Sulfaat",14,"SO4=","L111_1088SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1089","WITBEEK","Sulfaat",14,"SO4=","L111_1089SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1090","ZANDERBEEK","Sulfaat",14,"SO4=","L111_1090SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1091","KIKBEEK","Sulfaat",14,"SO4=","L111_1091SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1092","ZOUW","Sulfaat",14,"SO4=","L111_1092SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1093","EZELSBEEK","Sulfaat",14,"SO4=","L111_1093SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1094","HEULEBEEK L1","Sulfaat",14,"SO4=","L111_1094SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1095","KLEINE LAAK","Sulfaat",14,"SO4=","L111_1095SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1096","GROTE LAAK L1","Sulfaat",14,"SO4=","L111_1096SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1098","KEIBEEK","Sulfaat",14,"SO4=","L111_1098SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1099","GAVERSE BEEK (BECQUE DE NEUVILLE)","Sulfaat",14,"SO4=","L111_1099SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1102","KLEINE A - WILDERTSE BEEK","Sulfaat",14,"SO4=","L111_1102SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1104","DESPIERREBEEK","Sulfaat",14,"SO4=","L111_1104SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1105","MELSENBEEK","Sulfaat",14,"SO4=","L111_1105SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1106","DONKSE BEEK","Sulfaat",14,"SO4=","L111_1106SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["L111_1109","MOERDIJKVAART L1","Sulfaat",14,"SO4=","L111_1109SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1110","EDE","Sulfaat",14,"SO4=","L111_1110SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1112","ISABELLASTROOM","Sulfaat",14,"SO4=","L111_1112SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1113","LACHENEBEEK","Sulfaat",14,"SO4=","L111_1113SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1114","ANTITANKGRACHT ZUID","Sulfaat",14,"SO4=","L111_1114SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_1201","S HERTOGENDIJKSE BEEK","Sulfaat",14,"SO4=","L111_1201SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["L111_15","HEIDEBEEK (VLETEREN)","Sulfaat",14,"SO4=","L111_15SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["L111_298","OUDE DENDER","Sulfaat",14,"SO4=","L111_298SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_315","FONDATIEGRACHT","Sulfaat",14,"SO4=","L111_315SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_326","BARBIERBEEK","Sulfaat",14,"SO4=","L111_326SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_419","SCHOORBROEKBEEK","Sulfaat",14,"SO4=",{"$f":"_xlfn.CONCAT(A3267,E3267)","v":"L111_419SO4="},"jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_436","VELPE L1","Sulfaat",14,"SO4=","L111_436SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_624","TAPPELBEEK","Sulfaat",14,"SO4=","L111_624SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_627","KLEINE BEEK (ZANDHOVEN)","Sulfaat",14,"SO4=","L111_627SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_639","VISBEEK","Sulfaat",14,"SO4=","L111_639SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_674","BENEDENVLIET L1","Sulfaat",14,"SO4=","L111_674SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_676","WEZELSE BEEK","Sulfaat",14,"SO4=","L111_676SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_699","SCHERPENBERGLOOP","Sulfaat",14,"SO4=","L111_699SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_707","KLEINE HOOFDGRACHT","Sulfaat",14,"SO4=","L111_707SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_717","DESSELSE NEET","Sulfaat",14,"SO4=","L111_717SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_724","ANTITANKGRACHT NOORD","Sulfaat",14,"SO4=","L111_724SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L111_844","STIEMER","Sulfaat",14,"SO4=","L111_844SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L117_1036","ZUUNBEEK L1","Sulfaat",14,"SO4=","L117_1036SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L117_1068","HERTSBERGEBEEK - GETEBEEK","Sulfaat",14,"SO4=","L117_1068SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L117_1073","RIVIERBEEK","Sulfaat",14,"SO4=","L117_1073SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L117_1074","HERK L1","Sulfaat",14,"SO4=","L117_1074SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L117_1085","WILDERBEEK","Sulfaat",14,"SO4=","L117_1085SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L117_17","STEENVOORDEBEEK (WATOU)","Sulfaat",14,"SO4=","L117_17SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L117_219","BURGGRAVENSTROOM","Sulfaat",14,"SO4=","L117_219SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L117_232","JOBEEK","Sulfaat",14,"SO4=","L117_232SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L117_233","RINGBEEK","Sulfaat",14,"SO4=","L117_233SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L117_402","MOLENBEEK - SLAGVIJVERBEEK","Sulfaat",14,"SO4=","L117_402SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L117_659","KREKELBEEK","Sulfaat",14,"SO4=","L117_659SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L117_673","KLEIN SCHIJN (NOORDELIJK DEEL)","Sulfaat",14,"SO4=","L117_673SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L117_813","HERKEBEEK","Sulfaat",14,"SO4=","L117_813SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L118_238","KROMMEDIJKBEEK","Sulfaat",14,"SO4=","L118_238SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L119_675","KLEIN SCHIJN (ZUIDELIJK DEEL)","Sulfaat",14,"SO4=","L119_675SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L120_1097","KASSELRIJBEEK - OOST","Sulfaat",14,"SO4=","L120_1097SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L121_1045","GROTEBEEK - WINTERBEEK","Sulfaat",14,"SO4=","L121_1045SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L2 Bk","L2 Kleine Beek","Sulfaat",14,"SO4=","L2 BkSO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["L2 Bk","L2 kleine beek","Sulfaat",14,"SO4=","L2 BkSO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_102","DEMER V","Sulfaat",14,"SO4=","VL05_102SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_103","DEMER VI","Sulfaat",14,"SO4=","VL05_103SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_104","DEMER VII","Sulfaat",14,"SO4=","VL05_104SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_105","GETE I","Sulfaat",14,"SO4=","VL05_105SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_106","GETE II","Sulfaat",14,"SO4=","VL05_106SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_108","HERK + KLEINE HERK","Sulfaat",14,"SO4=","VL05_108SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_110","MANGELBEEK","Sulfaat",14,"SO4=","VL05_110SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_113","MOMBEEK","Sulfaat",14,"SO4=","VL05_113SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_114","MUNSTERBEEK","Sulfaat",14,"SO4=","VL05_114SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_115","VELPE","Sulfaat",14,"SO4=","VL05_115SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_116","WINGE","Sulfaat",14,"SO4=","VL05_116SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_118","ZWARTWATER","Sulfaat",14,"SO4=","VL05_118SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_119","VINNE","Sulfaat",14,"SO4=","VL05_119SO4=","jaargemiddelde","mg/L",100,"jaargemiddelde",100,100,150,300]
["VL05_12","POPERINGEVAART","Sulfaat",14,"SO4=","VL05_12SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_121","AA II","Sulfaat",14,"SO4=","VL05_121SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_122","GROTE LAAK","Sulfaat",14,"SO4=","VL05_122SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_124","GROTE NETE II","Sulfaat",14,"SO4=","VL05_124SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_130","WAMP","Sulfaat",14,"SO4=","VL05_130SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_131","WIMP","Sulfaat",14,"SO4=","VL05_131SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_134","BERWIJN","Sulfaat",14,"SO4=","VL05_134SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_135","BOSBEEK","Sulfaat",14,"SO4=","VL05_135SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_136","DOMMEL","Sulfaat",14,"SO4=","VL05_136SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_137","ITTERBEEK I","Sulfaat",14,"SO4=","VL05_137SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_138","ITTERBEEK II","Sulfaat",14,"SO4=","VL05_138SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_140","JEKER II","Sulfaat",14,"SO4=","VL05_140SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_141","LOSSING","Sulfaat",14,"SO4=","VL05_141SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_146","MERKSKE","Sulfaat",14,"SO4=","VL05_146SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_148","WEERIJSEBEEK","Sulfaat",14,"SO4=","VL05_148SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_150","AFLEIDINGSKANAAL van de LEIE/SCHIPDONKKANAAL I","Sulfaat",14,"SO4=","VL05_150SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_152","AVRIJEVAART + SLEIDINGSVAARDEKE","Sulfaat",14,"SO4=","VL05_152SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_159","KANAAL CHARLEROI-BRUSSEL","Sulfaat",14,"SO4=","VL05_159SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_163","KANAAL GENT-OOSTENDE II","Sulfaat",14,"SO4=","VL05_163SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_166","KANAAL IEPER-IJZER","Sulfaat",14,"SO4=","VL05_166SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_167","KANAAL LEUVEN-DIJLE","Sulfaat",14,"SO4=",{"$f":"_xlfn.CONCAT(A3331,E3331)","v":"VL05_167SO4="},"jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_170","KANAAL VAN BEVERLO","Sulfaat",14,"SO4=","VL05_170SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_171","LEDE","Sulfaat",14,"SO4=","VL05_171SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_175","MOERVAART","Sulfaat",14,"SO4=","VL05_175SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_177","NIEUWE KALE","Sulfaat",14,"SO4=","VL05_177SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_18","KERKEBEEK","Sulfaat",14,"SO4=","VL05_18SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_180","ZARRENBEEK","Sulfaat",14,"SO4=","VL05_180SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_182","ZUIDLEDE","Sulfaat",14,"SO4=","VL05_182SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_191","DESSELSE ZANDPUTTEN","Sulfaat",14,"SO4=","VL05_191SO4=","jaargemiddelde","mg/L",100,"jaargemiddelde",100,100,150,300]
["VL05_192","DONKMEER","Sulfaat",14,"SO4=","VL05_192SO4=","jaargemiddelde","mg/L",100,"jaargemiddelde",100,100,150,300]
["VL05_195","GAVERS HARELBEKE","Sulfaat",14,"SO4=","VL05_195SO4=","jaargemiddelde","mg/L",100,"jaargemiddelde",100,100,150,300]
["VL05_196","GRINDPLAS KESSENICH","Sulfaat",14,"SO4=","VL05_196SO4=","jaargemiddelde","mg/L",100,"jaargemiddelde",100,100,150,300]
["VL05_2","GROTE KEMMELBEEK","Sulfaat",14,"SO4=","VL05_2SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_20","RIVIERBEEK + HERTSBERGEBEEK","Sulfaat",14,"SO4=","VL05_20SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_200","SCHULENSMEER","Sulfaat",14,"SO4=","VL05_200SO4=","jaargemiddelde","mg/L",100,"jaargemiddelde",100,100,150,300]
["VL05_201","SPAANJERD + HEERENLAAK","Sulfaat",14,"SO4=","VL05_201SO4=","jaargemiddelde","mg/L",100,"jaargemiddelde",100,100,150,300]
["VL05_21","ZUIDERVAARTJE","Sulfaat",14,"SO4=","VL05_21SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_24","MEREBEEK + BORISGRACHT + LIEVE","Sulfaat",14,"SO4=","VL05_24SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_25","OUDE KALE","Sulfaat",14,"SO4=","VL05_25SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_28","BENEDENVLIET","Sulfaat",14,"SO4=","VL05_28SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_3","HANDZAMEVAART","Sulfaat",14,"SO4=","VL05_3SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_30","GROTE MOLENBEEK - DE VLIET","Sulfaat",14,"SO4=","VL05_30SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_31","KALKENSE VAART","Sulfaat",14,"SO4=","VL05_31SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_32","MOLENBEEK - GROTE BEEK","Sulfaat",14,"SO4=","VL05_32SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_38","ZIELBEEK - BOSBEEK","Sulfaat",14,"SO4=","VL05_38SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_4","HEIDEBEEK","Sulfaat",14,"SO4=","VL05_4SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_44","DEVEBEEK","Sulfaat",14,"SO4=","VL05_44SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_45","GAVERBEEK I","Sulfaat",14,"SO4=","VL05_45SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_46","GAVERBEEK II","Sulfaat",14,"SO4=","VL05_46SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_5","IEPERLEE + VERWEZEN KANAAL IEPER-KOMEN","Sulfaat",14,"SO4=","VL05_5SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_50","LEIE III","Sulfaat",14,"SO4=","VL05_50SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_51","MANDEL I","Sulfaat",14,"SO4=","VL05_51SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_52","MANDEL II","Sulfaat",14,"SO4=","VL05_52SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_53","OUDE MANDEL","Sulfaat",14,"SO4=","VL05_53SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_58","BOVEN-SCHELDE IV","Sulfaat",14,"SO4=","VL05_58SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_61","RONE","Sulfaat",14,"SO4=","VL05_61SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_62","STAMPKOTBEEK","Sulfaat",14,"SO4=","VL05_62SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_64","ZWARTE SPIEREBEEK","Sulfaat",14,"SO4=","VL05_64SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_67","DENDER I","Sulfaat",14,"SO4=","VL05_67SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_70","DENDER IV","Sulfaat",14,"SO4=","VL05_70SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_73","MOLENBEEK - PACHTBOSBEEK","Sulfaat",14,"SO4=","VL05_73SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_75","VONDELBEEK","Sulfaat",14,"SO4=","VL05_75SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_77","DIJLE I","Sulfaat",14,"SO4=","VL05_77SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_81","DIJLE V","Sulfaat",14,"SO4=","VL05_81SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_85","LEIBEEK - LAAKBEEK","Sulfaat",14,"SO4=","VL05_85SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_86","NETHEN","Sulfaat",14,"SO4=","VL05_86SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_87","VOER (Leuven)","Sulfaat",14,"SO4=","VL05_87SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_89","VUNT","Sulfaat",14,"SO4=","VL05_89SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_90","WEESBEEK","Sulfaat",14,"SO4=","VL05_90SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_93","ZENNE II","Sulfaat",14,"SO4=","VL05_93SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL05_98","DEMER I","Sulfaat",14,"SO4=","VL05_98SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL05_99","DEMER II","Sulfaat",14,"SO4=","VL05_99SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL08_125","GROTE NETE III","Sulfaat",14,"SO4=","VL08_125SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL08_132","GETIJDENETES","Sulfaat",14,"SO4=","VL08_132SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL08_157","ISABELLAWATERING","Sulfaat",14,"SO4=","VL08_157SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL08_162","KANAAL GENT-OOSTENDE I + COUPURE + VERBINDINGSKANAAL","Sulfaat",14,"SO4=","VL08_162SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL08_164","KANAAL GENT-OOSTENDE III","Sulfaat",14,"SO4=","VL08_164SO4=","jaargemiddelde","mg/L",200,"jaargemiddelde",200,200,250,300]
["VL08_172","LEOPOLDKANAAL I","Sulfaat",14,"SO4=","VL08_172SO4=","jaargemiddelde","mg/L",400,"jaargemiddelde",400,400,500,600]
["VL08_173","LEOPOLDKANAAL II","Sulfaat",14,"SO4=","VL08_173SO4=","jaargemiddelde","mg/L",200,"jaargemiddelde",200,200,50,300]
["VL08_176","NETEKANAAL","Sulfaat",14,"SO4=","VL08_176SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL08_178","NOORDELIJKE RINGVAART","Sulfaat",14,"SO4=","VL08_178SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL08_179","WESTELIJKE RINGVAART","Sulfaat",14,"SO4=","VL08_179SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL08_39","GETIJDEDURME","Sulfaat",14,"SO4=","VL08_39SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL08_41","ZEESCHELDE II","Sulfaat",14,"SO4=","VL08_41SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL08_55","BOVEN-SCHELDE I","Sulfaat",14,"SO4=",{"$f":"_xlfn.CONCAT(A3395,E3395)","v":"VL08_55SO4="},"jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL08_7","IJZER I","Sulfaat",14,"SO4=","VL08_7SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL08_71","DENDER V","Sulfaat",14,"SO4=","VL08_71SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL08_72","MARK (Denderbekken)","Sulfaat",14,"SO4=","VL08_72SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL08_80","DIJLE IV","Sulfaat",14,"SO4=","VL08_80SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL08_82","DIJLE VI","Sulfaat",14,"SO4=","VL08_82SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL08_92","ZENNE I","Sulfaat",14,"SO4=","VL08_92SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL08_95","GETIJDEDIJLE & GETIJDEZENNE","Sulfaat",14,"SO4=","VL08_95SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL09_78","DIJLE II","Sulfaat",14,"SO4=","VL09_78SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL11_10","MARTJEVAART","Sulfaat",14,"SO4=","VL11_10SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_109","KLEINE GETE + VLOEDGRACHT","Sulfaat",14,"SO4=","VL11_109SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_11","MOERDIJKVAART","Sulfaat",14,"SO4=","VL11_11SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_117","ZWARTEBEEK","Sulfaat",14,"SO4=","VL11_117SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_120","AA I","Sulfaat",14,"SO4=","VL11_120SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_123","GROTE NETE I","Sulfaat",14,"SO4=","VL11_123SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_126","KLEINE NETE I","Sulfaat",14,"SO4=","VL11_126SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_127","KLEINE NETE II","Sulfaat",14,"SO4=","VL11_127SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_128","MOL NEET","Sulfaat",14,"SO4=","VL11_128SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_133","ABEEK","Sulfaat",14,"SO4=","VL11_133SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_145","MARK (Maas)","Sulfaat",14,"SO4=","VL11_145SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_155","BRUGSE REIEN","Sulfaat",14,"SO4=","VL11_155SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL11_203","MAAS I+II+III","Sulfaat",14,"SO4=","VL11_203SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL11_205","DEMER III+IV","Sulfaat",14,"SO4=","VL11_205SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_207","MELSTERBEEK I+II","Sulfaat",14,"SO4=","VL11_207SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_40","ZEESCHELDE I","Sulfaat",14,"SO4=","VL11_40SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL11_59","GROTE SPIEREBEEK","Sulfaat",14,"SO4=","VL11_59SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_63","ZWALM","Sulfaat",14,"SO4=","VL11_63SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_76","BAREBEEK","Sulfaat",14,"SO4=","VL11_76SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_83","IJSSE","Sulfaat",14,"SO4=","VL11_83SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_84","LAAN","Sulfaat",14,"SO4=","VL11_84SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_88","VROUWVLIET","Sulfaat",14,"SO4=","VL11_88SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL11_91","WOLUWE","Sulfaat",14,"SO4=","VL11_91SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL17_147","WARMBEEK","Sulfaat",14,"SO4=","VL17_147SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL17_154","BRAKELEIKEN + LIEVE","Sulfaat",14,"SO4=","VL17_154SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL17_156","GENTSE BINNENWATEREN","Sulfaat",14,"SO4=","VL17_156SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL17_161","KANAAL DUINKERKE-NIEUWPOORT","Sulfaat",14,"SO4=","VL17_161SO4=","jaargemiddelde","mg/L",400,"jaargemiddelde",400,400,500,600]
["VL17_168","KANAAL PLASSENDALE-NIEUWPOORT","Sulfaat",14,"SO4=","VL17_168SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL17_169","KANAAL ROESELARE-LEIE","Sulfaat",14,"SO4=","VL17_169SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL17_174","LOKANAAL","Sulfaat",14,"SO4=","VL17_174SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL17_187","ANTWERPSE HAVENDOKKEN + SCHELDE-RIJNVERBINDING","Sulfaat",14,"SO4=","VL17_187SO4=","jaargemiddelde","mg/L",1000,"jaargemiddelde",1000,1000,1500,3000]
["VL17_204","BOVEN-SCHELDE II+III","Sulfaat",14,"SO4=","VL17_204SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL17_206","DENDER II+III","Sulfaat",14,"SO4=","VL17_206SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL17_29","GROOT SCHIJN","Sulfaat",14,"SO4=","VL17_29SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL17_35","VERLEGDE SCHIJN - HOOFDGRACHT","Sulfaat",14,"SO4=","VL17_35SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL17_48","LEIE I","Sulfaat",14,"SO4=","VL17_48SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL17_49","LEIE II","Sulfaat",14,"SO4=","VL17_49SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL17_54","TOERISTISCHE LEIE","Sulfaat",14,"SO4=","VL17_54SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL17_60","MOLENBEEK - MAARKEBEEK","Sulfaat",14,"SO4=","VL17_60SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL17_66","BELLEBEEK","Sulfaat",14,"SO4=","VL17_66SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL17_9","IJZER III","Sulfaat",14,"SO4=","VL17_9SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL20_36","VERLEGDE SCHIJN - VOORGRACHT","Sulfaat",14,"SO4=","VL20_36SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL20_96","BEGIJNENBEEK","Sulfaat",14,"SO4=","VL20_96SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL21_1","BLANKAART WATERLOPEN","Sulfaat",14,"SO4=","VL21_1SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL21_107","GROTE GETE + BORGGRACHT","Sulfaat",14,"SO4=","VL21_107SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL21_129","MOLENBEEK - BOLLAAK","Sulfaat",14,"SO4=","VL21_129SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL21_139","JEKER I","Sulfaat",14,"SO4=","VL21_139SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL21_26","POEKEBEEK","Sulfaat",14,"SO4=","VL21_26SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL21_33","MOLENBEEK - KOTTEMBEEK","Sulfaat",14,"SO4=","VL21_33SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL21_47","HEULEBEEK","Sulfaat",14,"SO4=","VL21_47SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL21_74","MOLENBEEK - TER ERPENBEEK","Sulfaat",14,"SO4=","VL21_74SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL21_79","DIJLE III","Sulfaat",14,"SO4=","VL21_79SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL21_8","IJZER II","Sulfaat",14,"SO4=","VL21_8SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL21_94","ZUUNBEEK","Sulfaat",14,"SO4=","VL21_94SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL21_97","DE HULPE - ZWART WATER","Sulfaat",14,"SO4=","VL21_97SO4=","jaargemiddelde","mg/L",90,"jaargemiddelde",90,90,120,150]
["VL22_208","ALBERTKANAAL - Maasbekken","Sulfaat",14,"SO4=",{"$f":"_xlfn.CONCAT(A3459,E3459)","v":"VL22_208SO4="},"jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL22_209","ALBERTKANAAL - Demerbekken","Sulfaat",14,"SO4=","VL22_209SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL22_210","ALBERTKANAAL - Netebekken","Sulfaat",14,"SO4=","VL22_210SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL22_211","ALBERTKANAAL - Benedenscheldebekken","Sulfaat",14,"SO4=","VL22_211SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL22_212","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Netebekken","Sulfaat",14,"SO4=","VL22_212SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL22_213","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Maasbekken","Sulfaat",14,"SO4=","VL22_213SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL22_214","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Benedenscheldebekken","Sulfaat",14,"SO4=","VL22_214SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL22_215","ZEEKANAAL BRUSSEL-SCHELDE - Dijle-Zennebekken","Sulfaat",14,"SO4=","VL22_215SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL22_216","ZEEKANAAL BRUSSEL-SCHELDE - Benedenscheldebekken","Sulfaat",14,"SO4=","VL22_216SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL22_217","AFLEIDINGSKANAAL van de LEIE II + KANAAL van EEKLO - Bekken van de Gentse kanalen","Sulfaat",14,"SO4=","VL22_217SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL22_218","AFLEIDINGSKANAAL van de LEIE II - Bekken van de Brugse polders","Sulfaat",14,"SO4=","VL22_218SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL22_219","KANAAL BOSSUIT-KORTRIJK - Bovenscheldebekken","Sulfaat",14,"SO4=","VL22_219SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL22_220","KANAAL BOSSUIT-KORTRIJK - Leiebekken","Sulfaat",14,"SO4=","VL22_220SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["VL22_221","ZUID-WILLEMSVAART + KANAAL BOCHOLT-HERENTALS (deels) + KANAAL BRIEGDEN-NEERHAREN","Sulfaat",14,"SO4=","VL22_221SO4=","jaargemiddelde","mg/L",150,"jaargemiddelde",150,150,200,250]
["L107_122","HET GELEED","Sulfaat",14,"SO4=","L107_122SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L107_130","KLEINE GEUL","Sulfaat",14,"SO4=","L107_130SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L107_133","BLANKENBERGSEVAART L1","Sulfaat",14,"SO4=","L107_133SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L107_143","GROOT ZWIN - NOORDGELEED","Sulfaat",14,"SO4=","L107_143SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L107_149","PROVINCIEGELEED","Sulfaat",14,"SO4=","L107_149SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L107_150","GRANINGATEVLIET","Sulfaat",14,"SO4=","L107_150SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L107_202","OOSTPOLDERKREEK","Sulfaat",14,"SO4=","L107_202SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L107_213","EEKLOSE WATERGANG","Sulfaat",14,"SO4=","L107_213SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L107_328","ZUIDELIJKE WATERGANG","Sulfaat",14,"SO4=","L107_328SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L107_33","BOMMELAREVAART","Sulfaat",14,"SO4=","L107_33SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L107_333","DOORLOOP","Sulfaat",14,"SO4=","L107_333SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L107_34","RINGSLOT","Sulfaat",14,"SO4=","L107_34SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L107_37","LANGGELEED","Sulfaat",14,"SO4=","L107_37SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L107_56","REYGAERTSVLIET","Sulfaat",14,"SO4=","L107_56SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L107_60","GROOTGELEED","Sulfaat",14,"SO4=","L107_60SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L111_1005","KALSIJDEADER","Sulfaat",14,"SO4=","L111_1005SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L111_1007","STEGERSZWIN","Sulfaat",14,"SO4=","L111_1007SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L111_1010","OOSTKERKEVAART","Sulfaat",14,"SO4=","L111_1010SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L111_1011","BOEREKREEK","Sulfaat",14,"SO4=","L111_1011SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L111_1015","OUDE AVAART","Sulfaat",14,"SO4=","L111_1015SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L111_1034","NIEUWE GRACHT","Sulfaat",14,"SO4=","L111_1034SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L111_1048","ZIJDELINGSGELEED","Sulfaat",14,"SO4=","L111_1048SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L111_1069","AFWATERINGSGRACHT","Sulfaat",14,"SO4=","L111_1069SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L111_1101","GROTE KEIGNAERT","Sulfaat",14,"SO4=","L111_1101SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L111_1107","SLIJKVAART","Sulfaat",14,"SO4=","L111_1107SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L111_1108","STEENGRACHT","Sulfaat",14,"SO4=","L111_1108SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L111_18","ST-MACHUITSBEEK","Sulfaat",14,"SO4=","L111_18SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["VL05_14","VLADSLOVAART","Sulfaat",14,"SO4=","VL05_14SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["VL05_153","BERGENVAART","Sulfaat",14,"SO4=","VL05_153SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["VL05_17","ISABELLAVAART","Sulfaat",14,"SO4=","VL05_17SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["VL05_22","ZWINNEVAART","Sulfaat",14,"SO4=","VL05_22SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["VL05_34","NOORD-ZUIDVERBINDING","Sulfaat",14,"SO4=","VL05_34SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["VL05_6","IEPERLEED","Sulfaat",14,"SO4=","VL05_6SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["VL08_16","BLANKENBERGSE VAART + NOORDEDE","Sulfaat",14,"SO4=","VL08_16SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["VL08_27","ZWARTESLUISBEEK","Sulfaat",14,"SO4=","VL08_27SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["VL11_13","VEURNE AMBACHT POLDER WATERLOPEN","Sulfaat",14,"SO4=","VL11_13SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["VL11_19","OOSTENDS KREKENGEBIED","Sulfaat",14,"SO4=","VL11_19SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["VL11_37","WATERLOOP VAN DE HOGE LANDEN + MELKADER","Sulfaat",14,"SO4=","VL11_37SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L107_10","KEMMELBEEK","Zwevende stoffen",113,"ZS","L107_10ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_104","NEERBEEK","Zwevende stoffen",113,"ZS","L107_104ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_105","PALINGBEEK","Zwevende stoffen",113,"ZS","L107_105ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_11","WANEBEEK","Zwevende stoffen",113,"ZS","L107_11ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_112","LA HAUTE PLANCHE","Zwevende stoffen",113,"ZS","L107_112ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_113","DOUVEBEEK","Zwevende stoffen",113,"ZS","L107_113ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_116","GROTE SPIERE","Zwevende stoffen",113,"ZS","L107_116ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_12","VLETERBEEK","Zwevende stoffen",113,"ZS","L107_12ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_120","SCHEEBEEK","Zwevende stoffen",113,"ZS","L107_120ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_122","HET GELEED","Zwevende stoffen",113,"ZS","L107_122ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_123","KANAAL VAN BRUGGE NAAR SLUIS","Zwevende stoffen",113,"ZS","L107_123ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_124","RONSELAREBEEK","Zwevende stoffen",113,"ZS","L107_124ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_130","KLEINE GEUL","Zwevende stoffen",113,"ZS",{"$f":"_xlfn.CONCAT(A3523,E3523)","v":"L107_130ZS"},"90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_131","LISSEWEEGSEVAART","Zwevende stoffen",113,"ZS","L107_131ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_133","BLANKENBERGSEVAART L1","Zwevende stoffen",113,"ZS","L107_133ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_135","JABBEEKSE BEEK","Zwevende stoffen",113,"ZS","L107_135ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_136","HOGE WATERING","Zwevende stoffen",113,"ZS","L107_136ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_140","SCHELLEVLIET","Zwevende stoffen",113,"ZS","L107_140ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_143","GROOT ZWIN - NOORDGELEED","Zwevende stoffen",113,"ZS","L107_143ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_149","PROVINCIEGELEED","Zwevende stoffen",113,"ZS","L107_149ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_150","GRANINGATEVLIET","Zwevende stoffen",113,"ZS","L107_150ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_16","HARINGEBEEK","Zwevende stoffen",113,"ZS","L107_16ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_202","OOSTPOLDERKREEK","Zwevende stoffen",113,"ZS","L107_202ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_209","ZWARTESLUISBEEK L1","Zwevende stoffen",113,"ZS","L107_209ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_213","EEKLOSE WATERGANG","Zwevende stoffen",113,"ZS","L107_213ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_218","SLEIDINGSVAARDEKEN","Zwevende stoffen",113,"ZS","L107_218ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_225","KEUTELBEEK","Zwevende stoffen",113,"ZS","L107_225ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_234","POEKEBEEK L1","Zwevende stoffen",113,"ZS","L107_234ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_235","REIGERBEEK","Zwevende stoffen",113,"ZS","L107_235ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_236","NEERSCHUURBEEK","Zwevende stoffen",113,"ZS","L107_236ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_237","SPEIBEEK","Zwevende stoffen",113,"ZS","L107_237ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_239","OUDE MANDEL L1","Zwevende stoffen",113,"ZS","L107_239ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_240","ZOUBEEK","Zwevende stoffen",113,"ZS","L107_240ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_241","KATTEBEEK","Zwevende stoffen",113,"ZS","L107_241ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_242","DUIVEBEEK","Zwevende stoffen",113,"ZS","L107_242ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_246","STAMPKOTBEEK - MOLENBEEK","Zwevende stoffen",113,"ZS","L107_246ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_247","STAMPKOTBEEK - WALLEBEEK","Zwevende stoffen",113,"ZS","L107_247ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_253","STAMPKOTBEEK - MUNKBOSBEEK","Zwevende stoffen",113,"ZS","L107_253ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_254","MOLENBEEK - BEIAARDBEEK","Zwevende stoffen",113,"ZS","L107_254ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_266","PEERDESTOKBEEK","Zwevende stoffen",113,"ZS","L107_266ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_272","OPHASSELTBEEK","Zwevende stoffen",113,"ZS","L107_272ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_273","MOLENBEEK - PACHTBOSBEEK L1","Zwevende stoffen",113,"ZS","L107_273ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_274","MOLENBEEK - KALSTERBEEK","Zwevende stoffen",113,"ZS","L107_274ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_275","TER ERPENBEEK","Zwevende stoffen",113,"ZS","L107_275ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_276","MOLENBEEK - GRAADBEEK","Zwevende stoffen",113,"ZS","L107_276ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_277","WILDEBEEK","Zwevende stoffen",113,"ZS","L107_277ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_279","MOLENBEEK - VOGELENZANGBEEK","Zwevende stoffen",113,"ZS","L107_279ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_282","MOLENBEEK - GONDEBEEK","Zwevende stoffen",113,"ZS","L107_282ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_287","MOLENBEEK - GROTE BEEK","Zwevende stoffen",113,"ZS","L107_287ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_289","DAMSLOOT","Zwevende stoffen",113,"ZS","L107_289ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_296","VOORSTESLOOT","Zwevende stoffen",113,"ZS","L107_296ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_299","VONDELBEEK L1","Zwevende stoffen",113,"ZS","L107_299ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_3","BROENBEEK","Zwevende stoffen",113,"ZS","L107_3ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_305","ZELEBEEK","Zwevende stoffen",113,"ZS","L107_305ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_325","GROTE ASTBEEK","Zwevende stoffen",113,"ZS","L107_325ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_328","ZUIDELIJKE WATERGANG","Zwevende stoffen",113,"ZS","L107_328ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_329","BLOKSTRAATBEEK","Zwevende stoffen",113,"ZS","L107_329ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_33","BOMMELAREVAART","Zwevende stoffen",113,"ZS","L107_33ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_330","WATERLOOP VAN DE HOGE LANDEN L1","Zwevende stoffen",113,"ZS","L107_330ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_333","DOORLOOP","Zwevende stoffen",113,"ZS","L107_333ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_335","MOLENBEEK - BEVERBEEK","Zwevende stoffen",113,"ZS","L107_335ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_336","DE RIJT","Zwevende stoffen",113,"ZS","L107_336ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_34","RINGSLOT","Zwevende stoffen",113,"ZS","L107_34ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_37","LANGGELEED","Zwevende stoffen",113,"ZS","L107_37ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_4","KORVERSBEEK","Zwevende stoffen",113,"ZS","L107_4ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_40","STENENSLUISVAART","Zwevende stoffen",113,"ZS","L107_40ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_403","MOLENBEEK - NEERPEDEBEEK","Zwevende stoffen",113,"ZS","L107_403ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_404","LOTBEEK","Zwevende stoffen",113,"ZS","L107_404ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_407","GROEBENGRACHT","Zwevende stoffen",113,"ZS","L107_407ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_409","KLEINE MAALBEEK","Zwevende stoffen",113,"ZS","L107_409ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_411","MOLENBEEK - PARKBEEK","Zwevende stoffen",113,"ZS","L107_411ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_413","TANGEBEEK","Zwevende stoffen",113,"ZS","L107_413ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_417","DE GROTE LAAK","Zwevende stoffen",113,"ZS","L107_417ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_418","MENE","Zwevende stoffen",113,"ZS","L107_418ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_421","GENOVEVABEEK","Zwevende stoffen",113,"ZS","L107_421ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_422","'S HERTOGENGRACHT","Zwevende stoffen",113,"ZS","L107_422ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_423","BEGIJNEBEEK L1","Zwevende stoffen",113,"ZS",{"$f":"_xlfn.CONCAT(A3587,E3587)","v":"L107_423ZS"},"90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_424","VIJVERSLOOP","Zwevende stoffen",113,"ZS","L107_424ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_431","ST-ODULPHUSBEEK","Zwevende stoffen",113,"ZS","L107_431ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_432","DORMAALBEEK","Zwevende stoffen",113,"ZS","L107_432ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_433","BEVERBEEK","Zwevende stoffen",113,"ZS","L107_433ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_434","SCHEIBEEK","Zwevende stoffen",113,"ZS","L107_434ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_435","AREBEEK","Zwevende stoffen",113,"ZS","L107_435ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_439","IJSE L1","Zwevende stoffen",113,"ZS","L107_439ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_441","LANGEGRACHT","Zwevende stoffen",113,"ZS","L107_441ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_449","VOER (BERTEM)","Zwevende stoffen",113,"ZS","L107_449ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_451","GROTE LAAK - GROTE LOOP - MESTENLOOP","Zwevende stoffen",113,"ZS","L107_451ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_452","LAARBEEK","Zwevende stoffen",113,"ZS","L107_452ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_453","ZWARTEBEEK (SCHERPENHEUVEL-ZICHEM)","Zwevende stoffen",113,"ZS","L107_453ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_454","KLEINEBEEK - RIJSELSESTRAATVLIET","Zwevende stoffen",113,"ZS","L107_454ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_462","LEMINGSBEEK","Zwevende stoffen",113,"ZS","L107_462ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_463","AABEEK (MECHELEN)","Zwevende stoffen",113,"ZS","L107_463ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_464","LEYBEEK","Zwevende stoffen",113,"ZS","L107_464ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_47","ZARRENBEEK L1","Zwevende stoffen",113,"ZS","L107_47ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_48","KANAAL VAN ESEN","Zwevende stoffen",113,"ZS","L107_48ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_5","BOLLAERTBEEK","Zwevende stoffen",113,"ZS","L107_5ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_56","REYGAERTSVLIET","Zwevende stoffen",113,"ZS","L107_56ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_6","DIKKEBUSBEEK","Zwevende stoffen",113,"ZS","L107_6ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_60","GROOTGELEED","Zwevende stoffen",113,"ZS","L107_60ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_600","LEYLOOP","Zwevende stoffen",113,"ZS","L107_600ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_601","DE AA (RAVELS)","Zwevende stoffen",113,"ZS","L107_601ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_602","BLAUWPUTTEN EN LEILOOP","Zwevende stoffen",113,"ZS","L107_602ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_603","HEERLESE LOOP","Zwevende stoffen",113,"ZS","L107_603ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_607","MERKSKE L1","Zwevende stoffen",113,"ZS","L107_607ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_609","KLEINE MARK","Zwevende stoffen",113,"ZS","L107_609ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_61","VAARTDIJKGELEED","Zwevende stoffen",113,"ZS","L107_61ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_610","MARK L1","Zwevende stoffen",113,"ZS","L107_610ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_613","SLUISKENSVIJVER","Zwevende stoffen",113,"ZS","L107_613ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_614","WEERIJSEBEEK L1","Zwevende stoffen",113,"ZS","L107_614ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_615","KLEINE BEEK (WUUSTWEZEL)","Zwevende stoffen",113,"ZS","L107_615ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_629","KLEIN WILBOEREBEEK","Zwevende stoffen",113,"ZS","L107_629ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_63","BOERGONJEVAART","Zwevende stoffen",113,"ZS","L107_63ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_631","MOLENBEEK - BOLLAAK L1","Zwevende stoffen",113,"ZS","L107_631ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_632","DE DELFTE BEEK","Zwevende stoffen",113,"ZS","L107_632ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_633","BOSBEEK - DIEPTELOOP","Zwevende stoffen",113,"ZS","L107_633ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_638","GROTE CALIE","Zwevende stoffen",113,"ZS","L107_638ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_640","DE AA - NATTENLOOP","Zwevende stoffen",113,"ZS","L107_640ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_644","ITTERBEEK (DUFFEL)","Zwevende stoffen",113,"ZS","L107_644ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_648","BRUINBEEK","Zwevende stoffen",113,"ZS","L107_648ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_650","REEHAGENBEEK","Zwevende stoffen",113,"ZS","L107_650ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_654","LARUMSE LOOP","Zwevende stoffen",113,"ZS","L107_654ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_655","DALEMANSLOOP","Zwevende stoffen",113,"ZS","L107_655ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_656","BEGGELBEEK","Zwevende stoffen",113,"ZS","L107_656ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_66","KERKBEEK","Zwevende stoffen",113,"ZS","L107_66ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_664","MOLENBEEK - ZIJP","Zwevende stoffen",113,"ZS","L107_664ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_665","BOUWBEEK","Zwevende stoffen",113,"ZS","L107_665ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_67","LIJSTERBEEK","Zwevende stoffen",113,"ZS","L107_67ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_677","DIEPE BEEK","Zwevende stoffen",113,"ZS","L107_677ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_681","KOUDE BEEK","Zwevende stoffen",113,"ZS","L107_681ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_684","SCHOON SCHIJN","Zwevende stoffen",113,"ZS","L107_684ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_688","LAARSE BEEK","Zwevende stoffen",113,"ZS","L107_688ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_695","VARENDONKSE BEEK","Zwevende stoffen",113,"ZS","L107_695ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_702","MILLEGEMLOOP","Zwevende stoffen",113,"ZS","L107_702ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_705","SCHEPPELIJKE NETE","Zwevende stoffen",113,"ZS","L107_705ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_706","MOLSE NETE L1","Zwevende stoffen",113,"ZS","L107_706ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_708","GROTE NETE L1","Zwevende stoffen",113,"ZS","L107_708ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_722","WAMP L1","Zwevende stoffen",113,"ZS","L107_722ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_723","RODE LOOP","Zwevende stoffen",113,"ZS","L107_723ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_729","STAPKENSLOOP","Zwevende stoffen",113,"ZS","L107_729ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_735","GESTELBEEK","Zwevende stoffen",113,"ZS","L107_735ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_740","BERGEBEEK","Zwevende stoffen",113,"ZS",{"$f":"_xlfn.CONCAT(A3651,E3651)","v":"L107_740ZS"},"90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_741","SPILLEBEEK","Zwevende stoffen",113,"ZS","L107_741ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_742","PLATTE BEEK","Zwevende stoffen",113,"ZS","L107_742ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_78","DEVEBEEK L1","Zwevende stoffen",113,"ZS","L107_78ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_8","IEPERLEE","Zwevende stoffen",113,"ZS","L107_8ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_809","KLEINE HERK L1","Zwevende stoffen",113,"ZS","L107_809ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_810","WINTERBEEK (KORTESSEM)","Zwevende stoffen",113,"ZS","L107_810ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_812","MOMBEEK L1","Zwevende stoffen",113,"ZS","L107_812ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_814","STEENLAAK","Zwevende stoffen",113,"ZS","L107_814ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_82","BABILLEBEEK","Zwevende stoffen",113,"ZS","L107_82ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_824","ROELBEEK","Zwevende stoffen",113,"ZS","L107_824ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_83","ROOBEEK","Zwevende stoffen",113,"ZS","L107_83ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_836","LAAMBEEK","Zwevende stoffen",113,"ZS","L107_836ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_839","ZONDERIKBEEK","Zwevende stoffen",113,"ZS","L107_839ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_84","KROMMEBEEK","Zwevende stoffen",113,"ZS","L107_84ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_846","KAATSBEEK","Zwevende stoffen",113,"ZS","L107_846ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_847","WINTERBEEK (BILZEN)","Zwevende stoffen",113,"ZS","L107_847ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_848","DEMER L1","Zwevende stoffen",113,"ZS","L107_848ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_852","MUNSTERBEEK L1","Zwevende stoffen",113,"ZS","L107_852ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_853","ZUTENDAALBEEK","Zwevende stoffen",113,"ZS","L107_853ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_854","BOLLISENBEEK","Zwevende stoffen",113,"ZS","L107_854ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_855","DOMMEL L1","Zwevende stoffen",113,"ZS","L107_855ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_856","HOLVENLOOP","Zwevende stoffen",113,"ZS","L107_856ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_857","EINDERGATLOOP","Zwevende stoffen",113,"ZS","L107_857ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_858","WARMBEEK L1","Zwevende stoffen",113,"ZS","L107_858ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_859","PRINSENLOOP","Zwevende stoffen",113,"ZS","L107_859ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_861","ABEEK L1","Zwevende stoffen",113,"ZS","L107_861ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_866","LOSSING L1","Zwevende stoffen",113,"ZS","L107_866ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_869","SOERBEEK","Zwevende stoffen",113,"ZS","L107_869ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_876","BOSBEEK L1","Zwevende stoffen",113,"ZS","L107_876ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_879","VRIETSELBEEK - OUDE MAAS (DILSEN)","Zwevende stoffen",113,"ZS","L107_879ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_883","ZIEPBEEK","Zwevende stoffen",113,"ZS","L107_883ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_885","HEESWATER","Zwevende stoffen",113,"ZS","L107_885ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_890","BEEK - DE BUTH (TONGEREN)","Zwevende stoffen",113,"ZS","L107_890ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_891","VOER (VOEREN)","Zwevende stoffen",113,"ZS","L107_891ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_892","BEEK (VOEREN)","Zwevende stoffen",113,"ZS","L107_892ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_893","GULP","Zwevende stoffen",113,"ZS","L107_893ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_91","PLAATSBEEK","Zwevende stoffen",113,"ZS","L107_91ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_92","MAALBEEK (LEIEBEKKEN)","Zwevende stoffen",113,"ZS","L107_92ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_97","KASSELRIJBEEK - WEST","Zwevende stoffen",113,"ZS","L107_97ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L107_98","GAVERBEEK","Zwevende stoffen",113,"ZS","L107_98ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L110_1100","ZILVERBEEK","Zwevende stoffen",113,"ZS","L110_1100ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1001","MARTJEVAART - LEKKERBOTERBEEK","Zwevende stoffen",113,"ZS","L111_1001ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1003","GELUWEBEEK","Zwevende stoffen",113,"ZS","L111_1003ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1004","RIJTGRACHT","Zwevende stoffen",113,"ZS","L111_1004ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1005","KALSIJDEADER","Zwevende stoffen",113,"ZS","L111_1005ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1006","HOOFDSLOOT","Zwevende stoffen",113,"ZS","L111_1006ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1007","STEGERSZWIN","Zwevende stoffen",113,"ZS","L111_1007ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1010","OOSTKERKEVAART","Zwevende stoffen",113,"ZS","L111_1010ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1011","BOEREKREEK","Zwevende stoffen",113,"ZS","L111_1011ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1014","MEREBEEK","Zwevende stoffen",113,"ZS","L111_1014ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1015","OUDE AVAART","Zwevende stoffen",113,"ZS","L111_1015ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1016","WANTEBEEK","Zwevende stoffen",113,"ZS","L111_1016ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1018","LEEBEEK","Zwevende stoffen",113,"ZS","L111_1018ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1019","MOLENBEEK - MARKEBEEK","Zwevende stoffen",113,"ZS","L111_1019ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1020","OOSSEBEEK","Zwevende stoffen",113,"ZS","L111_1020ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1021","ZWALMBEEK","Zwevende stoffen",113,"ZS","L111_1021ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1022","MOLENBEEK (RONSE)","Zwevende stoffen",113,"ZS","L111_1022ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1024","BAVEGEMSE BEEK","Zwevende stoffen",113,"ZS","L111_1024ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1025","MAANBEEK","Zwevende stoffen",113,"ZS","L111_1025ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1027","GROOTEBEEK","Zwevende stoffen",113,"ZS","L111_1027ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1028","LANGELEDE","Zwevende stoffen",113,"ZS","L111_1028ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1029","KLEINE WATERGANG","Zwevende stoffen",113,"ZS","L111_1029ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1030","WATERGANG VAN DE MOERBEKEPOLDER","Zwevende stoffen",113,"ZS","L111_1030ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1031","KANAAL VAN STEKENE","Zwevende stoffen",113,"ZS",{"$f":"_xlfn.CONCAT(A3715,E3715)","v":"L111_1031ZS"},"90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1032","DIJKGRACHT","Zwevende stoffen",113,"ZS","L111_1032ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1033","PAPENMEERSBEEK","Zwevende stoffen",113,"ZS","L111_1033ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1034","NIEUWE GRACHT","Zwevende stoffen",113,"ZS","L111_1034ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1035","KOEVAARDEKEN","Zwevende stoffen",113,"ZS","L111_1035ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1037","MOLENBEEK - LAKEBEEK","Zwevende stoffen",113,"ZS","L111_1037ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1038","MAALBEEK - AMELVONNEBEEK","Zwevende stoffen",113,"ZS","L111_1038ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1039","STEENVOORDBEEK (TERNAT)","Zwevende stoffen",113,"ZS","L111_1039ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1040","BELLEBEEK L1","Zwevende stoffen",113,"ZS","L111_1040ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1041","WINGE L1","Zwevende stoffen",113,"ZS","L111_1041ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1042","LEIBEEK - LIPSEBEEK L1","Zwevende stoffen",113,"ZS","L111_1042ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1043","WEESBEEK L1","Zwevende stoffen",113,"ZS","L111_1043ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1044","KASTEELBEEK","Zwevende stoffen",113,"ZS","L111_1044ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1046","GROTE MOTTE","Zwevende stoffen",113,"ZS","L111_1046ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1047","BAREBEEK L1","Zwevende stoffen",113,"ZS","L111_1047ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1048","ZIJDELINGSGELEED","Zwevende stoffen",113,"ZS","L111_1048ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1049","MUNTLOOP","Zwevende stoffen",113,"ZS","L111_1049ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1050","WEHAGENBEEK","Zwevende stoffen",113,"ZS","L111_1050ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1052","LAAKBEEK","Zwevende stoffen",113,"ZS","L111_1052ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1053","MOUBEEK","Zwevende stoffen",113,"ZS","L111_1053ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1054","GOORBOSBEEK","Zwevende stoffen",113,"ZS","L111_1054ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1056","VROUWVLIET L1","Zwevende stoffen",113,"ZS","L111_1056ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1057","GROTE MOLENBEEK L1","Zwevende stoffen",113,"ZS","L111_1057ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1058","ZWARTE BEEK (WILLEBROEK)","Zwevende stoffen",113,"ZS","L111_1058ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1059","ZIELBEEK - BOSBEEK L1","Zwevende stoffen",113,"ZS","L111_1059ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1060","GROOT SCHIJN L1","Zwevende stoffen",113,"ZS","L111_1060ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1062","HERSELTSELOOP","Zwevende stoffen",113,"ZS","L111_1062ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1063","STEENKENSBEEK","Zwevende stoffen",113,"ZS","L111_1063ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1064","ST. TRUDOLEKEN","Zwevende stoffen",113,"ZS","L111_1064ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1065","ASBEEK","Zwevende stoffen",113,"ZS","L111_1065ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1066","LOEIJENS NEETJE","Zwevende stoffen",113,"ZS","L111_1066ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1067","KLEINE NETE L1","Zwevende stoffen",113,"ZS","L111_1067ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1069","AFWATERINGSGRACHT","Zwevende stoffen",113,"ZS","L111_1069ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1070","WIMP L1","Zwevende stoffen",113,"ZS","L111_1070ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1071","GOORLOOP","Zwevende stoffen",113,"ZS","L111_1071ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1072","POVERSBEEK","Zwevende stoffen",113,"ZS","L111_1072ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1075","MELSTERBEEK L1","Zwevende stoffen",113,"ZS","L111_1075ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1076","CICINDRIA","Zwevende stoffen",113,"ZS","L111_1076ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1077","MOLENBEEK (SINT-TRUIDEN)","Zwevende stoffen",113,"ZS","L111_1077ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1078","GRONDBEEK","Zwevende stoffen",113,"ZS","L111_1078ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1079","HELDERBEEK","Zwevende stoffen",113,"ZS","L111_1079ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1080","ZWARTEBEEK L1","Zwevende stoffen",113,"ZS","L111_1080ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1081","MANGELBEEK L1","Zwevende stoffen",113,"ZS","L111_1081ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1082","SLANGBEEK","Zwevende stoffen",113,"ZS","L111_1082ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1083","MISERIKBEEK","Zwevende stoffen",113,"ZS","L111_1083ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1084","MANDEL L1","Zwevende stoffen",113,"ZS","L111_1084ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1086","LOZERBROEKBEEK","Zwevende stoffen",113,"ZS","L111_1086ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1087","HORSTGATERBEEK","Zwevende stoffen",113,"ZS","L111_1087ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1088","ITTERBEEK L1","Zwevende stoffen",113,"ZS","L111_1088ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1089","WITBEEK","Zwevende stoffen",113,"ZS","L111_1089ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1090","ZANDERBEEK","Zwevende stoffen",113,"ZS","L111_1090ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1091","KIKBEEK","Zwevende stoffen",113,"ZS","L111_1091ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1092","ZOUW","Zwevende stoffen",113,"ZS","L111_1092ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1093","EZELSBEEK","Zwevende stoffen",113,"ZS","L111_1093ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1094","HEULEBEEK L1","Zwevende stoffen",113,"ZS","L111_1094ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1095","KLEINE LAAK","Zwevende stoffen",113,"ZS","L111_1095ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1096","GROTE LAAK L1","Zwevende stoffen",113,"ZS","L111_1096ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1098","KEIBEEK","Zwevende stoffen",113,"ZS","L111_1098ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1099","GAVERSE BEEK (BECQUE DE NEUVILLE)","Zwevende stoffen",113,"ZS","L111_1099ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1101","GROTE KEIGNAERT","Zwevende stoffen",113,"ZS","L111_1101ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1102","KLEINE A - WILDERTSE BEEK","Zwevende stoffen",113,"ZS","L111_1102ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1104","DESPIERREBEEK","Zwevende stoffen",113,"ZS","L111_1104ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1105","MELSENBEEK","Zwevende stoffen",113,"ZS","L111_1105ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1106","DONKSE BEEK","Zwevende stoffen",113,"ZS","L111_1106ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1107","SLIJKVAART","Zwevende stoffen",113,"ZS",{"$f":"_xlfn.CONCAT(A3779,E3779)","v":"L111_1107ZS"},"90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1108","STEENGRACHT","Zwevende stoffen",113,"ZS","L111_1108ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1109","MOERDIJKVAART L1","Zwevende stoffen",113,"ZS","L111_1109ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1110","EDE","Zwevende stoffen",113,"ZS","L111_1110ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1111","GELEEDBEEK - PASSENDALEGELEED","Zwevende stoffen",113,"ZS","L111_1111ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1112","ISABELLASTROOM","Zwevende stoffen",113,"ZS","L111_1112ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1113","LACHENEBEEK","Zwevende stoffen",113,"ZS","L111_1113ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1114","ANTITANKGRACHT ZUID","Zwevende stoffen",113,"ZS","L111_1114ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_1201","S HERTOGENDIJKSE BEEK","Zwevende stoffen",113,"ZS","L111_1201ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_15","HEIDEBEEK (VLETEREN)","Zwevende stoffen",113,"ZS","L111_15ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_18","ST-MACHUITSBEEK","Zwevende stoffen",113,"ZS","L111_18ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_298","OUDE DENDER","Zwevende stoffen",113,"ZS","L111_298ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_315","FONDATIEGRACHT","Zwevende stoffen",113,"ZS","L111_315ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_326","BARBIERBEEK","Zwevende stoffen",113,"ZS","L111_326ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_419","SCHOORBROEKBEEK","Zwevende stoffen",113,"ZS","L111_419ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_436","VELPE L1","Zwevende stoffen",113,"ZS","L111_436ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_624","TAPPELBEEK","Zwevende stoffen",113,"ZS","L111_624ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_627","KLEINE BEEK (ZANDHOVEN)","Zwevende stoffen",113,"ZS","L111_627ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_639","VISBEEK","Zwevende stoffen",113,"ZS","L111_639ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_674","BENEDENVLIET L1","Zwevende stoffen",113,"ZS","L111_674ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_676","WEZELSE BEEK","Zwevende stoffen",113,"ZS","L111_676ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_699","SCHERPENBERGLOOP","Zwevende stoffen",113,"ZS","L111_699ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_707","KLEINE HOOFDGRACHT","Zwevende stoffen",113,"ZS","L111_707ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_717","DESSELSE NEET","Zwevende stoffen",113,"ZS","L111_717ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_724","ANTITANKGRACHT NOORD","Zwevende stoffen",113,"ZS","L111_724ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L111_844","STIEMER","Zwevende stoffen",113,"ZS","L111_844ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L117_1036","ZUUNBEEK L1","Zwevende stoffen",113,"ZS","L117_1036ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L117_1068","HERTSBERGEBEEK - GETEBEEK","Zwevende stoffen",113,"ZS","L117_1068ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L117_1073","RIVIERBEEK","Zwevende stoffen",113,"ZS","L117_1073ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L117_1074","HERK L1","Zwevende stoffen",113,"ZS","L117_1074ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L117_1085","WILDERBEEK","Zwevende stoffen",113,"ZS","L117_1085ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L117_17","STEENVOORDEBEEK (WATOU)","Zwevende stoffen",113,"ZS","L117_17ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L117_219","BURGGRAVENSTROOM","Zwevende stoffen",113,"ZS","L117_219ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L117_232","JOBEEK","Zwevende stoffen",113,"ZS","L117_232ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L117_233","RINGBEEK","Zwevende stoffen",113,"ZS","L117_233ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L117_402","MOLENBEEK - SLAGVIJVERBEEK","Zwevende stoffen",113,"ZS","L117_402ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L117_659","KREKELBEEK","Zwevende stoffen",113,"ZS","L117_659ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L117_673","KLEIN SCHIJN (NOORDELIJK DEEL)","Zwevende stoffen",113,"ZS","L117_673ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L117_813","HERKEBEEK","Zwevende stoffen",113,"ZS","L117_813ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L118_238","KROMMEDIJKBEEK","Zwevende stoffen",113,"ZS","L118_238ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L119_675","KLEIN SCHIJN (ZUIDELIJK DEEL)","Zwevende stoffen",113,"ZS","L119_675ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L120_1097","KASSELRIJBEEK - OOST","Zwevende stoffen",113,"ZS","L120_1097ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L121_1045","GROTEBEEK - WINTERBEEK","Zwevende stoffen",113,"ZS","L121_1045ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L2 Bk","L2 Kleine Beek","Zwevende stoffen",113,"ZS","L2 BkZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["L2 Bk","L2 kleine beek","Zwevende stoffen",113,"ZS","L2 BkZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_102","DEMER V","Zwevende stoffen",113,"ZS","VL05_102ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_103","DEMER VI","Zwevende stoffen",113,"ZS","VL05_103ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_104","DEMER VII","Zwevende stoffen",113,"ZS","VL05_104ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_105","GETE I","Zwevende stoffen",113,"ZS","VL05_105ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_106","GETE II","Zwevende stoffen",113,"ZS","VL05_106ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_108","HERK + KLEINE HERK","Zwevende stoffen",113,"ZS","VL05_108ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_110","MANGELBEEK","Zwevende stoffen",113,"ZS","VL05_110ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_113","MOMBEEK","Zwevende stoffen",113,"ZS","VL05_113ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_114","MUNSTERBEEK","Zwevende stoffen",113,"ZS","VL05_114ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_115","VELPE","Zwevende stoffen",113,"ZS","VL05_115ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_116","WINGE","Zwevende stoffen",113,"ZS","VL05_116ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_118","ZWARTWATER","Zwevende stoffen",113,"ZS","VL05_118ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_12","POPERINGEVAART","Zwevende stoffen",113,"ZS","VL05_12ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_121","AA II","Zwevende stoffen",113,"ZS","VL05_121ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_122","GROTE LAAK","Zwevende stoffen",113,"ZS","VL05_122ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_124","GROTE NETE II","Zwevende stoffen",113,"ZS","VL05_124ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_130","WAMP","Zwevende stoffen",113,"ZS","VL05_130ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_131","WIMP","Zwevende stoffen",113,"ZS","VL05_131ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_134","BERWIJN","Zwevende stoffen",113,"ZS","VL05_134ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_135","BOSBEEK","Zwevende stoffen",113,"ZS",{"$f":"_xlfn.CONCAT(A3843,E3843)","v":"VL05_135ZS"},"90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_136","DOMMEL","Zwevende stoffen",113,"ZS","VL05_136ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_137","ITTERBEEK I","Zwevende stoffen",113,"ZS","VL05_137ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_138","ITTERBEEK II","Zwevende stoffen",113,"ZS","VL05_138ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_14","VLADSLOVAART","Zwevende stoffen",113,"ZS","VL05_14ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_140","JEKER II","Zwevende stoffen",113,"ZS","VL05_140ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_141","LOSSING","Zwevende stoffen",113,"ZS","VL05_141ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_146","MERKSKE","Zwevende stoffen",113,"ZS","VL05_146ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_148","WEERIJSEBEEK","Zwevende stoffen",113,"ZS","VL05_148ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_150","AFLEIDINGSKANAAL van de LEIE/SCHIPDONKKANAAL I","Zwevende stoffen",113,"ZS","VL05_150ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_152","AVRIJEVAART + SLEIDINGSVAARDEKE","Zwevende stoffen",113,"ZS","VL05_152ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_153","BERGENVAART","Zwevende stoffen",113,"ZS","VL05_153ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_159","KANAAL CHARLEROI-BRUSSEL","Zwevende stoffen",113,"ZS","VL05_159ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_163","KANAAL GENT-OOSTENDE II","Zwevende stoffen",113,"ZS","VL05_163ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_166","KANAAL IEPER-IJZER","Zwevende stoffen",113,"ZS","VL05_166ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_167","KANAAL LEUVEN-DIJLE","Zwevende stoffen",113,"ZS","VL05_167ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_17","ISABELLAVAART","Zwevende stoffen",113,"ZS","VL05_17ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_170","KANAAL VAN BEVERLO","Zwevende stoffen",113,"ZS","VL05_170ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_171","LEDE","Zwevende stoffen",113,"ZS","VL05_171ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_175","MOERVAART","Zwevende stoffen",113,"ZS","VL05_175ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_177","NIEUWE KALE","Zwevende stoffen",113,"ZS","VL05_177ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_18","KERKEBEEK","Zwevende stoffen",113,"ZS","VL05_18ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_180","ZARRENBEEK","Zwevende stoffen",113,"ZS","VL05_180ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_182","ZUIDLEDE","Zwevende stoffen",113,"ZS","VL05_182ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_2","GROTE KEMMELBEEK","Zwevende stoffen",113,"ZS","VL05_2ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_20","RIVIERBEEK + HERTSBERGEBEEK","Zwevende stoffen",113,"ZS","VL05_20ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_21","ZUIDERVAARTJE","Zwevende stoffen",113,"ZS","VL05_21ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_22","ZWINNEVAART","Zwevende stoffen",113,"ZS","VL05_22ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_24","MEREBEEK + BORISGRACHT + LIEVE","Zwevende stoffen",113,"ZS","VL05_24ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_25","OUDE KALE","Zwevende stoffen",113,"ZS","VL05_25ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_28","BENEDENVLIET","Zwevende stoffen",113,"ZS","VL05_28ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_3","HANDZAMEVAART","Zwevende stoffen",113,"ZS","VL05_3ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_30","GROTE MOLENBEEK - DE VLIET","Zwevende stoffen",113,"ZS","VL05_30ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_31","KALKENSE VAART","Zwevende stoffen",113,"ZS","VL05_31ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_32","MOLENBEEK - GROTE BEEK","Zwevende stoffen",113,"ZS","VL05_32ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_34","NOORD-ZUIDVERBINDING","Zwevende stoffen",113,"ZS","VL05_34ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_38","ZIELBEEK - BOSBEEK","Zwevende stoffen",113,"ZS","VL05_38ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_4","HEIDEBEEK","Zwevende stoffen",113,"ZS","VL05_4ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_44","DEVEBEEK","Zwevende stoffen",113,"ZS","VL05_44ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_45","GAVERBEEK I","Zwevende stoffen",113,"ZS","VL05_45ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_46","GAVERBEEK II","Zwevende stoffen",113,"ZS","VL05_46ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_5","IEPERLEE + VERWEZEN KANAAL IEPER-KOMEN","Zwevende stoffen",113,"ZS","VL05_5ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_50","LEIE III","Zwevende stoffen",113,"ZS","VL05_50ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_51","MANDEL I","Zwevende stoffen",113,"ZS","VL05_51ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_52","MANDEL II","Zwevende stoffen",113,"ZS","VL05_52ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_53","OUDE MANDEL","Zwevende stoffen",113,"ZS","VL05_53ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_58","BOVEN-SCHELDE IV","Zwevende stoffen",113,"ZS","VL05_58ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_6","IEPERLEED","Zwevende stoffen",113,"ZS","VL05_6ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_61","RONE","Zwevende stoffen",113,"ZS","VL05_61ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_62","STAMPKOTBEEK","Zwevende stoffen",113,"ZS","VL05_62ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_64","ZWARTE SPIEREBEEK","Zwevende stoffen",113,"ZS","VL05_64ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_67","DENDER I","Zwevende stoffen",113,"ZS","VL05_67ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_70","DENDER IV","Zwevende stoffen",113,"ZS","VL05_70ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_73","MOLENBEEK - PACHTBOSBEEK","Zwevende stoffen",113,"ZS","VL05_73ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_75","VONDELBEEK","Zwevende stoffen",113,"ZS","VL05_75ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_77","DIJLE I","Zwevende stoffen",113,"ZS","VL05_77ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_81","DIJLE V","Zwevende stoffen",113,"ZS","VL05_81ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_85","LEIBEEK - LAAKBEEK","Zwevende stoffen",113,"ZS","VL05_85ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_86","NETHEN","Zwevende stoffen",113,"ZS","VL05_86ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_87","VOER (Leuven)","Zwevende stoffen",113,"ZS","VL05_87ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_89","VUNT","Zwevende stoffen",113,"ZS","VL05_89ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_90","WEESBEEK","Zwevende stoffen",113,"ZS","VL05_90ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_93","ZENNE II","Zwevende stoffen",113,"ZS","VL05_93ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_98","DEMER I","Zwevende stoffen",113,"ZS","VL05_98ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL05_99","DEMER II","Zwevende stoffen",113,"ZS",{"$f":"_xlfn.CONCAT(A3907,E3907)","v":"VL05_99ZS"},"90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_125","GROTE NETE III","Zwevende stoffen",113,"ZS","VL08_125ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_157","ISABELLAWATERING","Zwevende stoffen",113,"ZS","VL08_157ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_16","BLANKENBERGSE VAART + NOORDEDE","Zwevende stoffen",113,"ZS","VL08_16ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_162","KANAAL GENT-OOSTENDE I + COUPURE + VERBINDINGSKANAAL","Zwevende stoffen",113,"ZS","VL08_162ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_164","KANAAL GENT-OOSTENDE III","Zwevende stoffen",113,"ZS","VL08_164ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_172","LEOPOLDKANAAL I","Zwevende stoffen",113,"ZS","VL08_172ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_173","LEOPOLDKANAAL II","Zwevende stoffen",113,"ZS","VL08_173ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_176","NETEKANAAL","Zwevende stoffen",113,"ZS","VL08_176ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_178","NOORDELIJKE RINGVAART","Zwevende stoffen",113,"ZS","VL08_178ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_179","WESTELIJKE RINGVAART","Zwevende stoffen",113,"ZS","VL08_179ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_27","ZWARTESLUISBEEK","Zwevende stoffen",113,"ZS","VL08_27ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_55","BOVEN-SCHELDE I","Zwevende stoffen",113,"ZS","VL08_55ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_7","IJZER I","Zwevende stoffen",113,"ZS","VL08_7ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_71","DENDER V","Zwevende stoffen",113,"ZS","VL08_71ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_72","MARK (Denderbekken)","Zwevende stoffen",113,"ZS","VL08_72ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_80","DIJLE IV","Zwevende stoffen",113,"ZS","VL08_80ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_82","DIJLE VI","Zwevende stoffen",113,"ZS","VL08_82ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL08_92","ZENNE I","Zwevende stoffen",113,"ZS","VL08_92ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL09_78","DIJLE II","Zwevende stoffen",113,"ZS","VL09_78ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_10","MARTJEVAART","Zwevende stoffen",113,"ZS","VL11_10ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_109","KLEINE GETE + VLOEDGRACHT","Zwevende stoffen",113,"ZS","VL11_109ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_11","MOERDIJKVAART","Zwevende stoffen",113,"ZS","VL11_11ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_117","ZWARTEBEEK","Zwevende stoffen",113,"ZS","VL11_117ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_120","AA I","Zwevende stoffen",113,"ZS","VL11_120ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_123","GROTE NETE I","Zwevende stoffen",113,"ZS","VL11_123ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_126","KLEINE NETE I","Zwevende stoffen",113,"ZS","VL11_126ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_127","KLEINE NETE II","Zwevende stoffen",113,"ZS","VL11_127ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_128","MOL NEET","Zwevende stoffen",113,"ZS","VL11_128ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_13","VEURNE AMBACHT POLDER WATERLOPEN","Zwevende stoffen",113,"ZS","VL11_13ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_133","ABEEK","Zwevende stoffen",113,"ZS","VL11_133ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_145","MARK (Maas)","Zwevende stoffen",113,"ZS","VL11_145ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_165","KANAAL GENT-TERNEUZEN + GENTSE HAVENDOKKEN","Zwevende stoffen",113,"ZS","VL11_165ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_19","OOSTENDS KREKENGEBIED","Zwevende stoffen",113,"ZS","VL11_19ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_203","MAAS I+II+III","Zwevende stoffen",113,"ZS","VL11_203ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_205","DEMER III+IV","Zwevende stoffen",113,"ZS","VL11_205ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_207","MELSTERBEEK I+II","Zwevende stoffen",113,"ZS","VL11_207ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_37","WATERLOOP VAN DE HOGE LANDEN + MELKADER","Zwevende stoffen",113,"ZS","VL11_37ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_59","GROTE SPIEREBEEK","Zwevende stoffen",113,"ZS","VL11_59ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_63","ZWALM","Zwevende stoffen",113,"ZS","VL11_63ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_76","BAREBEEK","Zwevende stoffen",113,"ZS","VL11_76ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_83","IJSSE","Zwevende stoffen",113,"ZS","VL11_83ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_84","LAAN","Zwevende stoffen",113,"ZS","VL11_84ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_88","VROUWVLIET","Zwevende stoffen",113,"ZS","VL11_88ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL11_91","WOLUWE","Zwevende stoffen",113,"ZS","VL11_91ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_147","WARMBEEK","Zwevende stoffen",113,"ZS","VL17_147ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_154","BRAKELEIKEN + LIEVE","Zwevende stoffen",113,"ZS","VL17_154ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_156","GENTSE BINNENWATEREN","Zwevende stoffen",113,"ZS","VL17_156ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_161","KANAAL DUINKERKE-NIEUWPOORT","Zwevende stoffen",113,"ZS","VL17_161ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_168","KANAAL PLASSENDALE-NIEUWPOORT","Zwevende stoffen",113,"ZS","VL17_168ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_169","KANAAL ROESELARE-LEIE","Zwevende stoffen",113,"ZS","VL17_169ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_174","LOKANAAL","Zwevende stoffen",113,"ZS","VL17_174ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_204","BOVEN-SCHELDE II+III","Zwevende stoffen",113,"ZS","VL17_204ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_206","DENDER II+III","Zwevende stoffen",113,"ZS","VL17_206ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_29","GROOT SCHIJN","Zwevende stoffen",113,"ZS","VL17_29ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_35","VERLEGDE SCHIJN - HOOFDGRACHT","Zwevende stoffen",113,"ZS","VL17_35ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_48","LEIE I","Zwevende stoffen",113,"ZS","VL17_48ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_49","LEIE II","Zwevende stoffen",113,"ZS","VL17_49ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_54","TOERISTISCHE LEIE","Zwevende stoffen",113,"ZS","VL17_54ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_60","MOLENBEEK - MAARKEBEEK","Zwevende stoffen",113,"ZS","VL17_60ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_66","BELLEBEEK","Zwevende stoffen",113,"ZS","VL17_66ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL17_9","IJZER III","Zwevende stoffen",113,"ZS","VL17_9ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL20_36","VERLEGDE SCHIJN - VOORGRACHT","Zwevende stoffen",113,"ZS","VL20_36ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL20_96","BEGIJNENBEEK","Zwevende stoffen",113,"ZS","VL20_96ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL21_1","BLANKAART WATERLOPEN","Zwevende stoffen",113,"ZS",{"$f":"_xlfn.CONCAT(A3971,E3971)","v":"VL21_1ZS"},"90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL21_107","GROTE GETE + BORGGRACHT","Zwevende stoffen",113,"ZS","VL21_107ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL21_129","MOLENBEEK - BOLLAAK","Zwevende stoffen",113,"ZS","VL21_129ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL21_139","JEKER I","Zwevende stoffen",113,"ZS","VL21_139ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL21_26","POEKEBEEK","Zwevende stoffen",113,"ZS","VL21_26ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL21_33","MOLENBEEK - KOTTEMBEEK","Zwevende stoffen",113,"ZS","VL21_33ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL21_47","HEULEBEEK","Zwevende stoffen",113,"ZS","VL21_47ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL21_74","MOLENBEEK - TER ERPENBEEK","Zwevende stoffen",113,"ZS","VL21_74ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL21_79","DIJLE III","Zwevende stoffen",113,"ZS","VL21_79ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL21_8","IJZER II","Zwevende stoffen",113,"ZS","VL21_8ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL21_94","ZUUNBEEK","Zwevende stoffen",113,"ZS","VL21_94ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL21_97","DE HULPE - ZWART WATER","Zwevende stoffen",113,"ZS","VL21_97ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL22_208","ALBERTKANAAL - Maasbekken","Zwevende stoffen",113,"ZS","VL22_208ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL22_209","ALBERTKANAAL - Demerbekken","Zwevende stoffen",113,"ZS","VL22_209ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL22_210","ALBERTKANAAL - Netebekken","Zwevende stoffen",113,"ZS","VL22_210ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL22_211","ALBERTKANAAL - Benedenscheldebekken","Zwevende stoffen",113,"ZS","VL22_211ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL22_212","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Netebekken","Zwevende stoffen",113,"ZS","VL22_212ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL22_213","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Maasbekken","Zwevende stoffen",113,"ZS","VL22_213ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL22_214","KANAAL DESSEL-KWAADMECHELEN + KANAAL DESSEL-SCHOTEN + KANAAL BOCHOLT-HERENTALS - Benedenscheldebekken","Zwevende stoffen",113,"ZS","VL22_214ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL22_215","ZEEKANAAL BRUSSEL-SCHELDE - Dijle-Zennebekken","Zwevende stoffen",113,"ZS","VL22_215ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL22_216","ZEEKANAAL BRUSSEL-SCHELDE - Benedenscheldebekken","Zwevende stoffen",113,"ZS","VL22_216ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL22_217","AFLEIDINGSKANAAL van de LEIE II + KANAAL van EEKLO - Bekken van de Gentse kanalen","Zwevende stoffen",113,"ZS","VL22_217ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL22_218","AFLEIDINGSKANAAL van de LEIE II - Bekken van de Brugse polders","Zwevende stoffen",113,"ZS","VL22_218ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL22_219","KANAAL BOSSUIT-KORTRIJK - Bovenscheldebekken","Zwevende stoffen",113,"ZS","VL22_219ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL22_220","KANAAL BOSSUIT-KORTRIJK - Leiebekken","Zwevende stoffen",113,"ZS","VL22_220ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
["VL22_221","ZUID-WILLEMSVAART + KANAAL BOCHOLT-HERENTALS (deels) + KANAAL BRIEGDEN-NEERHAREN","Zwevende stoffen",113,"ZS","VL22_221ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]

{"sheet":"Criteria volgens stofcategorie","index":11,"n_rows":122,"n_cols":28,"rows_kept":122,"cut":false,"hidden":true,"merged":[[66,0,66,2],[97,0,97,2],[2,0,2,2],[4,0,4,2],[33,0,33,2],[35,0,35,2],[0,7,0,10],[1,8,1,9],[0,23,0,26],[1,24,1,25],[0,11,0,14],[0,15,0,18],[1,16,1,17],[0,19,0,22],[1,20,1,21]]}
["Cat 1","Milieuvoordeel primeert sterk tov haalbaarheid",null,null,null,null,null,"Bijkomende kostprijs tov huidige WZ",null,null,null,"Kostprijs technologie (EUR/m³)",null,null,null,"Kengetallen BBT - omzet",null,null,null,"Kengetallen BBT - toegevoegde waarde",null,null,null,"Kengetallen BBT - EBIDTA",null,null,null,"BBT/meer dan BBT"]
[null,null,null,null,null,null,null,"Aanvaardbaar ","Intermediair",null,"Niet aanvaardbaar",null,null,null,null,"betaalbaar","Intermediair",null,"Niet betaalbaar","betaalbaar","Intermediair",null,"Niet betaalbaar","betaalbaar","Intermediair",null,"Niet betaalbaar"]
["ENKEL VMM - aanpassing criteria (pas gele cellen aan)",null,null,null,null,"Stof x impactcategorie","Stof x impactcategorie weergave","Ondergrens","ondergrens","bovengrens","bovengrens",1,2,3,4,"ondergrens","Ondergrens","bovengrens","ondergrens","ondergrens","Ondergrens","bovengrens","Bovengrens","ondergrens","Ondergrens","bovengrens","Bovengrens"]
[null,null,null,null,null,1,1,{"$f":"B7","v":0.5},{"$f":"B8","v":0.5},{"$f":"C8","v":1},{"$f":"B9","v":1},{"$f":"B15","v":20},{"$f":"B16","v":12},{"$f":"B17","v":3},{"$f":"B18","v":"te bekijken"},{"$f":"B23","v":5.0000000000000001E-3},{"$f":"P4","v":5.0000000000000001E-3},{"$f":"C23","v":0.05},{"$f":"D23","v":0.05},{"$f":"B24","v":0.02},{"$f":"T4","v":0.02},{"$f":"C24","v":0.5},{"$f":"D24","v":0.5},{"$f":"B25","v":0.1},{"$f":"X4","v":0.1},{"$f":"C25","v":1},{"$f":"D25","v":1},{"$f":"A29","v":"Bovenste kostencurve"}]
["Bijkomende kostprijs tov huidige WZ",null,null,null,null,2,1,{"$f":"B38","v":0.5},{"$f":"B39","v":0.5},{"$f":"C39","v":1},{"$f":"B40","v":1},{"$f":"B46","v":20},{"$f":"B47","v":12},{"$f":"B48","v":3},{"$f":"B49","v":"te bekijken"},{"$f":"B54","v":5.0000000000000001E-3},{"$f":"P5","v":5.0000000000000001E-3},{"$f":"C54","v":0.05},{"$f":"D54","v":0.05},{"$f":"B55","v":0.02},{"$f":"T5","v":0.02},{"$f":"C55","v":0.5},{"$f":"D55","v":0.5},{"$f":"B56","v":0.1},{"$f":"X5","v":0.1},{"$f":"C56","v":1},{"$f":"D56","v":1},{"$f":"A60","v":"Bovenste kostencureve"}]
[null,null,null,null,null,3,2,{"$f":"B69","v":0.5},{"$f":"B70","v":0.5},{"$f":"C70","v":1},{"$f":"B71","v":1},{"$f":"B77","v":20},{"$f":"B78","v":12},{"$f":"B79","v":3},{"$f":"B80","v":"te bekijken"},{"$f":"B85","v":5.0000000000000001E-3},5.0000000000000001E-3,{"$f":"C85","v":0.05},{"$f":"D85","v":0.05},{"$f":"B86","v":0.02},0.02,{"$f":"C86","v":0.5},{"$f":"D86","v":0.5},{"$f":"B87","v":0.1},0.1,{"$f":"C87","v":1},{"$f":"D87","v":1},{"$f":"A91","v":"Onderste kostencurve"}]
["Aanvaardbaard (… <)",0.5,null,null,null,4,2,{"$f":"B100","v":0.5},{"$f":"B101","v":0.5},{"$f":"C101","v":1},{"$f":"B102","v":1},{"$f":"B108","v":20},{"$f":"B109","v":12},{"$f":"B110","v":3},{"$f":"B111","v":"te bekijken"},{"$f":"B116","v":5.0000000000000001E-3},5.0000000000000001E-3,{"$f":"C116","v":0.05},{"$f":"D116","v":0.05},{"$f":"B117","v":0.02},0.02,{"$f":"C117","v":0.5},{"$f":"D117","v":0.5},{"$f":"B118","v":0.1},0.1,{"$f":"C118","v":1},{"$f":"D118","v":1},{"$f":"A122","v":"Onderste kostencurve"}]
["Intermediair",0.5,1]
["Niet aanvaardbaar (> …)",1]
[]
[null,null,null,null,null,null,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22]
["Kostprijs (€/m³)"]
[null,"(info redelijkheid)",null,"(toetsing)"]
["Technologie","€/m³",null,"€/m³"]
[1,20,null,6]
[2,12,null,12]
[3,3]
[4,"te bekijken"]
[]
["Kengetallen BBT"]
[]
["Jaarlijkse kosten vs.","Betaalbaar (… <)","Intermediair bovengrens","Niet betaalbaar (> …)"]
["Omzet",5.0000000000000001E-3,0.05,0.05]
["Toegevoegde waarde",0.02,0.5,0.5]
["EBIDTA",0.1,1,1]
[]
[]
["KE"]
["Bovenste kostencurve"]
[]
[]
["Cat 2","Milieuvoordeel primeert tov haalbaarheid"]
[]
["ENKEL VMM - aanpassing criteria (pas gele cellen aan)"]
[]
["Bijkomende kostprijs tov huidige WZ"]
[]
["Aanvaardbaard (… <)",0.5]
["Intermediair",0.5,1]
["Niet aanvaardbaar (> …)",1]
[]
[]
["Kostprijs (€/m³)"]
[null,"(info redelijkheid)",null,"(toetsing)"]
["Technologie","€/m³",null,"€/m³"]
[1,20,null,6]
[2,12,null,12]
[3,3]
[4,"te bekijken"]
[]
["Kengetallen BBT"]
[]
["Jaarlijkse kosten vs.","Betaalbaar (… <)","Intermediair bovengrens","Niet betaalbaar (> …)"]
["Omzet",5.0000000000000001E-3,0.05,0.05]
["Toegevoegde waarde",0.02,0.5,0.5]
["EBIDTA",0.1,1,1]
[]
[]
["KE"]
["Bovenste kostencureve"]
[]
[]
["Cat 3","Milieuvoordeel staat gelijk aan haalbaarheid"]
[]
["ENKEL VMM - aanpassing criteria (pas gele cellen aan)"]
[]
["Bijkomende kostprijs tov huidige WZ"]
[]
["Aanvaardbaard (… <)",0.5]
["Intermediair",0.5,1]
["Niet aanvaardbaar (> …)",1]
[]
[]
["Kostprijs (€/m³)"]
[null,"(info redelijkheid)",null,"(toetsing)"]
["Technologie","€/m³",null,"€/m³"]
[1,20,null,6]
[2,12,null,12]
[3,3]
[4,"te bekijken"]
[]
["Kengetallen BBT"]
[]
["Jaarlijkse kosten vs.","Betaalbaar (… <)","Intermediair bovengrens","Niet betaalbaar (> …)"]
["Omzet",5.0000000000000001E-3,0.05,0.05]
["Toegevoegde waarde",0.02,0.5,0.5]
["EBIDTA",0.1,1,1]
[]
[]
["KE"]
["Onderste kostencurve"]
[]
[]
["Cat 4","Haalbaarheid primeert"]
[]
["ENKEL VMM - aanpassing criteria (pas gele cellen aan)"]
[]
["Bijkomende kostprijs tov huidige WZ"]
[]
["Aanvaardbaard (… <)",0.5]
["Intermediair",0.5,1]
["Niet aanvaardbaar (> …)",1]
[]
[]
["Kostprijs (€/m³)"]
[null,"(info redelijkheid)",null,"(toetsing)"]
["Technologie","€/m³",null,"€/m³"]
[1,20,null,6]
[2,12,null,12]
[3,3]
[4,"te bekijken"]
[]
["Kengetallen BBT"]
[]
["Jaarlijkse kosten vs.","Betaalbaar (… <)","Intermediair bovengrens","Niet betaalbaar (> …)"]
["Omzet",5.0000000000000001E-3,0.05,0.05]
["Toegevoegde waarde",0.02,0.5,0.5]
["EBIDTA",0.1,1,1]
[]
[]
["KE"]
["Onderste kostencurve"]

{"sheet":"Samenvatting econ kengetallen","index":12,"n_rows":87,"n_cols":10,"rows_kept":87,"cut":false,"hidden":true,"merged":[[67,8,67,9],[76,8,76,9]]}
[]
["Exploitatie-ID"]
["Vestegingsnaam",{"$f":"'Input financiële kengetallen'!B22","v":"Naam Vestiging"},null,null,null,"Toetsing gebeurt met data incl baten"]
[]
["Bijkomende kostprijs tov huidige WZ (enkel opex)",null,{"$f":"B35","v":{"$error":"#DIV/0!"}}]
["Bijkomende kostprijs (€/m³)",null,{"$f":"B28","v":{"$error":"#DIV/0!"}}]
["Huidige WZ"]
["YCC huidige WZ",{"$f":"'Input huidige maatreg. (fac.)'!D37","v":0},"EUR/jaar"]
["Opex huidige WZ",{"$f":"'Input huidige maatreg. (fac.)'!H37","v":0},"EUR/jaar"]
["Behandeld volume huidige WZ",{"$f":"'Input huidige maatreg. (fac.)'!D10","v":0},"m³/jaar"]
[]
["Jaarlijkse kost huidige WZ (Opex + YCC)",{"$f":"B9+B8","v":0},"EUR/jaar"]
["huidige kost WZ per m³ (capex+opex)",{"$f":"'Input huidige maatreg. (fac.)'!D42","v":0},"EUR/m³"]
["huidige kost WZ per m³ (enkel opex)",{"$f":"'Input huidige maatreg. (fac.)'!H38","v":0},"EUR/m³"]
[]
["Bijkomende WZ"]
["Investering (eenmalig)",{"$f":"'Input bijkomende maatregelen'!D68","v":0},"EUR"]
["Jaarlijkse kapitaalkost (YCC)",{"$f":"'Input bijkomende maatregelen'!D72","v":0},"EUR/jaar"]
["Werkingskosten (Opex)",{"$f":"'Input bijkomende maatregelen'!G72","v":0},"EUR/jaar"]
["Baten",{"$f":"'Input bijkomende maatregelen'!J72","v":0},"EUR/jaar"]
[]
["Behandeld volume via bijkomende WZ",{"$f":"'Input bijkomende maatregelen'!D8","v":0},"m³/jaar"]
["Totaal volume geloosd AW",{"$f":"'Input huidige maatreg. (fac.)'!D10","v":0},"m³/jaar"]
["Jaarlijkse kost bijkomende WZ (Opex + YCC)",{"$f":"B19+B18","v":0},"EUR/jaar"]
["Jaarlijkse kost bijkomende WZ, rekening houdende met baten (Opex + YCC - Baten)",{"$f":"B24-B20","v":0},"EUR/jaar"]
[]
["Bijkomende kost WZ per m³",{"$f":"B24/B22","v":{"$error":"#DIV/0!"}},"EUR/m³"]
["Bijkomende kost WZ per m³ (incl baten)",{"$f":"B25/B22","v":{"$error":"#DIV/0!"}},"EUR/m³"]
[]
["Huidige VS bijkomende WZ (%)"]
["Ratio kost bijkomende WZ vs opex huidige WZ - behandeling volledige stroom",{"$f":"B27/B14","v":{"$error":"#DIV/0!"}},"(opex + ycc) / (huidige opex)"]
["Ratio kost bijkomende WZ (incl. baten) vs opex & YCC huidige WZ - behandeling volledige stroom",{"$f":"B28/B14","v":{"$error":"#DIV/0!"}},"(opex + ycc - baten) / (huidige opex)"]
["Ratio kost bijkomende WZ (incl. baten) vs opex huidige WZ - behandeling volledige stroom",{"$f":"B28/B13","v":{"$error":"#DIV/0!"}},"(opex + ycc - baten) / (huidige opex + huidige ycc)"]
["Ratio kost bijkomende WZ vs opex huidige WZ - deelstroombehandeling",{"$f":"B24/B9","v":{"$error":"#DIV/0!"}},"(opex + ycc)/ (huidige opex)"]
["Ratio kost bijkomende WZ (incl. baten) vs opex & ycc huidige WZ - deelstroombehandeling",{"$f":"B25/B9","v":{"$error":"#DIV/0!"}},"(opex + ycc - baten) / (huidige opex)"]
["Ratio kost bijkomende WZ (incl. baten) vs opex & ycc huidige WZ - deelstroombehandeling",{"$f":"B25/B12","v":{"$error":"#DIV/0!"}},"(opex + ycc - baten) / (huidige opex + huidige ycc)"]
[]
[]
["Kostenefficiëntie per parameter"]
[]
[]
["Probleemparameters","Gem. Jaarlijkse verwijdering - huidige WZ","Kostenefficientie - huidige WZ - Opex+YCC","Kostenefficientie - huidige WZ - enkel opex","Gem. jaarlijkse verwijdering - bijkomende WZ","Kostenefficientie bijkomende WZ","Ratio KE bijkomende WZ vs KE huidige WZ"]
[null,"kg/jaar","EUR/kg","EUR/kg","kg/jaar","EUR/kg","%"]
[{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input impactbeoordeing'!B20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input huidige maatreg. (fac.)'!J17)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",$B$12/B44)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",$B$9/B44)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",'Input bijkomende maatregelen'!I27)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B20)=TRUE,\"\",$B$25/E44)","v":""},{"$f":"IFERROR(C44/F44,\"\")","v":""}]
[{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input impactbeoordeing'!B21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input huidige maatreg. (fac.)'!J18)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",$B$12/B45)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",$B$9/B45)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",'Input bijkomende maatregelen'!I28)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B21)=TRUE,\"\",$B$25/E45)","v":""},{"$f":"IFERROR(C45/F45,\"\")","v":""}]
[{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input impactbeoordeing'!B22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input huidige maatreg. (fac.)'!J19)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",$B$12/B46)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",$B$9/B46)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",'Input bijkomende maatregelen'!I29)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B22)=TRUE,\"\",$B$25/E46)","v":""},""]
[{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input impactbeoordeing'!B23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input huidige maatreg. (fac.)'!J20)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",$B$12/B47)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",$B$9/B47)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",'Input bijkomende maatregelen'!I30)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B23)=TRUE,\"\",$B$25/E47)","v":""},""]
[{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input impactbeoordeing'!B24)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input huidige maatreg. (fac.)'!J21)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",$B$12/B48)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",$B$9/B48)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",'Input bijkomende maatregelen'!I31)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B24)=TRUE,\"\",$B$25/E48)","v":""},""]
[{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input impactbeoordeing'!B25)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input huidige maatreg. (fac.)'!J22)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",$B$12/B49)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",$B$9/B49)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",'Input bijkomende maatregelen'!I32)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B25)=TRUE,\"\",$B$25/E49)","v":""},""]
[{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input impactbeoordeing'!B26)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input huidige maatreg. (fac.)'!J23)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",$B$12/B50)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",$B$9/B50)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",'Input bijkomende maatregelen'!I33)","v":""},{"$f":"IF(ISBLANK('Input impactbeoordeing'!B26)=TRUE,\"\",$B$25/E50)","v":""},""]
[null,null,null,null,null,{"$f":"IF(ISBLANK('Input impactbeoordeing'!B27)=TRUE,\"\",$B$25/E51)","v":""}]
[]
[]
[]
["Technologietoets"]
["Techniek"]
["ID",{"$f":"VLOOKUP('Input bijkomende maatregelen'!D6,'Input bijkomende maatregelen'!R3:S17,2,)","v":{"$error":"#N/A"}},{"$f":"'Input bijkomende maatregelen'!D6","v":0}]
[]
[]
[]
[]
["Toetsing Kengetallen BBT+"]
["- Vestiging","Omzet",{"$f":"I70","v":{"$error":"#DIV/0!"}},null,"Toegevoegde waarde",{"$f":"I71","v":{"$error":"#DIV/0!"}},null,"EBIDTA",{"$f":"I72","v":{"$error":"#DIV/0!"}}]
["- Group/holding","Omzet",{"$f":"I79","v":{"$error":"#DIV/0!"}},null,"Toegevoegde waarde",{"$f":"I80","v":{"$error":"#DIV/0!"}},null,"EBIDTA",{"$f":"I81","v":{"$error":"#DIV/0!"}}]
[]
["Financiële data van de vestiging"]
[]
[null,"Jaar",null,null,null,null,null,null,"Resultaat (incl baten)"]
[null,{"$f":"'Input financiële kengetallen'!B27","v":2024},{"$f":"'Input financiële kengetallen'!C27","v":2023},{"$f":"'Input financiële kengetallen'!D27","v":2022},{"$f":"'Input financiële kengetallen'!E27","v":2021},{"$f":"'Input financiële kengetallen'!F27","v":2020},"gemiddeld",null,"Opex+YCC-baten","2x"]
["Omzet EUR",{"$f":"IF('Input financiële kengetallen'!B29=0,\"\",'Input financiële kengetallen'!B29)","v":""},{"$f":"IF('Input financiële kengetallen'!C29=0,\"\",'Input financiële kengetallen'!C29)","v":""},{"$f":"IF('Input financiële kengetallen'!D29=0,\"\",'Input financiële kengetallen'!D29)","v":""},{"$f":"IF('Input financiële kengetallen'!E29=0,\"\",'Input financiële kengetallen'!E29)","v":""},{"$f":"IF('Input financiële kengetallen'!F29=0,\"\",'Input financiële kengetallen'!F29)","v":""},{"$f":"AVERAGE(B70:F70)","v":{"$error":"#DIV/0!"}},null,{"$f":"$B$25/($G70)","v":{"$error":"#DIV/0!"}},{"$f":"2*$B$25/($G70)","v":{"$error":"#DIV/0!"}}]
["Toegevoegde waarde EUR",{"$f":"IF('Input financiële kengetallen'!B31=0,\"\",'Input financiële kengetallen'!B31)","v":""},{"$f":"IF('Input financiële kengetallen'!C31=0,\"\",'Input financiële kengetallen'!C31)","v":""},{"$f":"IF('Input financiële kengetallen'!D31=0,\"\",'Input financiële kengetallen'!D31)","v":""},{"$f":"IF('Input financiële kengetallen'!E31=0,\"\",'Input financiële kengetallen'!E31)","v":""},{"$f":"IF('Input financiële kengetallen'!F31=0,\"\",'Input financiële kengetallen'!F31)","v":""},{"$f":"AVERAGE(B71:F71)","v":{"$error":"#DIV/0!"}},null,{"$f":"$B$25/($G71)","v":{"$error":"#DIV/0!"}},{"$f":"2*$B$25/($G71)","v":{"$error":"#DIV/0!"}}]
["EBIDTA",{"$f":"IF('Input financiële kengetallen'!B33=0,\"\",'Input financiële kengetallen'!B33)","v":""},{"$f":"IF('Input financiële kengetallen'!C33=0,\"\",'Input financiële kengetallen'!C33)","v":""},{"$f":"IF('Input financiële kengetallen'!D33=0,\"\",'Input financiële kengetallen'!D33)","v":""},{"$f":"IF('Input financiële kengetallen'!E33=0,\"\",'Input financiële kengetallen'!E33)","v":""},{"$f":"IF('Input financiële kengetallen'!F33=0,\"\",'Input financiële kengetallen'!F33)","v":""},{"$f":"AVERAGE(B72:F72)","v":{"$error":"#DIV/0!"}},null,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
[]
["Financiële data group/holding"]
[]
[null,"Jaar",null,null,null,null,null,null,"Resultaat (incl baten)"]
[null,{"$f":"'Input financiële kengetallen'!B12","v":2024},{"$f":"'Input financiële kengetallen'!C12","v":2023},{"$f":"'Input financiële kengetallen'!D12","v":2022},{"$f":"'Input financiële kengetallen'!E12","v":2021},{"$f":"'Input financiële kengetallen'!F12","v":2020},"gemiddeld",null,"Opex+YCC-baten","2x"]
["Omzet EUR",{"$f":"IF('Input financiële kengetallen'!B14=0,\"\",'Input financiële kengetallen'!B14)","v":""},{"$f":"IF('Input financiële kengetallen'!C14=0,\"\",'Input financiële kengetallen'!C14)","v":""},{"$f":"IF('Input financiële kengetallen'!D14=0,\"\",'Input financiële kengetallen'!D14)","v":""},{"$f":"IF('Input financiële kengetallen'!E14=0,\"\",'Input financiële kengetallen'!E14)","v":""},{"$f":"IF('Input financiële kengetallen'!F14=0,\"\",'Input financiële kengetallen'!F14)","v":""},{"$f":"AVERAGE(B79:F79)","v":{"$error":"#DIV/0!"}},null,{"$f":"$B$25/($G79)","v":{"$error":"#DIV/0!"}},{"$f":"2*$B$25/($G79)","v":{"$error":"#DIV/0!"}}]
["Toegevoegde waarde EUR",{"$f":"IF('Input financiële kengetallen'!B16=0,\"\",'Input financiële kengetallen'!B16)","v":""},{"$f":"IF('Input financiële kengetallen'!C16=0,\"\",'Input financiële kengetallen'!C16)","v":""},{"$f":"IF('Input financiële kengetallen'!D16=0,\"\",'Input financiële kengetallen'!D16)","v":""},{"$f":"IF('Input financiële kengetallen'!E16=0,\"\",'Input financiële kengetallen'!E16)","v":""},{"$f":"IF('Input financiële kengetallen'!F16=0,\"\",'Input financiële kengetallen'!F16)","v":""},{"$f":"AVERAGE(B80:F80)","v":{"$error":"#DIV/0!"}},null,{"$f":"$B$25/($G80)","v":{"$error":"#DIV/0!"}},{"$f":"2*$B$25/($G80)","v":{"$error":"#DIV/0!"}}]
["EBIDTA",{"$f":"IF('Input financiële kengetallen'!B18=0,\"\",'Input financiële kengetallen'!B18)","v":""},{"$f":"IF('Input financiële kengetallen'!C18=0,\"\",'Input financiële kengetallen'!C18)","v":""},{"$f":"IF('Input financiële kengetallen'!D18=0,\"\",'Input financiële kengetallen'!D18)","v":""},{"$f":"IF('Input financiële kengetallen'!E18=0,\"\",'Input financiële kengetallen'!E18)","v":""},{"$f":"IF('Input financiële kengetallen'!F18=0,\"\",'Input financiële kengetallen'!F18)","v":""},{"$f":"AVERAGE(B81:F81)","v":{"$error":"#DIV/0!"}},null,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
[]
["Overige investeringen","Totale jaarlijkse kost"]
["Bijkomende maatregel",{"$f":"B25","v":0}]
["Overige investeringen",{"$f":"'Input overige investeringen'!J16","v":0}]
["Totaal investeringen ikv wezer stappenplan",{"$f":"SUM(B85:B86)","v":0}]

{"sheet":"KE afleiding NL - Algemene par","index":13,"n_rows":97,"n_cols":34,"rows_kept":97,"cut":false,"hidden":true,"merged":[]}
["MKN (µg/L)","MKN mg/l","Bezwaarlijkheid","BBT (Basisjaar)","BBT+ (basisjaar)",null,null,null,null,null,null,null,null,null,null,"MKN (µg/L)","MKN mg/l","Bezwaarlijkheid","BBT (Index)","BBT+ (Index)",null,null,null,null,null,null,null,null,null,null,null,"Basisjaar (2013)","2021-01-01","index huidige jaar"]
[1000000,{"$f":"A2/1000","v":1000},{"$f":"1/A2","v":9.9999999999999995E-7},{"$f":"E2/10","v":0.03},0.3,null,null,null,null,null,null,null,null,null,null,1000000,{"$f":"P2/1000","v":1000},{"$f":"1/P2","v":9.9999999999999995E-7},{"$f":"D2*$AH$2/$AG$2","v":3.546421751386742E-2},{"$f":"E2*$AH$2/$AG$2","v":0.35464217513867419},null,null,null,null,null,null,null,null,null,null,null,100,109.97,130]
[{"$f":"A2/2","v":500000},{"$f":"A3/1000","v":500},{"$f":"1/A3","v":1.9999999999999999E-6},{"$f":"E3/10","v":0.06},0.6,null,null,null,null,null,null,null,null,null,null,{"$f":"P2/2","v":500000},{"$f":"P3/1000","v":500},{"$f":"1/P3","v":1.9999999999999999E-6},{"$f":"D3*$AH$2/$AG$2","v":7.092843502773484E-2},{"$f":"E3*$AH$2/$AG$2","v":0.70928435027734837}]
[400000,400,2.5000000000000002E-6,{"$f":"E4/10","v":6.9999999999999993E-2},0.7,null,null,null,null,null,null,null,null,null,null,400000,400,2.5000000000000002E-6,8.2749840865690635E-2,0.82749840865690649]
[300000,300,3.3333333333333333E-6,0.1,1,null,null,null,null,null,null,null,null,null,null,300000,300,3.3333333333333333E-6,0.11821405837955806,1.1821405837955807]
[200000,200,5.0000000000000004E-6,{"$f":"E6/10","v":0.16},1.6,null,null,null,null,null,null,null,null,null,null,200000,200,5.0000000000000004E-6,0.18914249340729292,1.891424934072929]
[100000,100,1.0000000000000001E-5,0.36,3.6,null,null,null,null,null,null,null,null,null,null,100000,100,1.0000000000000001E-5,0.42557061016640901,4.2557061016640905]
[90000,90,1.1111111111111112E-5,0.4,4,null,null,null,null,null,null,null,null,null,null,90000,90,1.1111111111111112E-5,0.47285623351823225,4.7285623351823229]
[80000,80,1.2500000000000001E-5,0.45999999999999996,4.5999999999999996,null,null,null,null,null,null,null,null,null,null,80000,80,1.2500000000000001E-5,0.54378466854596708,5.4378466854596708]
[70000,70,1.4285714285714285E-5,0.54,5.4,null,null,null,null,null,null,null,null,null,null,70000,70,1.4285714285714285E-5,0.63835591524961355,6.3835591524961357]
[60000,60,1.6666666666666667E-5,0.64,6.4,null,null,null,null,null,null,null,null,null,null,60000,60,1.6666666666666667E-5,0.75656997362917167,7.565699736291716]
[50000,50,2.0000000000000002E-5,0.79,7.9,null,null,null,null,null,null,null,null,null,null,50000,50,2.0000000000000002E-5,0.93389106119850873,9.3389106119850869]
[40000,40,2.5000000000000001E-5,1.02,10.199999999999999,null,null,null,null,null,null,null,null,null,null,40000,40,2.5000000000000001E-5,1.2057833954714923,12.057833954714923]
[30000,30,3.3333333333333335E-5,1.42,14.2,null,null,null,null,null,null,null,null,null,null,30000,30,3.3333333333333335E-5,1.6786396289897245,16.786396289897244]
[20000,20,5.0000000000000002E-5,2.2600000000000002,22.6,null,null,null,null,null,null,null,null,null,null,20000,20,5.0000000000000002E-5,2.6716377193780123,26.716377193780122]
[10000,10,{"$f":"1/A16","v":1E-4},5.0200000000000005,50.2,null,null,null,null,null,null,null,null,null,null,10000,10,1E-4,5.9343457306538152,59.343457306538149]
[9000,9,1.1111111111111112E-4,5.67,56.7,null,null,null,null,null,null,null,null,null,null,9000,9,1.1111111111111112E-4,6.7027371101209425,67.027371101209425]
[8000,8,1.25E-4,6.49,64.900000000000006,null,null,null,null,null,null,null,null,null,null,8000,8,1.25E-4,7.6720923888333186,76.720923888333189]
[7000,7,1.4285714285714287E-4,7.57,75.7,null,null,null,null,null,null,null,null,null,null,7000,7,1.4285714285714287E-4,8.9488042193325459,89.488042193325455]
[6000,6,{"$f":"1/A20","v":1.6666666666666666E-4},9.0400000000000009,90.4,null,null,null,null,null,null,null,null,null,null,6000,6,1.6666666666666666E-4,10.686550877512049,106.86550877512049]
[5000,5,2.0000000000000001E-4,11.15,111.5,null,null,null,null,null,null,null,null,null,null,5000,5,2.0000000000000001E-4,13.180867509320723,131.80867509320723]
[4000,4,2.5000000000000001E-4,14.41,144.1,null,null,null,null,null,null,null,null,null,null,4000,4,2.5000000000000001E-4,17.034645812494315,170.34645812494315]
[3000,3,3.3333333333333332E-4,20.059999999999999,200.6,null,null,null,null,null,null,null,null,null,null,3000,3,3.3333333333333332E-4,23.713740110939344,237.13740110939347]
[2000,2,5.0000000000000001E-4,31.98,319.8,null,null,null,null,null,null,null,null,null,null,2000,2,5.0000000000000001E-4,37.804855869782664,378.04855869782671]
[1000,1,1E-3,70.960000000000008,709.6,null,null,null,null,null,null,null,null,null,null,1000,1,1E-3,83.884695826134404,838.84695826134396]
[900,0.9,1.1111111111111111E-3,80.099999999999994,801,null,null,null,null,null,null,null,null,null,null,900,0.9,1.1111111111111111E-3,94.689460762026002,946.8946076202601]
[800,0.8,{"$f":"1/A27","v":1.25E-3},91.72,917.2,null,null,null,null,null,null,null,null,null,null,800,0.8,1.25E-3,108.42593434573065,1084.2593434573066]
[700,0.7,1.4285714285714286E-3,106.95,1069.5,null,null,null,null,null,null,null,null,null,null,700,0.7,1.4285714285714286E-3,126.42993543693734,1264.2993543693735]
[600,0.6,1.6666666666666668E-3,127.69000000000001,1276.9000000000001,null,null,null,null,null,null,null,null,null,null,600,0.6,1.6666666666666668E-3,150.94753114485769,1509.4753114485768]
[500,0.5,2E-3,157.47999999999999,1574.8,null,null,null,null,null,null,null,null,null,null,500,0.5,2E-3,186.16349913612802,1861.6349913612803]
[400,0.4,2.5000000000000001E-3,203.55,2035.5,null,null,null,null,null,null,null,null,null,null,400,0.4,2.5000000000000001E-3,240.62471583159044,2406.2471583159045]
[300,0.3,3.3333333333333335E-3,283.36,2833.6,null,null,null,null,null,null,null,null,null,null,300,0.3,3.3333333333333335E-3,334.97135582431576,3349.7135582431574]
[200,0.2,5.0000000000000001E-3,451.7,4517,"laatste punt lineair gebied log",null,null,null,null,null,null,null,null,null,200,0.2,5.0000000000000001E-3,533.97290170046381,5339.7290170046381,"laatste punt lineair gebied log"]
[100,0.1,0.01,910.6,9106,null,null,null,null,null,null,null,null,null,null,100,0.1,0.01,1076.4572156042557,10764.572156042557]
[90,0.09,1.1111111111111112E-2,980.12999999999988,9801.2999999999993,null,null,null,null,null,null,null,null,null,null,90,0.09,1.1111111111111112E-2,1158.6514503955623,11586.514503955625]
[80,0.08,1.2500000000000001E-2,1057.8600000000001,10578.6,null,null,null,null,null,null,null,null,null,null,80,0.08,1.2500000000000001E-2,1250.5392379739931,12505.392379739929]
[70,7.0000000000000007E-2,1.4285714285714285E-2,1145.99,11459.9,null,null,null,null,null,null,null,null,null,null,70,7.0000000000000007E-2,1.4285714285714285E-2,1354.7212876238975,13547.212876238975]
[60,0.06,1.6666666666666666E-2,{"$f":"E38/10","v":1247.73},12477.3,null,null,null,null,null,null,null,null,null,null,60,0.06,1.6666666666666666E-2,1474.9922706192597,14749.922706192598]
[50,0.05,0.02,1336.8,13368,null,null,null,null,null,null,null,null,null,null,50,0.05,0.02,1580.2855324179322,15802.855324179322]
[40,0.04,2.5000000000000001E-2,1515.34,15153.4,null,null,null,null,null,null,null,null,null,null,40,0.04,2.5000000000000001E-2,1791.344912248795,17913.449122487953]
[30,0.03,3.3333333333333333E-2,1705.2099999999998,17052.099999999999,null,null,null,null,null,null,null,null,null,null,30,0.03,3.3333333333333333E-2,2015.7979448940619,20157.979448940619]
[20,0.02,0.05,1972.8200000000002,19728.2,null,null,null,null,null,null,null,null,null,null,20,0.02,0.05,2332.1505865235977,23321.505865235973]
[10,0.01,0.1,2430.29,24302.9,null,null,null,null,null,null,null,null,null,null,10,0.01,0.1,2872.9444393925619,28729.444393925616]
[9,8.9999999999999993E-3,0.1111111111111111,2499.83,24998.3,null,null,null,null,null,null,null,null,null,null,9,8.9999999999999993E-3,0.1111111111111111,2955.1504955897058,29551.504955897064]
[8,8.0000000000000002E-3,0.125,2577.5700000000002,25775.7,null,null,null,null,null,null,null,null,null,null,8,8.0000000000000002E-3,0.125,3047.0501045739752,30470.501045739747]
[7,7.0000000000000001E-3,0.14285714285714285,2665.7,26657,null,null,null,null,null,null,null,null,null,null,7,7.0000000000000001E-3,0.14285714285714285,3151.2321542238792,31512.321542238791]
[6,6.0000000000000001E-3,0.16666666666666666,2767.44,27674.400000000001,null,null,null,null,null,null,null,null,null,null,6,6.0000000000000001E-3,0.16666666666666666,3271.5031372192416,32715.031372192418]
[5,5.0000000000000001E-3,0.2,2887.77,28877.7,null,null,null,null,null,null,null,null,null,null,5,5.0000000000000001E-3,0.2,3413.7501136673636,34137.501136673636]
[4,4.0000000000000001E-3,0.25,3035.05,30350.5,null,null,null,null,null,null,null,null,null,null,4,4.0000000000000001E-3,0.25,3587.8557788487769,35878.557788487771]
[3,3.0000000000000001E-3,0.33333333333333331,3224.92,32249.200000000001,null,null,null,null,null,null,null,null,null,null,3,3.0000000000000001E-3,0.33333333333333331,3812.3088114940442,38123.088114940438]
[2,2E-3,0.5,3492.5199999999995,34925.199999999997,null,null,null,null,null,null,null,null,null,null,2,2E-3,0.5,4128.6496317177407,41286.496317177414]
[1,1E-3,1,3950,39500,null,null,null,null,null,null,null,null,null,null,1,1E-3,1,4669.4553059925438,46694.553059925434]
[0.9,8.9999999999999998E-4,1.1111111111111112,4019.54,40195.4,null,null,null,null,null,null,null,null,null,null,0.9,8.9999999999999998E-4,1.1111111111111112,4751.6613621896886,47516.613621896882]
[0.8,8.0000000000000004E-4,1.25,4097.2699999999995,40972.699999999997,null,null,null,null,null,null,null,null,null,null,0.8,8.0000000000000004E-4,1.25,4843.5491497681187,48435.491497681185]
[0.7,6.9999999999999999E-4,1.4285714285714286,null,null,null,null,null,null,null,null,null,null,null,null,0.7,6.9999999999999999E-4,1.4285714285714286]
[0.6,5.9999999999999995E-4,1.6666666666666667,null,null,null,null,null,null,null,null,null,null,null,null,0.6,5.9999999999999995E-4,1.6666666666666667]
[0.5,5.0000000000000001E-4,2,null,null,null,null,null,null,null,null,null,null,null,null,0.5,5.0000000000000001E-4,2]
[0.4,4.0000000000000002E-4,2.5,null,null,null,null,null,null,null,null,null,null,null,null,0.4,4.0000000000000002E-4,2.5]
[0.3,2.9999999999999997E-4,3.3333333333333335,null,null,null,null,null,null,null,null,null,null,null,null,0.3,2.9999999999999997E-4,3.3333333333333335]
[0.2,2.0000000000000001E-4,5,null,null,null,null,null,null,null,null,null,null,null,null,0.2,2.0000000000000001E-4,5]
[0.1,1E-4,10,{"$f":"E61/10","v":5469.71},54697.1,null,null,null,null,null,null,null,null,null,null,0.1,1E-4,10,{"$f":"D61*$AH$2/$AG$2","v":6465.9661725925262},{"$f":"E61*$AH$2/$AG$2","v":64659.661725925253}]
[0.09,8.9999999999999992E-5,11.111111111111111,null,null,null,null,null,null,null,null,null,null,null,null,0.09,8.9999999999999992E-5,11.111111111111111]
[0.08,8.0000000000000007E-5,12.5,null,null,null,null,null,null,null,null,null,null,null,null,0.08,8.0000000000000007E-5,12.5]
[7.0000000000000007E-2,7.0000000000000007E-5,14.285714285714285,null,null,null,null,null,null,null,null,null,null,null,null,7.0000000000000007E-2,7.0000000000000007E-5,14.285714285714285]
[0.06,5.9999999999999995E-5,16.666666666666668,null,null,null,null,null,null,null,null,null,null,null,null,0.06,5.9999999999999995E-5,16.666666666666668]
[0.05,5.0000000000000002E-5,20,null,null,null,null,null,null,null,null,null,null,null,null,0.05,5.0000000000000002E-5,20]
[0.04,{"$f":"A67/1000","v":4.0000000000000003E-5},25,null,null,null,null,null,null,null,null,null,null,null,null,0.04,{"$f":"P67/1000","v":4.0000000000000003E-5},{"$f":"1/P67","v":25}]
[0.03,2.9999999999999997E-5,33.333333333333336,null,null,null,null,null,null,null,null,null,null,null,null,0.03,2.9999999999999997E-5,33.333333333333336]
[0.02,2.0000000000000002E-5,50,null,null,null,null,null,null,null,null,null,null,null,null,0.02,2.0000000000000002E-5,50]
[0.01,1.0000000000000001E-5,100,{"$f":"E70/10","v":6989.4100000000008},69894.100000000006,null,null,null,null,null,null,null,null,null,null,0.01,1.0000000000000001E-5,100,8262.4652177866701,82624.652177866694]
[8.9999999999999993E-3,8.9999999999999985E-6,111.11111111111111,null,null,null,null,null,null,null,null,null,null,null,null,8.9999999999999993E-3,8.9999999999999985E-6,111.11111111111111]
[8.0000000000000002E-3,7.9999999999999996E-6,{"$f":"1/A72","v":125},null,null,null,null,null,null,null,null,null,null,null,null,8.0000000000000002E-3,7.9999999999999996E-6,125]
[7.0000000000000001E-3,6.9999999999999999E-6,142.85714285714286,null,null,null,null,null,null,null,null,null,null,null,null,7.0000000000000001E-3,6.9999999999999999E-6,142.85714285714286]
[6.0000000000000001E-3,6.0000000000000002E-6,166.66666666666666,null,null,null,null,null,null,null,null,null,null,null,null,6.0000000000000001E-3,6.0000000000000002E-6,166.66666666666666]
[5.0000000000000001E-3,5.0000000000000004E-6,200,null,null,null,null,null,null,null,null,null,null,null,null,5.0000000000000001E-3,5.0000000000000004E-6,200]
[3.9999999999999897E-3,3.9999999999999897E-6,250.00000000000065,null,null,null,null,null,null,null,null,null,null,null,null,3.9999999999999897E-3,3.9999999999999897E-6,250.00000000000065]
[2.9999999999999901E-3,2.9999999999999899E-6,333.33333333333445,null,null,null,null,null,null,null,null,null,null,null,null,2.9999999999999901E-3,2.9999999999999899E-6,333.33333333333445]
[1.9999999999999901E-3,1.9999999999999902E-6,500.0000000000025,null,null,null,null,null,null,null,null,null,null,null,null,1.9999999999999901E-3,1.9999999999999902E-6,500.0000000000025]
[9.9999999999999005E-4,9.9999999999999E-7,1000.00000000001,{"$f":"E79/10","v":8509.119999999999},85091.199999999997,null,null,null,null,null,null,null,null,null,null,9.9999999999999005E-4,9.9999999999999E-7,1000.00000000001,10058.97608438665,100589.7608438665]
[8.9999999999999998E-4,8.9999999999999996E-7,1111.1111111111111,null,null,null,null,null,null,null,null,null,null,null,null,8.9999999999999998E-4,8.9999999999999996E-7,1111.1111111111111]
[8.0000000000001001E-4,8.0000000000001002E-7,{"$f":"1/A81","v":1249.9999999999843},null,null,null,null,null,null,null,null,null,null,null,null,8.0000000000001001E-4,8.0000000000001002E-7,1249.9999999999843]
[7.0000000000002005E-4,7.0000000000002009E-7,1428.5714285713877,null,null,null,null,null,null,null,null,null,null,null,null,7.0000000000002005E-4,7.0000000000002009E-7,1428.5714285713877]
[6.0000000000002998E-4,6.0000000000002994E-7,1666.6666666665833,null,null,null,null,null,null,null,null,null,null,null,null,6.0000000000002998E-4,6.0000000000002994E-7,1666.6666666665833]
[5.0000000000004002E-4,5.0000000000004E-7,1999.9999999998399,null,null,null,null,null,null,null,null,null,null,null,null,5.0000000000004002E-4,5.0000000000004E-7,1999.9999999998399]
[4.0000000000005E-4,4.0000000000005001E-7,2499.9999999996876,null,null,null,null,null,null,null,null,null,null,null,null,4.0000000000005E-4,4.0000000000005001E-7,2499.9999999996876]
[3.0000000000005998E-4,3.0000000000005997E-7,3333.3333333326668,null,null,null,null,null,null,null,null,null,null,null,null,3.0000000000005998E-4,3.0000000000005997E-7,3333.3333333326668]
[2.0000000000006899E-4,2.00000000000069E-7,4999.9999999982756,null,null,null,null,null,null,null,null,null,null,null,null,2.0000000000006899E-4,2.00000000000069E-7,4999.9999999982756]
[1.00000000000079E-4,1.0000000000007901E-7,9999.9999999921001,{"$f":"E88/10","v":10028.82},100288.2,null,null,null,null,null,null,null,null,null,null,1.00000000000079E-4,1.0000000000007901E-7,9999.9999999921001,11855.475129580793,118554.75129580795]
[9.0000000000000006E-5,9.0000000000000012E-8,11111.111111111111,null,null,null,null,null,null,null,null,null,null,null,null,9.0000000000000006E-5,9.0000000000000012E-8,11111.111111111111]
[7.9999999999920995E-5,7.9999999999920989E-8,{"$f":"1/A90","v":12500.000000012344},null,null,null,null,null,null,null,null,null,null,null,null,7.9999999999920995E-5,7.9999999999920989E-8,12500.000000012344]
[6.9999999999841999E-5,6.9999999999841993E-8,14285.714285746531,null,null,null,null,null,null,null,null,null,null,null,null,6.9999999999841999E-5,6.9999999999841993E-8,14285.714285746531]
[5.9999999999763002E-5,5.9999999999762997E-8,16666.666666732501,null,null,null,null,null,null,null,null,null,null,null,null,5.9999999999763002E-5,5.9999999999762997E-8,16666.666666732501]
[4.9999999999683998E-5,4.9999999999683995E-8,20000.000000126402,null,null,null,null,null,null,null,null,null,null,null,null,4.9999999999683998E-5,4.9999999999683995E-8,20000.000000126402]
[3.9999999999605001E-5,3.9999999999604999E-8,25000.000000246873,null,null,null,null,null,null,null,null,null,null,null,null,3.9999999999605001E-5,3.9999999999604999E-8,25000.000000246873]
[2.9999999999526001E-5,2.9999999999526003E-8,33333.333333859999,null,null,null,null,null,null,null,null,null,null,null,null,2.9999999999526001E-5,2.9999999999526003E-8,33333.333333859999]
[1.9999999999447001E-5,1.9999999999447E-8,50000.000001382497,null,null,null,null,null,null,null,null,null,null,null,null,1.9999999999447001E-5,1.9999999999447E-8,50000.000001382497]
[9.9999999993680007E-6,9.9999999993680011E-9,100000.00000632,{"$f":"E97/10","v":11548.53},115485.3,null,null,null,null,null,null,null,null,null,null,9.9999999993680007E-6,9.9999999993680011E-9,100000.00000632,13651.985996180778,136519.85996180776]

{"sheet":"MKN - Max","index":14,"n_rows":128,"n_cols":10,"rows_kept":128,"cut":false,"hidden":true,"merged":[]}
["Parameter ID","Parameter Symbool","Toets","Eenheid","toetswaarde stap 4","toetscriterium stap 5","toetswaarde stap 5 - halen doelstellingen","toetswaarde stap 5 - achteruitgang (goed-matig)","toetswaarde stap 5 - achteruitgang (matig-ontoereikend)","toetswaarde stap 5 - achteruitgang (ontoereikend-slecht)"]
[9,"NO2-","maximum","mgN/L",0.6,"maximum",0.6,0.6,null,3]
[19,"NH3","maximum","mgN/L",8.2239999999999994E-2,"maximum",8.2239999999999994E-2,8.2239999999999994E-2,null,0.41120000000000001]
[26,"CN- t","maximum","µg/L",75,"maximum",75,75,null,375]
[113,"ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]
[149,"Cd t","maximum","µg/L",4.5,"maximum",4.5,4.5,null,22.5]
[168,"Hg t","maximum","µg/L",0.15,"maximum",0.15,0.15,null,0.75]
[171,"Pb t","maximum","µg/L",97.22,"maximum",97.22,97.22,null,486.1]
[180,"Ni t","maximum","µg/L",51,"maximum",51,51,null,255]
[212,"Benzeen","maximum","µg/L",50,"maximum",50,50,null,250]
[213,"EyBz","maximum","µg/L",50,"maximum",50,50,null,250]
[221,"iPyBz","maximum","µg/L",10,"maximum",10,10,null,50]
[223,"Tolueen","maximum","µg/L",700,"maximum",700,700,null,3500]
[229,"245-T","maximum","ng/L",20000,"maximum",20000,20000,null,100000]
[230,"24-D","maximum","ng/L",200000,"maximum",200000,200000,null,1000000]
[231,"Propanil","maximum","ng/L",3000,"maximum",3000,3000,null,15000]
[233,"Cdaan","maximum","ng/L",40,"maximum",40,40,null,200]
[234,"24-DP","maximum","ng/L",200000,"maximum",200000,200000,null,1000000]
[244,"HCBz","maximum","ng/L",50,"maximum",50,50,null,250]
[245,"HCBdn","maximum","ng/L",600,"maximum",600,600,null,3000]
[252,"MCPA","maximum","ng/L",20000,"maximum",20000,20000,null,100000]
[253,"MCPP","maximum","ng/L",40000,"maximum",40000,40000,null,200000]
[259,"PCFol","maximum","ng/L",1000,"maximum",1000,1000,null,5000]
[268,"Atraz","maximum","ng/L",2000,"maximum",2000,2000,null,10000]
[273,"Diuron","maximum","ng/L",1800,"maximum",1800,1800,null,9000]
[274,"Iproturon","maximum","ng/L",1000,"maximum",1000,1000,null,5000]
[275,"Linuron","maximum","ng/L",700,"maximum",700,700,null,3500]
[278,"Mlinuron","maximum","ng/L",10000,"maximum",10000,10000,null,50000]
[280,"Simaz","maximum","ng/L",4000,"maximum",4000,4000,null,20000]
[281,"TrByaz","maximum","µg/L",1.8,"maximum",1.8,1.8,null,9]
[282,"Terbutryn","maximum","ng/L",340,"maximum",340,340,null,1700]
[287,"BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
[288,"CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
[308,"111CEa","maximum","µg/L",50,"maximum",50,50,null,250]
[309,"1122CEa","maximum","µg/L",900,"maximum",900,900,null,4500]
[310,"112CEa","maximum","µg/L",300,"maximum",300,300,null,1500]
[311,"11CEa","maximum","µg/L",8000,"maximum",8000,8000,null,40000]
[312,"11CEe","maximum","µg/L",500,"maximum",500,500,null,2500]
[316,"1245CBz","maximum","ng/L",30000,"maximum",30000,30000,null,150000]
[320,"12CEe","maximum","µg/L",100,"maximum",100,100,null,500]
[321,"12CPa","maximum","µg/L",1000,"maximum",1000,1000,null,5000]
[323,"13C2Pol","maximum","µg/L",2000,"maximum",2000,2000,null,10000]
[330,"1C24NiBz","maximum","µg/L",20,"maximum",20,20,null,100]
[343,"23CPe","maximum","µg/L",20,"maximum",20,20,null,100]
[346,"24CFol","maximum","ng/L",70000,"maximum",70000,70000,null,350000]
[351,"2CEol","maximum","µg/L",300,"maximum",300,300,null,1500]
[358,"3CPe","maximum","µg/L",30,"maximum",30,30,null,150]
[361,"4C2NiAn","maximum","µg/L",20,"maximum",20,20,null,100]
[363,"4C3MyFol","maximum","ng/L",90000,"maximum",90000,90000,null,450000]
[372,"CHAc","maximum","µg/L",3,"maximum",3,3,null,15]
[373,"CBz","maximum","µg/L",40,"maximum",40,40,null,200]
[381,"HCEa","maximum","µg/L",80,"maximum",80,80,null,400]
[391,"DCvos","maximum","ng/L",0.7,"maximum",0.7,0.7,null,3.5]
[392,"Mevinfos","maximum","ng/L",20,"maximum",20,20,null,100]
[393,"AzinfosEy","maximum","ng/L",100,"maximum",100,100,null,500]
[394,"AzinfosMy","maximum","ng/L",10,"maximum",10,10,null,50]
[396,"Dmetoat","maximum","ng/L",200,"maximum",200,200,null,1000]
[397,"Dsulfoton","maximum","ng/L",70,"maximum",70,70,null,350]
[399,"Fenithion","maximum","ng/L",2,"maximum",2,2,null,10]
[400,"Foxim","maximum","µg/L",0.2,"maximum",0.2,0.2,null,1]
[401,"Malathion","maximum","ng/L",3,"maximum",3,3,null,15]
[402,"Methamfos","maximum","µg/L",3,"maximum",3,3,null,15]
[403,"Omethoaat","maximum","µg/L",0.2,"maximum",0.2,0.2,null,1]
[404,"ODemeton-My","maximum","ng/L",4000,"maximum",4000,4000,null,20000]
[407,"TCfon","maximum","µg/L",0.01,"maximum",0.01,0.01,null,0.05]
[410,"TtBySn","maximum","ngSn/L",41,"maximum",41,41,null,205]
[419,"Ant","maximum","ng/L",100,"maximum",100,100,null,500]
[421,"B(a)P","maximum","ng/L",270,"maximum",270,270,null,1350]
[422,"B(b)Flu","maximum","ng/L",17,"maximum",17,17,null,85]
[423,"B(ghi)Pe","maximum","ng/L",8.1999999999999993,"maximum",8.1999999999999993,8.1999999999999993,null,41]
[424,"B(k)Flu","maximum","ng/L",17,"maximum",17,17,null,85]
[429,"Flu","maximum","ng/L",120,"maximum",120,120,null,600]
[432,"Naft","maximum","ng/L",130000,"maximum",130000,130000,null,650000]
[435,"Bzdine","maximum","µg/L",6,"maximum",6,6,null,30]
[445,"PCB t","maximum","ng/L",20,"maximum",20,20,null,100]
[456,"Bentazone","maximum","ng/L",500000,"maximum",500000,500000,null,2500000]
[471,"12BEa","maximum","µg/L",0.4,"maximum",0.4,0.4,null,2]
[481,"CNaft","maximum","µg/L",40,"maximum",40,40,null,200]
[482,"CNiTol","maximum","µg/L",40,"maximum",40,40,null,200]
[484,"CTine","maximum","µg/L",60,"maximum",60,60,null,300]
[486,"Cumafos","maximum","ng/L",10,"maximum",10,10,null,50]
[496,"DEyAm","maximum","µg/L",200,"maximum",200,200,null,1000]
[497,"DMyAm","maximum","µg/L",80,"maximum",80,80,null,400]
[498,"DFy","maximum","µg/L",10,"maximum",10,10,null,50]
[500,"Fenthion","maximum","ng/L",2,"maximum",2,2,null,10]
[502,"112CTFEa","maximum","µg/L",70,"maximum",70,70,null,350]
[508,"PathionMy","maximum","ng/L",20,"maximum",20,20,null,100]
[520,"TBP","maximum","ng/L",100000,"maximum",100000,100000,null,500000]
[521,"TCAcyde","maximum","µg/L",5000,"maximum",5000,5000,null,25000]
[526,"ompXyl","maximum","µg/L",40,"maximum",40,40,null,200]
[531,"PathionEy","maximum","ng/L",4,"maximum",4,4,null,20]
[670,"TBySn","maximum","ngSn/L",0.61,"maximum",0.61,0.61,null,3.05]
[675,"Cfvinfos","maximum","ng/L",300,"maximum",300,300,null,1500]
[686,"CpfosEy","maximum","ng/L",100,"maximum",100,100,null,500]
[724,"aCTol","maximum","µg/L",10,"maximum",10,10,null,50]
[751,"Alachloor","maximum","ng/L",700,"maximum",700,700,null,3500]
[753,"Cdazon","maximum","ng/L",20000,"maximum",20000,20000,null,100000]
[779,"eCHydrine","maximum","µg/L",100,"maximum",100,100,null,500]
[886,"DCBzdines","maximum","µg/L",5,"maximum",5,5,null,25]
[888,"DCAn t","maximum","µg/L",0.6,"maximum",0.6,0.6,null,3]
[895,"ct13CPe","maximum","µg/L",20,"maximum",20,20,null,100]
[898,"Demeton","maximum","ng/L",500,"maximum",500,500,null,2500]
[939,"HBCD","maximum","µg/L",0.5,"maximum",0.5,0.5,null,2.5]
[948,"HpC+Epx","maximum","ng/L",0.3,"maximum",0.3,0.3,null,1.5]
[949,"Alk c","maximum","µg/L",1.4,"maximum",1.4,1.4,null,7]
[972,"NyFol","maximum","ng/L",2000,"maximum",2000,2000,null,10000]
[976,"Flucet","maximum","ng/L",200,"maximum",200,200,null,1000]
[1020,"Dflucan","maximum","ng/L",50,"maximum",50,50,null,250]
[1038,"Quinofen","maximum","ng/L",2700,"maximum",2700,2700,null,13500]
[1044,"PFOS","maximum","ng/L",36000,"maximum",36000,36000,null,180000]
[1075,"Cypmethrin","maximum","ng/L",0.6,"maximum",0.6,0.6,null,3]
[1204,"a+bEndoS","maximum","ng/L",10,"maximum",10,10,null,50]
[1205,"a+b+d+gHCHS","maximum","ng/L",40,"maximum",40,40,null,200]
[1206,"CAnS","maximum","µg/L",5,"maximum",5,5,null,25]
[1208,"CFolS","maximum","ng/L",120000,"maximum",120000,120000,null,600000]
[1210,"1C2+3+4NiBzS","maximum","µg/L",60,"maximum",60,60,null,300]
[1212,"CTolS","maximum","µg/L",200,"maximum",200,200,null,1000]
[1216,"DBySn som","maximum","ngSn/L",700,"maximum",700,700,null,3500]
[1218,"CBzsom","maximum","µg/L",70,"maximum",70,70,null,350]
[1219,"diCNiBzsom","maximum","µg/L",60,"maximum",60,60,null,300]
[1228,"triCFolsom","maximum","ng/L",20000,"maximum",20000,20000,null,100000]
[1229,"TFySn som","maximum","ngSn/L",3,"maximum",3,3,null,15]
[1231,"DiMetamid","maximum","µg/L",6.7,"maximum",6.7,6.7,null,33.5]
[1388,"BDE t (6)","maximum","ng/L",140,"maximum",140,140,null,700]
[1440,"Imcloprid","maximum","µg/L",0.2,"maximum",0.2,0.2,null,1]
[1506,"Cybutrine","maximum","ng/L",16,"maximum",16,16,null,80]
[1522,"Bifenox","maximum","ng/L",40,"maximum",40,40,null,200]
[1523,"Aclonifen","maximum","ng/L",120,"maximum",120,120,null,600]

{"sheet":"MKN - JG","index":15,"n_rows":180,"n_cols":10,"rows_kept":180,"cut":false,"hidden":true,"merged":[]}
["Parameter ID","Parameter Symbool","Toets","Eenheid","toetswaarde stap 4","toetscriterium stap 5","toetswaarde stap 5 - halen doelstellingen","toetswaarde stap 5 - achteruitgang (goed-matig)","toetswaarde stap 5 - achteruitgang (matig-ontoereikend)","toetswaarde stap 5 - achteruitgang (ontoereikend-slecht)"]
[4,"Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
[9,"NO2-","jaargemiddelde","mgN/L",0.2,"jaargemiddelde",0.2,0.2,null,1]
[14,"SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
[19,"NH3","jaargemiddelde","mgN/L",2.4670000000000001E-2,"jaargemiddelde",2.4670000000000001E-2,2.4670000000000001E-2,null,0.12335]
[26,"CN- t","jaargemiddelde","µg/L",50,"jaargemiddelde",50,50,null,250]
[29,"P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
[31,"N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
[59,"b2EyHyFt","jaargemiddelde","µg/L",1.3,"jaargemiddelde",1.3,1.3,null,6.5]
[82,"EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
[134,"Sb t","jaargemiddelde","µg/L",100,"jaargemiddelde",100,100,null,500]
[137,"As t","jaargemiddelde","µg/L",5,"jaargemiddelde",5,5,null,25]
[140,"Ba t","jaargemiddelde","µg/L",70,"jaargemiddelde",70,70,null,350]
[143,"Be t","jaargemiddelde","µg/L",0.1,"jaargemiddelde",0.1,0.1,null,0.5]
[146,"B t","jaargemiddelde","µg/L",700,"jaargemiddelde",700,700,null,3500]
[149,"Cd t","jaargemiddelde","µg/L",0.8,"jaargemiddelde",0.8,0.8,null,4]
[155,"Cr t","jaargemiddelde","µg/L",50,"jaargemiddelde",50,50,null,250]
[162,"Co t","jaargemiddelde","µg/L",0.6,"jaargemiddelde",0.6,0.6,null,3]
[165,"Cu t","jaargemiddelde","µg/L",50,"jaargemiddelde",50,50,null,250]
[168,"Hg t","jaargemiddelde","µg/L",6.9999999999999994E-5,"jaargemiddelde",6.9999999999999994E-5,6.9999999999999994E-5,null,3.5E-4]
[171,"Pb t","jaargemiddelde","µg/L",50,"jaargemiddelde",50,50,null,250]
[177,"Mo t","jaargemiddelde","µg/L",350,"jaargemiddelde",350,350,null,1750]
[180,"Ni t","jaargemiddelde","µg/L",30,"jaargemiddelde",30,30,null,150]
[183,"Se t","jaargemiddelde","µg/L",3,"jaargemiddelde",3,3,null,15]
[190,"Tl t","jaargemiddelde","µg/L",0.2,"jaargemiddelde",0.2,0.2,null,1]
[193,"Sn t","jaargemiddelde","µg/L",40,"jaargemiddelde",40,40,null,200]
[196,"Ti t","jaargemiddelde","µg/L",100,"jaargemiddelde",100,100,null,500]
[199,"V t","jaargemiddelde","µg/L",5,"jaargemiddelde",5,5,null,25]
[202,"Ag t","jaargemiddelde","µg/L",0.4,"jaargemiddelde",0.4,0.4,null,2]
[205,"Zn t","jaargemiddelde","µg/L",200,"jaargemiddelde",200,200,null,1000]
[212,"Benzeen","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
[213,"EyBz","jaargemiddelde","µg/L",5,"jaargemiddelde",5,5,null,25]
[221,"iPyBz","jaargemiddelde","µg/L",1,"jaargemiddelde",1,1,null,5]
[223,"Tolueen","jaargemiddelde","µg/L",90,"jaargemiddelde",90,90,null,450]
[229,"245-T","jaargemiddelde","ng/L",2000,"jaargemiddelde",2000,2000,null,10000]
[230,"24-D","jaargemiddelde","ng/L",20000,"jaargemiddelde",20000,20000,null,100000]
[231,"Propanil","jaargemiddelde","ng/L",200,"jaargemiddelde",200,200,null,1000]
[233,"Cdaan","jaargemiddelde","ng/L",2,"jaargemiddelde",2,2,null,10]
[234,"24-DP","jaargemiddelde","ng/L",20000,"jaargemiddelde",20000,20000,null,100000]
[244,"HCBz","jaargemiddelde","ng/L",4.3999999999999997E-2,"jaargemiddelde",4.3999999999999997E-2,4.3999999999999997E-2,null,0.22]
[245,"HCBdn","jaargemiddelde","ng/L",0.55000000000000004,"jaargemiddelde",0.55000000000000004,0.55000000000000004,null,2.75]
[252,"MCPA","jaargemiddelde","ng/L",700,"jaargemiddelde",700,700,null,3500]
[253,"MCPP","jaargemiddelde","ng/L",10000,"jaargemiddelde",10000,10000,null,50000]
[259,"PCFol","jaargemiddelde","ng/L",400,"jaargemiddelde",400,400,null,2000]
[263,"44DDT","jaargemiddelde","ng/L",10,"jaargemiddelde",10,10,null,50]
[268,"Atraz","jaargemiddelde","ng/L",600,"jaargemiddelde",600,600,null,3000]
[273,"Diuron","jaargemiddelde","ng/L",200,"jaargemiddelde",200,200,null,1000]
[274,"Iproturon","jaargemiddelde","ng/L",300,"jaargemiddelde",300,300,null,1500]
[275,"Linuron","jaargemiddelde","ng/L",300,"jaargemiddelde",300,300,null,1500]
[278,"Mlinuron","jaargemiddelde","ng/L",300,"jaargemiddelde",300,300,null,1500]
[280,"Simaz","jaargemiddelde","ng/L",1000,"jaargemiddelde",1000,1000,null,5000]
[281,"TrByaz","jaargemiddelde","µg/L",0.32,"jaargemiddelde",0.32,0.32,null,1.6]
[282,"Terbutryn","jaargemiddelde","ng/L",65,"jaargemiddelde",65,65,null,325]
[284,"AOX","jaargemiddelde","µgCl/L",40,"jaargemiddelde",40,40,null,200]
[308,"111CEa","jaargemiddelde","µg/L",20,"jaargemiddelde",20,20,null,100]
[309,"1122CEa","jaargemiddelde","µg/L",100,"jaargemiddelde",100,100,null,500]
[310,"112CEa","jaargemiddelde","µg/L",20,"jaargemiddelde",20,20,null,100]
[311,"11CEa","jaargemiddelde","µg/L",100,"jaargemiddelde",100,100,null,500]
[312,"11CEe","jaargemiddelde","µg/L",50,"jaargemiddelde",50,50,null,250]
[316,"1245CBz","jaargemiddelde","ng/L",9000,"jaargemiddelde",9000,9000,null,45000]
[319,"12CEa","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
[320,"12CEe","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
[321,"12CPa","jaargemiddelde","µg/L",400,"jaargemiddelde",400,400,null,2000]
[323,"13C2Pol","jaargemiddelde","µg/L",100,"jaargemiddelde",100,100,null,500]
[330,"1C24NiBz","jaargemiddelde","µg/L",5,"jaargemiddelde",5,5,null,25]
[343,"23CPe","jaargemiddelde","µg/L",2,"jaargemiddelde",2,2,null,10]
[346,"24CFol","jaargemiddelde","ng/L",2000,"jaargemiddelde",2000,2000,null,10000]
[348,"2Am4CFol","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
[349,"2C13Bdn","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
[351,"2CEol","jaargemiddelde","µg/L",30,"jaargemiddelde",30,30,null,150]
[358,"3CPe","jaargemiddelde","µg/L",3,"jaargemiddelde",3,3,null,15]
[361,"4C2NiAn","jaargemiddelde","µg/L",2,"jaargemiddelde",2,2,null,10]
[363,"4C3MyFol","jaargemiddelde","ng/L",9000,"jaargemiddelde",9000,9000,null,45000]
[372,"CHAc","jaargemiddelde","µg/L",0.6,"jaargemiddelde",0.6,0.6,null,3]
[373,"CBz","jaargemiddelde","µg/L",6,"jaargemiddelde",6,6,null,30]
[379,"DCMa","jaargemiddelde","µg/L",20,"jaargemiddelde",20,20,null,100]
[381,"HCEa","jaargemiddelde","µg/L",3,"jaargemiddelde",3,3,null,15]
[382,"TtCEe","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
[383,"TtCMa","jaargemiddelde","µg/L",12,"jaargemiddelde",12,12,null,60]
[385,"TCEe","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
[388,"TCMa","jaargemiddelde","µg/L",2.5,"jaargemiddelde",2.5,2.5,null,12.5]
[391,"DCvos","jaargemiddelde","ng/L",0.6,"jaargemiddelde",0.6,0.6,null,3]
[392,"Mevinfos","jaargemiddelde","ng/L",2,"jaargemiddelde",2,2,null,10]
[393,"AzinfosEy","jaargemiddelde","ng/L",10,"jaargemiddelde",10,10,null,50]
[394,"AzinfosMy","jaargemiddelde","ng/L",2,"jaargemiddelde",2,2,null,10]
[396,"Dmetoat","jaargemiddelde","ng/L",20,"jaargemiddelde",20,20,null,100]
[397,"Dsulfoton","jaargemiddelde","ng/L",10,"jaargemiddelde",10,10,null,50]
[399,"Fenithion","jaargemiddelde","ng/L",0.9,"jaargemiddelde",0.9,0.9,null,4.5]
[400,"Foxim","jaargemiddelde","µg/L",0.02,"jaargemiddelde",0.02,0.02,null,0.1]
[401,"Malathion","jaargemiddelde","ng/L",0.8,"jaargemiddelde",0.8,0.8,null,4]
[402,"Methamfos","jaargemiddelde","µg/L",0.3,"jaargemiddelde",0.3,0.3,null,1.5]
[403,"Omethoaat","jaargemiddelde","µg/L",0.02,"jaargemiddelde",0.02,0.02,null,0.1]
[404,"ODemeton-My","jaargemiddelde","ng/L",400,"jaargemiddelde",400,400,null,2000]
[406,"Triazofos","jaargemiddelde","ng/L",30,"jaargemiddelde",30,30,null,150]
[407,"TCfon","jaargemiddelde","µg/L",1E-3,"jaargemiddelde",1E-3,1E-3,null,5.0000000000000001E-3]
[410,"TtBySn","jaargemiddelde","ngSn/L",4.0999999999999996,"jaargemiddelde",4.0999999999999996,4.0999999999999996,null,20.5]
[417,"Tfluralin","jaargemiddelde","ng/L",30,"jaargemiddelde",30,30,null,150]
[418,"Acenaft","jaargemiddelde","ng/L",60,"jaargemiddelde",60,60,null,300]
[419,"Ant","jaargemiddelde","ng/L",100,"jaargemiddelde",100,100,null,500]
[420,"B(a)A","jaargemiddelde","ng/L",300,"jaargemiddelde",300,300,null,1500]
[421,"B(a)P","jaargemiddelde","ng/L",0.17,"jaargemiddelde",0.17,0.17,null,0.85]
[425,"Chr","jaargemiddelde","ng/L",1000,"jaargemiddelde",1000,1000,null,5000]
[426,"dBz(ah)An","jaargemiddelde","ng/L",500,"jaargemiddelde",500,500,null,2500]
[428,"Fen","jaargemiddelde","ng/L",100,"jaargemiddelde",100,100,null,500]
[429,"Flu","jaargemiddelde","ng/L",6.3,"jaargemiddelde",6.3,6.3,null,31.5]
[430,"Fluoreen","jaargemiddelde","ng/L",2000,"jaargemiddelde",2000,2000,null,10000]
[432,"Naft","jaargemiddelde","ng/L",2000,"jaargemiddelde",2000,2000,null,10000]
[434,"Pyr","jaargemiddelde","ng/L",40,"jaargemiddelde",40,40,null,200]
[435,"Bzdine","jaargemiddelde","µg/L",0.6,"jaargemiddelde",0.6,0.6,null,3]
[445,"PCB t","jaargemiddelde","ng/L",2,"jaargemiddelde",2,2,null,10]
[456,"Bentazone","jaargemiddelde","ng/L",50000,"jaargemiddelde",50000,50000,null,250000]
[471,"12BEa","jaargemiddelde","µg/L",3.0000000000000001E-3,"jaargemiddelde",3.0000000000000001E-3,3.0000000000000001E-3,null,1.4999999999999999E-2]
[473,"246C135Az","jaargemiddelde","µg/L",0.1,"jaargemiddelde",0.1,0.1,null,0.5]
[478,"b2CiPyEt","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
[481,"CNaft","jaargemiddelde","µg/L",1,"jaargemiddelde",1,1,null,5]
[482,"CNiTol","jaargemiddelde","µg/L",3,"jaargemiddelde",3,3,null,15]
[484,"CTine","jaargemiddelde","µg/L",8,"jaargemiddelde",8,8,null,40]
[486,"Cumafos","jaargemiddelde","ng/L",1,"jaargemiddelde",1,1,null,5]
[496,"DEyAm","jaargemiddelde","µg/L",30,"jaargemiddelde",30,30,null,150]
[497,"DMyAm","jaargemiddelde","µg/L",6,"jaargemiddelde",6,6,null,30]
[498,"DFy","jaargemiddelde","µg/L",2,"jaargemiddelde",2,2,null,10]
[500,"Fenthion","jaargemiddelde","ng/L",0.2,"jaargemiddelde",0.2,0.2,null,1]
[502,"112CTFEa","jaargemiddelde","µg/L",7,"jaargemiddelde",7,7,null,35]
[508,"PathionMy","jaargemiddelde","ng/L",10,"jaargemiddelde",10,10,null,50]
[511,"Acenaftyl","jaargemiddelde","ng/L",4000,"jaargemiddelde",4000,4000,null,20000]
[517,"Te t","jaargemiddelde","µg/L",100,"jaargemiddelde",100,100,null,500]
[520,"TBP","jaargemiddelde","ng/L",40000,"jaargemiddelde",40000,40000,null,200000]
[521,"TCAcyde","jaargemiddelde","µg/L",500,"jaargemiddelde",500,500,null,2500]
[522,"TCBz","jaargemiddelde","µg/L",0.4,"jaargemiddelde",0.4,0.4,null,2]
[525,"U t","jaargemiddelde","µg/L",1,"jaargemiddelde",1,1,null,5]
[526,"ompXyl","jaargemiddelde","µg/L",4,"jaargemiddelde",4,4,null,20]
[531,"PathionEy","jaargemiddelde","ng/L",0.2,"jaargemiddelde",0.2,0.2,null,1]
[570,"VinCl","jaargemiddelde","µg/L",0.09,"jaargemiddelde",0.09,0.09,null,0.45]
[618,"AISurf","jaargemiddelde","mg/L",0.1,"jaargemiddelde",0.1,0.1,null,0.5]
[670,"TBySn","jaargemiddelde","ngSn/L",8.1000000000000003E-2,"jaargemiddelde",8.1000000000000003E-2,8.1000000000000003E-2,null,0.40500000000000003]
[675,"Cfvinfos","jaargemiddelde","ng/L",100,"jaargemiddelde",100,100,null,500]
[686,"CpfosEy","jaargemiddelde","ng/L",30,"jaargemiddelde",30,30,null,150]
[724,"aCTol","jaargemiddelde","µg/L",1,"jaargemiddelde",1,1,null,5]
[751,"Alachloor","jaargemiddelde","ng/L",300,"jaargemiddelde",300,300,null,1500]
[753,"Cdazon","jaargemiddelde","ng/L",10000,"jaargemiddelde",10000,10000,null,50000]
[756,"PCBz","jaargemiddelde","ng/L",7,"jaargemiddelde",7,7,null,35]
[770,"aaCTol","jaargemiddelde","µg/L",5,"jaargemiddelde",5,5,null,25]
[779,"eCHydrine","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
[886,"DCBzdines","jaargemiddelde","µg/L",0.5,"jaargemiddelde",0.5,0.5,null,2.5]
[888,"DCAn t","jaargemiddelde","µg/L",0.2,"jaargemiddelde",0.2,0.2,null,1]
[895,"ct13CPe","jaargemiddelde","µg/L",2,"jaargemiddelde",2,2,null,10]
[898,"Demeton","jaargemiddelde","ng/L",50,"jaargemiddelde",50,50,null,250]
[900,"bFol-A","jaargemiddelde","µg/L",1.5,"jaargemiddelde",1.5,1.5,null,7.5]
[907,"DDT t","jaargemiddelde","ng/L",25,"jaargemiddelde",25,25,null,125]
[939,"HBCD","jaargemiddelde","µg/L",1.6000000000000001E-3,"jaargemiddelde",1.6000000000000001E-3,1.6000000000000001E-3,null,8.0000000000000002E-3]
[948,"HpC+Epx","jaargemiddelde","ng/L",2.0000000000000001E-4,"jaargemiddelde",2.0000000000000001E-4,2.0000000000000001E-4,null,1E-3]
[949,"Alk c","jaargemiddelde","µg/L",0.4,"jaargemiddelde",0.4,0.4,null,2]
[972,"NyFol","jaargemiddelde","ng/L",300,"jaargemiddelde",300,300,null,1500]
[976,"Flucet","jaargemiddelde","ng/L",40,"jaargemiddelde",40,40,null,200]
[996,"ADEIdrin","jaargemiddelde","ng/L",10,"jaargemiddelde",10,10,null,50]
[1020,"Dflucan","jaargemiddelde","ng/L",30,"jaargemiddelde",30,30,null,150]
[1038,"Quinofen","jaargemiddelde","ng/L",150,"jaargemiddelde",150,150,null,750]
[1044,"PFOS","jaargemiddelde","ng/L",0.65,"jaargemiddelde",0.65,0.65,null,3.25]
[1075,"Cypmethrin","jaargemiddelde","ng/L",0.08,"jaargemiddelde",0.08,0.08,null,0.4]
[1204,"a+bEndoS","jaargemiddelde","ng/L",5,"jaargemiddelde",5,5,null,25]
[1205,"a+b+d+gHCHS","jaargemiddelde","ng/L",20,"jaargemiddelde",20,20,null,100]
[1206,"CAnS","jaargemiddelde","µg/L",1,"jaargemiddelde",1,1,null,5]
[1208,"CFolS","jaargemiddelde","ng/L",20000,"jaargemiddelde",20000,20000,null,100000]
[1210,"1C2+3+4NiBzS","jaargemiddelde","µg/L",3,"jaargemiddelde",3,3,null,15]
[1212,"CTolS","jaargemiddelde","µg/L",3,"jaargemiddelde",3,3,null,15]
[1216,"DBySn som","jaargemiddelde","ngSn/L",80,"jaargemiddelde",80,80,null,400]
[1218,"CBzsom","jaargemiddelde","µg/L",20,"jaargemiddelde",20,20,null,100]
[1219,"diCNiBzsom","jaargemiddelde","µg/L",3,"jaargemiddelde",3,3,null,15]
[1223,"OyFolsom","jaargemiddelde","ng/L",100,"jaargemiddelde",100,100,null,500]
[1228,"triCFolsom","jaargemiddelde","ng/L",6000,"jaargemiddelde",6000,6000,null,30000]
[1229,"TFySn som","jaargemiddelde","ngSn/L",0.3,"jaargemiddelde",0.3,0.3,null,1.5]
[1231,"DiMetamid","jaargemiddelde","µg/L",1.5,"jaargemiddelde",1.5,1.5,null,7.5]
[1328,"F- o","jaargemiddelde","mg/L",0.9,"jaargemiddelde",0.9,0.9,null,4.5]
[1388,"BDE t (6)","jaargemiddelde","ng/L",4.8999999999999998E-5,"jaargemiddelde",4.8999999999999998E-5,4.8999999999999998E-5,null,2.4499999999999999E-4]
[1440,"Imcloprid","jaargemiddelde","µg/L",8.0000000000000002E-3,"jaargemiddelde",8.0000000000000002E-3,8.0000000000000002E-3,null,0.04]
[1464,"Dicofol","jaargemiddelde","ng/L",1.3,"jaargemiddelde",1.3,1.3,null,6.5]
[1506,"Cybutrine","jaargemiddelde","ng/L",2.5,"jaargemiddelde",2.5,2.5,null,12.5]
[1522,"Bifenox","jaargemiddelde","ng/L",12,"jaargemiddelde",12,12,null,60]
[1523,"Aclonifen","jaargemiddelde","ng/L",120,"jaargemiddelde",120,120,null,600]
[1767,"Surf KID+NID","jaargemiddelde","mg/L",1,"jaargemiddelde",1,1,null,5]

{"sheet":"Toetswaarden STAP 4-7","index":16,"n_rows":308,"n_cols":13,"rows_kept":308,"cut":false,"hidden":true,"merged":[]}
["Toetswaarden voor het waterlichaam HET GELEED (L107_122)"]
["Code","Naam waterlichaam","Parameter","Parameter ID","Parameter Symbool","Toets","Eenheid","toetswaarde stap 4","toetscriterium stap 5","toetswaarde stap 5 - halen doelstellingen","toetswaarde stap 5 - achteruitgang (goed-matig)","toetswaarde stap 5 - achteruitgang (matig-ontoereikend)","toetswaarde stap 5 - achteruitgang (ontoereikend-slecht)"]
["L107_122","HET GELEED","(4-Chloor-2-methylfenoxy)azijnzuur",252,"MCPA","jaargemiddelde","ng/L",700,"jaargemiddelde",700,700,null,3500]
["L107_122","HET GELEED","(4-Chloor-2-methylfenoxy)azijnzuur",252,"MCPA","maximum","ng/L",20000,"maximum",20000,20000,null,100000]
["L107_122","HET GELEED","1,1,1-Trichloorethaan",308,"111CEa","jaargemiddelde","µg/L",20,"jaargemiddelde",20,20,null,100]
["L107_122","HET GELEED","1,1,1-Trichloorethaan",308,"111CEa","maximum","µg/L",50,"maximum",50,50,null,250]
["L107_122","HET GELEED","1,1,2,2-Tetrachloorethaan",309,"1122CEa","jaargemiddelde","µg/L",100,"jaargemiddelde",100,100,null,500]
["L107_122","HET GELEED","1,1,2,2-Tetrachloorethaan",309,"1122CEa","maximum","µg/L",900,"maximum",900,900,null,4500]
["L107_122","HET GELEED","1,1,2-Trichloorethaan",310,"112CEa","jaargemiddelde","µg/L",20,"jaargemiddelde",20,20,null,100]
["L107_122","HET GELEED","1,1,2-Trichloorethaan",310,"112CEa","maximum","µg/L",300,"maximum",300,300,null,1500]
["L107_122","HET GELEED","1,1,2-Trichloortrifluorethaan",502,"112CTFEa","jaargemiddelde","µg/L",7,"jaargemiddelde",7,7,null,35]
["L107_122","HET GELEED","1,1,2-Trichloortrifluorethaan",502,"112CTFEa","maximum","µg/L",70,"maximum",70,70,null,350]
["L107_122","HET GELEED","1,1-Dichloorethaan",311,"11CEa","jaargemiddelde","µg/L",100,"jaargemiddelde",100,100,null,500]
["L107_122","HET GELEED","1,1-Dichloorethaan",311,"11CEa","maximum","µg/L",8000,"maximum",8000,8000,null,40000]
["L107_122","HET GELEED","1,1-Dichlooretheen",312,"11CEe","jaargemiddelde","µg/L",50,"jaargemiddelde",50,50,null,250]
["L107_122","HET GELEED","1,1-Dichlooretheen",312,"11CEe","maximum","µg/L",500,"maximum",500,500,null,2500]
["L107_122","HET GELEED","1,2,4,5-Tetrachloorbenzeen",316,"1245CBz","jaargemiddelde","ng/L",9000,"jaargemiddelde",9000,9000,null,45000]
["L107_122","HET GELEED","1,2,4,5-Tetrachloorbenzeen",316,"1245CBz","maximum","ng/L",30000,"maximum",30000,30000,null,150000]
["L107_122","HET GELEED","1,2-Dibroomethaan",471,"12BEa","jaargemiddelde","µg/L",3.0000000000000001E-3,"jaargemiddelde",3.0000000000000001E-3,3.0000000000000001E-3,null,1.4999999999999999E-2]
["L107_122","HET GELEED","1,2-Dibroomethaan",471,"12BEa","maximum","µg/L",0.4,"maximum",0.4,0.4,null,2]
["L107_122","HET GELEED","1,2-Dichloorethaan",319,"12CEa","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
["L107_122","HET GELEED","1,2-Dichlooretheen",320,"12CEe","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
["L107_122","HET GELEED","1,2-Dichlooretheen",320,"12CEe","maximum","µg/L",100,"maximum",100,100,null,500]
["L107_122","HET GELEED","1,2-Dichloorpropaan",321,"12CPa","jaargemiddelde","µg/L",400,"jaargemiddelde",400,400,null,2000]
["L107_122","HET GELEED","1,2-Dichloorpropaan",321,"12CPa","maximum","µg/L",1000,"maximum",1000,1000,null,5000]
["L107_122","HET GELEED","1,3-Dichloor-2-propanol",323,"13C2Pol","jaargemiddelde","µg/L",100,"jaargemiddelde",100,100,null,500]
["L107_122","HET GELEED","1,3-Dichloor-2-propanol",323,"13C2Pol","maximum","µg/L",2000,"maximum",2000,2000,null,10000]
["L107_122","HET GELEED","1,3-Dichloorpropeen (cis+trans)",895,"ct13CPe","jaargemiddelde","µg/L",2,"jaargemiddelde",2,2,null,10]
["L107_122","HET GELEED","1,3-Dichloorpropeen (cis+trans)",895,"ct13CPe","maximum","µg/L",20,"maximum",20,20,null,100]
["L107_122","HET GELEED","1-Chloor-2,4-dinitrobenzeen",330,"1C24NiBz","jaargemiddelde","µg/L",5,"jaargemiddelde",5,5,null,25]
["L107_122","HET GELEED","1-Chloor-2,4-dinitrobenzeen",330,"1C24NiBz","maximum","µg/L",20,"maximum",20,20,null,100]
["L107_122","HET GELEED","2,3-Dichloorpropeen",343,"23CPe","jaargemiddelde","µg/L",2,"jaargemiddelde",2,2,null,10]
["L107_122","HET GELEED","2,3-Dichloorpropeen",343,"23CPe","maximum","µg/L",20,"maximum",20,20,null,100]
["L107_122","HET GELEED","2,4,5-Trichloorfenoxyazijnzuur",229,"245-T","jaargemiddelde","ng/L",2000,"jaargemiddelde",2000,2000,null,10000]
["L107_122","HET GELEED","2,4,5-Trichloorfenoxyazijnzuur",229,"245-T","maximum","ng/L",20000,"maximum",20000,20000,null,100000]
["L107_122","HET GELEED","2,4,6-Trichloor-1,3,5-triazine",473,"246C135Az","jaargemiddelde","µg/L",0.1,"jaargemiddelde",0.1,0.1,null,0.5]
["L107_122","HET GELEED","2,4-Dichloorfenol",346,"24CFol","jaargemiddelde","ng/L",2000,"jaargemiddelde",2000,2000,null,10000]
["L107_122","HET GELEED","2,4-Dichloorfenol",346,"24CFol","maximum","ng/L",70000,"maximum",70000,70000,null,350000]
["L107_122","HET GELEED","2,4-Dichloorfenoxyazijnzuur",230,"24-D","jaargemiddelde","ng/L",20000,"jaargemiddelde",20000,20000,null,100000]
["L107_122","HET GELEED","2,4-Dichloorfenoxyazijnzuur",230,"24-D","maximum","ng/L",200000,"maximum",200000,200000,null,1000000]
["L107_122","HET GELEED","2-Amino-4-chloorfenol",348,"2Am4CFol","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
["L107_122","HET GELEED","2-Chloor-1,3-butadieen",349,"2C13Bdn","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
["L107_122","HET GELEED","2-Chloorethanol",351,"2CEol","jaargemiddelde","µg/L",30,"jaargemiddelde",30,30,null,150]
["L107_122","HET GELEED","2-Chloorethanol",351,"2CEol","maximum","µg/L",300,"maximum",300,300,null,1500]
["L107_122","HET GELEED","3-Chloorpropeen",358,"3CPe","jaargemiddelde","µg/L",3,"jaargemiddelde",3,3,null,15]
["L107_122","HET GELEED","3-Chloorpropeen",358,"3CPe","maximum","µg/L",30,"maximum",30,30,null,150]
["L107_122","HET GELEED","4-Chloor-2-nitroaniline",361,"4C2NiAn","jaargemiddelde","µg/L",2,"jaargemiddelde",2,2,null,10]
["L107_122","HET GELEED","4-Chloor-2-nitroaniline",361,"4C2NiAn","maximum","µg/L",20,"maximum",20,20,null,100]
["L107_122","HET GELEED","4-Chloor-3-methylfenol",363,"4C3MyFol","jaargemiddelde","ng/L",9000,"jaargemiddelde",9000,9000,null,45000]
["L107_122","HET GELEED","4-Chloor-3-methylfenol",363,"4C3MyFol","maximum","ng/L",90000,"maximum",90000,90000,null,450000]
["L107_122","HET GELEED","Acenafteen",418,"Acenaft","jaargemiddelde","ng/L",60,"jaargemiddelde",60,60,null,300]
["L107_122","HET GELEED","Acenaftyleen",511,"Acenaftyl","jaargemiddelde","ng/L",4000,"jaargemiddelde",4000,4000,null,20000]
["L107_122","HET GELEED","Aclonifen",1523,"Aclonifen","jaargemiddelde","ng/L",120,"jaargemiddelde",120,120,null,600]
["L107_122","HET GELEED","Aclonifen",1523,"Aclonifen","maximum","ng/L",120,"maximum",120,120,null,600]
["L107_122","HET GELEED","Adsorbeerbare organohalogenen",284,"AOX","jaargemiddelde","µgCl/L",40,"jaargemiddelde",40,40,null,200]
["L107_122","HET GELEED","Alachloor",751,"Alachloor","jaargemiddelde","ng/L",300,"jaargemiddelde",300,300,null,1500]
["L107_122","HET GELEED","Alachloor",751,"Alachloor","maximum","ng/L",700,"maximum",700,700,null,3500]
["L107_122","HET GELEED","Aldrin+Dieldrin+Endrin+Isodrin",996,"ADEIdrin","jaargemiddelde","ng/L",10,"jaargemiddelde",10,10,null,50]
["L107_122","HET GELEED","alfa+beta Endosulfan",1204,"a+bEndoS","jaargemiddelde","ng/L",5,"jaargemiddelde",5,5,null,25]
["L107_122","HET GELEED","alfa+beta Endosulfan",1204,"a+bEndoS","maximum","ng/L",10,"maximum",10,10,null,50]
["L107_122","HET GELEED","alfa+beta+gamma+delta Hexachloorcyclohexaan",1205,"a+b+d+gHCHS","jaargemiddelde","ng/L",20,"jaargemiddelde",20,20,null,100]
["L107_122","HET GELEED","alfa+beta+gamma+delta Hexachloorcyclohexaan",1205,"a+b+d+gHCHS","maximum","ng/L",40,"maximum",40,40,null,200]
["L107_122","HET GELEED","alfa-alfa-Dichloortolueen",770,"aaCTol","jaargemiddelde","µg/L",5,"jaargemiddelde",5,5,null,25]
["L107_122","HET GELEED","alfa-Chloortolueen",724,"aCTol","jaargemiddelde","µg/L",1,"jaargemiddelde",1,1,null,5]
["L107_122","HET GELEED","alfa-Chloortolueen",724,"aCTol","maximum","µg/L",10,"maximum",10,10,null,50]
["L107_122","HET GELEED","Alkanen, gechloreerde",949,"Alk c","jaargemiddelde","µg/L",0.4,"jaargemiddelde",0.4,0.4,null,2]
["L107_122","HET GELEED","Alkanen, gechloreerde",949,"Alk c","maximum","µg/L",1.4,"maximum",1.4,1.4,null,7]
["L107_122","HET GELEED","Ammoniak",19,"NH3","jaargemiddelde","mgN/L",2.4670000000000001E-2,"jaargemiddelde",2.4670000000000001E-2,2.4670000000000001E-2,null,0.12335]
["L107_122","HET GELEED","Ammoniak",19,"NH3","maximum","mgN/L",8.2239999999999994E-2,"maximum",8.2239999999999994E-2,8.2239999999999994E-2,null,0.41120000000000001]
["L107_122","HET GELEED","Anthraceen",419,"Ant","jaargemiddelde","ng/L",100,"jaargemiddelde",100,100,null,500]
["L107_122","HET GELEED","Anthraceen",419,"Ant","maximum","ng/L",100,"maximum",100,100,null,500]
["L107_122","HET GELEED","Antimoon, totaal",134,"Sb t","jaargemiddelde","µg/L",100,"jaargemiddelde",100,100,null,500]
["L107_122","HET GELEED","Arseen, totaal",137,"As t","jaargemiddelde","µg/L",5,"jaargemiddelde",5,5,null,25]
["L107_122","HET GELEED","Atrazine",268,"Atraz","jaargemiddelde","ng/L",600,"jaargemiddelde",600,600,null,3000]
["L107_122","HET GELEED","Atrazine",268,"Atraz","maximum","ng/L",2000,"maximum",2000,2000,null,10000]
["L107_122","HET GELEED","Azinfos-ethyl",393,"AzinfosEy","jaargemiddelde","ng/L",10,"jaargemiddelde",10,10,null,50]
["L107_122","HET GELEED","Azinfos-ethyl",393,"AzinfosEy","maximum","ng/L",100,"maximum",100,100,null,500]
["L107_122","HET GELEED","Azinfos-methyl",394,"AzinfosMy","jaargemiddelde","ng/L",2,"jaargemiddelde",2,2,null,10]
["L107_122","HET GELEED","Azinfos-methyl",394,"AzinfosMy","maximum","ng/L",10,"maximum",10,10,null,50]
["L107_122","HET GELEED","Barium, totaal",140,"Ba t","jaargemiddelde","µg/L",70,"jaargemiddelde",70,70,null,350]
["L107_122","HET GELEED","Bentazone",456,"Bentazone","jaargemiddelde","ng/L",50000,"jaargemiddelde",50000,50000,null,250000]
["L107_122","HET GELEED","Bentazone",456,"Bentazone","maximum","ng/L",500000,"maximum",500000,500000,null,2500000]
["L107_122","HET GELEED","Benzeen",212,"Benzeen","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
["L107_122","HET GELEED","Benzeen",212,"Benzeen","maximum","µg/L",50,"maximum",50,50,null,250]
["L107_122","HET GELEED","Benzidine",435,"Bzdine","jaargemiddelde","µg/L",0.6,"jaargemiddelde",0.6,0.6,null,3]
["L107_122","HET GELEED","Benzidine",435,"Bzdine","maximum","µg/L",6,"maximum",6,6,null,30]
["L107_122","HET GELEED","Benzo(a)anthraceen",420,"B(a)A","jaargemiddelde","ng/L",300,"jaargemiddelde",300,300,null,1500]
["L107_122","HET GELEED","Benzo(a)pyreen",421,"B(a)P","jaargemiddelde","ng/L",0.17,"jaargemiddelde",0.17,0.17,null,0.85]
["L107_122","HET GELEED","Benzo(a)pyreen",421,"B(a)P","maximum","ng/L",270,"maximum",270,270,null,1350]
["L107_122","HET GELEED","Benzo(b)fluorantheen",422,"B(b)Flu","maximum","ng/L",17,"maximum",17,17,null,85]
["L107_122","HET GELEED","Benzo(g,h,i)peryleen",423,"B(ghi)Pe","maximum","ng/L",8.1999999999999993,"maximum",8.1999999999999993,8.1999999999999993,null,41]
["L107_122","HET GELEED","Benzo(k)fluorantheen",424,"B(k)Flu","maximum","ng/L",17,"maximum",17,17,null,85]
["L107_122","HET GELEED","Berylium, totaal",143,"Be t","jaargemiddelde","µg/L",0.1,"jaargemiddelde",0.1,0.1,null,0.5]
["L107_122","HET GELEED","Bifenox",1522,"Bifenox","jaargemiddelde","ng/L",12,"jaargemiddelde",12,12,null,60]
["L107_122","HET GELEED","Bifenox",1522,"Bifenox","maximum","ng/L",40,"maximum",40,40,null,200]
["L107_122","HET GELEED","Biochemisch zuurstofverbruik na 5d.",287,"BZV5","90 percentiel","mgO2/L",6,"maximum",9,9,15,37.5]
["L107_122","HET GELEED","bis-(2-Chloorisopropyl)-ether",478,"b2CiPyEt","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
["L107_122","HET GELEED","bis-(2-ethylhexyl)-ftalaat",59,"b2EyHyFt","jaargemiddelde","µg/L",1.3,"jaargemiddelde",1.3,1.3,null,6.5]
["L107_122","HET GELEED","bisfenol A",900,"bFol-A","jaargemiddelde","µg/L",1.5,"jaargemiddelde",1.5,1.5,null,7.5]
["L107_122","HET GELEED","Boor, totaal",146,"B t","jaargemiddelde","µg/L",700,"jaargemiddelde",700,700,null,3500]
["L107_122","HET GELEED","Cadmium, totaal",149,"Cd t","jaargemiddelde","µg/L",0.8,"jaargemiddelde",0.8,0.8,null,4]
["L107_122","HET GELEED","Cadmium, totaal",149,"Cd t","maximum","µg/L",4.5,"maximum",4.5,4.5,null,22.5]
["L107_122","HET GELEED","Chemisch zuurstofverbruik",288,"CZV","90 percentiel","mgO2/L",30,"maximum",45,45,60,120]
["L107_122","HET GELEED","Chlooranilines",1206,"CAnS","jaargemiddelde","µg/L",1,"jaargemiddelde",1,1,null,5]
["L107_122","HET GELEED","Chlooranilines",1206,"CAnS","maximum","µg/L",5,"maximum",5,5,null,25]
["L107_122","HET GELEED","Chloorazijnzuur",372,"CHAc","jaargemiddelde","µg/L",0.6,"jaargemiddelde",0.6,0.6,null,3]
["L107_122","HET GELEED","Chloorazijnzuur",372,"CHAc","maximum","µg/L",3,"maximum",3,3,null,15]
["L107_122","HET GELEED","Chloorbenzeen",373,"CBz","jaargemiddelde","µg/L",6,"jaargemiddelde",6,6,null,30]
["L107_122","HET GELEED","Chloorbenzeen",373,"CBz","maximum","µg/L",40,"maximum",40,40,null,200]
["L107_122","HET GELEED","Chloordaan",233,"Cdaan","jaargemiddelde","ng/L",2,"jaargemiddelde",2,2,null,10]
["L107_122","HET GELEED","Chloordaan",233,"Cdaan","maximum","ng/L",40,"maximum",40,40,null,200]
["L107_122","HET GELEED","Chloorfenolen",1208,"CFolS","jaargemiddelde","ng/L",20000,"jaargemiddelde",20000,20000,null,100000]
["L107_122","HET GELEED","Chloorfenolen",1208,"CFolS","maximum","ng/L",120000,"maximum",120000,120000,null,600000]
["L107_122","HET GELEED","Chloorfenvinfos",675,"Cfvinfos","jaargemiddelde","ng/L",100,"jaargemiddelde",100,100,null,500]
["L107_122","HET GELEED","Chloorfenvinfos",675,"Cfvinfos","maximum","ng/L",300,"maximum",300,300,null,1500]
["L107_122","HET GELEED","Chloornaftalenen (technisch)",481,"CNaft","jaargemiddelde","µg/L",1,"jaargemiddelde",1,1,null,5]
["L107_122","HET GELEED","Chloornaftalenen (technisch)",481,"CNaft","maximum","µg/L",40,"maximum",40,40,null,200]
["L107_122","HET GELEED","Chloornitrobenzenen",1210,"1C2+3+4NiBzS","jaargemiddelde","µg/L",3,"jaargemiddelde",3,3,null,15]
["L107_122","HET GELEED","Chloornitrobenzenen",1210,"1C2+3+4NiBzS","maximum","µg/L",60,"maximum",60,60,null,300]
["L107_122","HET GELEED","Chloornitrotoluenen",482,"CNiTol","jaargemiddelde","µg/L",3,"jaargemiddelde",3,3,null,15]
["L107_122","HET GELEED","Chloornitrotoluenen",482,"CNiTol","maximum","µg/L",40,"maximum",40,40,null,200]
["L107_122","HET GELEED","Chloorpyrifos-ethyl",686,"CpfosEy","jaargemiddelde","ng/L",30,"jaargemiddelde",30,30,null,150]
["L107_122","HET GELEED","Chloorpyrifos-ethyl",686,"CpfosEy","maximum","ng/L",100,"maximum",100,100,null,500]
["L107_122","HET GELEED","Chloortoluenen",1212,"CTolS","jaargemiddelde","µg/L",3,"jaargemiddelde",3,3,null,15]
["L107_122","HET GELEED","Chloortoluenen",1212,"CTolS","maximum","µg/L",200,"maximum",200,200,null,1000]
["L107_122","HET GELEED","Chloortoluidinen",484,"CTine","jaargemiddelde","µg/L",8,"jaargemiddelde",8,8,null,40]
["L107_122","HET GELEED","Chloortoluidinen",484,"CTine","maximum","µg/L",60,"maximum",60,60,null,300]
["L107_122","HET GELEED","Chloridazon",753,"Cdazon","jaargemiddelde","ng/L",10000,"jaargemiddelde",10000,10000,null,50000]
["L107_122","HET GELEED","Chloridazon",753,"Cdazon","maximum","ng/L",20000,"maximum",20000,20000,null,100000]
["L107_122","HET GELEED","Chloride",4,"Cl-","zomergemiddelde (apr-sept)","mg/L",10000,"jaargemiddelde",10000,10000,15000,0]
["L107_122","HET GELEED","Chroom, totaal",155,"Cr t","jaargemiddelde","µg/L",50,"jaargemiddelde",50,50,null,250]
["L107_122","HET GELEED","Chryseen",425,"Chr","jaargemiddelde","ng/L",1000,"jaargemiddelde",1000,1000,null,5000]
["L107_122","HET GELEED","Cumafos",486,"Cumafos","jaargemiddelde","ng/L",1,"jaargemiddelde",1,1,null,5]
["L107_122","HET GELEED","Cumafos",486,"Cumafos","maximum","ng/L",10,"maximum",10,10,null,50]
["L107_122","HET GELEED","Cyaniden, totaal",26,"CN- t","jaargemiddelde","µg/L",50,"jaargemiddelde",50,50,null,250]
["L107_122","HET GELEED","Cyaniden, totaal",26,"CN- t","maximum","µg/L",75,"maximum",75,75,null,375]
["L107_122","HET GELEED","Cybutrine",1506,"Cybutrine","jaargemiddelde","ng/L",2.5,"jaargemiddelde",2.5,2.5,null,12.5]
["L107_122","HET GELEED","Cybutrine",1506,"Cybutrine","maximum","ng/L",16,"maximum",16,16,null,80]
["L107_122","HET GELEED","Cypermethrin",1075,"Cypmethrin","jaargemiddelde","ng/L",0.08,"jaargemiddelde",0.08,0.08,null,0.4]
["L107_122","HET GELEED","Cypermethrin",1075,"Cypmethrin","maximum","ng/L",0.6,"maximum",0.6,0.6,null,3]
["L107_122","HET GELEED","DDT, totaal",907,"DDT t","jaargemiddelde","ng/L",25,"jaargemiddelde",25,25,null,125]
["L107_122","HET GELEED","Demeton",898,"Demeton","jaargemiddelde","ng/L",50,"jaargemiddelde",50,50,null,250]
["L107_122","HET GELEED","Demeton",898,"Demeton","maximum","ng/L",500,"maximum",500,500,null,2500]
["L107_122","HET GELEED","Dibenzo(a,h)anthraceen",426,"dBz(ah)An","jaargemiddelde","ng/L",500,"jaargemiddelde",500,500,null,2500]
["L107_122","HET GELEED","Dibutyltinverbindingen",1216,"DBySn som","jaargemiddelde","ngSn/L",80,"jaargemiddelde",80,80,null,400]
["L107_122","HET GELEED","Dibutyltinverbindingen",1216,"DBySn som","maximum","ngSn/L",700,"maximum",700,700,null,3500]
["L107_122","HET GELEED","Dichlooranilines, totaal",888,"DCAn t","jaargemiddelde","µg/L",0.2,"jaargemiddelde",0.2,0.2,null,1]
["L107_122","HET GELEED","Dichlooranilines, totaal",888,"DCAn t","maximum","µg/L",0.6,"maximum",0.6,0.6,null,3]
["L107_122","HET GELEED","Dichloorbenzenen",1218,"CBzsom","jaargemiddelde","µg/L",20,"jaargemiddelde",20,20,null,100]
["L107_122","HET GELEED","Dichloorbenzenen",1218,"CBzsom","maximum","µg/L",70,"maximum",70,70,null,350]
["L107_122","HET GELEED","Dichloorbenzidines",886,"DCBzdines","jaargemiddelde","µg/L",0.5,"jaargemiddelde",0.5,0.5,null,2.5]
["L107_122","HET GELEED","Dichloorbenzidines",886,"DCBzdines","maximum","µg/L",5,"maximum",5,5,null,25]
["L107_122","HET GELEED","Dichloormethaan",379,"DCMa","jaargemiddelde","µg/L",20,"jaargemiddelde",20,20,null,100]
["L107_122","HET GELEED","Dichloornitrobenzenen",1219,"diCNiBzsom","jaargemiddelde","µg/L",3,"jaargemiddelde",3,3,null,15]
["L107_122","HET GELEED","Dichloornitrobenzenen",1219,"diCNiBzsom","maximum","µg/L",60,"maximum",60,60,null,300]
["L107_122","HET GELEED","Dichloorprop",234,"24-DP","jaargemiddelde","ng/L",20000,"jaargemiddelde",20000,20000,null,100000]
["L107_122","HET GELEED","Dichloorprop",234,"24-DP","maximum","ng/L",200000,"maximum",200000,200000,null,1000000]
["L107_122","HET GELEED","Dichloorvos",391,"DCvos","jaargemiddelde","ng/L",0.6,"jaargemiddelde",0.6,0.6,null,3]
["L107_122","HET GELEED","Dichloorvos",391,"DCvos","maximum","ng/L",0.7,"maximum",0.7,0.7,null,3.5]
["L107_122","HET GELEED","Dicofol",1464,"Dicofol","jaargemiddelde","ng/L",1.3,"jaargemiddelde",1.3,1.3,null,6.5]
["L107_122","HET GELEED","Diethylamine",496,"DEyAm","jaargemiddelde","µg/L",30,"jaargemiddelde",30,30,null,150]
["L107_122","HET GELEED","Diethylamine",496,"DEyAm","maximum","µg/L",200,"maximum",200,200,null,1000]
["L107_122","HET GELEED","Difenyl",498,"DFy","jaargemiddelde","µg/L",2,"jaargemiddelde",2,2,null,10]
["L107_122","HET GELEED","Difenyl",498,"DFy","maximum","µg/L",10,"maximum",10,10,null,50]
["L107_122","HET GELEED","Diflufenican",1020,"Dflucan","jaargemiddelde","ng/L",30,"jaargemiddelde",30,30,null,150]
["L107_122","HET GELEED","Diflufenican",1020,"Dflucan","maximum","ng/L",50,"maximum",50,50,null,250]
["L107_122","HET GELEED","Dimethenamid",1231,"DiMetamid","jaargemiddelde","µg/L",1.5,"jaargemiddelde",1.5,1.5,null,7.5]
["L107_122","HET GELEED","Dimethenamid",1231,"DiMetamid","maximum","µg/L",6.7,"maximum",6.7,6.7,null,33.5]
["L107_122","HET GELEED","Dimethoaat",396,"Dmetoat","jaargemiddelde","ng/L",20,"jaargemiddelde",20,20,null,100]
["L107_122","HET GELEED","Dimethoaat",396,"Dmetoat","maximum","ng/L",200,"maximum",200,200,null,1000]
["L107_122","HET GELEED","Dimethylamine",497,"DMyAm","jaargemiddelde","µg/L",6,"jaargemiddelde",6,6,null,30]
["L107_122","HET GELEED","Dimethylamine",497,"DMyAm","maximum","µg/L",80,"maximum",80,80,null,400]
["L107_122","HET GELEED","Disulfoton",397,"Dsulfoton","jaargemiddelde","ng/L",10,"jaargemiddelde",10,10,null,50]
["L107_122","HET GELEED","Disulfoton",397,"Dsulfoton","maximum","ng/L",70,"maximum",70,70,null,350]
["L107_122","HET GELEED","Diuron",273,"Diuron","jaargemiddelde","ng/L",200,"jaargemiddelde",200,200,null,1000]
["L107_122","HET GELEED","Diuron",273,"Diuron","maximum","ng/L",1800,"maximum",1800,1800,null,9000]
["L107_122","HET GELEED","Epichloorhydrine",779,"eCHydrine","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
["L107_122","HET GELEED","Epichloorhydrine",779,"eCHydrine","maximum","µg/L",100,"maximum",100,100,null,500]
["L107_122","HET GELEED","Ethylbenzeen",213,"EyBz","jaargemiddelde","µg/L",5,"jaargemiddelde",5,5,null,25]
["L107_122","HET GELEED","Ethylbenzeen",213,"EyBz","maximum","µg/L",50,"maximum",50,50,null,250]
["L107_122","HET GELEED","Fenantreen",428,"Fen","jaargemiddelde","ng/L",100,"jaargemiddelde",100,100,null,500]
["L107_122","HET GELEED","Fenitrothion",399,"Fenithion","jaargemiddelde","ng/L",0.9,"jaargemiddelde",0.9,0.9,null,4.5]
["L107_122","HET GELEED","Fenitrothion",399,"Fenithion","maximum","ng/L",2,"maximum",2,2,null,10]
["L107_122","HET GELEED","Fenthion",500,"Fenthion","jaargemiddelde","ng/L",0.2,"jaargemiddelde",0.2,0.2,null,1]
["L107_122","HET GELEED","Fenthion",500,"Fenthion","maximum","ng/L",2,"maximum",2,2,null,10]
["L107_122","HET GELEED","Flufenacet",976,"Flucet","jaargemiddelde","ng/L",40,"jaargemiddelde",40,40,null,200]
["L107_122","HET GELEED","Flufenacet",976,"Flucet","maximum","ng/L",200,"maximum",200,200,null,1000]
["L107_122","HET GELEED","Fluorantheen",429,"Flu","jaargemiddelde","ng/L",6.3,"jaargemiddelde",6.3,6.3,null,31.5]
["L107_122","HET GELEED","Fluorantheen",429,"Flu","maximum","ng/L",120,"maximum",120,120,null,600]
["L107_122","HET GELEED","Fluoreen",430,"Fluoreen","jaargemiddelde","ng/L",2000,"jaargemiddelde",2000,2000,null,10000]
["L107_122","HET GELEED","Fluoride, opgelost",1328,"F- o","jaargemiddelde","mg/L",0.9,"jaargemiddelde",0.9,0.9,null,4.5]
["L107_122","HET GELEED","Fosfor, totaal",29,"P t","zomergemiddelde (apr-sept)","mgP/L",0.14000000000000001,"jaargemiddelde",0.14000000000000001,0.14000000000000001,0.35,0.7]
["L107_122","HET GELEED","Foxim",400,"Foxim","jaargemiddelde","µg/L",0.02,"jaargemiddelde",0.02,0.02,null,0.1]
["L107_122","HET GELEED","Foxim",400,"Foxim","maximum","µg/L",0.2,"maximum",0.2,0.2,null,1]
["L107_122","HET GELEED","Geleidbaarheid (20°C)",82,"EC 20","zomergemiddelde (apr-sept)","µS/cm",15000,"jaargemiddelde",15000,15000,18000,0]
["L107_122","HET GELEED","Heptachloor+epoxyde",948,"HpC+Epx","jaargemiddelde","ng/L",2.0000000000000001E-4,"jaargemiddelde",2.0000000000000001E-4,2.0000000000000001E-4,null,1E-3]
["L107_122","HET GELEED","Heptachloor+epoxyde",948,"HpC+Epx","maximum","ng/L",0.3,"maximum",0.3,0.3,null,1.5]
["L107_122","HET GELEED","Hexabroomcyclododecaan",939,"HBCD","jaargemiddelde","µg/L",1.6000000000000001E-3,"jaargemiddelde",1.6000000000000001E-3,1.6000000000000001E-3,null,8.0000000000000002E-3]
["L107_122","HET GELEED","Hexabroomcyclododecaan",939,"HBCD","maximum","µg/L",0.5,"maximum",0.5,0.5,null,2.5]
["L107_122","HET GELEED","Hexachloorbenzeen",244,"HCBz","jaargemiddelde","ng/L",4.3999999999999997E-2,"jaargemiddelde",4.3999999999999997E-2,4.3999999999999997E-2,null,0.22]
["L107_122","HET GELEED","Hexachloorbenzeen",244,"HCBz","maximum","ng/L",50,"maximum",50,50,null,250]
["L107_122","HET GELEED","Hexachloorbutadieen",245,"HCBdn","jaargemiddelde","ng/L",0.55000000000000004,"jaargemiddelde",0.55000000000000004,0.55000000000000004,null,2.75]
["L107_122","HET GELEED","Hexachloorbutadieen",245,"HCBdn","maximum","ng/L",600,"maximum",600,600,null,3000]
["L107_122","HET GELEED","Hexachloorethaan",381,"HCEa","jaargemiddelde","µg/L",3,"jaargemiddelde",3,3,null,15]
["L107_122","HET GELEED","Hexachloorethaan",381,"HCEa","maximum","µg/L",80,"maximum",80,80,null,400]
["L107_122","HET GELEED","Imidacloprid",1440,"Imcloprid","jaargemiddelde","µg/L",8.0000000000000002E-3,"jaargemiddelde",8.0000000000000002E-3,8.0000000000000002E-3,null,0.04]
["L107_122","HET GELEED","Imidacloprid",1440,"Imcloprid","maximum","µg/L",0.2,"maximum",0.2,0.2,null,1]
["L107_122","HET GELEED","Isopropylbenzeen",221,"iPyBz","jaargemiddelde","µg/L",1,"jaargemiddelde",1,1,null,5]
["L107_122","HET GELEED","Isopropylbenzeen",221,"iPyBz","maximum","µg/L",10,"maximum",10,10,null,50]
["L107_122","HET GELEED","Isoproturon",274,"Iproturon","jaargemiddelde","ng/L",300,"jaargemiddelde",300,300,null,1500]
["L107_122","HET GELEED","Isoproturon",274,"Iproturon","maximum","ng/L",1000,"maximum",1000,1000,null,5000]
["L107_122","HET GELEED","Kobalt, totaal",162,"Co t","jaargemiddelde","µg/L",0.6,"jaargemiddelde",0.6,0.6,null,3]
["L107_122","HET GELEED","Koper, totaal",165,"Cu t","jaargemiddelde","µg/L",50,"jaargemiddelde",50,50,null,250]
["L107_122","HET GELEED","Kwik, totaal",168,"Hg t","jaargemiddelde","µg/L",6.9999999999999994E-5,"jaargemiddelde",6.9999999999999994E-5,6.9999999999999994E-5,null,3.5E-4]
["L107_122","HET GELEED","Kwik, totaal",168,"Hg t","maximum","µg/L",0.15,"maximum",0.15,0.15,null,0.75]
["L107_122","HET GELEED","Linuron",275,"Linuron","jaargemiddelde","ng/L",300,"jaargemiddelde",300,300,null,1500]
["L107_122","HET GELEED","Linuron",275,"Linuron","maximum","ng/L",700,"maximum",700,700,null,3500]
["L107_122","HET GELEED","Lood, totaal",171,"Pb t","jaargemiddelde","µg/L",50,"jaargemiddelde",50,50,null,250]
["L107_122","HET GELEED","Lood, totaal",171,"Pb t","maximum","µg/L",97.22,"maximum",97.22,97.22,null,486.1]
["L107_122","HET GELEED","Malathion",401,"Malathion","jaargemiddelde","ng/L",0.8,"jaargemiddelde",0.8,0.8,null,4]
["L107_122","HET GELEED","Malathion",401,"Malathion","maximum","ng/L",3,"maximum",3,3,null,15]
["L107_122","HET GELEED","Mecoprop",253,"MCPP","jaargemiddelde","ng/L",10000,"jaargemiddelde",10000,10000,null,50000]
["L107_122","HET GELEED","Mecoprop",253,"MCPP","maximum","ng/L",40000,"maximum",40000,40000,null,200000]
["L107_122","HET GELEED","Methamidofos",402,"Methamfos","jaargemiddelde","µg/L",0.3,"jaargemiddelde",0.3,0.3,null,1.5]
["L107_122","HET GELEED","Methamidofos",402,"Methamfos","maximum","µg/L",3,"maximum",3,3,null,15]
["L107_122","HET GELEED","Mevinfos",392,"Mevinfos","jaargemiddelde","ng/L",2,"jaargemiddelde",2,2,null,10]
["L107_122","HET GELEED","Mevinfos",392,"Mevinfos","maximum","ng/L",20,"maximum",20,20,null,100]
["L107_122","HET GELEED","Molybdeen, totaal",177,"Mo t","jaargemiddelde","µg/L",350,"jaargemiddelde",350,350,null,1750]
["L107_122","HET GELEED","Monolinuron",278,"Mlinuron","jaargemiddelde","ng/L",300,"jaargemiddelde",300,300,null,1500]
["L107_122","HET GELEED","Monolinuron",278,"Mlinuron","maximum","ng/L",10000,"maximum",10000,10000,null,50000]
["L107_122","HET GELEED","Naftaleen",432,"Naft","jaargemiddelde","ng/L",2000,"jaargemiddelde",2000,2000,null,10000]
["L107_122","HET GELEED","Naftaleen",432,"Naft","maximum","ng/L",130000,"maximum",130000,130000,null,650000]
["L107_122","HET GELEED","Nikkel, totaal",180,"Ni t","jaargemiddelde","µg/L",30,"jaargemiddelde",30,30,null,150]
["L107_122","HET GELEED","Nikkel, totaal",180,"Ni t","maximum","µg/L",51,"maximum",51,51,null,255]
["L107_122","HET GELEED","Nitriet",9,"NO2-","jaargemiddelde","mgN/L",0.2,"jaargemiddelde",0.2,0.2,null,1]
["L107_122","HET GELEED","Nitriet",9,"NO2-","maximum","mgN/L",0.6,"maximum",0.6,0.6,null,3]
["L107_122","HET GELEED","Nonylfenol",972,"NyFol","jaargemiddelde","ng/L",300,"jaargemiddelde",300,300,null,1500]
["L107_122","HET GELEED","Nonylfenol",972,"NyFol","maximum","ng/L",2000,"maximum",2000,2000,null,10000]
["L107_122","HET GELEED","Octylfenolen",1223,"OyFolsom","jaargemiddelde","ng/L",100,"jaargemiddelde",100,100,null,500]
["L107_122","HET GELEED","Omethoaat",403,"Omethoaat","jaargemiddelde","µg/L",0.02,"jaargemiddelde",0.02,0.02,null,0.1]
["L107_122","HET GELEED","Omethoaat",403,"Omethoaat","maximum","µg/L",0.2,"maximum",0.2,0.2,null,1]
["L107_122","HET GELEED","Oxydemeton-methyl",404,"ODemeton-My","jaargemiddelde","ng/L",400,"jaargemiddelde",400,400,null,2000]
["L107_122","HET GELEED","Oxydemeton-methyl",404,"ODemeton-My","maximum","ng/L",4000,"maximum",4000,4000,null,20000]
["L107_122","HET GELEED","Parathion-ethyl",531,"PathionEy","jaargemiddelde","ng/L",0.2,"jaargemiddelde",0.2,0.2,null,1]
["L107_122","HET GELEED","Parathion-ethyl",531,"PathionEy","maximum","ng/L",4,"maximum",4,4,null,20]
["L107_122","HET GELEED","Parathion-methyl",508,"PathionMy","jaargemiddelde","ng/L",10,"jaargemiddelde",10,10,null,50]
["L107_122","HET GELEED","Parathion-methyl",508,"PathionMy","maximum","ng/L",20,"maximum",20,20,null,100]
["L107_122","HET GELEED","Pentachloorbenzeen",756,"PCBz","jaargemiddelde","ng/L",7,"jaargemiddelde",7,7,null,35]
["L107_122","HET GELEED","Pentachloorfenol",259,"PCFol","jaargemiddelde","ng/L",400,"jaargemiddelde",400,400,null,2000]
["L107_122","HET GELEED","Pentachloorfenol",259,"PCFol","maximum","ng/L",1000,"maximum",1000,1000,null,5000]
["L107_122","HET GELEED","perfluoroctaansulfonzuur (PFOS)",1044,"PFOS","jaargemiddelde","ng/L",0.65,"jaargemiddelde",0.65,0.65,null,3.25]
["L107_122","HET GELEED","perfluoroctaansulfonzuur (PFOS)",1044,"PFOS","maximum","ng/L",36000,"maximum",36000,36000,null,180000]
["L107_122","HET GELEED","Polybroomdifenylether, totaal (6)",1388,"BDE t (6)","jaargemiddelde","ng/L",4.8999999999999998E-5,"jaargemiddelde",4.8999999999999998E-5,4.8999999999999998E-5,null,2.4499999999999999E-4]
["L107_122","HET GELEED","Polybroomdifenylether, totaal (6)",1388,"BDE t (6)","maximum","ng/L",140,"maximum",140,140,null,700]
["L107_122","HET GELEED","Polychloorbifenyl, totaal",445,"PCB t","jaargemiddelde","ng/L",2,"jaargemiddelde",2,2,null,10]
["L107_122","HET GELEED","Polychloorbifenyl, totaal",445,"PCB t","maximum","ng/L",20,"maximum",20,20,null,100]
["L107_122","HET GELEED","pp'Dichloordifenyltrichloorethaan",263,"44DDT","jaargemiddelde","ng/L",10,"jaargemiddelde",10,10,null,50]
["L107_122","HET GELEED","Propanil",231,"Propanil","jaargemiddelde","ng/L",200,"jaargemiddelde",200,200,null,1000]
["L107_122","HET GELEED","Propanil",231,"Propanil","maximum","ng/L",3000,"maximum",3000,3000,null,15000]
["L107_122","HET GELEED","Pyreen",434,"Pyr","jaargemiddelde","ng/L",40,"jaargemiddelde",40,40,null,200]
["L107_122","HET GELEED","Quinoxyfen",1038,"Quinofen","jaargemiddelde","ng/L",150,"jaargemiddelde",150,150,null,750]
["L107_122","HET GELEED","Quinoxyfen",1038,"Quinofen","maximum","ng/L",2700,"maximum",2700,2700,null,13500]
["L107_122","HET GELEED","Seleen, totaal",183,"Se t","jaargemiddelde","µg/L",3,"jaargemiddelde",3,3,null,15]
["L107_122","HET GELEED","Simazine",280,"Simaz","jaargemiddelde","ng/L",1000,"jaargemiddelde",1000,1000,null,5000]
["L107_122","HET GELEED","Simazine",280,"Simaz","maximum","ng/L",4000,"maximum",4000,4000,null,20000]
["L107_122","HET GELEED","Stikstof, totaal",31,"N t","zomergemiddelde (apr-sept)","mgN/L",4,"jaargemiddelde",4,4,8,12]
["L107_122","HET GELEED","Sulfaat",14,"SO4=","zomergemiddelde (apr-sept)","mg/L",2250,"jaargemiddelde",2250,2250,2750,0]
["L107_122","HET GELEED","Surfactanten, anionische",618,"AISurf","jaargemiddelde","mg/L",0.1,"jaargemiddelde",0.1,0.1,null,0.5]
["L107_122","HET GELEED","Surfactanten, Kationische + Niet-ionogen",1767,"Surf KID+NID","jaargemiddelde","mg/L",1,"jaargemiddelde",1,1,null,5]
["L107_122","HET GELEED","Tellurium, totaal",517,"Te t","jaargemiddelde","µg/L",100,"jaargemiddelde",100,100,null,500]
["L107_122","HET GELEED","Terbutryn",282,"Terbutryn","jaargemiddelde","ng/L",65,"jaargemiddelde",65,65,null,325]
["L107_122","HET GELEED","Terbutryn",282,"Terbutryn","maximum","ng/L",340,"maximum",340,340,null,1700]
["L107_122","HET GELEED","Terbutylazine",281,"TrByaz","jaargemiddelde","µg/L",0.32,"jaargemiddelde",0.32,0.32,null,1.6]
["L107_122","HET GELEED","Terbutylazine",281,"TrByaz","maximum","µg/L",1.8,"maximum",1.8,1.8,null,9]
["L107_122","HET GELEED","Tetrabutyltin",410,"TtBySn","jaargemiddelde","ngSn/L",4.0999999999999996,"jaargemiddelde",4.0999999999999996,4.0999999999999996,null,20.5]
["L107_122","HET GELEED","Tetrabutyltin",410,"TtBySn","maximum","ngSn/L",41,"maximum",41,41,null,205]
["L107_122","HET GELEED","Tetrachlooretheen",382,"TtCEe","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
["L107_122","HET GELEED","Tetrachloormethaan",383,"TtCMa","jaargemiddelde","µg/L",12,"jaargemiddelde",12,12,null,60]
["L107_122","HET GELEED","Thallium, totaal",190,"Tl t","jaargemiddelde","µg/L",0.2,"jaargemiddelde",0.2,0.2,null,1]
["L107_122","HET GELEED","Tin, totaal",193,"Sn t","jaargemiddelde","µg/L",40,"jaargemiddelde",40,40,null,200]
["L107_122","HET GELEED","Titaan, totaal",196,"Ti t","jaargemiddelde","µg/L",100,"jaargemiddelde",100,100,null,500]
["L107_122","HET GELEED","Tolueen",223,"Tolueen","jaargemiddelde","µg/L",90,"jaargemiddelde",90,90,null,450]
["L107_122","HET GELEED","Tolueen",223,"Tolueen","maximum","µg/L",700,"maximum",700,700,null,3500]
["L107_122","HET GELEED","Triazofos",406,"Triazofos","jaargemiddelde","ng/L",30,"jaargemiddelde",30,30,null,150]
["L107_122","HET GELEED","Tributylfosfaat",520,"TBP","jaargemiddelde","ng/L",40000,"jaargemiddelde",40000,40000,null,200000]
["L107_122","HET GELEED","Tributylfosfaat",520,"TBP","maximum","ng/L",100000,"maximum",100000,100000,null,500000]
["L107_122","HET GELEED","Tributyltin",670,"TBySn","jaargemiddelde","ngSn/L",8.1000000000000003E-2,"jaargemiddelde",8.1000000000000003E-2,8.1000000000000003E-2,null,0.40500000000000003]
["L107_122","HET GELEED","Tributyltin",670,"TBySn","maximum","ngSn/L",0.61,"maximum",0.61,0.61,null,3.05]
["L107_122","HET GELEED","Trichlooracetaldehyde-hydraat",521,"TCAcyde","jaargemiddelde","µg/L",500,"jaargemiddelde",500,500,null,2500]
["L107_122","HET GELEED","Trichlooracetaldehyde-hydraat",521,"TCAcyde","maximum","µg/L",5000,"maximum",5000,5000,null,25000]
["L107_122","HET GELEED","Trichloorbenzenen",522,"TCBz","jaargemiddelde","µg/L",0.4,"jaargemiddelde",0.4,0.4,null,2]
["L107_122","HET GELEED","Trichlooretheen",385,"TCEe","jaargemiddelde","µg/L",10,"jaargemiddelde",10,10,null,50]
["L107_122","HET GELEED","Trichloorfenolen",1228,"triCFolsom","jaargemiddelde","ng/L",6000,"jaargemiddelde",6000,6000,null,30000]
["L107_122","HET GELEED","Trichloorfenolen",1228,"triCFolsom","maximum","ng/L",20000,"maximum",20000,20000,null,100000]
["L107_122","HET GELEED","Trichloorfon",407,"TCfon","jaargemiddelde","µg/L",1E-3,"jaargemiddelde",1E-3,1E-3,null,5.0000000000000001E-3]
["L107_122","HET GELEED","Trichloorfon",407,"TCfon","maximum","µg/L",0.01,"maximum",0.01,0.01,null,0.05]
["L107_122","HET GELEED","Trichloormethaan",388,"TCMa","jaargemiddelde","µg/L",2.5,"jaargemiddelde",2.5,2.5,null,12.5]
["L107_122","HET GELEED","Trifenyltinacetaat, chloride, hydroxide",1229,"TFySn som","jaargemiddelde","ngSn/L",0.3,"jaargemiddelde",0.3,0.3,null,1.5]
["L107_122","HET GELEED","Trifenyltinacetaat, chloride, hydroxide",1229,"TFySn som","maximum","ngSn/L",3,"maximum",3,3,null,15]
["L107_122","HET GELEED","Trifluralin",417,"Tfluralin","jaargemiddelde","ng/L",30,"jaargemiddelde",30,30,null,150]
["L107_122","HET GELEED","Uranium, totaal",525,"U t","jaargemiddelde","µg/L",1,"jaargemiddelde",1,1,null,5]
["L107_122","HET GELEED","Vanadium, totaal",199,"V t","jaargemiddelde","µg/L",5,"jaargemiddelde",5,5,null,25]
["L107_122","HET GELEED","Vinylchloride",570,"VinCl","jaargemiddelde","µg/L",0.09,"jaargemiddelde",0.09,0.09,null,0.45]
["L107_122","HET GELEED","Xylenen (o+m+p)",526,"ompXyl","jaargemiddelde","µg/L",4,"jaargemiddelde",4,4,null,20]
["L107_122","HET GELEED","Xylenen (o+m+p)",526,"ompXyl","maximum","µg/L",40,"maximum",40,40,null,200]
["L107_122","HET GELEED","Zilver, totaal",202,"Ag t","jaargemiddelde","µg/L",0.4,"jaargemiddelde",0.4,0.4,null,2]
["L107_122","HET GELEED","Zink, totaal",205,"Zn t","jaargemiddelde","µg/L",200,"jaargemiddelde",200,200,null,1000]
["L107_122","HET GELEED","Zwevende stoffen",113,"ZS","90 percentiel","mg/L",50,"maximum",75,75,150,225]

{"sheet":"MKN opgeschoond","index":17,"n_rows":261,"n_cols":12,"rows_kept":261,"cut":false,"hidden":true,"merged":[[0,4,0,5],[0,6,0,7],[1,0,4,0],[1,1,4,1],[1,2,4,2],[1,3,4,3],[1,10,4,10],[5,1,5,10],[6,8,9,8],[6,10,9,10],[22,1,23,1],[22,2,23,2],[22,3,23,3],[22,4,23,4],[22,5,23,5],[22,6,23,6],[257,1,257,10],[22,7,23,7],[22,8,23,8],[22,10,23,10],[134,9,135,9],[136,9,137,9],[229,1,229,10]]}
[null,null,null,null,"RIVIEREN EN MEREN",null,"OVERGANGSWATER"]
["Volgnummer Bijlage 2.3.1","CAS-nummer","Parameter","Eenheid","Milieu-","Milieu-","Milieu-","Milieu-","Bio-","Indelings-","Europese Context"]
[null,null,null,null,"kwaliteitsnorm","kwaliteitsnorm","kwaliteitsnorm","kwaliteitsnorm maximum","tanorm","criterium GS"]
[null,null,null,null,"gemiddelde","maximum","gemiddelde","(MAC-MKN)","(µg/kg nat gewicht)"]
[null,null,null,null,"(JG-MKN)","(MAC-MKN)","(JG-MKN)"]
[null,"gevaarlijke stoffen: organische stoffen",null,null,null,null,null,null,null,null,null,"Aandachtsstoffen Vlaanderen"]
[1,"309-00-2","aldrin","µg/l",0.01,"niet van toepassing",5.0000000000000001E-3,"niet van toepassing",null,0.01,"VS"]
[2,"60-57-1","dieldrin","µg/l",0.01,"niet van toepassing",5.0000000000000001E-3,"niet van toepassing",null,0.01]
[3,"72-20-8","endrin","µg/l",0.01,"niet van toepassing",5.0000000000000001E-3,"niet van toepassing",null,0.01]
[4,"465-73-6","isodrin","µg/l",0.01,"niet van toepassing",5.0000000000000001E-3,"niet van toepassing",null,0.01]
[4.5,null,"aldrin + dieldrin + endrin + isodrin","µg/l",0.01,"niet van toepassing",5.0000000000000001E-3,"niet van toepassing",null,0.01]
[5,"95-85-2","2-amino-4-chloorfenol","µg/l",10,"niet van toepassing",10,"niet van toepassing",null,10]
[6,"2642-71-9","azinfos-ethyl","µg/l",0.01,0.1,0.01,0.1,null,0.01]
[7,"86-50-0","azinfos-methyl","µg/l",2E-3,0.01,2E-3,0.01,null,2E-3]
[8,"71-43-2","benzeen","µg/l",10,50,8,50,null,10,"PS (4)"]
[9,"92-87-5","benzidine","µg/l",0.6,6,0.6,6,null,0.6]
[10,"100-44-7","alfa-chloortolueen (benzylchloride)","µg/l",1,10,1,10,null,1]
[11,"98-87-3","alfa-alfa-dichloortolueen (benzalchloride)","µg/l",5,"niet van toepassing",5,"niet van toepassing",null,5]
[12,"74070-46-5","aclonifen","µg/l",0.12,0.12,1.2E-2,1.2E-2,null,0.12,"PS (38)"]
[13,"42576-02-3","bifenox","µg/l",1.2E-2,0.04,1.1999999999999999E-3,4.0000000000000001E-3,null,1.2E-2,"PS (39)"]
[14,"28159-98-0","cybutryne","µg/l",2.5000000000000001E-3,1.6E-2,2.5000000000000001E-3,1.6E-2,null,2.5000000000000001E-3,"PS (40)"]
[15,"52315-07-8","cypermethrin","µg/l",8.0000000000000007E-5,5.9999999999999995E-4,7.9999999999999996E-6,6.0000000000000002E-5,null,8.0000000000000007E-5,"PS (41)"]
[16,"(A)","dioxinen en dioxineachtige verbindingen","µg/l",null,null,null,null,"0.0065 (B)(C)","rapportage-","PGS (37)"]
[17,null,null,null,null,null,null,null,null,"grens"]
[18,"92-52-4","difenyl","µg/l",2,10,2,10,null,2]
[19,"56-23-5","koolstoftetrachloride","µg/l",12,"niet van toepassing",12,"niet van toepassing",null,12,"VS"]
[20,"302-17-0","trichlooracetal-dehyde-hydraat","µg/l",500,5000,500,5000,null,500]
[21,"57-74-9","cis-chloordaan trans-chloordaan","µg/l","Σ = 0.002","Σ = 0.04","Σ = 0.002","Σ = 0.04",null,"Σ = 0.002"]
[22,"79-11-8","chloorazijnzuur","µg/l",0.6,3,0.6,3,null,0.6]
[23,"95-51-2","o-chlooraniline","µg/l",1,5,1,5,null,1]
[24,"108-42-9","m-chlooraniline","µg/l",1,5,1,5,null,1]
[25,"106-47-8","p-chlooraniline","µg/l",1,5,1,5,null,1]
[25.5,null,"o-chlooraniline + m-chlooraniline + p-chlooraniline","µg/l",1,5,1,5,null,1]
[26,"108-90-7","chloorbenzeen","µg/l",6,40,6,40,null,6]
[27,"97-00-7","1-chloor-2,4-dinitrobenzeen","µg/l",5,20,5,20,null,5]
[28,"107-07-3","2-chloorethanol","µg/l",30,300,30,300,null,30]
[29,"67-66-3","chloroform","µg/l",2.5,"niet van toepassing",2.5,"niet van toepassing",null,2.5,"PS (32)"]
[30,"59-50-7","4-chloor-3-methylfenol","µg/l",9,90,9,90,null,9]
[31,"90-13-1","1-chloornaftaleen","µg/l",1,40,1,40,null,1]
[32,"91-58-7","2-chloornaftaleen","µg/l",1,40,1,40,null,1]
[32.5,null,"1-chloornaftaleen + 2-chloornaftaleen","µg/l",1,40,1,40,null,1]
[33,"89-63-4","4-chloor-2-nitroaniline","µg/l",2,20,2,20,null,2]
[34,"88-73-3","1-chloor-2-nitrobenzeen","µg/l",3,60,3,60,null,3]
[35,"121-73-3","1-chloor-3-nitrobenzeen","µg/l",3,60,3,60,null,3]
[36,"100-00-5","1-chloor-4-nitrobenzeen","µg/l",3,60,3,60,null,3]
[36.5,null,"1-chloor-2-nitrobenzeen + 1-chloor-3-nitrobenzeen + 1-chloor-4-nitrobenzeen","µg/l",3,60,3,60,null,3]
[37,null,"chloornitrotoluenen","µg/l",3,40,3,40,null,3]
[38,"95-57-8","2-chloorfenol","µg/l",20,120,20,120,null,20]
[39,"108-43-0","3-chloorfenol","µg/l",20,120,20,120,null,20]
[40,"106-48-9","4-chloorfenol","µg/l",20,120,20,120,null,20]
[40.5,null,"2-chloorfenol + 3-chloorfenol + 4-chloorfenol","µg/l",20,120,20,120,null,20]
[41,"126-99-8","2-chloor-1,3-butadieen","µg/l",10,"niet van toepassing",10,"niet van toepassing",null,10]
[42,"107-05-1","3-chloorpropeen","µg/l",3,30,3,30,null,3]
[43,"95-49-8","2-chloortolueen","µg/l",3,200,3,200,null,3]
[44,"108-41-8","3-chloortolueen","µg/l",3,200,3,200,null,3]
[45,"106-43-4","4-chloortolueen","µg/l",3,200,3,200,null,3]
[45.5,null,"2-chloortolueen + 3-chloortolueen + 4-chloortolueen","µg/l",3,200,3,200,null,3]
[46,"615-65-6","2-chloor-para-toluïdine","µg/l",8,60,8,60,null,8]
[47,null,"chloortoluïdinen (andere dan 2-chloor-para-toluïdine)","µg/l",8,60,8,60,null,8]
[47.5,null,"2-chloor-para-toluïdine + chloortoluïdinen (andere dan 2-chloor-para-toluïdine)","µg/l",8,60,8,60,null,8]
[48,"56-72-4","cumafos","µg/l",1E-3,0.01,1E-3,0.01,null,1E-3]
[49,"108-77-0","2,4,6-trichloor-1,3,5-triazine","µg/l",0.1,"niet van toepassing",0.1,"niet van toepassing",null,0.1]
[50,"94-75-7","(2,4-dichloorfenoxy)-azijnzuur (2,4-D)","µg/l",20,200,20,200,null,20]
[51,"(D)","DDT totaal","µg/l",2.5000000000000001E-2,"niet van toepassing",2.5000000000000001E-2,"niet van toepassing",null,2.5000000000000001E-2,"VS"]
[52,"50-29-3","p,p'-DDT","µg/l",0.01,"niet van toepassing",0.01,"niet van toepassing",null,0.01,"VS"]
[53,"8065-48-3","demeton","µg/l",0.05,0.5,0.05,0.5,null,0.05]
[54,"106-93-4","1,2-dibroomethaan","µg/l",3.0000000000000001E-3,0.4,3.0000000000000001E-3,0.4,null,3.0000000000000001E-3]
[55,"683-18-1","dibutyltindichloride","µg Sn/l",0.08,0.7,0.08,0.7,null,0.08]
[56,"818-08-6","dibutyltinoxide","µg Sn/l",0.08,0.7,0.08,0.7,null,0.08]
[57,null,"dibutyltinzouten","µg Sn/l",0.08,0.7,0.08,0.7,null,0.08]
[null,null,"dibutyltindichloride + dibutyltinoxide + dibutyltinzouten","µg Sn/l",0.08,0.7,0.08,0.7,null,0.08]
[58,"608-27-5","2,3-dichlooraniline","µg/L",0.2,0.6,0.2,0.6,null,0.2]
[59,"554-00-7","2,4-dichlooraniline","µg/L",0.2,0.6,0.2,0.6,null,0.2]
[60,"95-82-9","2,5-dichlooraniline","µg/L",0.2,0.6,0.2,0.6,null,0.2]
[61,"608-31-1","2,6-dichlooraniline","µg/L",0.2,0.6,0.2,0.6,null,0.2]
[62,"626-43-7","3,5-dichlooraniline","µg/L",0.2,0.6,0.2,0.6,null,0.2]
[63,"95-76-1","3,4-dichlooraniline","µg/L",0.2,0.6,0.2,0.6,null,0.2]
[63.5,null,{"$f":"_xlfn.CONCAT(C72,\" + \",C73,\" + \",C74,\" + \",C75,\" + \",C76,\" + \",C77)","v":"2,3-dichlooraniline + 2,4-dichlooraniline + 2,5-dichlooraniline + 2,6-dichlooraniline + 3,5-dichlooraniline + 3,4-dichlooraniline"},"µg/L",0.2,0.6,0.2,0.6,null,0.2]
[64,"95-50-1","1,2-dichloorbenzeen"," µg/l ",20,70,20,70,null,20]
[65,"541-73-1","1,3-dichloorbenzeen "," µg/l ",20,70,20,70,null,20]
[66,"106-46-7","1,4-dichloorbenzeen"," µg/l ",20,70,20,70,null,20]
[66.5,null,{"$f":"_xlfn.CONCAT(C79,\" + \",C80,\" + \",C81)","v":"1,2-dichloorbenzeen + 1,3-dichloorbenzeen  + 1,4-dichloorbenzeen"}," µg/l ",20,70,20,70,null,20]
[67,null,"dichloorbenzidines","µg/l",0.5,5,0.5,5,null,0.5]
[68,"108-60-1","bis-(2-chloorisopropyl)-ether","µg/l",10,"niet van toepassing",10,"niet van toepassing",null,10]
[69,"75-34-3","1,1-dichloorethaan","µg/l",100,8000,100,8000,null,100]
[70,"107-06-2","1,2-dichloorethaan (EDC)","µg/l",10,"niet van toepassing",10,"niet van toepassing",null,10,"PS (10)"]
[71,"75-35-4","1,1-dichlooretheen","µg/l",50,500,50,500,null,50]
[72,"540-59-0","1,2-dichlooretheen, cis","µg/l",10,100,10,100,null,10]
[73,"540-59-0","1,2-dichlooretheen, trans","µg/l",10,100,10,100,null,10]
[73.5,"540-59-0",{"$f":"_xlfn.CONCAT(C88,\" + \",C89)","v":"1,2-dichlooretheen, cis + 1,2-dichlooretheen, trans"},"µg/l",10,100,10,100,null,10]
[74,"75-09-2","dichloormethaan","µg/l",20,"niet van toepassing",20,"niet van toepassing",null,20,"PS (11)"]
[75,null,"dichloornitrobenze-nen","µg/l",3,60,3,60,null,3]
[76,"120-83-2","2,4-dichloorfenol","µg/l",2,70,2,70,null,2]
[77,"78-87-5","1,2-dichloorpropaan","µg/l",400,1000,400,1000,null,400]
[78,"96-23-1","1,3-dichloor-2-propanol","µg/l",100,2000,100,2000,null,100]
[79,"542-75-6","1,3-dichloorpropeen, cis","µg/l",2,20,2,20,null,2]
[80,"542-75-6","1,3-dichloorpropeen, trans","µg/l",2,20,2,20,null,2]
[80.5,"542-75-6",{"$f":"_xlfn.CONCAT(C96,\" + \",C97)","v":"1,3-dichloorpropeen, cis + 1,3-dichloorpropeen, trans"},"µg/l",2,20,2,20,null,2]
[81,"78-88-6","2,3-dichloorpropeen","µg/l",2,20,2,20,null,2]
[82,"120-36-5","dichlorprop","µg/l",20,200,20,200,null,20]
[83,"115-32-2","dicofol","µg/l",1.2999999999999999E-3,"niet van toepassing (E)",3.1999999999999999E-5,"niet van toepassing (E)",33,"rapportagegrens","PGS (34)"]
[84,"62-73-7","dichloorvos","µg/l",5.9999999999999995E-4,6.9999999999999999E-4,6.0000000000000002E-5,6.9999999999999994E-5,null,5.9999999999999995E-4,"PS (42)"]
[85,"109-89-7","diethylamine","µg/l",30,200,30,200,null,30]
[86,"60-51-5","dimethoaat","µg/l",0.02,0.2,0.02,0.2,null,0.02]
[87,"124-40-3","dimethylamine","µg/l",6,80,6,80,null,6]
[88,"298-04-4","disulfoton","µg/l",0.01,7.0000000000000007E-2,0.01,7.0000000000000007E-2,null,0.01]
[89,"115-29-7","α-endosulfan","µg/l",5.0000000000000001E-3,0.01,5.0000000000000001E-4,4.0000000000000001E-3,null,5.0000000000000001E-3,"PGS (14)"]
[90,"115-29-7","β-endosulfan","µg/l",5.0000000000000001E-3,0.01,5.0000000000000001E-4,4.0000000000000001E-3,null,5.0000000000000001E-3,"PGS (14)"]
[90.5,"115-29-7",{"$f":"_xlfn.CONCAT(C107,\" + \",C108)","v":"α-endosulfan + β-endosulfan"},"µg/l",5.0000000000000001E-3,0.01,5.0000000000000001E-4,4.0000000000000001E-3,null,5.0000000000000001E-3,"PGS (14)"]
[91,"106-89-8","1-chloor-2,3-epoxypropaan (epichloorhydrine)","µg/l",10,100,10,100,null,10]
[92,"100-41-4","ethylbenzeen","µg/l",5,50,5,50,null,5]
[93,"122-14-5","fenitrothion","µg/l",8.9999999999999998E-4,2E-3,8.9999999999999998E-4,2E-3,null,8.9999999999999998E-4]
[94,"55-38-9","fenthion","µg/l",2.0000000000000001E-4,2E-3,2.0000000000000001E-4,2E-3,null,2.0000000000000001E-4]
[95,"118-74-1","hexachloorbenzeen (HCB)","µg/l",null,0.05,null,0.05,"10 (F)","rapportagegrens","PGS (16)"]
[96,"87-68-3","hexachloorbutadieen (HCBD)","µg/l",null,0.6,null,0.6,"55 (G)","rapportagegrens","PGS (17)"]
[97,"(H)","hexabroom-cyclododecaan (HBCDD)","µg/l",1.6000000000000001E-3,0.5,8.0000000000000004E-4,0.05,167,"rapportagegrens","PGS (43)"]
[98,"76-44-8 / 1024-57-3","heptachloor en heptachloorepoxide","µg/l",1.9999999999999999E-7,2.9999999999999997E-4,1E-8,3.0000000000000001E-5,6.7000000000000002E-3,"rapportagegrens","PGS (44)"]
[99,"608-73-1","α-hexachloorcyclo-hexaan (α-HCH)","µg/l",0.02,0.04,2E-3,0.02,null,0.02,"PGS (18)"]
[100,"608-73-1","β-hexachloorcyclo-hexaan (β-HCH)","µg/l",0.02,0.04,2E-3,0.02,null,0.02,"PGS (18)"]
[101,"608-73-1","Y-hexachloorcyclo-hexaan (Y-HCH)","µg/l",0.02,0.04,2E-3,0.02,null,0.02,"PGS (18)"]
[102,"608-73-1","σ-hexachloorcyclo-hexaan (σ-HCH)","µg/l",0.02,0.04,2E-3,0.02,null,0.02,"PGS (18)"]
[102.5,"608-73-1","α-HCH + β-HCH + Y-HCH + σ-HCH","µg/l",0.02,0.04,2E-3,0.02,null,0.02,"PGS (18)"]
[103,"67-72-1","hexachloorethaan","µg/l",3,80,3,80,null,3]
[104,"98-82-8","isopropylbenzeen","µg/l",1,10,1,10,null,1]
[105,"330-55-2","linuron","µg/l",0.3,0.7,0.3,0.7,null,0.3]
[106,"121-75-5","malathion","µg/l",8.0000000000000004E-4,3.0000000000000001E-3,8.0000000000000004E-4,3.0000000000000001E-3,null,8.0000000000000004E-4]
[107,"94-74-6","MCPA","µg/l",0.7,20,0.7,20,null,0.7]
[108,"93-65-2","mecoprop (MCPP)","µg/l",10,40,10,40,null,10]
[109,"10265-92-6","methamidofos","µg/l",0.3,3,0.3,3,null,0.3]
[110,"7786-34-7","mevinfos","µg/l",2E-3,0.02,2E-3,0.02,null,2E-3]
[111,"1746-81-2","monolinuron","µg/l",0.3,10,0.3,10,null,0.3]
[112,"1113-02-6","omethoaat","µg/l",0.02,0.2,0.02,0.2,null,0.02]
[113,"301-12-2","oxydemeton-methyl","µg/l",0.4,4,0.4,4,null,0.4]
[114,"50-32-8","benzo(a)pyreen","µg/l",1.7000000000000001E-4,0.27,1.7000000000000001E-4,2.7E-2,5,"rapportagegrens","PGS (28)"]
[115,"205-99-2","benzo(b)fluoran-teen","µg/l","(I)",1.7000000000000001E-2,"(I)",1.7000000000000001E-2,"(I)","Σ = 0.03","PGS (28)"]
[116,"207-08-9","benzo(k)fluoran-teen","µg/l","(I)",1.7000000000000001E-2,"(I)",1.7000000000000001E-2,"(I)",null,"PGS (28)"]
[117,"191-24-2","benzo(g,h,i)pery-leen","µg/l","(I)",8.2000000000000007E-3,"(I)",8.1999999999999998E-4,"(I)","Σ = 0.002","PGS (28)"]
[118,"193-39-5","indeno(1,2,3-cd)pyreen","µg/l","(I)","niet van toepassing","(I)","niet van toepassing","(I)",null,"PGS (28)"]
[119,"206-44-0","fluoranteen","µg/l",6.3E-3,0.12,6.3E-3,0.12,30,"rapportagegrens","PS (15)"]
[120,"120-12-7","antraceen","µg/l",0.1,0.1,0.1,0.1,null,0.1,"PGS (2)"]
[121,"91-20-3","naftaleen","µg/l",2,130,2,130,null,2,"PS (22)"]
[122,"85-01-8","fenantreen","µg/l",0.1,"niet van toepassing",0.1,"niet van toepassing",null,0.1]
[123,"83-32-9","acenafteen","µg/l",0.06,"niet van toepassing",0.06,"niet van toepassing",null,0.06]
[124,"218-01-9","chryseen","µg/l",1,"niet van toepassing",1,"niet van toepassing",null,1]
[125,"56-55-3","benzo(a)antra-ceen","µg/l",0.3,"niet van toepassing",0.3,"niet van toepassing",null,0.3]
[126,"86-73-7","fluoreen","µg/l",2,"niet van toepassing",2,"niet van toepassing",null,2]
[127,"129-00-0","pyreen","µg/l",0.04,"niet van toepassing",0.04,"niet van toepassing",null,0.04]
[128,"208-96-8","acenaftyleen","µg/l",4,"niet van toepassing",4,"niet van toepassing",null,4]
[129,"53-70-3","dibenzo(a,h)an-traceen","µg/l",0.5,"niet van toepassing",0.5,"niet van toepassing",null,0.5]
[130,"56-38-2","parathion-ethyl","µg/l",2.0000000000000001E-4,4.0000000000000001E-3,2.0000000000000001E-4,4.0000000000000001E-3,null,2.0000000000000001E-4]
[131,"298-00-0","parathion-methyl","µg/l",0.01,0.02,0.01,0.02,null,0.01]
[132,"7012-37-5","PCB 28","µg/l",2E-3,0.02,2E-3,0.02,null,2E-3]
[133,"35693-99-3","PCB 52","µg/l",2E-3,0.02,2E-3,0.02,null,2E-3]
[134,"37680-73-2","PCB 101","µg/l",2E-3,0.02,2E-3,0.02,null,2E-3]
[135,"31508-00-6","PCB 118","µg/l",2E-3,0.02,2E-3,0.02,null,2E-3]
[136,"35065-28-2","PCB 138","µg/l",2E-3,0.02,2E-3,0.02,null,2E-3]
[137,"35065-27-1","PCB 153","µg/l",2E-3,0.02,2E-3,0.02,null,2E-3]
[138,"35065-29-3","PCB 180","µg/l",2E-3,0.02,2E-3,0.02,null,2E-3]
[138.5,null,"PCB totaal","µg/L",2E-3,0.02,2E-3,0.02,null,2E-3]
[139,"87-86-5","pentachloorfenol","µg/l",0.4,1,0.4,1,null,0.4,"PS (27)"]
[140,"1763-23-1","perfluoroctaansul-fonzuur en zijn derivaten (PFOS)","µg/l",6.4999999999999997E-4,36,1.2999999999999999E-4,7.2,9.1,"rapportagegrens","PGS (35)"]
[141,"124495-18-7","quinoxyfen","µg/l",0.15,2.7,1.4999999999999999E-2,0.54,null,0.15,"PGS(36)"]
[142,"14816-18-3","foxim","µg/l",0.02,0.2,0.02,0.2,null,0.02]
[143,"709-98-8","propanil","µg/l",0.2,3,0.2,3,null,0.2]
[144,"1698-60-8","chloridazon (pyrazon)","µg/l",10,20,10,20,null,10]
[145,"122-34-9","simazine","µg/l",1,4,1,4,null,1,"PS (29)"]
[146,"93-76-5","(2,4,5-trichloorfenoxy)-azijnzuur (2,4,5-T)","µg/l",2,20,2,20,null,2]
[147,"1461-25-2","tetrabutyltin","µg/l",1.2E-2,0.12,1.2E-2,0.12,null,0.01]
[148,"95-94-3","1,2,4,5-tetrachloorbenzeen","µg/l",9,30,9,30,null,9]
[149,"79-34-5","1,1,2,2-tetrachloorethaan","µg/l",100,900,100,900,null,100]
[150,"886-50-0","terbutryn","µg/l",6.5000000000000002E-2,0.34,6.4999999999999997E-3,3.4000000000000002E-2,null,6.5000000000000002E-2,"PS (45)"]
[151,"127-18-4","tetrachlooretheen (PER)","µg/l",10,"niet van toepassing",10,"niet van toepassing",null,10,"VS"]
[152,"108-88-3","tolueen","µg/l",90,700,90,700,null,90]
[153,"24017-47-8","triazofos","µg/l",0.03,"niet van toepassing",0.03,"niet van toepassing",null,0.03]
[154,"126-73-8","tri-n-butylfosfaat","µg/l",40,100,40,100,null,40]
[155,"36643-28-4","tributyltin","µg/l",2.0000000000000001E-4,1.5E-3,2.0000000000000001E-4,1.5E-3,null,2.0000000000000001E-4,"PGS (30)"]
[156,"52-68-6","trichloorfon","µg/l",1E-3,0.01,1E-3,0.01,null,1E-3]
[157,"12002-48-1","1,2,3-trichloorbenzeen","µg/l",0.4,"niet van toepassing",0.4,"niet van toepassing",null,0.4,"PS (31)"]
[161,"12002-48-1","1,2,4-trichloorbenzeen","µg/l",0.4,"niet van toepassing",0.4,"niet van toepassing",null,0.4,"PS (31)"]
[162,"12002-48-1","1,3,5-trichloorbenzeen","µg/l",0.4,"niet van toepassing",0.4,"niet van toepassing",null,0.4,"PS (31)"]
[162.5,"12002-48-1",{"$f":"_xlfn.CONCAT(C178,\" + \",C179,\" + \",C180)","v":"1,2,3-trichloorbenzeen + 1,2,4-trichloorbenzeen + 1,3,5-trichloorbenzeen"},"µg/l",0.4,"niet van toepassing",0.4,"niet van toepassing",null,0.4,"PS (31)"]
[163,"71-55-6","1,1,1-trichloorethaan","µg/l",20,50,20,50,null,20]
[164,"79-00-5","1,1,2-trichloorethaan","µg/l",20,300,20,300,null,20]
[165,"79-01-6","trichloorethyleen (TRI)","µg/l",10,"niet van toepassing",10,"niet van toepassing",null,10,"VS"]
[166,"933-78-8","2,3,5-trichloorfenol","µg/l",6,20,6,20,null,6]
[167,"88-06-2","2,4,6-trichloorfenol","µg/l",6,20,6,20,null,6]
[168,"95-95-4","2,4,5-trichloorfenol","µg/l",6,20,6,20,null,6]
[169,"15950-66-0","2,3,4-trichloorfenol","µg/l",6,20,6,20,null,6]
[170,"933-75-5","2,3,6-trichloorfenol","µg/l",6,20,6,20,null,6]
[171,"609-19-8","3,4,5-trichloorfenol","µg/l",6,20,6,20,null,6]
[171.5,null,{"$f":"_xlfn.CONCAT(C185,\" + \",C186,\" + \",C187,\" + \",C188,\" + \",C189,\" + \",C190)","v":"2,3,5-trichloorfenol + 2,4,6-trichloorfenol + 2,4,5-trichloorfenol + 2,3,4-trichloorfenol + 2,3,6-trichloorfenol + 3,4,5-trichloorfenol"},"µg/l",6,20,6,20,null,6]
[172,"76-13-1","1,1,2-trichloortrifluor-ethaan","µg/l",7,70,7,70,null,7]
[173,"1582-09-8","trifluraline","µg/l",0.03,"niet van toepassing",0.03,"niet van toepassing",null,0.03,"PGS (33)"]
[174,"900-95-8","trifenyltinacetaat","µg/l",2.9999999999999997E-4,3.0000000000000001E-3,2.9999999999999997E-4,3.0000000000000001E-3,null,2.9999999999999997E-4]
[175,"639-58-7","trifenyltinchloride","µg/l",2.9999999999999997E-4,3.0000000000000001E-3,2.9999999999999997E-4,3.0000000000000001E-3,null,2.9999999999999997E-4]
[176,"76-87-9","trifenyltinhydroxide","µg/l",2.9999999999999997E-4,3.0000000000000001E-3,2.9999999999999997E-4,3.0000000000000001E-3,null,2.9999999999999997E-4]
[176.5,null,{"$f":"_xlfn.CONCAT(C194,\" + \",C195,\" + \",C196)","v":"trifenyltinacetaat + trifenyltinchloride + trifenyltinhydroxide"},"µg/l",2.9999999999999997E-4,3.0000000000000001E-3,2.9999999999999997E-4,3.0000000000000001E-3,null,2.9999999999999997E-4]
[177,"75-01-4","vinylchloride","µg/l",0.09,"niet van toepassing",0.09,"niet van toepassing",null,0.09]
[178,"1330-20-7","xylenen","µg/l",4,40,4,40,null,4]
[179,"1912-24-9","atrazine","µg/l",0.6,2,0.6,2,null,0.6,"PS (3)"]
[180,"25057-89-0","bentazon","µg/l",50,500,50,500,null,50]
[181,"25154-52-3","nonylfenol","µg/l",0.3,2,0.3,2,null,0.3,"PGS (24)"]
[182,"104-40-5","nonylfenol","µg/l",0.3,2,0.3,2,null,0.3,"PGS (24)"]
[183,"84852-15-3","nonylfenol","µg/l",0.3,2,0.3,2,null,0.3,"PGS (24)"]
[null,null,"totaal nonylfenol","µg/l",0.3,2,0.3,2,null,0.3,"PGS (24)"]
[184,"15972-60-8","alachloor","µg/l",0.3,0.7,0.3,0.7,null,0.3,"PS (1)"]
[185,"85535-84-8","C10-13-chlooralkanen (J)","µg/l",0.4,1.4,0.4,1.4,null,0.4,"PGS (7)"]
[186,"470-90-6","chloorfenvinphos","µg/l",0.1,0.3,0.1,0.3,null,0.1,"PS (8)"]
[187,"2921-88-2","chloorpyrifos","µg/l",0.03,0.1,0.03,0.1,null,0.03,"PS (9)"]
[188,"117-81-7","di(2-ethylhexyl)-ftalaat (DEHP)","µg/l",1.3,"niet van toepassing",1.3,"niet van toepassing",null,1,"PGS (12)"]
[189,"330-54-1","diuron","µg/l",0.2,1.8,0.2,1.8,null,0.2,"PS (13)"]
[190,"41318-75-6 (BDE-28)","gebromeerde difenylethers (K)","µg/l",null,0.14000000000000001,null,1.4E-2,"0.0085 (L)","rapportagegrens","PGS (5)"]
[191,"5436-43-1 (BDE-47)","gebromeerde difenylethers (K)","µg/l",null,0.14000000000000001,null,1.4E-2,"0.0085 (L)","rapportagegrens","PGS (5)"]
[192,"60348-60-9 (BDE-99)","gebromeerde difenylethers (K)","µg/l",null,0.14000000000000001,null,1.4E-2,"0.0085 (L)","rapportagegrens","PGS (5)"]
[193,"189084-64-8 (BDE-100)","gebromeerde difenylethers (K)","µg/l",null,0.14000000000000001,null,1.4E-2,"0.0085 (L)","rapportagegrens","PGS (5)"]
[194,"67774-32-7 (BDE-153)","gebromeerde difenylethers (K)","µg/l",null,0.14000000000000001,null,1.4E-2,"0.0085 (L)","rapportagegrens","PGS (5)"]
[195,"207122-15-4 (BDE-154)","gebromeerde difenylethers (K)","µg/l",null,0.14000000000000001,null,1.4E-2,"0.0085 (L)","rapportagegrens","PGS (5)"]
[195.5,"BDE totaal","gebromeerde difenylethers (K)","µg/l",null,0.14000000000000001,null,1.4E-2,"0.0085 (L)","rapportagegrens","PGS (5)"]
[196,"34123-59-6","isoproturon","µg/l",0.3,1,0.3,1,null,0.3,"PS (19)"]
[197,"1806-26-4","octylfenol","µg/l",0.1,"niet van toepassing",0.01,"niet van toepassing",null,0.1,"PS (25)"]
[198,"140-66-9","octylfenol","µg/l",0.1,"niet van toepassing",0.01,"niet van toepassing",null,0.1,"PS (25)"]
[198.5,null,"totaal octylfenol","µg/l",0.1,"niet van toepassing",0.01,"niet van toepassing",null,0.1,"PS (25)"]
[199,"608-93-5","pentachloorben-zeen","µg/l",7.0000000000000001E-3,"niet van toepassing",6.9999999999999999E-4,"niet van toepassing",null,7.0000000000000001E-3,"PGS (26)"]
[200,"83164-33-4","diflufenican","µg/l",0.03,0.05,0.03,0.05,null,0.03]
[201,"142459-58-3","flufenacet","µg/l",0.04,0.2,0.04,0.2,null,0.04]
[202,"80-05-7","Bisfenol A","µg/l",1.5,"niet van toepassing",1.5,"niet van toepassing",null,1.5]
[203,"5915-41-3","Terbutylazine","µg/l",0.32,1.8,0.32,1.8,null,0.3]
[204,"138261-41-3","Imidacloprid","µg/l",8.0000000000000002E-3,0.2,8.0000000000000002E-3,0.2,null,8.0000000000000002E-3]
[205,"87674-68-8","Dimethenamid","µg/l",1.5,6.7,1.5,6.7,null,1.5]
[206,"gevaarlijke stoffen: anorganische stoffen"]
[207,"7440-38-2","arseen","µg/l",3,"niet van toepassing",3,"niet van toepassing",null,5]
[208,"7440-43-9","cadmium (M)","µg/l",0.08,0.45,0.2,0.45,null,"0,8","PGS (6)"]
[218,"7439-97-6","kwik","µg/l",null,"0,07 ",null,"0,07 ","20 (N)","rapportagegrens","PGS (21)"]
[219,"7440-39-3","barium","µg/l",60,"niet van toepassing",60,"niet van toepassing",null,70]
[220,"7440-41-7","beryllium","µg/l","0,08 ","niet van toepassing","0,08 ","niet van toepassing",null,"0,1 "]
[221,"7440-42-8","boor","µg/l",700,"niet van toepassing",700,"niet van toepassing",null,700]
[222,"7440-47-3","chroom","µg/l",5,"niet van toepassing",5,"niet van toepassing",null,50]
[223,"7440-48-4","kobalt","µg/l","0,5 ","niet van toepassing","0,5 ","niet van toepassing",null,"0,6 "]
[224,"7440-50-8","koper","µg/l",7,"niet van toepassing",7,"niet van toepassing",null,50]
[225,"7439-92-1","lood","µg/l","1,2",14,"1,3 ",14,null,50,"PS (20)"]
[226,"7439-98-7","molybdeen","µg/l",340,"niet van toepassing",340,"niet van toepassing",null,350]
[227,"7440-02-0","nikkel","µg/l",4,34,"8,6 ",34,null,30,"PS (23)"]
[228,"7782-49-2","seleen","µg/l",2,"niet van toepassing",2,"niet van toepassing",null,3]
[229,"7440-28-0","thallium","µg/l","0,2 ","niet van toepassing","0,2 ","niet van toepassing",null,"0,2 "]
[230,"7440-31-5","tin","µg/l",3,"niet van toepassing",3,"niet van toepassing",null,40]
[231,"7440-61-1","uranium","µg/l",1,"niet van toepassing",1,"niet van toepassing",null,1]
[232,"7440-62-2","vanadium","µg/l",4,"niet van toepassing",4,"niet van toepassing",null,5]
[233,"7440-22-4","zilver","µg/l","0,08 ","niet van toepassing","0,08 ","niet van toepassing",null,"0,4 "]
[234,"7440-66-6","zink","µg/l",20,"niet van toepassing",20,"niet van toepassing",null,200]
[235,"7440-36-0","antimoon","µg/l",100,"niet van toepassing",100,"niet van toepassing",null,100]
[236,"13494-80-9","tellurium","µg/l",100,"niet van toepassing",100,"niet van toepassing",null,100]
[237,"7440-32-6","titanium","µg/l",20,"niet van toepassing",20,"niet van toepassing",null,100]
[238,null,"totaal fosfor","µg/l",140,"niet van toepassing",null,"niet van toepassing",null,1000]
[239,"7664-41-7","ammoniak","µg/l",30,100,30,100,null,"30 (P)"]
[240,"14797-65-0","nitriet","µg N/l",200,600,200,600,null,"200 (P)"]
[241,"57-12-5","totaal cyanide","µg/l",50,75,50,75,null,50]
[242,"16984-48-8","opgelost fluoride","µg/l",900,"niet van toepassing",900,"niet van toepassing",null,900]
[243,"gevaarlijke stoffen: groepsnormen"]
[244,null,"adsorbeerbare organische halogeenverbindingen (AOX)","µg/l",40,"niet van toepassing",40,"niet van toepassing",null,40]
[245,null,"anionische oppervlakteactieve stoffen","µg/l",100,"niet van toepassing",100,"niet van toepassing",null,100]
[246,null,"niet-ionogene en kationische oppervlakteactieve stoffen","µg/l",1000,"niet van toepassing",1000,"niet van toepassing",null,1000]

{"sheet":"BBT+ Criteria","index":18,"n_rows":23,"n_cols":4,"rows_kept":23,"cut":false,"hidden":true,"merged":[]}
["ENKEL VMM - aanpassing criteria (pas gele cellen aan)"]
[]
["Bijkomende kostprijs tov huidige WZ"]
[]
["Aanvaardbaard (… <)",0.5]
["Intermediair",0.5,1]
["Niet aanvaardbaar (> …)",1]
[]
[]
["Kostprijs (€/m³)"]
[null,"(info redelijkheid)",null,"(toetsing)"]
["Technologie","€/m³",null,"€/m³"]
[1,20,null,6]
[2,12,null,12]
[3,3]
[4,"te bekijken"]
[]
["Kengetallen BBT"]
[]
["Jaarlijkse kosten vs.","Betaalbaar (… <)","Intermediair","Niet betaalbaar (> …)"]
["Omzet",5.0000000000000001E-3,"0,5 – 5 %",0.05]
["Toegevoegde waarde",0.02,"2-50 %",0.5]
["Investering tov totale investering",0.1,"10-100 %",1]